Version: 1.5
*START 1
N Originating Program: RUSLE2
N Skel Format Version: 1.1
N This management file was originally converted from the NRCS standard XML format on - Thu Jun 21 09:32:39 PDT 2012
N This management file was updated to contain the most current crop and operation records for WEPS on - Tue Jun 26 16:03:28 PDT 2012
#------------
D 20/04/01
O 04 Sprayer, kill crop
+ 1.2160101 0.15
T All crop types are killed, green grow turned to residue, standing.  MAS 12-27-11
T
T Added Flattening to the operation to match R2 (P-24).  This will tend to increase erosion on systems that using
T cover crops by causing less standing residue from the crop or cover crop killed.  MAS 4-3-12
T
T After a conference call, Linda Scheffe, Dave Lightle, Mike Sporcic, and Fred Fox, we decided to change the flattening
T from 0.7-0.5 to 0.05 for all residue type due to wheel traffic only.  Plant canopy change over time is not considered.
T Normal plant senescence built into the model will handle plant changes.  MAS 4-5-12
+ 
G 02 Biomass Manipulation
+ 1.0
P 24 Flatten Standing Biomass
+ 0 0.05 0.05 0.05 0.05 0.05
P 31 Kill or Defoliate Growing Crop
+ 2
P 40 End crop Biomass Manipulation
#------------
D 22/05/01
O 04 Fert applic. surface broadcast
+ 1.4966278 0.0609375
T R2 Notes: Broadcast fertilizer spreader.  Wheel traffic only.  rev 082107 DTL
T
T Added to DB 4-12-12 MAS
+
G 01 Tillage
+ 0.0 0 0.05 0.0 0.0 0.0
P 01 Break Crust
P 02 Random Roughness
+ 1 8.8900175
P 11 Aggregate Crushing
+ 4.3 2.0
P 24 Flatten Standing Biomass
+ 0 0.25 0.2 0.15 0.1 1.0
P 26 Resurface Buried Biomass
+ 0.07 0.08 0.1 0.12 0.07
P 34 Change Standing Biomass Fall Rate
+ 0 1.0 1.0 1.0 1.0 1.0
+ 1.0 1.0 1.0 1.0 1.0
#------------
D 01/06/01
O 03 Planter, ridge till
+ 5.799433 10.56 2.2351363 0.0 2.2351363 1.5645955 2.9056773
T RUSLE:6/7/01 DTL  This is a planter on 30 in sp where 65% of the area is tilled with a 4 in ridge.  MAS 8/8/07
T G2 was added into file in front of the flattening (P24), burial (P25), and resurfacing (P26) factors because the area affected is less than 1.0 and
T the RUSLE values were normalized to 1.0.  This change will imulate the correct residue changes based on the method set forth in RUSLE.
T RUSLE's factors have been redused to based on the area affected.
T The stalk fall rate factor (P34) was moved ahead of the new (G2) factor to set the fall rate to the  less than 1.0 area affected.  8/8/07 MAS
+
G 01 Tillage
+ 63.500126 0.5 .65 63.500126 50.800102 101.600204
P 01 Break Crust
P 02 Random Roughness
+ 1 10.160021
P 05 Ridges and Dikes
+ 1 101.600204 762.0015 558.8011 0.0 0.0
P 11 Aggregate Crushing
+ 2.8 0.75
P 12 Soil Loosening
+ 0.75
P 13 Soil Layer Mixing
+ 0.35
P 34 Change Standing Biomass Fall Rate
+ 7 3.0 2.5 2.0 1.5 1.0
+ 0.5 0.6 0.7 0.8 1.0
G 02 Biomass Manipulation
+ 1.0
P 24 Flatten Standing Biomass
+ 0 .3 .25 .2 0.1 1.0
P 25 Bury Flat Biomass
+ 1 .15 .12 .09 .078 .114
P 26 Resurface Buried Biomass
+ .01 .01 .01 .02 .01
G 03 Crop Name
+ Sunflower
P 51 Seeding Configuration
+ 1 0.0 2
+ 5.0 1.0 1 1400 1.0 1.0 0
+ lb/ac
+ 10 8930.0 4 0.8 0.9 0.8
+ 2.5 0.025 2.0 6.0 25.0 0 115 1500.0
+ -5.0 -15.0 0.15 0.95 0.0 40.0
+ 0.023 0.8063 0.3146 -0.061 -0.024 0.9911 0.6435 0.0494
+ 0.3146 -0.061 0.13925274 0.68 17.3 0.05 0 0.8
+ 76.92308 76.92308 2.0 0.03 0.0 0.0 0.0 2
+ 0.025 0.025 0.025 0.025 0.15 0.02 20.0 1.97163
+ -0.604267 0.711259 1.8615 0.037413973 0.0 0.0 0.0 0.0
T Enter crop notes here.
#------------
D 25/06/01
O 03 Cultivator, row - 1st pass ridge till
+ 5.799433 17.55 2.2351363 0.0 1.7881091 1.5645955 2.9056773
T 8/4/06 MAS from RUSLE
T G2 was added into file in front of the flattening (P24), burial (P25), and resurfacing (P26) factors because the area affected is less than 1.0 and
T the RUSLE values were normalized to 1.0.  This change will imulate the correct residue changes based on the method set forth in RUSLE.
T RUSLE's factors have been redused to based on the area affected.
T The stalk fall rate factor (P34) was moved ahead of the new (G2) factor to set the fall rate to the less than 1.0 area affected.  8/8/07 MAS
+
G 01 Tillage
+ 63.50013 .75 0.85 63.500134 50.800102 101.600204
P 01 Break Crust
P 02 Random Roughness
+ 1 17.780035
P 05 Ridges and Dikes
+ 1 101.600204 762.0015 152.4003 0.0 0.0
P 11 Aggregate Crushing
+ 3.0 1.0
P 12 Soil Loosening
+ 0.75
P 13 Soil Layer Mixing
+ .6
P 34 Change Standing Biomass Fall Rate
+ 4 3.0 2.5 2.0 1.5 1.0
+ 0.5 0.6 0.7 0.8 1.0
G 02 Biomass Manipulation
+ 1.0
P 24 Flatten Standing Biomass
+ 14 0.8 .7 .7 0.1 1.0
P 25 Bury Flat Biomass
+ 1 .43 .34 .26 .22 .32
P 26 Resurface Buried Biomass
+ 0.04 0.045 .05 .22 0.04
#------------
D 15/07/01
O 03 Cultivator, row - 2nd pass ridge till
+ 6.921904 19.5 2.2351363 0.0 2.2351363 1.3410819 2.9056773
T Enter Operation notes here
+
G 01 Tillage
+ 76.20015 0.75 1.0 76.20015 50.800102 101.600204
P 01 Break Crust
P 02 Random Roughness
+ 1 17.780035
P 05 Ridges and Dikes
+ 1 152.4003 762.0015 152.4003 0.0 0.0
P 11 Aggregate Crushing
+ 3.0 1.0
P 12 Soil Loosening
+ 0.75
P 13 Soil Layer Mixing
+ 0.6
P 24 Flatten Standing Biomass
+ 14 0.8 0.7 0.7 0.2 1.0
P 25 Bury Flat Biomass
+ 1 0.8 0.75 0.7 0.2 0.5
P 26 Resurface Buried Biomass
+ 0.05 0.05 0.05 0.07 0.05
P 34 Change Standing Biomass Fall Rate
+ 4 3.0 2.5 2.0 1.5 1.0
+ 0.5 0.6 0.7 0.8 1.0
#------------
D 01/08/01
O 04 Sprayer, insecticide post emergence
+ 1.2160101 0.15
T Spray pest control chemicals on growing crop.   Crop is not killed.  11/17/01 DTL
T
T Added to the DB.  This assumes no crop flattening.  4-5-12 MAS
+
#------------
D 25/10/01
O 04 Harvest, killing crop 50pct standing stubble
+ 14.311503 .15
T ARS record - filename is:  Harvest Wheat - grain (combine cutterbar header).oprn
T This operation record is designed to represent actual field harvesting operation
T of removing the grain from small grain crops with a cutterbar head on a combine.
T This harvesting operation record removes all the reproductive component of a crop above the
T cutting height.  Typically this is specified as the "yield" component in the crop record.
T The non-harvested crop plant material above the specified cut height becomes flat residue.
T The remaining above ground crop material below the specified cut height becomes standing residue.
T Nov 02, 2005	Created - Larry Wagner
T Detailed info regarding this operation record:
T This harvest record specifies the actual cut height dependent upon the height
T of the crop.  The cut height is specified as a fraction of the crop height.
T Added 0.2 for the flatting of the combine and tire trafic for haulling grain.
T MAS 1-18-07
T The harvesting operation could also have an effect on the "standing stalk"
T fall rate and fall threshold values.  The default "biomass pool" flag parameter
T is set to "No adjustments applied" so that no "stalk residue decay rate change" will occur.
T However, this flag value can be changed along with the default parameter values
T to change the "stalk residue decay processes".
+
G 02 Biomass Manipulation
+ 1.0
P 31 Kill or Defoliate Growing Crop
+ 2
P 43 Cut/Remove Biomass by Fraction (flags)
+ 1 1 0 1 0.2 1 0 0
P 34 Change Standing Biomass Fall Rate
+ 0 1.0 1.0 1.0 1.0 1.0
+ 1.0 1.0 1.0 1.0 1.0
P 40 End crop Biomass Manipulation
P 24 Flatten Standing Biomass
+ 0 0.2 0.2 0.15 0.2 1
#------------
*END
*EOF
