Version: 1.5
*START 2
N Originating Program: RUSLE2
N Skel Format Version: 1.1
N This management file was originally converted from the NRCS standard XML format on - Thu Jun 21 09:32:48 PDT 2012
N This management file was updated to contain the most current crop and operation records for WEPS on - Tue Jun 26 16:02:37 PDT 2012
#------------
D 05/07/01
O 04 Burn residue, high intensity
+ 9.353924E-8 0
T Burn residue 100% of standing residue and 100% of flat residue 032207 DTL
T Added remove fruit percentage for removal of reproductive parts. MAS 9-10-08
T Changed report harvest to "no report" to better work with the crop yr interval MAS 7-26-11
+
G 02 Biomass Manipulation
+ 1
P 62 Remove (by age pool) Plant/Residue Material
+ 0 0 1 0 1 6 0 1 1 1 0 0
P 62 Remove (by age pool) Plant/Residue Material
+ 0 0 1 0 2 6 0 0.93 0.93 0.93 0 0
#------------
D 15/07/01
O 03 Chisel, st. pt
+ 9.353924 45.5 2.2351363 0.0 2.2351363 1.5645955 2.9056773
T Enter Operation notes here
+
G 01 Tillage
+ 177.80035 0.75 1.0 177.80035 101.600204 203.20041
P 01 Break Crust
P 02 Random Roughness
+ 1 38.100075
P 05 Ridges and Dikes
+ 1 76.20015 381.00076 101.600204 0.0 0.0
P 11 Aggregate Crushing
+ 2.4 -2.0
P 12 Soil Loosening
+ 0.85
P 13 Soil Layer Mixing
+ 0.37
P 31 Kill or Defoliate Growing Crop
+ 2
P 40 End crop Biomass Manipulation
P 24 Flatten Standing Biomass
+ 0 0.6 0.4 0.25 0.1 1.0
P 25 Bury Flat Biomass
+ 1 0.76 0.68 0.58 0.5 0.9
P 26 Resurface Buried Biomass
+ 0.05 0.06 0.07 0.2 0.05
P 34 Change Standing Biomass Fall Rate
+ 7 3.0 2.5 2.0 1.5 1.0
+ 0.5 0.6 0.7 0.8 1.0
#------------
D 15/08/01
O 03 Disk, tandem secondary op
+ 4.4898834 32.5 2.2351363 0.0 2.2351363 1.3410819 2.6821637
T 9-in. Spacing, Front and Rear; Good for seedbed preparation/chemical incorporation in medium to heavy soils
T Works well in primary tillage in light to medium soils
T Provides good residue-handling capability.  MAS 10-26-06
+
G 01 Tillage
+ 127.00027 0.75 1.0 127.00026 76.20015 152.4003
P 01 Break Crust
P 02 Random Roughness
+ 1 15.240031
P 05 Ridges and Dikes
+ 1 50.800102 228.60046 0.0 0.0 0.0
P 11 Aggregate Crushing
+ 2.8 0.75
P 12 Soil Loosening
+ 0.85
P 13 Soil Layer Mixing
+ 0.4
P 31 Kill or Defoliate Growing Crop
+ 2
P 40 End crop Biomass Manipulation
P 24 Flatten Standing Biomass
+ 0 0.85 0.7 0.6 0.5 1.0
P 25 Bury Flat Biomass
+ 1 0.73 0.63 0.55 0.4 0.73
P 26 Resurface Buried Biomass
+ 0.02 0.04 0.02 0.05 0.02
P 34 Change Standing Biomass Fall Rate
+ 7 3.0 2.5 2.0 1.5 1.0
+ 0.5 0.6 0.7 0.8 1.0
#------------
D 10/09/01
O 03 Cultivator, field 6-12 in sweeps
+ 6.921904 26 2.2351363 0.0 2.2351363 1.5645955 2.9056773
T Corrected Speed of operation numbers 11-1-11 MAS
+
G 01 Tillage
+ 101.600204 0.4 1.0 101.600204 50.800102 152.4003
P 01 Break Crust
P 02 Random Roughness
+ 1 15.240031
P 05 Ridges and Dikes
+ 1 50.800102 228.60045 0.0 0.0 0.0
P 11 Aggregate Crushing
+ 3.0 1.0
P 12 Soil Loosening
+ 0.65
P 13 Soil Layer Mixing
+ 0.3
P 31 Kill or Defoliate Growing Crop
+ 2
P 40 End crop Biomass Manipulation
P 24 Flatten Standing Biomass
+ 0 0.7 0.4 0.3 0.2 1.0
P 25 Bury Flat Biomass
+ 1 0.4 0.35 0.3 0.2 0.85
P 26 Resurface Buried Biomass
+ 0.05 0.06 0.07 0.2 0.05
P 34 Change Standing Biomass Fall Rate
+ 7 3.0 2.5 2.0 1.5 1.0
+ 0.5 0.6 0.7 0.8 1.0
#------------
D 15/09/01
O 03 Drill or airseeder, double disk
+ 3.3674128 6.34 2.2351363 0.0 2.2351363 1.5645955 2.9056773
T Drill or air seeder with double disk openers on 7 to 10 inch spacings.  Rev102403 DTL  RUSLE MAS 10-26-06
T G2 was added into file in front of the flattening (P24), burial (P25), and resurfacing (P26) factors because the area affected is less than 1.0 and
T the RUSLE values were normalized to 1.0.  This change will imulate the correct residue changes based on the method set forth in RUSLE.
T RUSLE's factors have been redused to based on the area affected.
T The stalk fall rate factor (P34) was moved ahead of the new (G2) factor to set the fall rate to the  less than 1.0 area affected.  8/8/07 MAS
T
T Deleted the G2 process because all process only affect 0.65 of the surface.  This is set a 0.65 with G1 process in the beginning. 5-11-11 MAS
+ 
G 01 Tillage
+ 38.100075 0.4 0.65 38.100075 25.400051 50.800102
P 01 Break Crust
P 02 Random Roughness
+ 1 7.6200156
P 05 Ridges and Dikes
+ 1 25.400051 203.20041 25.400051 0.0 0.0
P 11 Aggregate Crushing
+ 2.8 0.75
P 12 Soil Loosening
+ 0.6
P 13 Soil Layer Mixing
+ 0.3
P 34 Change Standing Biomass Fall Rate
+ 7 3.0 2.5 2.0 1.5 1.0
+ 0.5 0.6 0.7 0.8 1.0
P 24 Flatten Standing Biomass
+ 0 0.6 0.4 0.35 0.15 1.0
P 25 Bury Flat Biomass
+ 1 0.2275 0.1625 0.13 0.065 0.13
P 26 Resurface Buried Biomass
+ 0.01 0.01 0.01 0.02 0.01
G 03 Crop Name
+ Wheat, winter
P 51 Seeding Configuration
+ 1 0.0 0
+ 220.0 8.0 1 40.0 1.0 1.0 0
+ bu/ac
+ 10.9 148.833 5 0.8 0.6 0.8
+ 1.2 0.025 2.0 0.0 25.0 1 270 1333.3334
+ -5.0 -15.0 0.005 0.05 0.035 30.0
+ 0.013 0.8013 0.4293 -0.086 -0.018 0.932 0.556 0.0736
+ 0.3293 -0.086 2.87 1.0 20.0 0.05 0 0.3
+ 28.571428 335.0 1.4 0.012 0.1 0.1 0.0 2
+ 0.0133 0.0133 0.0133 0.0133 0.04 0.0050 17.1 5.227942
+ -2.08165 0.548606 1.4111 0.077708535 0.0 0.0 0.0 0.0
T Orginal record from ARS, wheat, winter.  Res to Grain ratio based on core 5/2/94 40 bu/ac yield incl. winter dormant period
T excl. NW Wheat & Range Region adj. dorm. for winter growth REV 61901 DTL
T
T Standing Fall rate reduced from 0.12 to 0.04 #/(# days) because
T WW-Chem fallow in SW KS showed too much standing residue was falling down.  Larry Wagner recommended we
T reduce fall rate. Dave L, Linda S., and I made runs to get the wt to match the standing stalk wt from Fred Fox stalk residue
T samples WERU Lab.  This rate left 24% of the starting count standing.  This is well within the range of values of two paper.
T Both paper showed about 46% left standing at the 440 day after harvest time.  David Nelson, ARS Akron, CO also confirmed
T that the orginal 8% standing was too low.  He thought that the 24% was much more resonable.  MAS 6-7-11
#------------
D 15/06/02
O 04 Harvest, killing crop 50pct standing stubble
+ 14.311503 .15
T ARS record - filename is:  Harvest Wheat - grain (combine cutterbar header).oprn
T This operation record is designed to represent actual field harvesting operation
T of removing the grain from small grain crops with a cutterbar head on a combine.
T This harvesting operation record removes all the reproductive component of a crop above the
T cutting height.  Typically this is specified as the "yield" component in the crop record.
T The non-harvested crop plant material above the specified cut height becomes flat residue.
T The remaining above ground crop material below the specified cut height becomes standing residue.
T Nov 02, 2005	Created - Larry Wagner
T Detailed info regarding this operation record:
T This harvest record specifies the actual cut height dependent upon the height
T of the crop.  The cut height is specified as a fraction of the crop height.
T Added 0.2 for the flatting of the combine and tire trafic for haulling grain.
T MAS 1-18-07
T The harvesting operation could also have an effect on the "standing stalk"
T fall rate and fall threshold values.  The default "biomass pool" flag parameter
T is set to "No adjustments applied" so that no "stalk residue decay rate change" will occur.
T However, this flag value can be changed along with the default parameter values
T to change the "stalk residue decay processes".
+
G 02 Biomass Manipulation
+ 1.0
P 31 Kill or Defoliate Growing Crop
+ 2
P 43 Cut/Remove Biomass by Fraction (flags)
+ 1 1 0 1 0.2 1 0 0
P 34 Change Standing Biomass Fall Rate
+ 0 1.0 1.0 1.0 1.0 1.0
+ 1.0 1.0 1.0 1.0 1.0
P 40 End crop Biomass Manipulation
P 24 Flatten Standing Biomass
+ 0 0.2 0.2 0.15 0.2 1
#------------
*END
*EOF
