Version: 1.5
*START 4
N Originating Program: RUSLE2
N Skel Format Version: 1.1
N This management file was originally converted from the NRCS standard XML format on - Thu Jun 21 11:15:47 PDT 2012
N This management file was updated to contain the most current crop and operation records for WEPS on - Tue Jun 26 15:41:25 PDT 2012
N This management file was updated to contain the most current crop and operation records for WEPS on - Tue Dec 17 19:24:30 CST 2013
#------------
D 22/03/01
O 03 Plow, moldboard
+ 17.491838 65 2.2351363 0.0 2.2351363 1.5645955 2.6821637
T Moldboard plow 8 inch operating depth.  060701 DTL  Modified flattening and burial per McCool and Foster 05/21/02 DTL RUSLE MAS 10-26-06
+
G 01 Tillage
+ 203.20041 1.0 1.0 203.20041 152.4003 254.0005
P 01 Break Crust
P 02 Random Roughness
+ 1 48.260098
P 05 Ridges and Dikes
+ 1 25.400051 406.40082 0.0 0.0 0.0
P 11 Aggregate Crushing
+ 2.8 1.0
P 12 Soil Loosening
+ 1.0
P 13 Soil Layer Mixing
+ 0.7
P 14 Soil Layer Inversion
P 31 Kill or Defoliate Growing Crop
+ 2
P 40 End crop Biomass Manipulation
P 24 Flatten Standing Biomass
+ 0 1 1 1 0.75 1.0
P 25 Bury Flat Biomass
+ 3 0.99 0.99 0.99 0.85 0.97
P 26 Resurface Buried Biomass
+ 0.01 0.02 0.04 0.1 0.02
P 34 Change Standing Biomass Fall Rate
+ 7 3.0 2.5 2.0 1.5 1.0
+ 0.5 0.6 0.7 0.8 1.0
#------------
D 25/04/01
O 03 Disk, tandem heavy primary op
+ 7.0154433 39 2.2351363 0.0 2.2351363 1.3410819 2.6821637
T 11-12in. Spacing, Front and Rear
T Recommended for primary tillage in medium to heavy soils
T Excellent residue-handling capability. MAS 10-26-06
+
G 01 Tillage
+ 152.4003 1.0 1.0 152.4003 101.600204 177.80035
P 01 Break Crust
P 02 Random Roughness
+ 1 38.100075
P 05 Ridges and Dikes
+ 1 101.600204 279.40057 0.0 0.0 0.0
P 11 Aggregate Crushing
+ 2.8 0.75
P 12 Soil Loosening
+ 0.9
P 13 Soil Layer Mixing
+ 0.4
P 31 Kill or Defoliate Growing Crop
+ 2
P 40 End crop Biomass Manipulation
P 24 Flatten Standing Biomass
+ 0 1.0 0.9 0.8 0.5 1.0
P 25 Bury Flat Biomass
+ 1 0.95 0.85 0.8 0.6 0.95
P 26 Resurface Buried Biomass
+ 0.05 0.06 0.07 0.08 0.05
P 34 Change Standing Biomass Fall Rate
+ 7 3.0 2.5 2.0 1.5 1.0
+ 0.5 0.6 0.7 0.8 1.0
#------------
D 27/04/01
O 04 Fert applic. surface broadcast
+ 1.4966278 0.0609375
T R2 Notes: Broadcast fertilizer spreader.  Wheel traffic only.  rev 082107 DTL
T
T Added to DB 4-12-12 MAS
+
G 01 Tillage
+ 0.0 0 0.05 0.0 0.0 0.0
P 01 Break Crust
P 02 Random Roughness
+ 1 8.8900175
P 11 Aggregate Crushing
+ 4.3 2.0
P 24 Flatten Standing Biomass
+ 0 0.25 0.2 0.15 0.1 1.0
P 26 Resurface Buried Biomass
+ 0.07 0.08 0.1 0.12 0.07
P 34 Change Standing Biomass Fall Rate
+ 0 1.0 1.0 1.0 1.0 1.0
+ 1.0 1.0 1.0 1.0 1.0
#------------
D 27/04/01
O 03 Disk, tandem secondary op
+ 4.4898834 32.5 2.2351363 0.0 2.2351363 1.3410819 2.6821637
T 9-in. Spacing, Front and Rear; Good for seedbed preparation/chemical incorporation in medium to heavy soils
T Works well in primary tillage in light to medium soils
T Provides good residue-handling capability.  MAS 10-26-06
+
G 01 Tillage
+ 127.00027 0.75 1.0 127.00026 76.20015 152.4003
P 01 Break Crust
P 02 Random Roughness
+ 1 15.240031
P 05 Ridges and Dikes
+ 1 50.800102 228.60046 0.0 0.0 0.0
P 11 Aggregate Crushing
+ 2.8 0.75
P 12 Soil Loosening
+ 0.85
P 13 Soil Layer Mixing
+ 0.4
P 31 Kill or Defoliate Growing Crop
+ 2
P 40 End crop Biomass Manipulation
P 24 Flatten Standing Biomass
+ 0 0.85 0.7 0.6 0.5 1.0
P 25 Bury Flat Biomass
+ 1 0.73 0.63 0.55 0.4 0.73
P 26 Resurface Buried Biomass
+ 0.02 0.04 0.02 0.05 0.02
P 34 Change Standing Biomass Fall Rate
+ 7 3.0 2.5 2.0 1.5 1.0
+ 0.5 0.6 0.7 0.8 1.0
#------------
D 30/04/01
O 03 Planter, double disk opnr
+ 4.1157265 2.4375 2.2351363 0.0 2.2351363 1.5645955 2.9056773
T This is a standard planter on 30 in sp with a 1 in ridge.  Created in RUSLE 6/7/01.  MAS 8/7/07
T G2 was added into file in front of the flattening (P24), burial (P25), and resurfacing (P26) factors because the area affected is less than 1.0 and
T the RUSLE values were normalized to 1.0.  This change will imulate the correct residue changes based on the method set forth in RUSLE.
T RUSLE's factors have been redused to based on the area affected.
T The stalk fall rate factor (P34) was moved ahead of the new (G2) factor to set the fall rate to the less than 1.0 area affected.  8/7/07 MAS
+
G 01 Tillage
+ 63.500126 0.5 .15 63.500126 50.800102 101.600204
P 01 Break Crust
P 02 Random Roughness
+ 1 10.160021
P 05 Ridges and Dikes
+ 1 50.800102 762.0015 635.0013 0.0 0.0
P 11 Aggregate Crushing
+ 2.8 0.75
P 12 Soil Loosening
+ 0.6
P 13 Soil Layer Mixing
+ 0.35
P 34 Change Standing Biomass Fall Rate
+ 7 3.0 2.5 2.0 1.5 1.0
+ 0.5 0.6 0.7 0.8 1.0
G 02 Biomass Manipulation
+ 1.0
P 24 Flatten Standing Biomass
+ 0 .3 .25 .2 0.1 1.0
P 25 Bury Flat Biomass
+ 1 .0525 0.0375 .03 .015 .03
P 26 Resurface Buried Biomass
+ .01 .01 .01 .02 .01
G 03 Crop Name
+ Corn, sweet
P 51 Seeding Configuration
+ 1 0.0 2
+ 6.4249883 3.0 1 14000 1.0 1.0 0
+ lbs/ac
+ 79 8930 4 0.95 0.65 0.8
+ 2.0 0.05 1.5240185 10.0 30.0 0 65 1000.0
+ -5.0 -15.0 0.15 0.95 0.0 35.0
+ 0.0031 0.9233 0.3266 -0.044 0.0 0.976 0.511 0.0287
+ 0.3266 -0.044 0.22259772 0.72 17.4 0.05 0 0.8
+ 250.0 250.0 3.0 0.03 0.0 0.0 0.0 3
+ 0.01 0.01 0.01 0.01 0.153 0.01 20.0 3.3722901
+ -1.20379 0.604887 .4192 0.038108904 0.0 0.0 0.0 0.0
T Rusle note: 4/21/03 gaw. High production, related to one or more of the following - irrigation, high fertility, favorable climate,
T productive soils and varieties. Type locations:  CA, CO, FL, GA, OR, WA.
T Adjusted days to mature to 65 based on NY data.  MAS 3-5-07
#------------
D 15/05/01
O 03 Cultivator, row 1 in ridge
+ 5.799433 14.63 2.2351363 0.0 2.2351363 0.89405453 2.4586499
T RUSLE:Row crop cultivator w/ sweeps leaving a 1" ridge 05-14-02 DTL
T G2 was added into file in front of the flattening (P24), burial (P25), and resurfacing (P26) factors because the area affected is less than 1.0 and
T the RUSLE values were normalized to 1.0.  This change will imulate the correct residue changes based on the method set forth in RUSLE.
T RUSLE's factors have been redused to based on the area affected.
T The stalk fall rate factor (P34) was moved ahead of the new (G2) factor to set the fall rate to the less than 1.0 area affected.  8/8/07 MAS
+
G 01 Tillage
+ 76.20015 0.5 .75 76.20015 50.800102 101.600204
P 01 Break Crust
P 02 Random Roughness
+ 1 7.6200156
P 05 Ridges and Dikes
+ 1 25.400051 762.0015 0.0 0.0 0.0
P 11 Aggregate Crushing
+ 3.0 1.0
P 12 Soil Loosening
+ 0.75
P 13 Soil Layer Mixing
+ 0.35
P 34 Change Standing Biomass Fall Rate
+ 4 3.0 2.5 2.0 1.5 1.0
+ 0.5 0.6 0.7 0.8 1.0
G 02 Biomass Manipulation
+ 1.0
P 24 Flatten Standing Biomass
+ 14 0.7 0.3 0.3 0.1 1.0
P 25 Bury Flat Biomass
+ 1 .57 0.5 0.44 0.32 0.64
P 26 Resurface Buried Biomass
+ 0.01 0.01 0.01 0.01 0.01
#------------
D 29/05/01
O 03 Cultivator, row 1 in ridge
+ 5.799433 14.63 2.2351363 0.0 2.2351363 0.89405453 2.4586499
T RUSLE:Row crop cultivator w/ sweeps leaving a 1" ridge 05-14-02 DTL
T G2 was added into file in front of the flattening (P24), burial (P25), and resurfacing (P26) factors because the area affected is less than 1.0 and
T the RUSLE values were normalized to 1.0.  This change will imulate the correct residue changes based on the method set forth in RUSLE.
T RUSLE's factors have been redused to based on the area affected.
T The stalk fall rate factor (P34) was moved ahead of the new (G2) factor to set the fall rate to the less than 1.0 area affected.  8/8/07 MAS
+
G 01 Tillage
+ 76.20015 0.5 .75 76.20015 50.800102 101.600204
P 01 Break Crust
P 02 Random Roughness
+ 1 7.6200156
P 05 Ridges and Dikes
+ 1 25.400051 762.0015 0.0 0.0 0.0
P 11 Aggregate Crushing
+ 3.0 1.0
P 12 Soil Loosening
+ 0.75
P 13 Soil Layer Mixing
+ 0.35
P 34 Change Standing Biomass Fall Rate
+ 4 3.0 2.5 2.0 1.5 1.0
+ 0.5 0.6 0.7 0.8 1.0
G 02 Biomass Manipulation
+ 1.0
P 24 Flatten Standing Biomass
+ 14 0.7 0.3 0.3 0.1 1.0
P 25 Bury Flat Biomass
+ 1 .57 0.5 0.44 0.32 0.64
P 26 Resurface Buried Biomass
+ 0.01 0.01 0.01 0.01 0.01
#------------
D 11/07/01
O 04 Harvest, stripper header
+ 14.311503 .15
T Represents a combine or picker with a snapper header.  Ears and husks are snapped from stalks
T as they pass between snapping rolls.  Ears complete with kernels, cob and husks are harvested and removed
T from the field leaving only the stem and leaf residues. Rev 021109 DTL
+
G 02 Biomass Manipulation
+ 1.0
P 31 Kill or Defoliate Growing Crop
+ 2
P 62 Remove (by age pool) Plant/Residue Material
+ 1 1 0 1 1 3 0 1.0 0.0 0.0 0.0 0.0
P 34 Change Standing Biomass Fall Rate
+ 3 2.5 2.0 1.5 1.25 1.0
+ 0.6 0.7 0.8 0.9 1.0
P 40 End crop Biomass Manipulation
P 24 Flatten Standing Biomass
+ 0 0.2 .2 .2 0.5 1.0
#------------
D 26/09/01
O 03 Disk, tandem heavy primary op
+ 7.0154433 39 2.2351363 0.0 2.2351363 1.3410819 2.6821637
T 11-12in. Spacing, Front and Rear
T Recommended for primary tillage in medium to heavy soils
T Excellent residue-handling capability. MAS 10-26-06
+
G 01 Tillage
+ 152.4003 1.0 1.0 152.4003 101.600204 177.80035
P 01 Break Crust
P 02 Random Roughness
+ 1 38.100075
P 05 Ridges and Dikes
+ 1 101.600204 279.40057 0.0 0.0 0.0
P 11 Aggregate Crushing
+ 2.8 0.75
P 12 Soil Loosening
+ 0.9
P 13 Soil Layer Mixing
+ 0.4
P 31 Kill or Defoliate Growing Crop
+ 2
P 40 End crop Biomass Manipulation
P 24 Flatten Standing Biomass
+ 0 1.0 0.9 0.8 0.5 1.0
P 25 Bury Flat Biomass
+ 1 0.95 0.85 0.8 0.6 0.95
P 26 Resurface Buried Biomass
+ 0.05 0.06 0.07 0.08 0.05
P 34 Change Standing Biomass Fall Rate
+ 7 3.0 2.5 2.0 1.5 1.0
+ 0.5 0.6 0.7 0.8 1.0
#------------
D 15/10/01
O 04 Fert applic. surface broadcast
+ 1.4966278 0.0609375
T R2 Notes: Broadcast fertilizer spreader.  Wheel traffic only.  rev 082107 DTL
T
T Added to DB 4-12-12 MAS
+
G 01 Tillage
+ 0.0 0 0.05 0.0 0.0 0.0
P 01 Break Crust
P 02 Random Roughness
+ 1 8.8900175
P 11 Aggregate Crushing
+ 4.3 2.0
P 24 Flatten Standing Biomass
+ 0 0.25 0.2 0.15 0.1 1.0
P 26 Resurface Buried Biomass
+ 0.07 0.08 0.1 0.12 0.07
P 34 Change Standing Biomass Fall Rate
+ 0 1.0 1.0 1.0 1.0 1.0
+ 1.0 1.0 1.0 1.0 1.0
#------------
D 15/10/01
O 03 Disk, tandem secondary op
+ 4.4898834 32.5 2.2351363 0.0 2.2351363 1.3410819 2.6821637
T 9-in. Spacing, Front and Rear; Good for seedbed preparation/chemical incorporation in medium to heavy soils
T Works well in primary tillage in light to medium soils
T Provides good residue-handling capability.  MAS 10-26-06
+
G 01 Tillage
+ 127.00027 0.75 1.0 127.00026 76.20015 152.4003
P 01 Break Crust
P 02 Random Roughness
+ 1 15.240031
P 05 Ridges and Dikes
+ 1 50.800102 228.60046 0.0 0.0 0.0
P 11 Aggregate Crushing
+ 2.8 0.75
P 12 Soil Loosening
+ 0.85
P 13 Soil Layer Mixing
+ 0.4
P 31 Kill or Defoliate Growing Crop
+ 2
P 40 End crop Biomass Manipulation
P 24 Flatten Standing Biomass
+ 0 0.85 0.7 0.6 0.5 1.0
P 25 Bury Flat Biomass
+ 1 0.73 0.63 0.55 0.4 0.73
P 26 Resurface Buried Biomass
+ 0.02 0.04 0.02 0.05 0.02
P 34 Change Standing Biomass Fall Rate
+ 7 3.0 2.5 2.0 1.5 1.0
+ 0.5 0.6 0.7 0.8 1.0
#------------
D 16/10/01
O 03 Drill or air seeder single disk openers 7-10 in spac
+ 3.2738733 2.44 2.2351363 0.0 2.2351363 1.5645955 2.9056773
T Drill or Air seeder with single disk no-till openers  JD 750 or similar openers. (No-till air drill)
T Based on Drill, no-till single disk 7-10 spacing. 102403 DTL. RUSLE MAS 10-26-06
T G2 was added into file in front of the flattening (P24), burial (P25), and resurfacing (P26) factors because the area affected is less than 1.0 and
T the RUSLE values were normalized to 1.0.  This change will imulate the correct residue changes based on the method set forth in RUSLE.
T RUSLE's factors have been redused to based on the area affected.
T The stalk fall rate factor (P34) was moved ahead of the new (G2) factor to set the fall rate to the less than 1.0 area affected.  8/7/07 MAS
+
G 01 Tillage
+ 63.500134 0.4 0.15 63.50013 50.800102 101.600204
P 01 Break Crust
P 02 Random Roughness
+ 1 7.6200156
P 05 Ridges and Dikes
+ 1 25.400051 203.20041 0.0 0.0 0.0
P 11 Aggregate Crushing
+ 2.8 0.75
P 12 Soil Loosening
+ 0.4
P 13 Soil Layer Mixing
+ 0.20
P 34 Change Standing Biomass Fall Rate
+ 7 3.0 2.5 2.0 1.5 1.0
+ 0.5 0.6 0.7 0.8 1.0
G 02 Biomass Manipulation
+ 1.0
P 24 Flatten Standing Biomass
+ 0 0.6 0.4 0.35 0.15 1.0
P 25 Bury Flat Biomass
+ 1 0.05 0.04 0.03 0.02 0.03
P 26 Resurface Buried Biomass
+ 0.01 0.01 0.01 0.05 0.01
G 03 Crop Name
+ Barley, winter
P 51 Seeding Configuration
+ 1 0.0 0
+ 173.0 8.0 1 50.0 1.0 1.0 0
+ bu/ac
+ 9.6 186.0 5 0.8 0.64 0.8
+ 1.0 0.025 2.0 4.0 25.0 1 270 1333.3334
+ -5.0 -15.0 0.005 0.05 0.02 30.0
+ 0.013 0.6013 0.4293 -0.086 -0.018 0.932 0.556 0.0736
+ 0.4293 -0.086 2.5 1.0 25.0 0.05 0 0.3
+ 33.333332 385.0 1.4 0.012 0.1 0.1 0.0 2
+ 0.015 0.015 0.015 0.015 0.18 0.0050 17.1 5.183335
+ -2.08165 0.548606 1.3792 0.058508374 0.0 0.0 0.0 0.0
T Adjusted the Heat Units from the 3150 down to 2400 (same as WW)
T Tested in Delaware with John Timmons run.  8-18-09  MAS
#------------
D 18/06/02
O 04 Harvest, killing crop 50pct standing stubble
+ 14.311503 .15
T ARS record - filename is:  Harvest Wheat - grain (combine cutterbar header).oprn
T This operation record is designed to represent actual field harvesting operation
T of removing the grain from small grain crops with a cutterbar head on a combine.
T This harvesting operation record removes all the reproductive component of a crop above the
T cutting height.  Typically this is specified as the "yield" component in the crop record.
T The non-harvested crop plant material above the specified cut height becomes flat residue.
T The remaining above ground crop material below the specified cut height becomes standing residue.
T Nov 02, 2005	Created - Larry Wagner
T Detailed info regarding this operation record:
T This harvest record specifies the actual cut height dependent upon the height
T of the crop.  The cut height is specified as a fraction of the crop height.
T Added 0.2 for the flatting of the combine and tire trafic for haulling grain.
T MAS 1-18-07
T The harvesting operation could also have an effect on the "standing stalk"
T fall rate and fall threshold values.  The default "biomass pool" flag parameter
T is set to "No adjustments applied" so that no "stalk residue decay rate change" will occur.
T However, this flag value can be changed along with the default parameter values
T to change the "stalk residue decay processes".
+
G 02 Biomass Manipulation
+ 1.0
P 31 Kill or Defoliate Growing Crop
+ 2
P 43 Cut/Remove Biomass by Fraction (flags)
+ 1 1 0 1 0.2 1 0 0
P 34 Change Standing Biomass Fall Rate
+ 0 1.0 1.0 1.0 1.0 1.0
+ 1.0 1.0 1.0 1.0 1.0
P 40 End crop Biomass Manipulation
P 24 Flatten Standing Biomass
+ 0 0.2 0.2 0.15 0.2 1
#------------
D 01/08/02
O 03 Plow, moldboard
+ 17.491838 65 2.2351363 0.0 2.2351363 1.5645955 2.6821637
T Moldboard plow 8 inch operating depth.  060701 DTL  Modified flattening and burial per McCool and Foster 05/21/02 DTL RUSLE MAS 10-26-06
+
G 01 Tillage
+ 203.20041 1.0 1.0 203.20041 152.4003 254.0005
P 01 Break Crust
P 02 Random Roughness
+ 1 48.260098
P 05 Ridges and Dikes
+ 1 25.400051 406.40082 0.0 0.0 0.0
P 11 Aggregate Crushing
+ 2.8 1.0
P 12 Soil Loosening
+ 1.0
P 13 Soil Layer Mixing
+ 0.7
P 14 Soil Layer Inversion
P 31 Kill or Defoliate Growing Crop
+ 2
P 40 End crop Biomass Manipulation
P 24 Flatten Standing Biomass
+ 0 1 1 1 0.75 1.0
P 25 Bury Flat Biomass
+ 3 0.99 0.99 0.99 0.85 0.97
P 26 Resurface Buried Biomass
+ 0.01 0.02 0.04 0.1 0.02
P 34 Change Standing Biomass Fall Rate
+ 7 3.0 2.5 2.0 1.5 1.0
+ 0.5 0.6 0.7 0.8 1.0
#------------
D 10/08/02
O 03 Disk, tandem heavy primary op
+ 7.0154433 39 2.2351363 0.0 2.2351363 1.3410819 2.6821637
T 11-12in. Spacing, Front and Rear
T Recommended for primary tillage in medium to heavy soils
T Excellent residue-handling capability. MAS 10-26-06
+
G 01 Tillage
+ 152.4003 1.0 1.0 152.4003 101.600204 177.80035
P 01 Break Crust
P 02 Random Roughness
+ 1 38.100075
P 05 Ridges and Dikes
+ 1 101.600204 279.40057 0.0 0.0 0.0
P 11 Aggregate Crushing
+ 2.8 0.75
P 12 Soil Loosening
+ 0.9
P 13 Soil Layer Mixing
+ 0.4
P 31 Kill or Defoliate Growing Crop
+ 2
P 40 End crop Biomass Manipulation
P 24 Flatten Standing Biomass
+ 0 1.0 0.9 0.8 0.5 1.0
P 25 Bury Flat Biomass
+ 1 0.95 0.85 0.8 0.6 0.95
P 26 Resurface Buried Biomass
+ 0.05 0.06 0.07 0.08 0.05
P 34 Change Standing Biomass Fall Rate
+ 7 3.0 2.5 2.0 1.5 1.0
+ 0.5 0.6 0.7 0.8 1.0
#------------
D 12/08/02
O 04 Fert applic. surface broadcast
+ 1.4966278 0.0609375
T R2 Notes: Broadcast fertilizer spreader.  Wheel traffic only.  rev 082107 DTL
T
T Added to DB 4-12-12 MAS
+
G 01 Tillage
+ 0.0 0 0.05 0.0 0.0 0.0
P 01 Break Crust
P 02 Random Roughness
+ 1 8.8900175
P 11 Aggregate Crushing
+ 4.3 2.0
P 24 Flatten Standing Biomass
+ 0 0.25 0.2 0.15 0.1 1.0
P 26 Resurface Buried Biomass
+ 0.07 0.08 0.1 0.12 0.07
P 34 Change Standing Biomass Fall Rate
+ 0 1.0 1.0 1.0 1.0 1.0
+ 1.0 1.0 1.0 1.0 1.0
#------------
D 12/08/02
O 03 Disk, tandem light finishing
+ 3.7415698 19.5 2.2351363 0.0 2.2351363 1.3410819 2.6821637
T 6/8/01 DTL RUSLE.  7in sp.  This is tool used to finish a seedbed.  MAS 10-26-06
+
G 01 Tillage
+ 101.600204 0.5 1.0 101.600204 76.20015 127.00026
P 01 Break Crust
P 02 Random Roughness
+ 1 15.240031
P 05 Ridges and Dikes
+ 1 12.700026 177.80035 0.0 0.0 0.0
P 11 Aggregate Crushing
+ 2.8 0.75
P 12 Soil Loosening
+ 0.75
P 13 Soil Layer Mixing
+ 0.35
P 31 Kill or Defoliate Growing Crop
+ 2
P 40 End crop Biomass Manipulation
P 24 Flatten Standing Biomass
+ 0 0.85 0.7 0.6 0.5 1.0
P 25 Bury Flat Biomass
+ 1 0.73 0.63 0.55 0.4 0.73
P 26 Resurface Buried Biomass
+ 0.02 0.04 0.02 0.05 0.02
P 34 Change Standing Biomass Fall Rate
+ 7 3.0 2.5 2.0 1.5 1.0
+ 0.5 0.6 0.7 0.8 1.0
#------------
D 15/08/02
O 03 Drill or airseeder, double disk
+ 3.3674128 6.34 2.2351363 0.0 2.2351363 1.5645955 2.9056773
T Drill or air seeder with double disk openers on 7 to 10 inch spacings.  Rev102403 DTL  RUSLE MAS 10-26-06
T G2 was added into file in front of the flattening (P24), burial (P25), and resurfacing (P26) factors because the area affected is less than 1.0 and
T the RUSLE values were normalized to 1.0.  This change will imulate the correct residue changes based on the method set forth in RUSLE.
T RUSLE's factors have been redused to based on the area affected.
T The stalk fall rate factor (P34) was moved ahead of the new (G2) factor to set the fall rate to the  less than 1.0 area affected.  8/8/07 MAS
T
T Deleted the G2 process because all process only affect 0.65 of the surface.  This is set a 0.65 with G1 process in the beginning. 5-11-11 MAS
+ 
G 01 Tillage
+ 38.100075 0.4 0.65 38.100075 25.400051 50.800102
P 01 Break Crust
P 02 Random Roughness
+ 1 7.6200156
P 05 Ridges and Dikes
+ 1 25.400051 203.20041 25.400051 0.0 0.0
P 11 Aggregate Crushing
+ 2.8 0.75
P 12 Soil Loosening
+ 0.6
P 13 Soil Layer Mixing
+ 0.3
P 34 Change Standing Biomass Fall Rate
+ 7 3.0 2.5 2.0 1.5 1.0
+ 0.5 0.6 0.7 0.8 1.0
P 24 Flatten Standing Biomass
+ 0 0.6 0.4 0.35 0.15 1.0
P 25 Bury Flat Biomass
+ 1 0.2275 0.1625 0.13 0.065 0.13
P 26 Resurface Buried Biomass
+ 0.01 0.01 0.01 0.02 0.01
G 03 Crop Name
+ Spinach
P 51 Seeding Configuration
+ 1 0.0 0
+ 38 1 0 17500 1 1 2
+ lbs/ac
+ 92 8930 4 1 0.65 0.95
+ 0.2 0.01 0.8 0 18.199999999999996 1 55 1388.8889
+ -5 -15 0.01 0.95 0 35
+ 0.3128 0.576 0.6898 -0.1533 0 1 1.1 0.01
+ 0.4995 -0.0944 1.2 1 30 0.05 0 0.2562663
+ 10.10101 10.10101 1.5 0.015 0.1 0.1 0 1
+ 0.02 0.02 0.02 0.02 0.2 0.0050 20 5.227942
+ -1.20379 0.604887 0 0 0 0.0 0.0 0.0
T Squash.   High production, related to one or more of the following - irrigation, high fertility, favorable climate, productive soils and varieties.
T Type locations: CA, FL, GA, NY, OR.
T
T Adjusted the heat units from 5000 to 2500 and the Biomass eff from 19 to 35 to make growth needed for
T Suessex Co. DE.  Certified Crop 12-19-08 MAS
#------------
D 22/10/02
O 04 Harvest, leafy veg
+ 3.2738733 .15
T Harvest greens with no regrowth. Use to harvest crops like    Spinach, kale, chard, beet greens 12-10-01 DTL
T Crops are not killed to allow winter annuals like spinach to regrow through the winter months.  MAS 8-13-07
+
G 02 Biomass Manipulation
+ 1.0
P 31 Kill or Defoliate Growing Crop
+ 0
P 62 Remove (by age pool) Plant/Residue Material
+ 1 1 0 0 1 3 0 1.0 1.0 0.0 0.0 0.0
P 34 Change Standing Biomass Fall Rate
+ 3 1.0 1.0 1.0 1.0 1.0
+ 1.0 1.0 1.0 1.0 1.0
P 40 End crop Biomass Manipulation
P 24 Flatten Standing Biomass
+ 0 0.0 0.0 0.0 0.0 0.0
#------------
D 20/05/03
O 04 Harvest, leafy veg
+ 3.2738733 .15
T Harvest greens with no regrowth. Use to harvest crops like    Spinach, kale, chard, beet greens 12-10-01 DTL
T Crops are not killed to allow winter annuals like spinach to regrow through the winter months.  MAS 8-13-07
+
G 02 Biomass Manipulation
+ 1.0
P 31 Kill or Defoliate Growing Crop
+ 0
P 62 Remove (by age pool) Plant/Residue Material
+ 1 1 0 0 1 3 0 1.0 1.0 0.0 0.0 0.0
P 34 Change Standing Biomass Fall Rate
+ 3 1.0 1.0 1.0 1.0 1.0
+ 1.0 1.0 1.0 1.0 1.0
P 40 End crop Biomass Manipulation
P 24 Flatten Standing Biomass
+ 0 0.0 0.0 0.0 0.0 0.0
#------------
D 16/06/03
O 04 Harvest, leafy veg
+ 3.2738733 .15
T Harvest greens with no regrowth. Use to harvest crops like    Spinach, kale, chard, beet greens 12-10-01 DTL
T Crops are not killed to allow winter annuals like spinach to regrow through the winter months.  MAS 8-13-07
+
G 02 Biomass Manipulation
+ 1.0
P 31 Kill or Defoliate Growing Crop
+ 0
P 62 Remove (by age pool) Plant/Residue Material
+ 1 1 0 0 1 3 0 1.0 1.0 0.0 0.0 0.0
P 34 Change Standing Biomass Fall Rate
+ 3 1.0 1.0 1.0 1.0 1.0
+ 1.0 1.0 1.0 1.0 1.0
P 40 End crop Biomass Manipulation
P 24 Flatten Standing Biomass
+ 0 0.0 0.0 0.0 0.0 0.0
#------------
D 17/06/03
O 03 Plow, moldboard
+ 17.491838 65 2.2351363 0.0 2.2351363 1.5645955 2.6821637
T Moldboard plow 8 inch operating depth.  060701 DTL  Modified flattening and burial per McCool and Foster 05/21/02 DTL RUSLE MAS 10-26-06
+
G 01 Tillage
+ 203.20041 1.0 1.0 203.20041 152.4003 254.0005
P 01 Break Crust
P 02 Random Roughness
+ 1 48.260098
P 05 Ridges and Dikes
+ 1 25.400051 406.40082 0.0 0.0 0.0
P 11 Aggregate Crushing
+ 2.8 1.0
P 12 Soil Loosening
+ 1.0
P 13 Soil Layer Mixing
+ 0.7
P 14 Soil Layer Inversion
P 31 Kill or Defoliate Growing Crop
+ 2
P 40 End crop Biomass Manipulation
P 24 Flatten Standing Biomass
+ 0 1 1 1 0.75 1.0
P 25 Bury Flat Biomass
+ 3 0.99 0.99 0.99 0.85 0.97
P 26 Resurface Buried Biomass
+ 0.01 0.02 0.04 0.1 0.02
P 34 Change Standing Biomass Fall Rate
+ 7 3.0 2.5 2.0 1.5 1.0
+ 0.5 0.6 0.7 0.8 1.0
#------------
D 18/06/03
O 03 Disk, tandem heavy primary op
+ 7.0154433 39 2.2351363 0.0 2.2351363 1.3410819 2.6821637
T 11-12in. Spacing, Front and Rear
T Recommended for primary tillage in medium to heavy soils
T Excellent residue-handling capability. MAS 10-26-06
+
G 01 Tillage
+ 152.4003 1.0 1.0 152.4003 101.600204 177.80035
P 01 Break Crust
P 02 Random Roughness
+ 1 38.100075
P 05 Ridges and Dikes
+ 1 101.600204 279.40057 0.0 0.0 0.0
P 11 Aggregate Crushing
+ 2.8 0.75
P 12 Soil Loosening
+ 0.9
P 13 Soil Layer Mixing
+ 0.4
P 31 Kill or Defoliate Growing Crop
+ 2
P 40 End crop Biomass Manipulation
P 24 Flatten Standing Biomass
+ 0 1.0 0.9 0.8 0.5 1.0
P 25 Bury Flat Biomass
+ 1 0.95 0.85 0.8 0.6 0.95
P 26 Resurface Buried Biomass
+ 0.05 0.06 0.07 0.08 0.05
P 34 Change Standing Biomass Fall Rate
+ 7 3.0 2.5 2.0 1.5 1.0
+ 0.5 0.6 0.7 0.8 1.0
#------------
D 19/06/03
O 04 Fert applic. surface broadcast
+ 1.4966278 0.0609375
T R2 Notes: Broadcast fertilizer spreader.  Wheel traffic only.  rev 082107 DTL
T
T Added to DB 4-12-12 MAS
+
G 01 Tillage
+ 0.0 0 0.05 0.0 0.0 0.0
P 01 Break Crust
P 02 Random Roughness
+ 1 8.8900175
P 11 Aggregate Crushing
+ 4.3 2.0
P 24 Flatten Standing Biomass
+ 0 0.25 0.2 0.15 0.1 1.0
P 26 Resurface Buried Biomass
+ 0.07 0.08 0.1 0.12 0.07
P 34 Change Standing Biomass Fall Rate
+ 0 1.0 1.0 1.0 1.0 1.0
+ 1.0 1.0 1.0 1.0 1.0
#------------
D 19/06/03
O 03 Disk, tandem light finishing
+ 3.7415698 19.5 2.2351363 0.0 2.2351363 1.3410819 2.6821637
T 6/8/01 DTL RUSLE.  7in sp.  This is tool used to finish a seedbed.  MAS 10-26-06
+
G 01 Tillage
+ 101.600204 0.5 1.0 101.600204 76.20015 127.00026
P 01 Break Crust
P 02 Random Roughness
+ 1 15.240031
P 05 Ridges and Dikes
+ 1 12.700026 177.80035 0.0 0.0 0.0
P 11 Aggregate Crushing
+ 2.8 0.75
P 12 Soil Loosening
+ 0.75
P 13 Soil Layer Mixing
+ 0.35
P 31 Kill or Defoliate Growing Crop
+ 2
P 40 End crop Biomass Manipulation
P 24 Flatten Standing Biomass
+ 0 0.85 0.7 0.6 0.5 1.0
P 25 Bury Flat Biomass
+ 1 0.73 0.63 0.55 0.4 0.73
P 26 Resurface Buried Biomass
+ 0.02 0.04 0.02 0.05 0.02
P 34 Change Standing Biomass Fall Rate
+ 7 3.0 2.5 2.0 1.5 1.0
+ 0.5 0.6 0.7 0.8 1.0
#------------
D 19/06/03
O 03 Planter, double disk opnr
+ 4.1157265 2.4375 2.2351363 0.0 2.2351363 1.5645955 2.9056773
T This is a standard planter on 30 in sp with a 1 in ridge.  Created in RUSLE 6/7/01.  MAS 8/7/07
T G2 was added into file in front of the flattening (P24), burial (P25), and resurfacing (P26) factors because the area affected is less than 1.0 and
T the RUSLE values were normalized to 1.0.  This change will imulate the correct residue changes based on the method set forth in RUSLE.
T RUSLE's factors have been redused to based on the area affected.
T The stalk fall rate factor (P34) was moved ahead of the new (G2) factor to set the fall rate to the less than 1.0 area affected.  8/7/07 MAS
+
G 01 Tillage
+ 63.500126 0.5 .15 63.500126 50.800102 101.600204
P 01 Break Crust
P 02 Random Roughness
+ 1 10.160021
P 05 Ridges and Dikes
+ 1 50.800102 762.0015 635.0013 0.0 0.0
P 11 Aggregate Crushing
+ 2.8 0.75
P 12 Soil Loosening
+ 0.6
P 13 Soil Layer Mixing
+ 0.35
P 34 Change Standing Biomass Fall Rate
+ 7 3.0 2.5 2.0 1.5 1.0
+ 0.5 0.6 0.7 0.8 1.0
G 02 Biomass Manipulation
+ 1.0
P 24 Flatten Standing Biomass
+ 0 .3 .25 .2 0.1 1.0
P 25 Bury Flat Biomass
+ 1 .0525 0.0375 .03 .015 .03
P 26 Resurface Buried Biomass
+ .01 .01 .01 .02 .01
G 03 Crop Name
+ Bean, green snap mech harv
P 51 Seeding Configuration
+ 1 0.0 2
+ 25.0 1.0 1 8100 1.0 1.0 0
+ lb/ac
+ 90 8930.0 1 1.0 0.8 0.95
+ 0.6 0.025 0.91441107 10.0 25.0 0 65 900.0
+ -5.0 -15.0 0.1 0.95 0.0 25.0
+ -0.017 0.738 0.4148 -0.082 0.0040 0.9357 0.4993 0.053
+ 0.4148 -0.082 3.3 1.0 33.0 0.05 0 0.3159463
+ 250.0 250.0 2.0 0.03 0.0 0.0 0.0 1
+ 0.02 0.02 0.02 0.02 0.2 0.0050 20.0 5.227942
+ -1.20379 0.604887 .2741 0.023537852 0.0 0.0 0.0 0.0
T Enter crop notes here.
#------------
D 10/07/03
O 03 Cultivator, row 1 in ridge
+ 5.799433 14.63 2.2351363 0.0 2.2351363 0.89405453 2.4586499
T RUSLE:Row crop cultivator w/ sweeps leaving a 1" ridge 05-14-02 DTL
T G2 was added into file in front of the flattening (P24), burial (P25), and resurfacing (P26) factors because the area affected is less than 1.0 and
T the RUSLE values were normalized to 1.0.  This change will imulate the correct residue changes based on the method set forth in RUSLE.
T RUSLE's factors have been redused to based on the area affected.
T The stalk fall rate factor (P34) was moved ahead of the new (G2) factor to set the fall rate to the less than 1.0 area affected.  8/8/07 MAS
+
G 01 Tillage
+ 76.20015 0.5 .75 76.20015 50.800102 101.600204
P 01 Break Crust
P 02 Random Roughness
+ 1 7.6200156
P 05 Ridges and Dikes
+ 1 25.400051 762.0015 0.0 0.0 0.0
P 11 Aggregate Crushing
+ 3.0 1.0
P 12 Soil Loosening
+ 0.75
P 13 Soil Layer Mixing
+ 0.35
P 34 Change Standing Biomass Fall Rate
+ 4 3.0 2.5 2.0 1.5 1.0
+ 0.5 0.6 0.7 0.8 1.0
G 02 Biomass Manipulation
+ 1.0
P 24 Flatten Standing Biomass
+ 14 0.7 0.3 0.3 0.1 1.0
P 25 Bury Flat Biomass
+ 1 .57 0.5 0.44 0.32 0.64
P 26 Resurface Buried Biomass
+ 0.01 0.01 0.01 0.01 0.01
#------------
D 31/07/03
O 03 Cultivator, row 1 in ridge
+ 5.799433 14.63 2.2351363 0.0 2.2351363 0.89405453 2.4586499
T RUSLE:Row crop cultivator w/ sweeps leaving a 1" ridge 05-14-02 DTL
T G2 was added into file in front of the flattening (P24), burial (P25), and resurfacing (P26) factors because the area affected is less than 1.0 and
T the RUSLE values were normalized to 1.0.  This change will imulate the correct residue changes based on the method set forth in RUSLE.
T RUSLE's factors have been redused to based on the area affected.
T The stalk fall rate factor (P34) was moved ahead of the new (G2) factor to set the fall rate to the less than 1.0 area affected.  8/8/07 MAS
+
G 01 Tillage
+ 76.20015 0.5 .75 76.20015 50.800102 101.600204
P 01 Break Crust
P 02 Random Roughness
+ 1 7.6200156
P 05 Ridges and Dikes
+ 1 25.400051 762.0015 0.0 0.0 0.0
P 11 Aggregate Crushing
+ 3.0 1.0
P 12 Soil Loosening
+ 0.75
P 13 Soil Layer Mixing
+ 0.35
P 34 Change Standing Biomass Fall Rate
+ 4 3.0 2.5 2.0 1.5 1.0
+ 0.5 0.6 0.7 0.8 1.0
G 02 Biomass Manipulation
+ 1.0
P 24 Flatten Standing Biomass
+ 14 0.7 0.3 0.3 0.1 1.0
P 25 Bury Flat Biomass
+ 1 .57 0.5 0.44 0.32 0.64
P 26 Resurface Buried Biomass
+ 0.01 0.01 0.01 0.01 0.01
#------------
D 20/08/03
O 04 Harvest, vine crops, mechanical
+ 3.2738733 2.6
T Represents harvest equipment like a tomato harvester that pulls the vine and runs the entire plant through,
T separating the fruits from the residue and placing the residue back on the ground. Some slight soil disturbance .   121604DTL
T
T ARS template (tool) record - filename is:  Harvest Tool (combine cutterbar header - fixed height cut).oprn
T This operation record is designed to represent actual field harvesting operations such as
T removing the grain yield of small grain crops like soybeans with a cutter bar head on a combine.
T This harvesting operation record removes all the reproductive component of a crop above the
T cutting height.  Typically this is specified as the "yield" component in the crop record.
T The non-harvested crop plant material above the specified cut height becomes flat residue.
T The remaining above ground crop material below the specified cut height becomes standing residue.
T Note that the harvested component can be changed from the "reproductive material"
T to other plant parts, so it can be used for non-grain type harvesting operations as well.
T Any crops harvested with this operation will default to killing the crop unless the appropriate
T "kill" process parameter is changed.
T 
T 200x	Created - Fred Fox
T Oct 31, 2005	Updated notes - Larry Wagner
T Detailed info regarding this operation record:
T This harvest record specifies the actual cut height independent upon the height
T of the crop.  If the crop is too short for the specified cut height, the operation may
T not harvest all of the intended material (yield).
T If one wants a variable cut height, based upon the height of the crop at harvest
T time, they should use the "Harvest Template (fraction crop height cut and remove)" operation.
T Some standing crop stalks could be flattened during the harvesting process,
T e.g. by the harvester's tire tracks.  Therefore, a flattening process is also a part of this
T operation record.  The default values are set to zero, assuming no flattening of standing
T stalks are occuring.  However, these can be set as necessary for the specific harvesting
T device used in the operation.
T The harvesting operation could also have an effect on the "standing stalk"
T fall rate and fall threshold values.  The default "biomass pool" flag parameter
T is set to "No adjustments applied" so that no "stalk residue decay rate change" will occur.
T However, this flag value can be changed along with the default parameter values
T to change the "stalk residue decay processes".
T
T Reworked the values MAS 2-24-09
T
T Changed the parts harvested to include flat to correct yield-residue issue with GA run on
T watermelons.  8-27-10  MAS
+
G 01 Tillage
+ 38.1000762001524 0.75 1 38.1000762001524 25.4000508001016 101.60020400000002
P 01 Break Crust
P 02 Random Roughness
+ 1 8.8900175
P 11 Aggregate Crushing
+ 1.4 -1.2
P 12 Soil Loosening
+ 0.85
P 13 Soil Layer Mixing
+ 0.05
G 02 Biomass Manipulation
+ 1.0
P 31 Kill or Defoliate Growing Crop
+ 2
P 62 Remove (by age pool) Plant/Residue Material
+ 1 1 0 1 3 3 2 1.0 0.0 0.0 0.0 0.0
P 34 Change Standing Biomass Fall Rate
+ 3 1.0 1.0 1.0 1.0 1.0
+ 1.0 1.0 1.0 1.0 1.0
P 40 End crop Biomass Manipulation
P 24 Flatten Standing Biomass
+ 14 1.0 1.0 1.0 1.0 1.0
#------------
D 30/09/03
O 03 Disk, tandem heavy primary op
+ 7.0154433 39 2.2351363 0.0 2.2351363 1.3410819 2.6821637
T 11-12in. Spacing, Front and Rear
T Recommended for primary tillage in medium to heavy soils
T Excellent residue-handling capability. MAS 10-26-06
+
G 01 Tillage
+ 152.4003 1.0 1.0 152.4003 101.600204 177.80035
P 01 Break Crust
P 02 Random Roughness
+ 1 38.100075
P 05 Ridges and Dikes
+ 1 101.600204 279.40057 0.0 0.0 0.0
P 11 Aggregate Crushing
+ 2.8 0.75
P 12 Soil Loosening
+ 0.9
P 13 Soil Layer Mixing
+ 0.4
P 31 Kill or Defoliate Growing Crop
+ 2
P 40 End crop Biomass Manipulation
P 24 Flatten Standing Biomass
+ 0 1.0 0.9 0.8 0.5 1.0
P 25 Bury Flat Biomass
+ 1 0.95 0.85 0.8 0.6 0.95
P 26 Resurface Buried Biomass
+ 0.05 0.06 0.07 0.08 0.05
P 34 Change Standing Biomass Fall Rate
+ 7 3.0 2.5 2.0 1.5 1.0
+ 0.5 0.6 0.7 0.8 1.0
#------------
D 09/10/03
O 03 Disk, tandem secondary op
+ 4.4898834 32.5 2.2351363 0.0 2.2351363 1.3410819 2.6821637
T 9-in. Spacing, Front and Rear; Good for seedbed preparation/chemical incorporation in medium to heavy soils
T Works well in primary tillage in light to medium soils
T Provides good residue-handling capability.  MAS 10-26-06
+
G 01 Tillage
+ 127.00027 0.75 1.0 127.00026 76.20015 152.4003
P 01 Break Crust
P 02 Random Roughness
+ 1 15.240031
P 05 Ridges and Dikes
+ 1 50.800102 228.60046 0.0 0.0 0.0
P 11 Aggregate Crushing
+ 2.8 0.75
P 12 Soil Loosening
+ 0.85
P 13 Soil Layer Mixing
+ 0.4
P 31 Kill or Defoliate Growing Crop
+ 2
P 40 End crop Biomass Manipulation
P 24 Flatten Standing Biomass
+ 0 0.85 0.7 0.6 0.5 1.0
P 25 Bury Flat Biomass
+ 1 0.73 0.63 0.55 0.4 0.73
P 26 Resurface Buried Biomass
+ 0.02 0.04 0.02 0.05 0.02
P 34 Change Standing Biomass Fall Rate
+ 7 3.0 2.5 2.0 1.5 1.0
+ 0.5 0.6 0.7 0.8 1.0
#------------
D 11/10/03
O 03 Drill or airseeder, double disk
+ 3.3674128 6.34 2.2351363 0.0 2.2351363 1.5645955 2.9056773
T Drill or air seeder with double disk openers on 7 to 10 inch spacings.  Rev102403 DTL  RUSLE MAS 10-26-06
T G2 was added into file in front of the flattening (P24), burial (P25), and resurfacing (P26) factors because the area affected is less than 1.0 and
T the RUSLE values were normalized to 1.0.  This change will imulate the correct residue changes based on the method set forth in RUSLE.
T RUSLE's factors have been redused to based on the area affected.
T The stalk fall rate factor (P34) was moved ahead of the new (G2) factor to set the fall rate to the  less than 1.0 area affected.  8/8/07 MAS
T
T Deleted the G2 process because all process only affect 0.65 of the surface.  This is set a 0.65 with G1 process in the beginning. 5-11-11 MAS
+ 
G 01 Tillage
+ 38.100075 0.4 0.65 38.100075 25.400051 50.800102
P 01 Break Crust
P 02 Random Roughness
+ 1 7.6200156
P 05 Ridges and Dikes
+ 1 25.400051 203.20041 25.400051 0.0 0.0
P 11 Aggregate Crushing
+ 2.8 0.75
P 12 Soil Loosening
+ 0.6
P 13 Soil Layer Mixing
+ 0.3
P 34 Change Standing Biomass Fall Rate
+ 7 3.0 2.5 2.0 1.5 1.0
+ 0.5 0.6 0.7 0.8 1.0
P 24 Flatten Standing Biomass
+ 0 0.6 0.4 0.35 0.15 1.0
P 25 Bury Flat Biomass
+ 1 0.2275 0.1625 0.13 0.065 0.13
P 26 Resurface Buried Biomass
+ 0.01 0.01 0.01 0.02 0.01
G 03 Crop Name
+ Barley, winter
P 51 Seeding Configuration
+ 1 0.0 0
+ 173.0 8.0 1 50.0 1.0 1.0 0
+ bu/ac
+ 9.6 186.0 5 0.8 0.64 0.8
+ 1.0 0.025 2.0 4.0 25.0 1 270 1333.3334
+ -5.0 -15.0 0.005 0.05 0.02 30.0
+ 0.013 0.6013 0.4293 -0.086 -0.018 0.932 0.556 0.0736
+ 0.4293 -0.086 2.5 1.0 25.0 0.05 0 0.3
+ 33.333332 385.0 1.4 0.012 0.1 0.1 0.0 2
+ 0.015 0.015 0.015 0.015 0.18 0.0050 17.1 5.183335
+ -2.08165 0.548606 1.3792 0.058508374 0.0 0.0 0.0 0.0
T Adjusted the Heat Units from the 3150 down to 2400 (same as WW)
T Tested in Delaware with John Timmons run.  8-18-09  MAS
#------------
D 18/06/04
O 04 Harvest, killing crop 70pct standing stubble
+ 14.311503 .15
T ARS record - filename is:  Harvest Wheat - grain (combine cutterbar header).oprn
T This operation record is designed to represent actual field harvesting operation
T of removing the grain from small grain crops with a cutterbar head on a combine.
T This harvesting operation record removes all the reproductive component of a crop above the
T cutting height.  Typically this is specified as the "yield" component in the crop record.
T The non-harvested crop plant material above the specified cut height becomes flat residue.
T The remaining above ground crop material below the specified cut height becomes standing residue.
T Nov 02, 2005	Created - Larry Wagner
T Detailed info regarding this operation record:
T This harvest record specifies the actual cut height dependent upon the height
T of the crop.  The cut height is specified as a fraction of the crop height.
T The harvesting operation could also have an effect on the "standing stalk"
T fall rate and fall threshold values.  The default "biomass pool" flag parameter
T is set to "No adjustments applied" so that no "stalk residue decay rate change" will occur.
T However, this flag value can be changed along with the default parameter values
T to change the "stalk residue decay processes".
T Added 0.2 for the flatting of the combine and tire trafic for haulling grain.
T MAS 1-18-07
+
G 02 Biomass Manipulation
+ 1.0
P 31 Kill or Defoliate Growing Crop
+ 2
P 43 Cut/Remove Biomass by Fraction (flags)
+ 1 1 0 1 0.03 1 0 0
P 34 Change Standing Biomass Fall Rate
+ 0 1.0 1.0 1.0 1.0 1.0
+ 1.0 1.0 1.0 1.0 1.0
P 40 End crop Biomass Manipulation
P 24 Flatten Standing Biomass
+ 0 0.1 0.1 0.1 0.1 1
#------------
D 18/06/04
O 04 Begin weed growth
+ 9.353924E-8 0
T Enter Operation notes here
+
G 03 Crop Name
+ Weeds, less than 6 mo growth
P 51 Seeding Configuration
+ 0 0.0 0
+ 9 1 0 1000 1 1 2
+ lbs/ac
+ 0 8930.0 4 1 0.65 0.95
+ 0.3048037 0.025 0.8 0 18.199999999999996 0 75 1100
+ -5 -15 0.01 0.95 0 19
+ 0.3128 0.576 0.6898 -0.1533 0 1 1.1 0.01
+ 0.4995 -0.0944 0.1 1 30 0.05 0 0.2562663
+ 500 500 1.5 0.01 0 0 0 1
+ 0.02 0.02 0.02 0.02 0.2 0.0050 20 5.227942
+ -1.20379 0.604887 0 0 0 0.0 0.0 0.0
T This record was replaced by Collard, greens.  The old record using winter peas did not grow in the south.
T The collard green produce 1400 lbs of biomass in the N part of N Dakota and 2356 lbs S FL.
T Edits were made to show just biomass above ground produced.  MAS 11-16-10
#------------
*END
*EOF
