Version: 1.5
*START 1
N Originating Program: RUSLE2
N Skel Format Version: 1.1
N This management file was originally converted from the NRCS standard XML format on - Thu Jun 21 11:13:41 PDT 2012
N This management file was updated to contain the most current crop and operation records for WEPS on - Tue Jun 26 15:43:20 PDT 2012
N This management file was updated to contain the most current crop and operation records for WEPS on - Tue Dec 17 19:26:21 CST 2013
#------------
D 01/03/01
O 03 Chisel, twisted shovel
+ 10.289317 65 2.9056773 0.0 2.9056773 1.5645955 2.9056773
T This is a stanard 3 inch twisted point chisel plow.  This is a 12 in sp machine placed staggered on three tool bars. MAS 6-4-09
+
G 01 Tillage
+ 165.10033 0.9 1.0 165.10033 101.600204 203.20041
P 01 Break Crust
P 02 Random Roughness
+ 1 48.260098
P 05 Ridges and Dikes
+ 1 152.4003 304.8006 101.600204 0.0 0.0
P 11 Aggregate Crushing
+ 2.4 -2.0
P 12 Soil Loosening
+ 0.85
P 13 Soil Layer Mixing
+ 0.42
P 31 Kill or Defoliate Growing Crop
+ 2
P 40 End crop Biomass Manipulation
P 24 Flatten Standing Biomass
+ 0 0.85 0.8 0.7 0.6 1.0
P 25 Bury Flat Biomass
+ 1 0.9 0.8 0.75 0.6 0.93
P 26 Resurface Buried Biomass
+ 0.05 0.06 0.07 0.15 0.05
P 34 Change Standing Biomass Fall Rate
+ 7 3.0 2.5 2.0 1.5 1.0
+ 0.5 0.6 0.7 0.8 1.0
#------------
D 01/04/01
O 03 Disk, tandem secondary op
+ 4.4898834 32.5 2.2351363 0.0 2.2351363 1.3410819 2.6821637
T 9-in. Spacing, Front and Rear; Good for seedbed preparation/chemical incorporation in medium to heavy soils
T Works well in primary tillage in light to medium soils
T Provides good residue-handling capability.  MAS 10-26-06
+
G 01 Tillage
+ 127.00027 0.75 1.0 127.00026 76.20015 152.4003
P 01 Break Crust
P 02 Random Roughness
+ 1 15.240031
P 05 Ridges and Dikes
+ 1 50.800102 228.60046 0.0 0.0 0.0
P 11 Aggregate Crushing
+ 2.8 0.75
P 12 Soil Loosening
+ 0.85
P 13 Soil Layer Mixing
+ 0.4
P 31 Kill or Defoliate Growing Crop
+ 2
P 40 End crop Biomass Manipulation
P 24 Flatten Standing Biomass
+ 0 0.85 0.7 0.6 0.5 1.0
P 25 Bury Flat Biomass
+ 1 0.73 0.63 0.55 0.4 0.73
P 26 Resurface Buried Biomass
+ 0.02 0.04 0.02 0.05 0.02
P 34 Change Standing Biomass Fall Rate
+ 7 3.0 2.5 2.0 1.5 1.0
+ 0.5 0.6 0.7 0.8 1.0
#------------
D 01/05/01
O 04 Fert applic. surface broadcast
+ 1.4966278 0.0609375
T R2 Notes: Broadcast fertilizer spreader.  Wheel traffic only.  rev 082107 DTL
T
T Added to DB 4-12-12 MAS
+
G 01 Tillage
+ 0.0 0 0.05 0.0 0.0 0.0
P 01 Break Crust
P 02 Random Roughness
+ 1 8.8900175
P 11 Aggregate Crushing
+ 4.3 2.0
P 24 Flatten Standing Biomass
+ 0 0.25 0.2 0.15 0.1 1.0
P 26 Resurface Buried Biomass
+ 0.07 0.08 0.1 0.12 0.07
P 34 Change Standing Biomass Fall Rate
+ 0 1.0 1.0 1.0 1.0 1.0
+ 1.0 1.0 1.0 1.0 1.0
#------------
D 01/05/01
O 03 Disk, tandem light finishing
+ 3.7415698 19.5 2.2351363 0.0 2.2351363 1.3410819 2.6821637
T 6/8/01 DTL RUSLE.  7in sp.  This is tool used to finish a seedbed.  MAS 10-26-06
+
G 01 Tillage
+ 101.600204 0.5 1.0 101.600204 76.20015 127.00026
P 01 Break Crust
P 02 Random Roughness
+ 1 15.240031
P 05 Ridges and Dikes
+ 1 12.700026 177.80035 0.0 0.0 0.0
P 11 Aggregate Crushing
+ 2.8 0.75
P 12 Soil Loosening
+ 0.75
P 13 Soil Layer Mixing
+ 0.35
P 31 Kill or Defoliate Growing Crop
+ 2
P 40 End crop Biomass Manipulation
P 24 Flatten Standing Biomass
+ 0 0.85 0.7 0.6 0.5 1.0
P 25 Bury Flat Biomass
+ 1 0.73 0.63 0.55 0.4 0.73
P 26 Resurface Buried Biomass
+ 0.02 0.04 0.02 0.05 0.02
P 34 Change Standing Biomass Fall Rate
+ 7 3.0 2.5 2.0 1.5 1.0
+ 0.5 0.6 0.7 0.8 1.0
#------------
D 05/05/01
O 03 Planter, small veg seed
+ 3.3674128 .59 0.89405453 0.0 0.89405453 0.44702727 1.3410819
T Small seed planter like used in planting small seeded vegetables in 25 to 30" rows.
T Shallow depth and minimal disturbance in fine seedbed.  Like Planet Junior.  12-10-01 DTL
T G2 was added into file in front of the flattening (P24), burial (P25), and resurfacing (P26) factors because the area affected is less than 1.0 and
T the RUSLE values were normalized to 1.0.  This change will imulate the correct residue changes based on the method set forth in RUSLE.
T RUSLE's factors have been redused to based on the area affected.
T The stalk fall rate factor (P34) was moved ahead of the new (G2) factor to set the fall rate to theless than 1.0 area affected.  8/7/07 MAS
T
T Changed the P5 to allow the preexisting ridges and furrows to set the ridge roughness.  MAS  12-30-2010
+
G 01 Tillage
+ 25.400051 0.5 .15 25.400051 12.700026 50.800102
P 01 Break Crust
P 02 Random Roughness
+ 1 7.6200156
P 05 Ridges and Dikes
+ 0 25.400051 762.0015 711.2014 0.0 0.0
P 11 Aggregate Crushing
+ 2.8 0.75
P 12 Soil Loosening
+ 0.6
P 13 Soil Layer Mixing
+ 0.35
P 34 Change Standing Biomass Fall Rate
+ 7 3.0 2.5 2.0 1.5 1.0
+ 0.5 0.6 0.7 0.8 1.0
G 02 Biomass Manipulation
+ 1.0
P 24 Flatten Standing Biomass
+ 0 .3 .25 .2 0.1 1.0
P 25 Bury Flat Biomass
+ 1 .0525 .0375 .03 .015 .03
P 26 Resurface Buried Biomass
+ 0.01 .01 .01 0.05 .01
G 03 Crop Name
+ Cucumber
P 51 Seeding Configuration
+ 1 0.0 2
+ 24.711494 1.0 1 29000 1.0 1.0 0
+ lb/ac
+ 96.1 8930 4 0.8 0.65 0.9
+ 0.4 0.025 1.1 10.0 32.0 0 70 900.0
+ -5.0 -15.0 0.15 0.95 0.0 30.0
+ -0.0062 0.9478 0.3633 -0.0721 -0.0083 1.005 0.7292 0.0562
+ 0.3633 -0.0721 2.0 1.0 20.0 0.05 0 6.0957026
+ 25.641026 25.641026 1.3 0.011 0.0 0.0 0.0 1
+ 0.02 0.02 0.02 0.02 0.2 0.0050 20.0 5.227942
+ -1.20379 0.604887 0.0688 0.024658702 0.0 0.0 0.0 0.0
T RUSLE2 notes.  4/17/03 gaw.   Yield for machine harvest. High production, related to one or more of the following - irrigation,
T high fertility, favorable climate, productive soils and varieties.  Type locations: CA, FL, TX.
T
T I made changes to the harvest index to match the Cucumber, HIGH PRO record in RUSLE2.  MAS 11-24-08
T Corrected the plant pop and yield.  MAS 5-11-09
#------------
D 05/05/01
O 04 Sprayer, pre-emergence
+ 1.2160101 .15
T Spray pest control chemicals on growing crop.  Crop is not killed.
T In the MCREW management screen the user must select the kind of weeds killed in the growing crop as external residue.   080404 DTL
T Cloned from Defoliate (spray) crop.oprn, Changed the P31 to No crop kill and added G4 to add material to field MAS 9-28-06
+
G 03 Crop Name
+ weed residue; 0-3 mo
P 65 Add Crop Residue Amounts
+ 0.0 0.0 0.0 0.0 1
+ 0.0 0.0 0.0056042504 152.4003
+ 0.025 0.025 0.025 0.025 0.169 0.0050 17.1 5.227942
+ -1.20379 0.604887
T Enter crop notes here.
#------------
D 15/05/01
O 03 Cultivator, row 1 in ridge
+ 5.799433 14.63 2.2351363 0.0 2.2351363 0.89405453 2.4586499
T RUSLE:Row crop cultivator w/ sweeps leaving a 1" ridge 05-14-02 DTL
T G2 was added into file in front of the flattening (P24), burial (P25), and resurfacing (P26) factors because the area affected is less than 1.0 and
T the RUSLE values were normalized to 1.0.  This change will imulate the correct residue changes based on the method set forth in RUSLE.
T RUSLE's factors have been redused to based on the area affected.
T The stalk fall rate factor (P34) was moved ahead of the new (G2) factor to set the fall rate to the less than 1.0 area affected.  8/8/07 MAS
+
G 01 Tillage
+ 76.20015 0.5 .75 76.20015 50.800102 101.600204
P 01 Break Crust
P 02 Random Roughness
+ 1 7.6200156
P 05 Ridges and Dikes
+ 1 25.400051 762.0015 0.0 0.0 0.0
P 11 Aggregate Crushing
+ 3.0 1.0
P 12 Soil Loosening
+ 0.75
P 13 Soil Layer Mixing
+ 0.35
P 34 Change Standing Biomass Fall Rate
+ 4 3.0 2.5 2.0 1.5 1.0
+ 0.5 0.6 0.7 0.8 1.0
G 02 Biomass Manipulation
+ 1.0
P 24 Flatten Standing Biomass
+ 14 0.7 0.3 0.3 0.1 1.0
P 25 Bury Flat Biomass
+ 1 .57 0.5 0.44 0.32 0.64
P 26 Resurface Buried Biomass
+ 0.01 0.01 0.01 0.01 0.01
#------------
D 05/06/01
O 04 Sprayer, insecticide post emergence
+ 1.2160101 0.15
T Spray pest control chemicals on growing crop.   Crop is not killed.  11/17/01 DTL
T
T Added to the DB.  This assumes no crop flattening.  4-5-12 MAS
+
#------------
D 05/06/01
O 03 Cultivator, row 1 in ridge
+ 5.799433 14.63 2.2351363 0.0 2.2351363 0.89405453 2.4586499
T RUSLE:Row crop cultivator w/ sweeps leaving a 1" ridge 05-14-02 DTL
T G2 was added into file in front of the flattening (P24), burial (P25), and resurfacing (P26) factors because the area affected is less than 1.0 and
T the RUSLE values were normalized to 1.0.  This change will imulate the correct residue changes based on the method set forth in RUSLE.
T RUSLE's factors have been redused to based on the area affected.
T The stalk fall rate factor (P34) was moved ahead of the new (G2) factor to set the fall rate to the less than 1.0 area affected.  8/8/07 MAS
+
G 01 Tillage
+ 76.20015 0.5 .75 76.20015 50.800102 101.600204
P 01 Break Crust
P 02 Random Roughness
+ 1 7.6200156
P 05 Ridges and Dikes
+ 1 25.400051 762.0015 0.0 0.0 0.0
P 11 Aggregate Crushing
+ 3.0 1.0
P 12 Soil Loosening
+ 0.75
P 13 Soil Layer Mixing
+ 0.35
P 34 Change Standing Biomass Fall Rate
+ 4 3.0 2.5 2.0 1.5 1.0
+ 0.5 0.6 0.7 0.8 1.0
G 02 Biomass Manipulation
+ 1.0
P 24 Flatten Standing Biomass
+ 14 0.7 0.3 0.3 0.1 1.0
P 25 Bury Flat Biomass
+ 1 .57 0.5 0.44 0.32 0.64
P 26 Resurface Buried Biomass
+ 0.01 0.01 0.01 0.01 0.01
#------------
D 05/06/01
O 04 Fert applic. side-dress, liquid
+ 1.2160101 0.15
T Spray or dribble side-dress application of fertilizer into row crop.   Crop is not affected.
T Created from DTL's Sprayer, insecticide post emergence" record.  04/13/11 GGF
T
T Added to WEPS 3-1-12
+ 
#------------
D 15/06/01
O 03 Cultivator, row 1 in ridge
+ 5.799433 14.63 2.2351363 0.0 2.2351363 0.89405453 2.4586499
T RUSLE:Row crop cultivator w/ sweeps leaving a 1" ridge 05-14-02 DTL
T G2 was added into file in front of the flattening (P24), burial (P25), and resurfacing (P26) factors because the area affected is less than 1.0 and
T the RUSLE values were normalized to 1.0.  This change will imulate the correct residue changes based on the method set forth in RUSLE.
T RUSLE's factors have been redused to based on the area affected.
T The stalk fall rate factor (P34) was moved ahead of the new (G2) factor to set the fall rate to the less than 1.0 area affected.  8/8/07 MAS
+
G 01 Tillage
+ 76.20015 0.5 .75 76.20015 50.800102 101.600204
P 01 Break Crust
P 02 Random Roughness
+ 1 7.6200156
P 05 Ridges and Dikes
+ 1 25.400051 762.0015 0.0 0.0 0.0
P 11 Aggregate Crushing
+ 3.0 1.0
P 12 Soil Loosening
+ 0.75
P 13 Soil Layer Mixing
+ 0.35
P 34 Change Standing Biomass Fall Rate
+ 4 3.0 2.5 2.0 1.5 1.0
+ 0.5 0.6 0.7 0.8 1.0
G 02 Biomass Manipulation
+ 1.0
P 24 Flatten Standing Biomass
+ 14 0.7 0.3 0.3 0.1 1.0
P 25 Bury Flat Biomass
+ 1 .57 0.5 0.44 0.32 0.64
P 26 Resurface Buried Biomass
+ 0.01 0.01 0.01 0.01 0.01
#------------
D 15/06/01
O 04 Sprayer, insecticide post emergence
+ 1.2160101 0.15
T Spray pest control chemicals on growing crop.   Crop is not killed.  11/17/01 DTL
T
T Added to the DB.  This assumes no crop flattening.  4-5-12 MAS
+
#------------
D 01/07/01
O 04 Harvest, vine crops, mechanical
+ 3.2738733 2.6
T Represents harvest equipment like a tomato harvester that pulls the vine and runs the entire plant through,
T separating the fruits from the residue and placing the residue back on the ground. Some slight soil disturbance .   121604DTL
T
T ARS template (tool) record - filename is:  Harvest Tool (combine cutterbar header - fixed height cut).oprn
T This operation record is designed to represent actual field harvesting operations such as
T removing the grain yield of small grain crops like soybeans with a cutter bar head on a combine.
T This harvesting operation record removes all the reproductive component of a crop above the
T cutting height.  Typically this is specified as the "yield" component in the crop record.
T The non-harvested crop plant material above the specified cut height becomes flat residue.
T The remaining above ground crop material below the specified cut height becomes standing residue.
T Note that the harvested component can be changed from the "reproductive material"
T to other plant parts, so it can be used for non-grain type harvesting operations as well.
T Any crops harvested with this operation will default to killing the crop unless the appropriate
T "kill" process parameter is changed.
T 
T 200x	Created - Fred Fox
T Oct 31, 2005	Updated notes - Larry Wagner
T Detailed info regarding this operation record:
T This harvest record specifies the actual cut height independent upon the height
T of the crop.  If the crop is too short for the specified cut height, the operation may
T not harvest all of the intended material (yield).
T If one wants a variable cut height, based upon the height of the crop at harvest
T time, they should use the "Harvest Template (fraction crop height cut and remove)" operation.
T Some standing crop stalks could be flattened during the harvesting process,
T e.g. by the harvester's tire tracks.  Therefore, a flattening process is also a part of this
T operation record.  The default values are set to zero, assuming no flattening of standing
T stalks are occuring.  However, these can be set as necessary for the specific harvesting
T device used in the operation.
T The harvesting operation could also have an effect on the "standing stalk"
T fall rate and fall threshold values.  The default "biomass pool" flag parameter
T is set to "No adjustments applied" so that no "stalk residue decay rate change" will occur.
T However, this flag value can be changed along with the default parameter values
T to change the "stalk residue decay processes".
T
T Reworked the values MAS 2-24-09
T
T Changed the parts harvested to include flat to correct yield-residue issue with GA run on
T watermelons.  8-27-10  MAS
+
G 01 Tillage
+ 38.1000762001524 0.75 1 38.1000762001524 25.4000508001016 101.60020400000002
P 01 Break Crust
P 02 Random Roughness
+ 1 8.8900175
P 11 Aggregate Crushing
+ 1.4 -1.2
P 12 Soil Loosening
+ 0.85
P 13 Soil Layer Mixing
+ 0.05
G 02 Biomass Manipulation
+ 1.0
P 31 Kill or Defoliate Growing Crop
+ 2
P 62 Remove (by age pool) Plant/Residue Material
+ 1 1 0 1 3 3 2 1.0 0.0 0.0 0.0 0.0
P 34 Change Standing Biomass Fall Rate
+ 3 1.0 1.0 1.0 1.0 1.0
+ 1.0 1.0 1.0 1.0 1.0
P 40 End crop Biomass Manipulation
P 24 Flatten Standing Biomass
+ 14 1.0 1.0 1.0 1.0 1.0
#------------
*END
*EOF
