Version: 1.5
*START 2
N Originating Program: RUSLE2
N Skel Format Version: 1.1
N This management file was originally converted from the NRCS standard XML format on - Thu Jun 21 11:15:53 PDT 2012
N This management file was updated to contain the most current crop and operation records for WEPS on - Tue Jun 26 15:41:09 PDT 2012
N This management file was updated to contain the most current crop and operation records for WEPS on - Tue Dec 17 19:24:17 CST 2013
#------------
D 18/06/01
O 04 Harvest, killing crop 50pct standing stubble
+ 14.311503 .15
T ARS record - filename is:  Harvest Wheat - grain (combine cutterbar header).oprn
T This operation record is designed to represent actual field harvesting operation
T of removing the grain from small grain crops with a cutterbar head on a combine.
T This harvesting operation record removes all the reproductive component of a crop above the
T cutting height.  Typically this is specified as the "yield" component in the crop record.
T The non-harvested crop plant material above the specified cut height becomes flat residue.
T The remaining above ground crop material below the specified cut height becomes standing residue.
T Nov 02, 2005	Created - Larry Wagner
T Detailed info regarding this operation record:
T This harvest record specifies the actual cut height dependent upon the height
T of the crop.  The cut height is specified as a fraction of the crop height.
T Added 0.2 for the flatting of the combine and tire trafic for haulling grain.
T MAS 1-18-07
T The harvesting operation could also have an effect on the "standing stalk"
T fall rate and fall threshold values.  The default "biomass pool" flag parameter
T is set to "No adjustments applied" so that no "stalk residue decay rate change" will occur.
T However, this flag value can be changed along with the default parameter values
T to change the "stalk residue decay processes".
+
G 02 Biomass Manipulation
+ 1.0
P 31 Kill or Defoliate Growing Crop
+ 2
P 43 Cut/Remove Biomass by Fraction (flags)
+ 1 1 0 1 0.2 1 0 0
P 34 Change Standing Biomass Fall Rate
+ 0 1.0 1.0 1.0 1.0 1.0
+ 1.0 1.0 1.0 1.0 1.0
P 40 End crop Biomass Manipulation
P 24 Flatten Standing Biomass
+ 0 0.2 0.2 0.15 0.2 1
#------------
D 20/06/01
O 03 Drill or air seeder single disk openers 7-10 in spac
+ 3.2738733 2.44 2.2351363 0.0 2.2351363 1.5645955 2.9056773
T Drill or Air seeder with single disk no-till openers  JD 750 or similar openers. (No-till air drill)
T Based on Drill, no-till single disk 7-10 spacing. 102403 DTL. RUSLE MAS 10-26-06
T G2 was added into file in front of the flattening (P24), burial (P25), and resurfacing (P26) factors because the area affected is less than 1.0 and
T the RUSLE values were normalized to 1.0.  This change will imulate the correct residue changes based on the method set forth in RUSLE.
T RUSLE's factors have been redused to based on the area affected.
T The stalk fall rate factor (P34) was moved ahead of the new (G2) factor to set the fall rate to the less than 1.0 area affected.  8/7/07 MAS
+
G 01 Tillage
+ 63.500134 0.4 0.15 63.50013 50.800102 101.600204
P 01 Break Crust
P 02 Random Roughness
+ 1 7.6200156
P 05 Ridges and Dikes
+ 1 25.400051 203.20041 0.0 0.0 0.0
P 11 Aggregate Crushing
+ 2.8 0.75
P 12 Soil Loosening
+ 0.4
P 13 Soil Layer Mixing
+ 0.20
P 34 Change Standing Biomass Fall Rate
+ 7 3.0 2.5 2.0 1.5 1.0
+ 0.5 0.6 0.7 0.8 1.0
G 02 Biomass Manipulation
+ 1.0
P 24 Flatten Standing Biomass
+ 0 0.6 0.4 0.35 0.15 1.0
P 25 Bury Flat Biomass
+ 1 0.05 0.04 0.03 0.02 0.03
P 26 Resurface Buried Biomass
+ 0.01 0.01 0.01 0.05 0.01
G 03 Crop Name
+ Soybean, group II, III and IV
P 51 Seeding Configuration
+ 1 0.0 0
+ 27.0 1.0 1 45 1.0 1.0 0
+ bu/ac
+ 13 148.7 1 0.8 0.65 .8
+ 1.5 0.05 1.5240185 10.0 25.0 0 100 1200.0
+ -5.0 -15.0 0.01 0.95 0.0 25.0
+ 0.023 0.8063 0.4146 -0.061 -0.024 0.9911 0.6435 0.0494
+ 0.4146 -0.061 2.83 1.0 26.0 0.05 0 0.5
+ 111.111115 111.111115 1.5 0.015 0.0 0.0 0.0 1
+ 0.03 0.03 0.03 0.03 0.2 0.01 20.0 5.227942
+ -1.20379 0.604887 1.34 0.0313838 0.0 0.0 0.0 0.0
T RUSLE Notes: Soybeans in Maturity group II, III, and IV.  7 inch row spacing Midwest growing conditions  REV 071104DTL
T This was cloned from the WEPS MG II file. MAS 10-19-06
T Days to mature set to losest maturity group days from planting minus 10 days.
T group II is 110 days - 10 = 100 days MAS 3-21-07
T
T WEPS yields are adjusted to the middle of the yield for the group
T and different than the RUSLE records (RUSLE gives the bottom of the group).
T MAS 7/31/07
#------------
D 20/06/01
O 04 Sprayer, pre-emergence
+ 1.2160101 .15
T Spray pest control chemicals on growing crop.  Crop is not killed.
T In the MCREW management screen the user must select the kind of weeds killed in the growing crop as external residue.   080404 DTL
T Cloned from Defoliate (spray) crop.oprn, Changed the P31 to No crop kill and added G4 to add material to field MAS 9-28-06
+
G 03 Crop Name
+ weed residue; 0-3 mo
P 65 Add Crop Residue Amounts
+ 0.0 0.0 0.0 0.0 1
+ 0.0 0.0 0.0056042504 152.4003
+ 0.025 0.025 0.025 0.025 0.169 0.0050 17.1 5.227942
+ -1.20379 0.604887
T Enter crop notes here.
#------------
D 15/07/01
O 04 Sprayer, post emergence
+ 1.2160101 .15
T Spray pest control chemicals on growing crop.  Crop is not killed.
T In the MCREW management screen the user must select the kind of weeds killed in the growing crop as external residue.   080404 DTL
T Cloned from Defoliate (spray) crop.oprn, Changed the P31 to No crop kill and added G4 to add material to field MAS 9-28-06
T DO NOT LEAVE CROP COLUMN SET TO "no crop".  User must select the crop and then drill into the operation and specify the amount of weed
T mass that will be killed and turned into residue.
+
G 03 Crop Name
+ weed residue; 0-3 mo
P 65 Add Crop Residue Amounts
+ 0.0 0.0 0.0 0.028021252 1
+ 0.0 0.0 0.0056042504 152.4003
+ 0.025 0.025 0.025 0.025 0.169 0.0050 17.1 5.227942
+ -1.20379 0.604887
T Enter crop notes here.
#------------
D 30/10/01
O 04 Harvest, killing crop 50pct standing stubble
+ 14.311503 .15
T ARS record - filename is:  Harvest Wheat - grain (combine cutterbar header).oprn
T This operation record is designed to represent actual field harvesting operation
T of removing the grain from small grain crops with a cutterbar head on a combine.
T This harvesting operation record removes all the reproductive component of a crop above the
T cutting height.  Typically this is specified as the "yield" component in the crop record.
T The non-harvested crop plant material above the specified cut height becomes flat residue.
T The remaining above ground crop material below the specified cut height becomes standing residue.
T Nov 02, 2005	Created - Larry Wagner
T Detailed info regarding this operation record:
T This harvest record specifies the actual cut height dependent upon the height
T of the crop.  The cut height is specified as a fraction of the crop height.
T Added 0.2 for the flatting of the combine and tire trafic for haulling grain.
T MAS 1-18-07
T The harvesting operation could also have an effect on the "standing stalk"
T fall rate and fall threshold values.  The default "biomass pool" flag parameter
T is set to "No adjustments applied" so that no "stalk residue decay rate change" will occur.
T However, this flag value can be changed along with the default parameter values
T to change the "stalk residue decay processes".
+
G 02 Biomass Manipulation
+ 1.0
P 31 Kill or Defoliate Growing Crop
+ 2
P 43 Cut/Remove Biomass by Fraction (flags)
+ 1 1 0 1 0.2 1 0 0
P 34 Change Standing Biomass Fall Rate
+ 0 1.0 1.0 1.0 1.0 1.0
+ 1.0 1.0 1.0 1.0 1.0
P 40 End crop Biomass Manipulation
P 24 Flatten Standing Biomass
+ 0 0.2 0.2 0.15 0.2 1
#------------
D 31/10/01
O 03 Chisel, st. pt. 12 in deep
+ 10.289317 62.4 2.2351363 0.0 2.2351363 1.5645955 2.9056773
T Chisel plow with straight points at 12 inch operating depth  02-28-02  DTL REV 110207 DTL
T Cloned from Chisel plow st pt.  Edit to RUSLE MAS 11-19-07
+
G 01 Tillage
+ 177.80035 0.75 1.0 177.80035 101.600204 203.20041
P 01 Break Crust
P 02 Random Roughness
+ 1 38.100075
P 05 Ridges and Dikes
+ 1 76.20015 381.00076 101.600204 0.0 0.0
P 11 Aggregate Crushing
+ 2.4 -2.0
P 12 Soil Loosening
+ 0.85
P 13 Soil Layer Mixing
+ 0.37
P 31 Kill or Defoliate Growing Crop
+ 2
P 40 End crop Biomass Manipulation
P 24 Flatten Standing Biomass
+ 0 0.6 0.4 0.25 0.1 1.0
P 25 Bury Flat Biomass
+ 1 0.76 0.68 0.58 0.5 0.9
P 26 Resurface Buried Biomass
+ 0.05 0.06 0.07 0.2 0.05
P 34 Change Standing Biomass Fall Rate
+ 7 3.0 2.5 2.0 1.5 1.0
+ 0.5 0.6 0.7 0.8 1.0
#------------
D 10/03/02
O 03 Disk, tandem heavy primary op
+ 7.0154433 39 2.2351363 0.0 2.2351363 1.3410819 2.6821637
T 11-12in. Spacing, Front and Rear
T Recommended for primary tillage in medium to heavy soils
T Excellent residue-handling capability. MAS 10-26-06
+
G 01 Tillage
+ 152.4003 1.0 1.0 152.4003 101.600204 177.80035
P 01 Break Crust
P 02 Random Roughness
+ 1 38.100075
P 05 Ridges and Dikes
+ 1 101.600204 279.40057 0.0 0.0 0.0
P 11 Aggregate Crushing
+ 2.8 0.75
P 12 Soil Loosening
+ 0.9
P 13 Soil Layer Mixing
+ 0.4
P 31 Kill or Defoliate Growing Crop
+ 2
P 40 End crop Biomass Manipulation
P 24 Flatten Standing Biomass
+ 0 1.0 0.9 0.8 0.5 1.0
P 25 Bury Flat Biomass
+ 1 0.95 0.85 0.8 0.6 0.95
P 26 Resurface Buried Biomass
+ 0.05 0.06 0.07 0.08 0.05
P 34 Change Standing Biomass Fall Rate
+ 7 3.0 2.5 2.0 1.5 1.0
+ 0.5 0.6 0.7 0.8 1.0
#------------
D 10/03/02
O 04 Fert applic. surface broadcast
+ 1.4966278 0.0609375
T R2 Notes: Broadcast fertilizer spreader.  Wheel traffic only.  rev 082107 DTL
T
T Added to DB 4-12-12 MAS
+
G 01 Tillage
+ 0.0 0 0.05 0.0 0.0 0.0
P 01 Break Crust
P 02 Random Roughness
+ 1 8.8900175
P 11 Aggregate Crushing
+ 4.3 2.0
P 24 Flatten Standing Biomass
+ 0 0.25 0.2 0.15 0.1 1.0
P 26 Resurface Buried Biomass
+ 0.07 0.08 0.1 0.12 0.07
P 34 Change Standing Biomass Fall Rate
+ 0 1.0 1.0 1.0 1.0 1.0
+ 1.0 1.0 1.0 1.0 1.0
#------------
D 10/03/02
O 03 Disk, tandem secondary op
+ 4.4898834 32.5 2.2351363 0.0 2.2351363 1.3410819 2.6821637
T 9-in. Spacing, Front and Rear; Good for seedbed preparation/chemical incorporation in medium to heavy soils
T Works well in primary tillage in light to medium soils
T Provides good residue-handling capability.  MAS 10-26-06
+
G 01 Tillage
+ 127.00027 0.75 1.0 127.00026 76.20015 152.4003
P 01 Break Crust
P 02 Random Roughness
+ 1 15.240031
P 05 Ridges and Dikes
+ 1 50.800102 228.60046 0.0 0.0 0.0
P 11 Aggregate Crushing
+ 2.8 0.75
P 12 Soil Loosening
+ 0.85
P 13 Soil Layer Mixing
+ 0.4
P 31 Kill or Defoliate Growing Crop
+ 2
P 40 End crop Biomass Manipulation
P 24 Flatten Standing Biomass
+ 0 0.85 0.7 0.6 0.5 1.0
P 25 Bury Flat Biomass
+ 1 0.73 0.63 0.55 0.4 0.73
P 26 Resurface Buried Biomass
+ 0.02 0.04 0.02 0.05 0.02
P 34 Change Standing Biomass Fall Rate
+ 7 3.0 2.5 2.0 1.5 1.0
+ 0.5 0.6 0.7 0.8 1.0
#------------
D 18/03/02
O 03 Planter, runner opener
+ 4.1157265 2.6 1.7881090746535537 0 2.2351363 0.8940545373267769 2.6821636119803305
+
G 01 Tillage
+ 63.500127000254 0.5 0.2 63.500126 25.4000508001016 88.90017780035559
P 01 Break Crust
P 02 Random Roughness
+ 1 10.160021
P 05 Ridges and Dikes
+ 1 76.2001524003048 762.0015 635.0013 0 0
P 11 Aggregate Crushing
+ 2.8 0.75
P 12 Soil Loosening
+ 0.6
P 13 Soil Layer Mixing
+ 0.35
P 34 Change Standing Biomass Fall Rate
+ 7 3.0 2.5 2.0 1.5 1.0
+ 0.5 0.6 0.7 0.8 1.0
G 02 Biomass Manipulation
+ 1.0
P 24 Flatten Standing Biomass
+ 0 .3 .25 .2 0.1 1.0
P 25 Bury Flat Biomass
+ 1 0.07 0.05 0.04 0.02 0.03
P 26 Resurface Buried Biomass
+ 0.01 0.01 0.01 0.05 0.01
G 03 Crop Name
+ Potato, late, harvest
P 51 Seeding Configuration
+ 1 0.0 2
+ 5.0 4.0 1 600 1.0 1.0 5
+ cwt/ac
+ 79.0 89.3 7 1.0 0.65 0.8
+ 0.8 0.05 0.6096074 2.0 25.0 0 120 1600.0
+ -5.0 -15.0 0.01 0.95 0.0 32
+ 0.0 0.6553 0.3159 -0.061 -3.0E-4 0.9911 0.3415 0.0494
+ 0.4163 -0.061 2.6 1.0 30.0 0.05 0 1.0
+ 12000.0 2700.0 3.0 0.03 0.0 0.0 0.9 1
+ 0.02 0.02 0.02 0.02 0.2 0.0050 20.0 5.227942
+ -1.20379 0.604887 0.0313 0.024658702 0.0 0.0 0.0 0.0
T Represents high yielding typically irrigated Potatoes - white, russet, red (all but sweet). 60,000 lb (600 cwt), 30 ton/ac yield .  36" rows.
T Residue at harvest includes mass before chemical kill.  Base location ID, WA, NM.
T
T File was tested in Grant Co. WA and Bingham Co. ID.  Biomas Conv Eff factor was at 32.  Yields were low.
T At 40 the yields were 553 cwt/ac in WA and 485 cwt/ac in ID.  I have made the change to get the yields closer
T to the actual field values.  MAS 9-26-07
T
T Harvest biomass ratio is set using two studies.  One from the PNW irrigated and the other in MN.
T Both sites are were sandy soils with irrigation.  Yields were 600 cwt/ac.  MAS 7-3-08
#------------
D 18/03/02
O 03 Bedder, hipper, disk hiller
+ 4.2092657 26 2.0116227 0.0 2.0116227 1.5645955 2.2351363
T This is an 8 in high tool to reform beds from RUSLE 6-7-01 DTL
T
T Corrected the tillage depths and other residue values 11-1-11
+
G 01 Tillage
+ 101.600204 0.9 1.0 101.600204 50.800102 127.00025
P 01 Break Crust
P 02 Random Roughness
+ 1 15.240031
P 11 Aggregate Crushing
+ 3.0 2.0
P 12 Soil Loosening
+ 0.75
P 13 Soil Layer Mixing
+ 0.75
P 05 Ridges and Dikes
+ 1 203.20041 760.0 381.00076 0.0 0.0
P 31 Kill or Defoliate Growing Crop
+ 2
P 40 End crop Biomass Manipulation
P 24 Flatten Standing Biomass
+ 0 1 0.90 0.9 0.5 1.00
P 25 Bury Flat Biomass
+ 1 0.95 0.92 0.85 0.5 0.6
P 26 Resurface Buried Biomass
+ 0.02 0.02 0.02 0.05 0.03
P 34 Change Standing Biomass Fall Rate
+ 7 3.0 2.5 2.0 1.5 1.0
+ 0.5 0.6 0.7 0.8 1.0
#------------
D 25/04/02
O 03 Cultivator, row between beds
+ 5.799433 10.56 2.2351363 0.0 2.2351363 0.89405453 2.4586499
T Cultivator w/ opposing gangs of disk hillers.  Used to cultivate between Sugarcane beds. 020106 DTL
T G2 was added into file in front of the flattening (P24), burial (P25), and resurfacing (P26) factors because the area affected is less than 1.0 and
T the RUSLE values were normalized to 1.0.  This change will imulate the correct residue changes based on the method set forth in RUSLE.
T RUSLE's factors have been redused to based on the area affected.
T The stalk fall rate factor (P34) was moved ahead of the new (G2) factor to set the fall rate to the  less than 1.0 area affected.  8/7/07 MAS
T Cloned from row cultivator.  11-22-07 MAS
T
T Changed the P5 Ridge and Dikes to reflect the height of the previous tillage.  The operation now will show the ridge height of the planter or
T the previous tillage.  MAS 6-3-11
+
G 01 Tillage
+ 63.500126 0.5 .65 63.500126 50.800102 101.600204
P 01 Break Crust
P 02 Random Roughness
+ 1 15.240031
P 05 Ridges and Dikes
+ 0 76.20015 762.0015 355.6007 0.0 0.0
P 11 Aggregate Crushing
+ 3.0 1.0
P 12 Soil Loosening
+ 0.75
P 13 Soil Layer Mixing
+ 0.35
P 34 Change Standing Biomass Fall Rate
+ 4 3.0 2.5 2.0 1.5 1.0
+ 0.5 0.6 0.7 0.8 1.0
G 02 Biomass Manipulation
+ 1.0
P 24 Flatten Standing Biomass
+ 14 0.7 0.3 0.3 0.1 1.0
P 25 Bury Flat Biomass
+ 1 0.49 0.44 0.38 0.28 0.55
P 26 Resurface Buried Biomass
+ 0.7 0.3 0.3 0.1 1
#------------
D 23/05/02
O 03 Cultivator, row between beds
+ 5.799433 10.56 2.2351363 0.0 2.2351363 0.89405453 2.4586499
T Cultivator w/ opposing gangs of disk hillers.  Used to cultivate between Sugarcane beds. 020106 DTL
T G2 was added into file in front of the flattening (P24), burial (P25), and resurfacing (P26) factors because the area affected is less than 1.0 and
T the RUSLE values were normalized to 1.0.  This change will imulate the correct residue changes based on the method set forth in RUSLE.
T RUSLE's factors have been redused to based on the area affected.
T The stalk fall rate factor (P34) was moved ahead of the new (G2) factor to set the fall rate to the  less than 1.0 area affected.  8/7/07 MAS
T Cloned from row cultivator.  11-22-07 MAS
T
T Changed the P5 Ridge and Dikes to reflect the height of the previous tillage.  The operation now will show the ridge height of the planter or
T the previous tillage.  MAS 6-3-11
+
G 01 Tillage
+ 63.500126 0.5 .65 63.500126 50.800102 101.600204
P 01 Break Crust
P 02 Random Roughness
+ 1 15.240031
P 05 Ridges and Dikes
+ 0 76.20015 762.0015 355.6007 0.0 0.0
P 11 Aggregate Crushing
+ 3.0 1.0
P 12 Soil Loosening
+ 0.75
P 13 Soil Layer Mixing
+ 0.35
P 34 Change Standing Biomass Fall Rate
+ 4 3.0 2.5 2.0 1.5 1.0
+ 0.5 0.6 0.7 0.8 1.0
G 02 Biomass Manipulation
+ 1.0
P 24 Flatten Standing Biomass
+ 14 0.7 0.3 0.3 0.1 1.0
P 25 Bury Flat Biomass
+ 1 0.49 0.44 0.38 0.28 0.55
P 26 Resurface Buried Biomass
+ 0.7 0.3 0.3 0.1 1
#------------
D 18/07/02
O 03 Harvest, dig root crops res. on surf
+ 17.491838 13.752375 1.3410819 0.0 1.5645955 1.3410819 2.9056773
T Harvest, root crops like potatoes, sugar beets, carrots, and onions.
T Surface is rough with 4 ridges and much of the residue is buried.
T Rev 11-18-04 DTL RUSLE MAS 10-26-06
T
T P24 was changed to show that all residue types are flattened.
T This havest now flattens all residue types 100%.  MAS 1-18-11
T Corrected P25 decimal value "bury flat residue"  07 to 0.07:  jkp 130910
+
G 01 Tillage
+ 177.80035 1.0 1.0 177.80035 152.4003 203.20041
P 01 Break Crust
P 02 Random Roughness
+ 1 16.510033
P 05 Ridges and Dikes
+ 1 101.600204 3657.6072 3048.006 0.0 0.0
P 11 Aggregate Crushing
+ 1.4 -1.2
P 12 Soil Loosening
+ 0.7
P 13 Soil Layer Mixing
+ 0.9
P 31 Kill or Defoliate Growing Crop
+ 2
G 02 Biomass Manipulation
+ 1.0
P 62 Remove (by age pool) Plant/Residue Material
+ 1 1 0 1 1 3 2 0.0 0.0 0.0 1.0 0.0
P 40 End crop Biomass Manipulation
P 24 Flatten Standing Biomass
+ 0 1.0 1.0 1.0 1.0 1.0
P 25 Bury Flat Biomass
+ 2 0.07 .08 .1 .12 .07
P 26 Resurface Buried Biomass
+ 0.01 0.01 0.03 0.01 0.01
#------------
D 26/09/02
O 03 Disk, tandem heavy primary op
+ 7.0154433 39 2.2351363 0.0 2.2351363 1.3410819 2.6821637
T 11-12in. Spacing, Front and Rear
T Recommended for primary tillage in medium to heavy soils
T Excellent residue-handling capability. MAS 10-26-06
+
G 01 Tillage
+ 152.4003 1.0 1.0 152.4003 101.600204 177.80035
P 01 Break Crust
P 02 Random Roughness
+ 1 38.100075
P 05 Ridges and Dikes
+ 1 101.600204 279.40057 0.0 0.0 0.0
P 11 Aggregate Crushing
+ 2.8 0.75
P 12 Soil Loosening
+ 0.9
P 13 Soil Layer Mixing
+ 0.4
P 31 Kill or Defoliate Growing Crop
+ 2
P 40 End crop Biomass Manipulation
P 24 Flatten Standing Biomass
+ 0 1.0 0.9 0.8 0.5 1.0
P 25 Bury Flat Biomass
+ 1 0.95 0.85 0.8 0.6 0.95
P 26 Resurface Buried Biomass
+ 0.05 0.06 0.07 0.08 0.05
P 34 Change Standing Biomass Fall Rate
+ 7 3.0 2.5 2.0 1.5 1.0
+ 0.5 0.6 0.7 0.8 1.0
#------------
D 26/09/02
O 04 Fert applic. surface broadcast
+ 1.4966278 0.0609375
T R2 Notes: Broadcast fertilizer spreader.  Wheel traffic only.  rev 082107 DTL
T
T Added to DB 4-12-12 MAS
+
G 01 Tillage
+ 0.0 0 0.05 0.0 0.0 0.0
P 01 Break Crust
P 02 Random Roughness
+ 1 8.8900175
P 11 Aggregate Crushing
+ 4.3 2.0
P 24 Flatten Standing Biomass
+ 0 0.25 0.2 0.15 0.1 1.0
P 26 Resurface Buried Biomass
+ 0.07 0.08 0.1 0.12 0.07
P 34 Change Standing Biomass Fall Rate
+ 0 1.0 1.0 1.0 1.0 1.0
+ 1.0 1.0 1.0 1.0 1.0
#------------
D 26/09/02
O 03 Disk, tandem secondary op
+ 4.4898834 32.5 2.2351363 0.0 2.2351363 1.3410819 2.6821637
T 9-in. Spacing, Front and Rear; Good for seedbed preparation/chemical incorporation in medium to heavy soils
T Works well in primary tillage in light to medium soils
T Provides good residue-handling capability.  MAS 10-26-06
+
G 01 Tillage
+ 127.00027 0.75 1.0 127.00026 76.20015 152.4003
P 01 Break Crust
P 02 Random Roughness
+ 1 15.240031
P 05 Ridges and Dikes
+ 1 50.800102 228.60046 0.0 0.0 0.0
P 11 Aggregate Crushing
+ 2.8 0.75
P 12 Soil Loosening
+ 0.85
P 13 Soil Layer Mixing
+ 0.4
P 31 Kill or Defoliate Growing Crop
+ 2
P 40 End crop Biomass Manipulation
P 24 Flatten Standing Biomass
+ 0 0.85 0.7 0.6 0.5 1.0
P 25 Bury Flat Biomass
+ 1 0.73 0.63 0.55 0.4 0.73
P 26 Resurface Buried Biomass
+ 0.02 0.04 0.02 0.05 0.02
P 34 Change Standing Biomass Fall Rate
+ 7 3.0 2.5 2.0 1.5 1.0
+ 0.5 0.6 0.7 0.8 1.0
#------------
D 27/09/02
O 03 Drill or air seeder single disk openers 7-10 in spac
+ 3.2738733 2.44 2.2351363 0.0 2.2351363 1.5645955 2.9056773
T Drill or Air seeder with single disk no-till openers  JD 750 or similar openers. (No-till air drill)
T Based on Drill, no-till single disk 7-10 spacing. 102403 DTL. RUSLE MAS 10-26-06
T G2 was added into file in front of the flattening (P24), burial (P25), and resurfacing (P26) factors because the area affected is less than 1.0 and
T the RUSLE values were normalized to 1.0.  This change will imulate the correct residue changes based on the method set forth in RUSLE.
T RUSLE's factors have been redused to based on the area affected.
T The stalk fall rate factor (P34) was moved ahead of the new (G2) factor to set the fall rate to the less than 1.0 area affected.  8/7/07 MAS
+
G 01 Tillage
+ 63.500134 0.4 0.15 63.50013 50.800102 101.600204
P 01 Break Crust
P 02 Random Roughness
+ 1 7.6200156
P 05 Ridges and Dikes
+ 1 25.400051 203.20041 0.0 0.0 0.0
P 11 Aggregate Crushing
+ 2.8 0.75
P 12 Soil Loosening
+ 0.4
P 13 Soil Layer Mixing
+ 0.20
P 34 Change Standing Biomass Fall Rate
+ 7 3.0 2.5 2.0 1.5 1.0
+ 0.5 0.6 0.7 0.8 1.0
G 02 Biomass Manipulation
+ 1.0
P 24 Flatten Standing Biomass
+ 0 0.6 0.4 0.35 0.15 1.0
P 25 Bury Flat Biomass
+ 1 0.05 0.04 0.03 0.02 0.03
P 26 Resurface Buried Biomass
+ 0.01 0.01 0.01 0.05 0.01
G 03 Crop Name
+ Barley, winter
P 51 Seeding Configuration
+ 1 0.0 0
+ 173.0 8.0 1 50.0 1.0 1.0 0
+ bu/ac
+ 9.6 186.0 5 0.8 0.64 0.8
+ 1.0 0.025 2.0 4.0 25.0 1 270 1333.3334
+ -5.0 -15.0 0.005 0.05 0.02 30.0
+ 0.013 0.6013 0.4293 -0.086 -0.018 0.932 0.556 0.0736
+ 0.4293 -0.086 2.5 1.0 25.0 0.05 0 0.3
+ 33.333332 385.0 1.4 0.012 0.1 0.1 0.0 2
+ 0.015 0.015 0.015 0.015 0.18 0.0050 17.1 5.183335
+ -2.08165 0.548606 1.3792 0.058508374 0.0 0.0 0.0 0.0
T Adjusted the Heat Units from the 3150 down to 2400 (same as WW)
T Tested in Delaware with John Timmons run.  8-18-09  MAS
#------------
*END
*EOF
