Version: 1.5
*START 1
N Originating Program: RUSLE2
N Skel Format Version: 1.1
N This management file was originally converted from the NRCS standard XML format on - Thu Jun 28 13:58:06 PDT 2012
N This management file was updated to contain the most current crop and operation records for WEPS on - Tue Dec 17 19:18:06 CST 2013
#------------
D 08/05/01
O 03 Manure spreader, solid and semi-solid
+ 11.505327 .20 1.7881091 0.0 1.7881091 1.3410819 3.5762181
T Created from RUSLE file MAS 9/19/06.
T This assumes a defult residue type of  manure solid significant bedding and the RUSLE may contain some bedding.
T User may need to change to the correct manure type, make a calulation on the dry matter applied, and change the application rate in MCREW.
T This opn is built for an application of 10 ton/ac 60% dry matter surface applied manure.
T 10 tons x 2000 lbs/ac = 20,000 lbs/ac x 0.6 = 12,000 lbs/ac applied.
T MAS 12-5-07
+
G 01 Tillage
+ 0.0 0 1 0.0 0.0 0.0
P 24 Flatten Standing Biomass
+ 14 .1 .1 .1 .1 1.0
G 03 Crop Name
+ manure, solid, signif. bedding
P 66 Add Manure Residue Amount
+ 0.0 0.0 0.0 0.0 1
+ 0.0 0.0 0.0 0.0
+ 1.34502 0.0
+ .017 .017 .017 .017 0.169 0.0050 1 5.227942
+ -2.08165 0.548606
T Enter crop notes here.
#------------
D 11/05/01
O 03 Chisel, st. pt
+ 9.353924 45.5 2.2351363 0.0 2.2351363 1.5645955 2.9056773
T Enter Operation notes here
+
G 01 Tillage
+ 177.80035 0.75 1.0 177.80035 101.600204 203.20041
P 01 Break Crust
P 02 Random Roughness
+ 1 38.100075
P 05 Ridges and Dikes
+ 1 76.20015 381.00076 101.600204 0.0 0.0
P 11 Aggregate Crushing
+ 2.4 -2.0
P 12 Soil Loosening
+ 0.85
P 13 Soil Layer Mixing
+ 0.37
P 31 Kill or Defoliate Growing Crop
+ 2
P 40 End crop Biomass Manipulation
P 24 Flatten Standing Biomass
+ 0 0.6 0.4 0.25 0.1 1.0
P 25 Bury Flat Biomass
+ 1 0.76 0.68 0.58 0.5 0.9
P 26 Resurface Buried Biomass
+ 0.05 0.06 0.07 0.2 0.05
P 34 Change Standing Biomass Fall Rate
+ 7 3.0 2.5 2.0 1.5 1.0
+ 0.5 0.6 0.7 0.8 1.0
#------------
D 16/05/01
O 03 Planter, double disk opnr
+ 4.1157265 2.4375 2.2351363 0.0 2.2351363 1.5645955 2.9056773
T This is a standard planter on 30 in sp with a 1 in ridge.  Created in RUSLE 6/7/01.  MAS 8/7/07
T G2 was added into file in front of the flattening (P24), burial (P25), and resurfacing (P26) factors because the area affected is less than 1.0 and
T the RUSLE values were normalized to 1.0.  This change will imulate the correct residue changes based on the method set forth in RUSLE.
T RUSLE's factors have been redused to based on the area affected.
T The stalk fall rate factor (P34) was moved ahead of the new (G2) factor to set the fall rate to the less than 1.0 area affected.  8/7/07 MAS
+
G 01 Tillage
+ 63.500126 0.5 .15 63.500126 50.800102 101.600204
P 01 Break Crust
P 02 Random Roughness
+ 1 10.160021
P 05 Ridges and Dikes
+ 1 50.800102 762.0015 635.0013 0.0 0.0
P 11 Aggregate Crushing
+ 2.8 0.75
P 12 Soil Loosening
+ 0.6
P 13 Soil Layer Mixing
+ 0.35
P 34 Change Standing Biomass Fall Rate
+ 7 3.0 2.5 2.0 1.5 1.0
+ 0.5 0.6 0.7 0.8 1.0
G 02 Biomass Manipulation
+ 1.0
P 24 Flatten Standing Biomass
+ 0 .3 .25 .2 0.1 1.0
P 25 Bury Flat Biomass
+ 1 .0525 0.0375 .03 .015 .03
P 26 Resurface Buried Biomass
+ .01 .01 .01 .02 .01
G 03 Crop Name
+ Soybean, group 0 and I
P 51 Seeding Configuration
+ 1 0.0 2
+ 27.0 1.0 1 40 1.0 1.0 0
+ bu/ac
+ 13 148.7 1 0.8 0.65 0.8
+ 1.5 0.05 1.5240185 10.0 25.0 0 85 700.0
+ -5.0 -15.0 0.01 0.95 0.0 25.0
+ 0.023 0.8063 0.4146 -0.061 -0.024 0.9911 0.6435 0.0494
+ 0.4146 -0.061 2.83 1.0 26.0 0.05 0 0.5
+ 111.111115 111.111115 1.5 0.015 0.0 0.0 0.0 1
+ 0.03 0.03 0.03 0.03 0.2 0.01 20.0 5.227942
+ -1.20379 0.604887 .9 0.013450201 0.0 0.0 0.0 0.0
T RUSLE Notes: Soybeans in Maturity group 0 to group 1 in Northern cornbelt and northern Great Plains,  7 inch row spacing.   071104DTL
T This was cloned from the WEPS MG 0 file. MAS 10-19-06
T Days to mature set to lowest maturity group days from planting minus 10 days.
T group 00 is 95 days - 10 = 85 days MAS 3-21-07
T
T WEPS yields are adjusted to the middle of the yield for the group
T and different than the RUSLE records (RUSLE gives the bottom of the group).
T MAS 7/31/07
#------------
D 15/10/01
O 04 Harvest, killing crop 50pct standing stubble
+ 14.311503 .15
T ARS record - filename is:  Harvest Wheat - grain (combine cutterbar header).oprn
T This operation record is designed to represent actual field harvesting operation
T of removing the grain from small grain crops with a cutterbar head on a combine.
T This harvesting operation record removes all the reproductive component of a crop above the
T cutting height.  Typically this is specified as the "yield" component in the crop record.
T The non-harvested crop plant material above the specified cut height becomes flat residue.
T The remaining above ground crop material below the specified cut height becomes standing residue.
T Nov 02, 2005	Created - Larry Wagner
T Detailed info regarding this operation record:
T This harvest record specifies the actual cut height dependent upon the height
T of the crop.  The cut height is specified as a fraction of the crop height.
T Added 0.2 for the flatting of the combine and tire trafic for haulling grain.
T MAS 1-18-07
T The harvesting operation could also have an effect on the "standing stalk"
T fall rate and fall threshold values.  The default "biomass pool" flag parameter
T is set to "No adjustments applied" so that no "stalk residue decay rate change" will occur.
T However, this flag value can be changed along with the default parameter values
T to change the "stalk residue decay processes".
+
G 02 Biomass Manipulation
+ 1.0
P 31 Kill or Defoliate Growing Crop
+ 2
P 43 Cut/Remove Biomass by Fraction (flags)
+ 1 1 0 1 0.2 1 0 0
P 34 Change Standing Biomass Fall Rate
+ 0 1.0 1.0 1.0 1.0 1.0
+ 1.0 1.0 1.0 1.0 1.0
P 40 End crop Biomass Manipulation
P 24 Flatten Standing Biomass
+ 0 0.2 0.2 0.15 0.2 1
#------------
*END
*EOF
