Version: 1.5
*START 1
N Originating Program: RUSLE2
N Skel Format Version: 1.1
N This management file was originally converted from the NRCS standard XML format on - Thu Jun 28 13:58:31 PDT 2012
N This management file was updated to contain the most current crop and operation records for WEPS on - Tue Dec 17 19:16:29 CST 2013
#------------
D 15/05/01
O 03 Disk, tandem heavy primary op
+ 7.0154433 39 2.2351363 0.0 2.2351363 1.3410819 2.6821637
T 11-12in. Spacing, Front and Rear
T Recommended for primary tillage in medium to heavy soils
T Excellent residue-handling capability. MAS 10-26-06
+
G 01 Tillage
+ 152.4003 1.0 1.0 152.4003 101.600204 177.80035
P 01 Break Crust
P 02 Random Roughness
+ 1 38.100075
P 05 Ridges and Dikes
+ 1 101.600204 279.40057 0.0 0.0 0.0
P 11 Aggregate Crushing
+ 2.8 0.75
P 12 Soil Loosening
+ 0.9
P 13 Soil Layer Mixing
+ 0.4
P 31 Kill or Defoliate Growing Crop
+ 2
P 40 End crop Biomass Manipulation
P 24 Flatten Standing Biomass
+ 0 1.0 0.9 0.8 0.5 1.0
P 25 Bury Flat Biomass
+ 1 0.95 0.85 0.8 0.6 0.95
P 26 Resurface Buried Biomass
+ 0.05 0.06 0.07 0.08 0.05
P 34 Change Standing Biomass Fall Rate
+ 7 3.0 2.5 2.0 1.5 1.0
+ 0.5 0.6 0.7 0.8 1.0
#------------
D 25/05/01
O 03 Harrow, coiled tine
+ 4.1157265 15.6 2.6821637 0.0 2.6821637 1.3410819 3.129191
T This oprn is from a RUSLE record created 6/7/01.  10-25-06 MAS
T
T Corrected ridge height and spacing to match RUSLE2. 10-26-11 LOS
T
T Changed spacing from 0 to 1 in. The 0 caused the operation to fail.  12-12-11 MAS
+
G 01 Tillage
+ 50.800102 0.25 1.0 50.800102 25.400051 76.20015
P 01 Break Crust
P 02 Random Roughness
+ 1 10.160021
P 05 Ridges and Dikes
+ 1 25.400051 101.600204 0.0 0.0 0.0
P 11 Aggregate Crushing
+ 3.0 -0.22
P 12 Soil Loosening
+ 0.6
P 13 Soil Layer Mixing
+ 0.2
P 31 Kill or Defoliate Growing Crop
+ 2
P 40 End crop Biomass Manipulation
P 24 Flatten Standing Biomass
+ 0 0.5 0.3 0.2 0.1 1.0
P 25 Bury Flat Biomass
+ 1 0.25 0.2 0.15 0.1 0.25
P 26 Resurface Buried Biomass
+ 0.01 0.01 0.01 0.02 0.01
P 34 Change Standing Biomass Fall Rate
+ 7 3.0 2.5 2.0 1.5 1.0
+ 0.5 0.6 0.7 0.8 1.0
#------------
D 25/05/01
O 03 Plastic mulch applicator
+ 2.5255597 1.56 0.89405453 0.0 0.89405453 0.44702727 1.7881091
T Plastic mulch application covering 100% of the surface.  May include drip tape installation. 11/08/01 DTL
T
T This operation follows tillage  for crops such as strawberries and green pepers.
T Uses crop names with small letter to indicate mulch type and high mass weights of woody mulch type.
T MAS 6-9-09
+
G 01 Tillage
+ 76.20015 .1 .2 76.20015 50.800102 101.600204
P 01 Break Crust
P 02 Random Roughness
+ 1 15.240031
P 05 Ridges and Dikes
+ 1 50.800102 1422.4028 1016.002 0.0 0.0
P 11 Aggregate Crushing
+ 3.0 -0.22
P 25 Bury Flat Biomass
+ 1 0.1 0.08 0.06 0.052 0.076
P 26 Resurface Buried Biomass
+ 0.02 0.02 0.02 0.05 0.03
P 34 Change Standing Biomass Fall Rate
+ 7 3.0 2.5 2.0 1.5 1.0
+ 0.5 0.6 0.7 0.8 1.0
G 03 Crop Name
+ plastic mulch
P 65 Add Crop Residue Amounts
+ 0.0 0.0 0.0 0.22417001 4
+ 0.0 0.0 0.0 0.0
+ .0001 .0001 .0001 .001 0.169 0.0050 17.1 6.244982
+ -0.604267 0.711259
T Enter crop notes here.
#------------
D 25/05/01
O 03 Planter, transplanter, vegetable
+ 7.4831395 3.12 0.89405453 0.0 0.89405453 0.44702727 1.3410819
T G2 was added into file in front of the flattening (P24), burial (P25), and resurfacing (P26) factors because the area affected is less than 1.0 and
T the RUSLE values were normalized to 1.0.  This change will imulate the correct residue changes based on the method set forth in RUSLE.
T RUSLE's factors have been redused to based on the area affected.
T The stalk fall rate factor (P34) was moved ahead of the new (G2) factor to set the fall rate to theless than 1.0 area affected.  8/7/07 MAS
T
T Changed the P5 to allow the preexisting ridges and furrows to set the ridge roughness.  MAS  12-30-2010
+
G 01 Tillage
+ 152.4003 0.4 0.2 152.4003 101.600204 203.20041
P 01 Break Crust
P 02 Random Roughness
+ 1 10.160021
P 05 Ridges and Dikes
+ 0 50.800102 762.0015 635.0013 0.0 0.0
P 11 Aggregate Crushing
+ 2.4 2.0
P 12 Soil Loosening
+ 0.6
P 13 Soil Layer Mixing
+ 0.3
P 34 Change Standing Biomass Fall Rate
+ 7 3.0 2.5 2.0 1.5 1.0
+ 0.5 0.6 0.7 0.8 1.0
G 02 Biomass Manipulation
+ 1.0
P 24 Flatten Standing Biomass
+ 0 0.3 0.25 0.2 0.1 1.0
P 25 Bury Flat Biomass
+ 1 .07 0.05 .04 .02 .03
P 26 Resurface Buried Biomass
+ 0.01 0.01 0.01 0.02 0.01
G 03 Crop Name
+ Tomato, fresh mkt
P 51 Seeding Configuration
+ 1 0.0 2
+ 2.0 1.0 1 300 1.0 1.0 0
+ cwt/ac
+ 94.0 89.3 4 1.0 0.65 0.95
+ 0.8 0.025 1.5 10.0 27.0 0 70 750.0
+ -1.0 -4.0 0.15 0.95 0.0 30.0
+ -0.0198 0.6575 0.4807 -0.1453 -0.336 1.3726 0.5408 0.1081
+ 0.4807 -0.1453 3.08 1.0 31.1 0.01 1 1.1170388
+ 1700.0 1700.0 3.0 0.03 0.0 0.0 0.0 1
+ 0.02 0.02 0.02 0.02 0.2 0.0050 20.0 2.7
+ -1.20379 0.604887 0.0767 0.012329351 0.0 0.0 0.0 0.0
T This records comes from ARS tomato transplant record and has the yield,
T Residue yield ration and the yield intercept changed to RUSLE values MAS 3-6-07
T Made changes as Fred instructed, mass of planting MAS 3/15/07
#------------
D 15/09/01
O 04 Harvest, hand pick
+ 3.2738733 0.15
T Hand pick lettuce or similar crops or to represent one final picking of fruit or berry crops.
T Do not use for multiple pickings of fruit or berry crops unless a regrowth vegetation file representing
T regrowth between pickings is available in the database to be called in.
T This is not the case for strawberries.  12132011 DTL
T Added 3/29/07 MAS
T Reworked the values MAS 2-24-09
T Added the change to flat on the crop type.  8-27-10
T This operation takes all of the yield, and can be used to calibrate the yield. 12-27-11 MAS
T Adjusted the Energy use to 0.000000010 gal/ac  2-23-12
T
T Changed the fuel use from 0.000000010 to 0.36 g/ac 4-17-12 MAS
+
G 02 Biomass Manipulation
+ 1.0
P 31 Kill or Defoliate Growing Crop
+ 0
P 62 Remove (by age pool) Plant/Residue Material
+ 1 1 0 1 3 3 2 1.0 0.0 0.0 0.0 0.0
P 40 End crop Biomass Manipulation
#------------
D 20/09/01
O 04 Kill crop
+ 0.0 0
T Enter Operation notes here
+
G 02 Biomass Manipulation
+ 1.0
P 31 Kill or Defoliate Growing Crop
+ 2
P 40 End crop Biomass Manipulation
#------------
D 20/09/01
O 04 Plastic mulch, remove
+ 3.6480303 .52
T Added a kill crop process to cause the crop residue to be changed after the picking operations  MAS 1-22-08
+
G 02 Biomass Manipulation
+ 1
P 62 Remove (by age pool) Plant/Residue Material
+ 0 0 1 0 2 4 2 1 1 1 0 0
P 31 Kill or Defoliate Growing Crop
+ 2
P 40 End crop Biomass Manipulation
#------------
D 25/09/01
O 03 Manure spreader, solid and semi-solid
+ 11.505327 .20 1.7881091 0.0 1.7881091 1.3410819 3.5762181
T Created from RUSLE file MAS 9/19/06.
T This assumes a defult residue type of  manure solid significant bedding and the RUSLE may contain some bedding.
T User may need to change to the correct manure type, make a calulation on the dry matter applied, and change the application rate in MCREW.
T This opn is built for an application of 10 ton/ac 60% dry matter surface applied manure.
T 10 tons x 2000 lbs/ac = 20,000 lbs/ac x 0.6 = 12,000 lbs/ac applied.
T MAS 12-5-07
+
G 01 Tillage
+ 0.0 0 1 0.0 0.0 0.0
P 24 Flatten Standing Biomass
+ 14 .1 .1 .1 .1 1.0
G 03 Crop Name
+ manure, solid, signif. bedding
P 66 Add Manure Residue Amount
+ 0.0 0.0 0.0 0.0 1
+ 0.0 0.0 0.0 0.0
+ 1.34502 0.0
+ .017 .017 .017 .017 0.169 0.0050 1 5.227942
+ -2.08165 0.548606
T Enter crop notes here.
#------------
D 25/09/01
O 03 Disk, tandem light finishing
+ 3.7415698 19.5 2.2351363 0.0 2.2351363 1.3410819 2.6821637
T 6/8/01 DTL RUSLE.  7in sp.  This is tool used to finish a seedbed.  MAS 10-26-06
+
G 01 Tillage
+ 101.600204 0.5 1.0 101.600204 76.20015 127.00026
P 01 Break Crust
P 02 Random Roughness
+ 1 15.240031
P 05 Ridges and Dikes
+ 1 12.700026 177.80035 0.0 0.0 0.0
P 11 Aggregate Crushing
+ 2.8 0.75
P 12 Soil Loosening
+ 0.75
P 13 Soil Layer Mixing
+ 0.35
P 31 Kill or Defoliate Growing Crop
+ 2
P 40 End crop Biomass Manipulation
P 24 Flatten Standing Biomass
+ 0 0.85 0.7 0.6 0.5 1.0
P 25 Bury Flat Biomass
+ 1 0.73 0.63 0.55 0.4 0.73
P 26 Resurface Buried Biomass
+ 0.02 0.04 0.02 0.05 0.02
P 34 Change Standing Biomass Fall Rate
+ 7 3.0 2.5 2.0 1.5 1.0
+ 0.5 0.6 0.7 0.8 1.0
#------------
D 25/09/01
O 04 Planting, broadcast seeder
+ 1.2160101 .15
T Broadcast seeding. Begins growth .    11/30/01 DTL
T No tillage processes added. MAS 3-28-07
+
G 03 Crop Name
+ Rye, winter cover
P 51 Seeding Configuration
+ 1 0.0 0
+ 220.0 8.0 0 2240 1.0 1.0 2
+ lbs/ac
+ 0 8930 5 1.0 0.6 0.8
+ 1.2 0.025 1.2192148 0.0 25.0 1 60 1472.2223
+ -5.0 -15.0 0.005 0.05 0.035 30.0
+ 0.013 0.8013 0.4293 -0.086 -0.018 0.932 0.556 0.0736
+ 0.3293 -0.086 2.87 1.0 20.0 0.05 0 0.3
+ 28.571428 335.0 1.4 0.012 0.1 0.1 0.0 2
+ 0.0133 0.0133 0.0133 0.0133 0.12 0.0050 17.1 5.227942
+ -2.08165 0.548606 0 0.0 0.0 0.0 0.0 0.0
T RUSLE Notes: Rye, as winter cover. Killed in vegetative stage the following spring.
T Decomposition  0.017 like grass forages. Rev 021705 DTL
T
T Cloned 2-16-07 MAS
T Lowered the heat units from 3600 to 2650 to match the core crop runs for OK  MAS 10-29-08
#------------
*END
*EOF
