Version: 1.5
*START 1
N Originating Program: RUSLE2
N Skel Format Version: 1.1
N This management file was originally converted from the NRCS standard XML format on - Thu Jun 28 13:58:01 PDT 2012
N This management file was updated to contain the most current crop and operation records for WEPS on - Tue Dec 17 19:18:32 CST 2013
#------------
D 25/04/01
O 03 Manure spreader, solid and semi-solid
+ 11.505327 .20 1.7881091 0.0 1.7881091 1.3410819 3.5762181
T Created from RUSLE file MAS 9/19/06.
T This assumes a defult residue type of  manure solid significant bedding and the RUSLE may contain some bedding.
T User may need to change to the correct manure type, make a calulation on the dry matter applied, and change the application rate in MCREW.
T This opn is built for an application of 10 ton/ac 60% dry matter surface applied manure.
T 10 tons x 2000 lbs/ac = 20,000 lbs/ac x 0.6 = 12,000 lbs/ac applied.
T MAS 12-5-07
+
G 01 Tillage
+ 0.0 0 1 0.0 0.0 0.0
P 24 Flatten Standing Biomass
+ 14 .1 .1 .1 .1 1.0
G 03 Crop Name
+ manure, solid, signif. bedding
P 66 Add Manure Residue Amount
+ 0.0 0.0 0.0 0.0 1
+ 0.0 0.0 0.0 0.0
+ 1.34502 0.0
+ .017 .017 .017 .017 0.169 0.0050 1 5.227942
+ -2.08165 0.548606
T Enter crop notes here.
#------------
D 30/04/01
O 03 Disk, tandem heavy primary op
+ 7.0154433 39 2.2351363 0.0 2.2351363 1.3410819 2.6821637
T 11-12in. Spacing, Front and Rear
T Recommended for primary tillage in medium to heavy soils
T Excellent residue-handling capability. MAS 10-26-06
+
G 01 Tillage
+ 152.4003 1.0 1.0 152.4003 101.600204 177.80035
P 01 Break Crust
P 02 Random Roughness
+ 1 38.100075
P 05 Ridges and Dikes
+ 1 101.600204 279.40057 0.0 0.0 0.0
P 11 Aggregate Crushing
+ 2.8 0.75
P 12 Soil Loosening
+ 0.9
P 13 Soil Layer Mixing
+ 0.4
P 31 Kill or Defoliate Growing Crop
+ 2
P 40 End crop Biomass Manipulation
P 24 Flatten Standing Biomass
+ 0 1.0 0.9 0.8 0.5 1.0
P 25 Bury Flat Biomass
+ 1 0.95 0.85 0.8 0.6 0.95
P 26 Resurface Buried Biomass
+ 0.05 0.06 0.07 0.08 0.05
P 34 Change Standing Biomass Fall Rate
+ 7 3.0 2.5 2.0 1.5 1.0
+ 0.5 0.6 0.7 0.8 1.0
#------------
D 05/05/01
O 03 Harrow, coiled tine
+ 4.1157265 15.6 2.6821637 0.0 2.6821637 1.3410819 3.129191
T This oprn is from a RUSLE record created 6/7/01.  10-25-06 MAS
T
T Corrected ridge height and spacing to match RUSLE2. 10-26-11 LOS
T
T Changed spacing from 0 to 1 in. The 0 caused the operation to fail.  12-12-11 MAS
+
G 01 Tillage
+ 50.800102 0.25 1.0 50.800102 25.400051 76.20015
P 01 Break Crust
P 02 Random Roughness
+ 1 10.160021
P 05 Ridges and Dikes
+ 1 25.400051 101.600204 0.0 0.0 0.0
P 11 Aggregate Crushing
+ 3.0 -0.22
P 12 Soil Loosening
+ 0.6
P 13 Soil Layer Mixing
+ 0.2
P 31 Kill or Defoliate Growing Crop
+ 2
P 40 End crop Biomass Manipulation
P 24 Flatten Standing Biomass
+ 0 0.5 0.3 0.2 0.1 1.0
P 25 Bury Flat Biomass
+ 1 0.25 0.2 0.15 0.1 0.25
P 26 Resurface Buried Biomass
+ 0.01 0.01 0.01 0.02 0.01
P 34 Change Standing Biomass Fall Rate
+ 7 3.0 2.5 2.0 1.5 1.0
+ 0.5 0.6 0.7 0.8 1.0
#------------
D 05/05/01
O 03 Drill or airseeder, double disk
+ 3.3674128 6.34 2.2351363 0.0 2.2351363 1.5645955 2.9056773
T Drill or air seeder with double disk openers on 7 to 10 inch spacings.  Rev102403 DTL  RUSLE MAS 10-26-06
T G2 was added into file in front of the flattening (P24), burial (P25), and resurfacing (P26) factors because the area affected is less than 1.0 and
T the RUSLE values were normalized to 1.0.  This change will imulate the correct residue changes based on the method set forth in RUSLE.
T RUSLE's factors have been redused to based on the area affected.
T The stalk fall rate factor (P34) was moved ahead of the new (G2) factor to set the fall rate to the  less than 1.0 area affected.  8/8/07 MAS
T
T Deleted the G2 process because all process only affect 0.65 of the surface.  This is set a 0.65 with G1 process in the beginning. 5-11-11 MAS
+ 
G 01 Tillage
+ 38.100075 0.4 0.65 38.100075 25.400051 50.800102
P 01 Break Crust
P 02 Random Roughness
+ 1 7.6200156
P 05 Ridges and Dikes
+ 1 25.400051 203.20041 25.400051 0.0 0.0
P 11 Aggregate Crushing
+ 2.8 0.75
P 12 Soil Loosening
+ 0.6
P 13 Soil Layer Mixing
+ 0.3
P 34 Change Standing Biomass Fall Rate
+ 7 3.0 2.5 2.0 1.5 1.0
+ 0.5 0.6 0.7 0.8 1.0
P 24 Flatten Standing Biomass
+ 0 0.6 0.4 0.35 0.15 1.0
P 25 Bury Flat Biomass
+ 1 0.2275 0.1625 0.13 0.065 0.13
P 26 Resurface Buried Biomass
+ 0.01 0.01 0.01 0.02 0.01
G 03 Crop Name
+ Barley, spring, hay
P 51 Seeding Configuration
+ 1 0.0 0
+ 173.0 8.0 0 2 1 1.0 2
+ ton/ac
+ 15 4.465 6 0.8 0.64 0.8
+ 1.0 0.025 0.91441107 1.6666667 25.0 0 120 1750.0
+ -5.0 -15.0 0.001 0.01 0.0 30.0
+ 0.013 0.6013 0.4293 -0.086 -0.018 0.932 0.556 0.0736
+ 0.4293 -0.086 2.5 1.0 25.0 0.05 0 0.3
+ 33.333332 385.0 1.4 0.012 0.1 0.1 0.0 2
+ 0.015 0.015 0.015 0.015 0.18 0.0050 17.1 5.227942
+ -2.08165 0.548606 0 0.0 0.0 0.0 0.0 0.0
T Cloned from spring barley, changed yield and harvest index to Alfalfa hay 10-1-06 MAS
T
T Spring oats hay 2.5 ton/ac yield based on Spring oats Core  Revised for RUSLE2 12/29/00 DTL REV 61801 DTL
T Rev growth curve and yield and residue :yield ratio 032907 DTL
T
T In response to poor growth in Alamosa, Co., (with consultation with Fred Fox, ARS),
T Crop growth was annual spring crop and now is Perennial pasture (to get it to regrow after cutting),
T Min Temp was change from 39 to 35 degrees F; Maturity was changed from HU to 120 days;
T Fraction of leaf mass partition was changed from 0 to 0.1;  and Fraction of stem mass partition was changed from 0 to 0.1.
T Crop now grows in the two cut example from CO.  MAS 11-7-11
#------------
D 15/07/01
O 04 Harvest, killing crop 50pct standing stubble
+ 14.311503 .15
T ARS record - filename is:  Harvest Wheat - grain (combine cutterbar header).oprn
T This operation record is designed to represent actual field harvesting operation
T of removing the grain from small grain crops with a cutterbar head on a combine.
T This harvesting operation record removes all the reproductive component of a crop above the
T cutting height.  Typically this is specified as the "yield" component in the crop record.
T The non-harvested crop plant material above the specified cut height becomes flat residue.
T The remaining above ground crop material below the specified cut height becomes standing residue.
T Nov 02, 2005	Created - Larry Wagner
T Detailed info regarding this operation record:
T This harvest record specifies the actual cut height dependent upon the height
T of the crop.  The cut height is specified as a fraction of the crop height.
T Added 0.2 for the flatting of the combine and tire trafic for haulling grain.
T MAS 1-18-07
T The harvesting operation could also have an effect on the "standing stalk"
T fall rate and fall threshold values.  The default "biomass pool" flag parameter
T is set to "No adjustments applied" so that no "stalk residue decay rate change" will occur.
T However, this flag value can be changed along with the default parameter values
T to change the "stalk residue decay processes".
+
G 02 Biomass Manipulation
+ 1.0
P 31 Kill or Defoliate Growing Crop
+ 2
P 43 Cut/Remove Biomass by Fraction (flags)
+ 1 1 0 1 0.2 1 0 0
P 34 Change Standing Biomass Fall Rate
+ 0 1.0 1.0 1.0 1.0 1.0
+ 1.0 1.0 1.0 1.0 1.0
P 40 End crop Biomass Manipulation
P 24 Flatten Standing Biomass
+ 0 0.2 0.2 0.15 0.2 1
#------------
D 15/07/01
O 03 Plow, moldboard
+ 17.491838 65 2.2351363 0.0 2.2351363 1.5645955 2.6821637
T Moldboard plow 8 inch operating depth.  060701 DTL  Modified flattening and burial per McCool and Foster 05/21/02 DTL RUSLE MAS 10-26-06
+
G 01 Tillage
+ 203.20041 1.0 1.0 203.20041 152.4003 254.0005
P 01 Break Crust
P 02 Random Roughness
+ 1 48.260098
P 05 Ridges and Dikes
+ 1 25.400051 406.40082 0.0 0.0 0.0
P 11 Aggregate Crushing
+ 2.8 1.0
P 12 Soil Loosening
+ 1.0
P 13 Soil Layer Mixing
+ 0.7
P 14 Soil Layer Inversion
P 31 Kill or Defoliate Growing Crop
+ 2
P 40 End crop Biomass Manipulation
P 24 Flatten Standing Biomass
+ 0 1 1 1 0.75 1.0
P 25 Bury Flat Biomass
+ 3 0.99 0.99 0.99 0.85 0.97
P 26 Resurface Buried Biomass
+ 0.01 0.02 0.04 0.1 0.02
P 34 Change Standing Biomass Fall Rate
+ 7 3.0 2.5 2.0 1.5 1.0
+ 0.5 0.6 0.7 0.8 1.0
#------------
*END
*EOF
