Version: 1.5
*START 10
N Originating Program: RUSLE2
N Skel Format Version: 1.1
N This management file was originally converted from the NRCS standard XML format on - Thu Jun 28 13:59:09 PDT 2012
N This management file was updated to contain the most current crop and operation records for WEPS on - Tue Dec 17 19:15:06 CST 2013
#------------
D 08/05/01
O 03 Manure spreader, solid and semi-solid
+ 11.505327 .20 1.7881091 0.0 1.7881091 1.3410819 3.5762181
T Created from RUSLE file MAS 9/19/06.
T This assumes a defult residue type of  manure solid significant bedding and the RUSLE may contain some bedding.
T User may need to change to the correct manure type, make a calulation on the dry matter applied, and change the application rate in MCREW.
T This opn is built for an application of 10 ton/ac 60% dry matter surface applied manure.
T 10 tons x 2000 lbs/ac = 20,000 lbs/ac x 0.6 = 12,000 lbs/ac applied.
T MAS 12-5-07
+
G 01 Tillage
+ 0.0 0 1 0.0 0.0 0.0
P 24 Flatten Standing Biomass
+ 14 .1 .1 .1 .1 1.0
G 03 Crop Name
+ manure, solid, signif. bedding
P 66 Add Manure Residue Amount
+ 0.0 0.0 0.0 0.0 1
+ 0.0 0.0 0.0 0.0
+ 1.34502 0.0
+ .017 .017 .017 .017 0.169 0.0050 1 5.227942
+ -2.08165 0.548606
T Enter crop notes here.
#------------
D 11/05/01
O 03 Disk, tandem heavy primary op
+ 7.0154433 39 2.2351363 0.0 2.2351363 1.3410819 2.6821637
T 11-12in. Spacing, Front and Rear
T Recommended for primary tillage in medium to heavy soils
T Excellent residue-handling capability. MAS 10-26-06
+
G 01 Tillage
+ 152.4003 1.0 1.0 152.4003 101.600204 177.80035
P 01 Break Crust
P 02 Random Roughness
+ 1 38.100075
P 05 Ridges and Dikes
+ 1 101.600204 279.40057 0.0 0.0 0.0
P 11 Aggregate Crushing
+ 2.8 0.75
P 12 Soil Loosening
+ 0.9
P 13 Soil Layer Mixing
+ 0.4
P 31 Kill or Defoliate Growing Crop
+ 2
P 40 End crop Biomass Manipulation
P 24 Flatten Standing Biomass
+ 0 1.0 0.9 0.8 0.5 1.0
P 25 Bury Flat Biomass
+ 1 0.95 0.85 0.8 0.6 0.95
P 26 Resurface Buried Biomass
+ 0.05 0.06 0.07 0.08 0.05
P 34 Change Standing Biomass Fall Rate
+ 7 3.0 2.5 2.0 1.5 1.0
+ 0.5 0.6 0.7 0.8 1.0
#------------
D 16/05/01
O 03 Disk, tandem light finishing
+ 3.7415698 19.5 2.2351363 0.0 2.2351363 1.3410819 2.6821637
T 6/8/01 DTL RUSLE.  7in sp.  This is tool used to finish a seedbed.  MAS 10-26-06
+
G 01 Tillage
+ 101.600204 0.5 1.0 101.600204 76.20015 127.00026
P 01 Break Crust
P 02 Random Roughness
+ 1 15.240031
P 05 Ridges and Dikes
+ 1 12.700026 177.80035 0.0 0.0 0.0
P 11 Aggregate Crushing
+ 2.8 0.75
P 12 Soil Loosening
+ 0.75
P 13 Soil Layer Mixing
+ 0.35
P 31 Kill or Defoliate Growing Crop
+ 2
P 40 End crop Biomass Manipulation
P 24 Flatten Standing Biomass
+ 0 0.85 0.7 0.6 0.5 1.0
P 25 Bury Flat Biomass
+ 1 0.73 0.63 0.55 0.4 0.73
P 26 Resurface Buried Biomass
+ 0.02 0.04 0.02 0.05 0.02
P 34 Change Standing Biomass Fall Rate
+ 7 3.0 2.5 2.0 1.5 1.0
+ 0.5 0.6 0.7 0.8 1.0
#------------
D 16/05/01
O 03 Fert applic. shank low disturbance, 12 in
+ 8.418531 3.25 2.2351363 0.0 2.2351363 1.5645955 2.9056773
T Minimum disturbance fertilizer injector shank.012904 DTL RUSLE MAS 10-26-06
T G2 was added into file in front of the flattening (P24), burial (P25), and resurfacing (P26) factors because the area affected is less than 1.0 and
T the RUSLE values were normalized to 1.0.  This change will imulate the correct residue changes based on the method set forth in RUSLE.
T RUSLE's factors have been redused to based on the area affected.
T The stalk fall rate factor (P34) was moved ahead of the new (G2) factor to set the fall rate to the less than 1.0 area affected.  8/7/07 MAS
+ 
G 01 Tillage
+ 101.600204 0.8 0.25 101.600204 76.20015 152.4003
P 01 Break Crust
P 02 Random Roughness
+ 1 15.240031
P 05 Ridges and Dikes
+ 1 50.800102 304.8006 25.400051 0.0 0.0
P 11 Aggregate Crushing
+ 2.4 2.0
P 12 Soil Loosening
+ 0.7
P 13 Soil Layer Mixing
+ 0.2
P 40 End crop Biomass Manipulation
P 34 Change Standing Biomass Fall Rate
+ 7 3.0 2.5 2.0 1.5 1.0
+ 0.5 0.6 0.7 0.8 1.0
P 24 Flatten Standing Biomass
+ 0 0.5 0.45 0.4 0.4 1.0
P 25 Bury Flat Biomass
+ 4 0.2 .15 .1 0.08 0.14
P 26 Resurface Buried Biomass
+ 0.06 0.06 0.06 0.1 0.06
#------------
D 16/05/01
O 03 Planter, double disk opnr
+ 4.1157265 2.4375 2.2351363 0.0 2.2351363 1.5645955 2.9056773
T This is a standard planter on 30 in sp with a 1 in ridge.  Created in RUSLE 6/7/01.  MAS 8/7/07
T G2 was added into file in front of the flattening (P24), burial (P25), and resurfacing (P26) factors because the area affected is less than 1.0 and
T the RUSLE values were normalized to 1.0.  This change will imulate the correct residue changes based on the method set forth in RUSLE.
T RUSLE's factors have been redused to based on the area affected.
T The stalk fall rate factor (P34) was moved ahead of the new (G2) factor to set the fall rate to the less than 1.0 area affected.  8/7/07 MAS
+
G 01 Tillage
+ 63.500126 0.5 .15 63.500126 50.800102 101.600204
P 01 Break Crust
P 02 Random Roughness
+ 1 10.160021
P 05 Ridges and Dikes
+ 1 50.800102 762.0015 635.0013 0.0 0.0
P 11 Aggregate Crushing
+ 2.8 0.75
P 12 Soil Loosening
+ 0.6
P 13 Soil Layer Mixing
+ 0.35
P 34 Change Standing Biomass Fall Rate
+ 7 3.0 2.5 2.0 1.5 1.0
+ 0.5 0.6 0.7 0.8 1.0
G 02 Biomass Manipulation
+ 1.0
P 24 Flatten Standing Biomass
+ 0 .3 .25 .2 0.1 1.0
P 25 Bury Flat Biomass
+ 1 .0525 0.0375 .03 .015 .03
P 26 Resurface Buried Biomass
+ .01 .01 .01 .02 .01
G 03 Crop Name
+ Corn, silage
P 51 Seeding Configuration
+ 1 0.0 2
+ 6.0 1.0 1 23 1.0 1.0 2
+ ton/ac
+ 65.0 4.465 4 1.0 0.65 0.8
+ 2.5 0.05 1.5240185 10.0 30.0 0 100 1700.0
+ -5.0 -15.0 0.01 0.05 0.0 40.0
+ 0.0031 0.9233 0.3266 -0.044 0.0 0.976 0.511 0.0287
+ 0.3266 -0.044 0.22259772 0.72 17.4 0.05 0 0.9
+ 333.33334 333.33334 3.0 0.03 0.0 0.0 0.0 3
+ 0.016 0.016 0.016 0.01 0.153 0.01 20.0 3.3812115
+ -1.20379 0.604887 0.3081 0.21615593 0.0 0.0 0.0 0.0
T corn silage 23 ton yield, 30" rows  Columbia, Mo DTL
T
T This record was cloned from ARS records and the revenant data adjusted to RUSLE values.
T The Biomass Conv Factor was changed from 40 to 47 based on runs made in Clovis, NM with full irrigation.
T MAS 9-27-07
T
T R2 Note - Rev residue : yield ratio 091108 DTL with 35% dry matter content. rev biomass-yield ratio 032012 DTL
T
T Added the Yield intercept and Res:Yield ratio. 
T If a cover crop is inter planted into Corn, silage users must use a harvest that call in a growing
T cover crop.  Only one crop can be grown at a time in WEPS. 4-3-12 MAS
#------------
D 22/09/01
O 04 Harvest, silage, release cover crop
+ 8.886228 .15
T This record cuts and removes a crop to a height, kills the crop, then calls in another crop file to start or continue the growth of
T an existing cover crop.  It cuts to a 5 in ht. MAS 6-30-08
T
T This harvest record specifies the actual cut height dependent upon the height
T of the crop.  The cut height is specified as a fraction of the crop height.
T Added 0.2 for the flatting of the combine and tire trafic for haulling grain.
T MAS 1-18-07
T
T ARS record - filename is:  Harvest Wheat - grain (combine cutterbar header).oprn
T This operation record is designed to represent actual field harvesting operation
T of removing the grain from small grain crops with a cutterbar head on a combine.
T This harvesting operation record removes all the reproductive component of a crop above the
T cutting height.  Typically this is specified as the "yield" component in the crop record.
T The non-harvested crop plant material above the specified cut height becomes flat residue.
T The remaining above ground crop material below the specified cut height becomes standing residue.
T Nov 02, 2005	Created - Larry Wagner
T Detailed info regarding this operation record:
T
T The harvesting operation could also have an effect on the "standing stalk"
T fall rate and fall threshold values.  The default "biomass pool" flag parameter
T is set to "No adjustments applied" so that no "stalk residue decay rate change" will occur.
T However, this flag value can be changed along with the default parameter values
T to change the "stalk residue decay processes".
+
G 02 Biomass Manipulation
+ 1.0
P 31 Kill or Defoliate Growing Crop
+ 2
P 42 Cut/Remove Biomass to Height (flags)
+ 1 1 0 1 0 127.00025 1 1 1
P 34 Change Standing Biomass Fall Rate
+ 0 1.0 1.0 1.0 1.0 1.0
+ 1.0 1.0 1.0 1.0 1.0
P 40 End crop Biomass Manipulation
P 24 Flatten Standing Biomass
+ 0 0.2 0.2 0.2 0.2 1
G 03 Crop Name
+ Ryegrass, annual, forage
P 51 Seeding Configuration
+ 1 0.0 0
+ 400.0 1 0 2000 1.0 1.0 2
+ lbs/ac
+ 0 8930.0 4 1.0 0.6 0.8
+ 1.2 0.025 1.2192148 0.0 25.0 1 100 1800.0
+ -5.0 -15.0 0.005 0.05 0.035 30.0
+ 0.013 0.8013 0.4293 -0.086 -0.018 0.932 0.556 0.0736
+ 0.3293 -0.086 2.87 1.0 20.0 0.05 0 0.3
+ 28.571428 335.0 1.4 0.012 0.1 0.1 0.0 2
+ 0.0133 0.0133 0.0133 0.0133 0.12 0.0050 17.1 5.227942
+ -2.08165 0.548606 0 0.0 0.0 0.0 0.0 0.0
T Rusle Notes: Winter wheat cover.   Drilled in 7 inch rows.   Chemically killed  in late boot stage.  Not harvested for grain.
T Base location Columbia, MO. REV 61901 DTL
T
T Not calibrated grown on heat units.
T
T Cloned from WW cover file. 12-26-07 MAS
#------------
D 08/05/02
O 03 Manure spreader, solid and semi-solid
+ 11.505327 .20 1.7881091 0.0 1.7881091 1.3410819 3.5762181
T Created from RUSLE file MAS 9/19/06.
T This assumes a defult residue type of  manure solid significant bedding and the RUSLE may contain some bedding.
T User may need to change to the correct manure type, make a calulation on the dry matter applied, and change the application rate in MCREW.
T This opn is built for an application of 10 ton/ac 60% dry matter surface applied manure.
T 10 tons x 2000 lbs/ac = 20,000 lbs/ac x 0.6 = 12,000 lbs/ac applied.
T MAS 12-5-07
+
G 01 Tillage
+ 0.0 0 1 0.0 0.0 0.0
P 24 Flatten Standing Biomass
+ 14 .1 .1 .1 .1 1.0
G 03 Crop Name
+ manure, solid, signif. bedding
P 66 Add Manure Residue Amount
+ 0.0 0.0 0.0 0.0 1
+ 0.0 0.0 0.0 0.0
+ 1.34502 0.0
+ .017 .017 .017 .017 0.169 0.0050 1 5.227942
+ -2.08165 0.548606
T Enter crop notes here.
#------------
D 11/05/02
O 03 Disk, tandem heavy primary op
+ 7.0154433 39 2.2351363 0.0 2.2351363 1.3410819 2.6821637
T 11-12in. Spacing, Front and Rear
T Recommended for primary tillage in medium to heavy soils
T Excellent residue-handling capability. MAS 10-26-06
+
G 01 Tillage
+ 152.4003 1.0 1.0 152.4003 101.600204 177.80035
P 01 Break Crust
P 02 Random Roughness
+ 1 38.100075
P 05 Ridges and Dikes
+ 1 101.600204 279.40057 0.0 0.0 0.0
P 11 Aggregate Crushing
+ 2.8 0.75
P 12 Soil Loosening
+ 0.9
P 13 Soil Layer Mixing
+ 0.4
P 31 Kill or Defoliate Growing Crop
+ 2
P 40 End crop Biomass Manipulation
P 24 Flatten Standing Biomass
+ 0 1.0 0.9 0.8 0.5 1.0
P 25 Bury Flat Biomass
+ 1 0.95 0.85 0.8 0.6 0.95
P 26 Resurface Buried Biomass
+ 0.05 0.06 0.07 0.08 0.05
P 34 Change Standing Biomass Fall Rate
+ 7 3.0 2.5 2.0 1.5 1.0
+ 0.5 0.6 0.7 0.8 1.0
#------------
D 16/05/02
O 03 Disk, tandem light finishing
+ 3.7415698 19.5 2.2351363 0.0 2.2351363 1.3410819 2.6821637
T 6/8/01 DTL RUSLE.  7in sp.  This is tool used to finish a seedbed.  MAS 10-26-06
+
G 01 Tillage
+ 101.600204 0.5 1.0 101.600204 76.20015 127.00026
P 01 Break Crust
P 02 Random Roughness
+ 1 15.240031
P 05 Ridges and Dikes
+ 1 12.700026 177.80035 0.0 0.0 0.0
P 11 Aggregate Crushing
+ 2.8 0.75
P 12 Soil Loosening
+ 0.75
P 13 Soil Layer Mixing
+ 0.35
P 31 Kill or Defoliate Growing Crop
+ 2
P 40 End crop Biomass Manipulation
P 24 Flatten Standing Biomass
+ 0 0.85 0.7 0.6 0.5 1.0
P 25 Bury Flat Biomass
+ 1 0.73 0.63 0.55 0.4 0.73
P 26 Resurface Buried Biomass
+ 0.02 0.04 0.02 0.05 0.02
P 34 Change Standing Biomass Fall Rate
+ 7 3.0 2.5 2.0 1.5 1.0
+ 0.5 0.6 0.7 0.8 1.0
#------------
D 16/05/02
O 03 Fert applic. shank low disturbance, 12 in
+ 8.418531 3.25 2.2351363 0.0 2.2351363 1.5645955 2.9056773
T Minimum disturbance fertilizer injector shank.012904 DTL RUSLE MAS 10-26-06
T G2 was added into file in front of the flattening (P24), burial (P25), and resurfacing (P26) factors because the area affected is less than 1.0 and
T the RUSLE values were normalized to 1.0.  This change will imulate the correct residue changes based on the method set forth in RUSLE.
T RUSLE's factors have been redused to based on the area affected.
T The stalk fall rate factor (P34) was moved ahead of the new (G2) factor to set the fall rate to the less than 1.0 area affected.  8/7/07 MAS
+ 
G 01 Tillage
+ 101.600204 0.8 0.25 101.600204 76.20015 152.4003
P 01 Break Crust
P 02 Random Roughness
+ 1 15.240031
P 05 Ridges and Dikes
+ 1 50.800102 304.8006 25.400051 0.0 0.0
P 11 Aggregate Crushing
+ 2.4 2.0
P 12 Soil Loosening
+ 0.7
P 13 Soil Layer Mixing
+ 0.2
P 40 End crop Biomass Manipulation
P 34 Change Standing Biomass Fall Rate
+ 7 3.0 2.5 2.0 1.5 1.0
+ 0.5 0.6 0.7 0.8 1.0
P 24 Flatten Standing Biomass
+ 0 0.5 0.45 0.4 0.4 1.0
P 25 Bury Flat Biomass
+ 4 0.2 .15 .1 0.08 0.14
P 26 Resurface Buried Biomass
+ 0.06 0.06 0.06 0.1 0.06
#------------
D 16/05/02
O 03 Planter, double disk opnr
+ 4.1157265 2.4375 2.2351363 0.0 2.2351363 1.5645955 2.9056773
T This is a standard planter on 30 in sp with a 1 in ridge.  Created in RUSLE 6/7/01.  MAS 8/7/07
T G2 was added into file in front of the flattening (P24), burial (P25), and resurfacing (P26) factors because the area affected is less than 1.0 and
T the RUSLE values were normalized to 1.0.  This change will imulate the correct residue changes based on the method set forth in RUSLE.
T RUSLE's factors have been redused to based on the area affected.
T The stalk fall rate factor (P34) was moved ahead of the new (G2) factor to set the fall rate to the less than 1.0 area affected.  8/7/07 MAS
+
G 01 Tillage
+ 63.500126 0.5 .15 63.500126 50.800102 101.600204
P 01 Break Crust
P 02 Random Roughness
+ 1 10.160021
P 05 Ridges and Dikes
+ 1 50.800102 762.0015 635.0013 0.0 0.0
P 11 Aggregate Crushing
+ 2.8 0.75
P 12 Soil Loosening
+ 0.6
P 13 Soil Layer Mixing
+ 0.35
P 34 Change Standing Biomass Fall Rate
+ 7 3.0 2.5 2.0 1.5 1.0
+ 0.5 0.6 0.7 0.8 1.0
G 02 Biomass Manipulation
+ 1.0
P 24 Flatten Standing Biomass
+ 0 .3 .25 .2 0.1 1.0
P 25 Bury Flat Biomass
+ 1 .0525 0.0375 .03 .015 .03
P 26 Resurface Buried Biomass
+ .01 .01 .01 .02 .01
G 03 Crop Name
+ Corn, silage
P 51 Seeding Configuration
+ 1 0.0 2
+ 6.0 1.0 1 23 1.0 1.0 2
+ ton/ac
+ 65.0 4.465 4 1.0 0.65 0.8
+ 2.5 0.05 1.5240185 10.0 30.0 0 100 1700.0
+ -5.0 -15.0 0.01 0.05 0.0 40.0
+ 0.0031 0.9233 0.3266 -0.044 0.0 0.976 0.511 0.0287
+ 0.3266 -0.044 0.22259772 0.72 17.4 0.05 0 0.9
+ 333.33334 333.33334 3.0 0.03 0.0 0.0 0.0 3
+ 0.016 0.016 0.016 0.01 0.153 0.01 20.0 3.3812115
+ -1.20379 0.604887 0.3081 0.21615593 0.0 0.0 0.0 0.0
T corn silage 23 ton yield, 30" rows  Columbia, Mo DTL
T
T This record was cloned from ARS records and the revenant data adjusted to RUSLE values.
T The Biomass Conv Factor was changed from 40 to 47 based on runs made in Clovis, NM with full irrigation.
T MAS 9-27-07
T
T R2 Note - Rev residue : yield ratio 091108 DTL with 35% dry matter content. rev biomass-yield ratio 032012 DTL
T
T Added the Yield intercept and Res:Yield ratio. 
T If a cover crop is inter planted into Corn, silage users must use a harvest that call in a growing
T cover crop.  Only one crop can be grown at a time in WEPS. 4-3-12 MAS
#------------
D 22/09/02
O 04 Harvest, silage, release cover crop
+ 8.886228 .15
T This record cuts and removes a crop to a height, kills the crop, then calls in another crop file to start or continue the growth of
T an existing cover crop.  It cuts to a 5 in ht. MAS 6-30-08
T
T This harvest record specifies the actual cut height dependent upon the height
T of the crop.  The cut height is specified as a fraction of the crop height.
T Added 0.2 for the flatting of the combine and tire trafic for haulling grain.
T MAS 1-18-07
T
T ARS record - filename is:  Harvest Wheat - grain (combine cutterbar header).oprn
T This operation record is designed to represent actual field harvesting operation
T of removing the grain from small grain crops with a cutterbar head on a combine.
T This harvesting operation record removes all the reproductive component of a crop above the
T cutting height.  Typically this is specified as the "yield" component in the crop record.
T The non-harvested crop plant material above the specified cut height becomes flat residue.
T The remaining above ground crop material below the specified cut height becomes standing residue.
T Nov 02, 2005	Created - Larry Wagner
T Detailed info regarding this operation record:
T
T The harvesting operation could also have an effect on the "standing stalk"
T fall rate and fall threshold values.  The default "biomass pool" flag parameter
T is set to "No adjustments applied" so that no "stalk residue decay rate change" will occur.
T However, this flag value can be changed along with the default parameter values
T to change the "stalk residue decay processes".
+
G 02 Biomass Manipulation
+ 1.0
P 31 Kill or Defoliate Growing Crop
+ 2
P 42 Cut/Remove Biomass to Height (flags)
+ 1 1 0 1 0 127.00025 1 1 1
P 34 Change Standing Biomass Fall Rate
+ 0 1.0 1.0 1.0 1.0 1.0
+ 1.0 1.0 1.0 1.0 1.0
P 40 End crop Biomass Manipulation
P 24 Flatten Standing Biomass
+ 0 0.2 0.2 0.2 0.2 1
G 03 Crop Name
+ Ryegrass, annual, forage
P 51 Seeding Configuration
+ 1 0.0 0
+ 400.0 1 0 2000 1.0 1.0 2
+ lbs/ac
+ 0 8930.0 4 1.0 0.6 0.8
+ 1.2 0.025 1.2192148 0.0 25.0 1 100 1800.0
+ -5.0 -15.0 0.005 0.05 0.035 30.0
+ 0.013 0.8013 0.4293 -0.086 -0.018 0.932 0.556 0.0736
+ 0.3293 -0.086 2.87 1.0 20.0 0.05 0 0.3
+ 28.571428 335.0 1.4 0.012 0.1 0.1 0.0 2
+ 0.0133 0.0133 0.0133 0.0133 0.12 0.0050 17.1 5.227942
+ -2.08165 0.548606 0 0.0 0.0 0.0 0.0 0.0
T Rusle Notes: Winter wheat cover.   Drilled in 7 inch rows.   Chemically killed  in late boot stage.  Not harvested for grain.
T Base location Columbia, MO. REV 61901 DTL
T
T Not calibrated grown on heat units.
T
T Cloned from WW cover file. 12-26-07 MAS
#------------
D 08/05/03
O 03 Manure spreader, solid and semi-solid
+ 11.505327 .20 1.7881091 0.0 1.7881091 1.3410819 3.5762181
T Created from RUSLE file MAS 9/19/06.
T This assumes a defult residue type of  manure solid significant bedding and the RUSLE may contain some bedding.
T User may need to change to the correct manure type, make a calulation on the dry matter applied, and change the application rate in MCREW.
T This opn is built for an application of 10 ton/ac 60% dry matter surface applied manure.
T 10 tons x 2000 lbs/ac = 20,000 lbs/ac x 0.6 = 12,000 lbs/ac applied.
T MAS 12-5-07
+
G 01 Tillage
+ 0.0 0 1 0.0 0.0 0.0
P 24 Flatten Standing Biomass
+ 14 .1 .1 .1 .1 1.0
G 03 Crop Name
+ manure, solid, signif. bedding
P 66 Add Manure Residue Amount
+ 0.0 0.0 0.0 0.0 1
+ 0.0 0.0 0.0 0.0
+ 1.34502 0.0
+ .017 .017 .017 .017 0.169 0.0050 1 5.227942
+ -2.08165 0.548606
T Enter crop notes here.
#------------
D 11/05/03
O 03 Disk, tandem heavy primary op
+ 7.0154433 39 2.2351363 0.0 2.2351363 1.3410819 2.6821637
T 11-12in. Spacing, Front and Rear
T Recommended for primary tillage in medium to heavy soils
T Excellent residue-handling capability. MAS 10-26-06
+
G 01 Tillage
+ 152.4003 1.0 1.0 152.4003 101.600204 177.80035
P 01 Break Crust
P 02 Random Roughness
+ 1 38.100075
P 05 Ridges and Dikes
+ 1 101.600204 279.40057 0.0 0.0 0.0
P 11 Aggregate Crushing
+ 2.8 0.75
P 12 Soil Loosening
+ 0.9
P 13 Soil Layer Mixing
+ 0.4
P 31 Kill or Defoliate Growing Crop
+ 2
P 40 End crop Biomass Manipulation
P 24 Flatten Standing Biomass
+ 0 1.0 0.9 0.8 0.5 1.0
P 25 Bury Flat Biomass
+ 1 0.95 0.85 0.8 0.6 0.95
P 26 Resurface Buried Biomass
+ 0.05 0.06 0.07 0.08 0.05
P 34 Change Standing Biomass Fall Rate
+ 7 3.0 2.5 2.0 1.5 1.0
+ 0.5 0.6 0.7 0.8 1.0
#------------
D 16/05/03
O 03 Disk, tandem light finishing
+ 3.7415698 19.5 2.2351363 0.0 2.2351363 1.3410819 2.6821637
T 6/8/01 DTL RUSLE.  7in sp.  This is tool used to finish a seedbed.  MAS 10-26-06
+
G 01 Tillage
+ 101.600204 0.5 1.0 101.600204 76.20015 127.00026
P 01 Break Crust
P 02 Random Roughness
+ 1 15.240031
P 05 Ridges and Dikes
+ 1 12.700026 177.80035 0.0 0.0 0.0
P 11 Aggregate Crushing
+ 2.8 0.75
P 12 Soil Loosening
+ 0.75
P 13 Soil Layer Mixing
+ 0.35
P 31 Kill or Defoliate Growing Crop
+ 2
P 40 End crop Biomass Manipulation
P 24 Flatten Standing Biomass
+ 0 0.85 0.7 0.6 0.5 1.0
P 25 Bury Flat Biomass
+ 1 0.73 0.63 0.55 0.4 0.73
P 26 Resurface Buried Biomass
+ 0.02 0.04 0.02 0.05 0.02
P 34 Change Standing Biomass Fall Rate
+ 7 3.0 2.5 2.0 1.5 1.0
+ 0.5 0.6 0.7 0.8 1.0
#------------
D 16/05/03
O 03 Fert applic. shank low disturbance, 12 in
+ 8.418531 3.25 2.2351363 0.0 2.2351363 1.5645955 2.9056773
T Minimum disturbance fertilizer injector shank.012904 DTL RUSLE MAS 10-26-06
T G2 was added into file in front of the flattening (P24), burial (P25), and resurfacing (P26) factors because the area affected is less than 1.0 and
T the RUSLE values were normalized to 1.0.  This change will imulate the correct residue changes based on the method set forth in RUSLE.
T RUSLE's factors have been redused to based on the area affected.
T The stalk fall rate factor (P34) was moved ahead of the new (G2) factor to set the fall rate to the less than 1.0 area affected.  8/7/07 MAS
+ 
G 01 Tillage
+ 101.600204 0.8 0.25 101.600204 76.20015 152.4003
P 01 Break Crust
P 02 Random Roughness
+ 1 15.240031
P 05 Ridges and Dikes
+ 1 50.800102 304.8006 25.400051 0.0 0.0
P 11 Aggregate Crushing
+ 2.4 2.0
P 12 Soil Loosening
+ 0.7
P 13 Soil Layer Mixing
+ 0.2
P 40 End crop Biomass Manipulation
P 34 Change Standing Biomass Fall Rate
+ 7 3.0 2.5 2.0 1.5 1.0
+ 0.5 0.6 0.7 0.8 1.0
P 24 Flatten Standing Biomass
+ 0 0.5 0.45 0.4 0.4 1.0
P 25 Bury Flat Biomass
+ 4 0.2 .15 .1 0.08 0.14
P 26 Resurface Buried Biomass
+ 0.06 0.06 0.06 0.1 0.06
#------------
D 16/05/03
O 03 Planter, double disk opnr
+ 4.1157265 2.4375 2.2351363 0.0 2.2351363 1.5645955 2.9056773
T This is a standard planter on 30 in sp with a 1 in ridge.  Created in RUSLE 6/7/01.  MAS 8/7/07
T G2 was added into file in front of the flattening (P24), burial (P25), and resurfacing (P26) factors because the area affected is less than 1.0 and
T the RUSLE values were normalized to 1.0.  This change will imulate the correct residue changes based on the method set forth in RUSLE.
T RUSLE's factors have been redused to based on the area affected.
T The stalk fall rate factor (P34) was moved ahead of the new (G2) factor to set the fall rate to the less than 1.0 area affected.  8/7/07 MAS
+
G 01 Tillage
+ 63.500126 0.5 .15 63.500126 50.800102 101.600204
P 01 Break Crust
P 02 Random Roughness
+ 1 10.160021
P 05 Ridges and Dikes
+ 1 50.800102 762.0015 635.0013 0.0 0.0
P 11 Aggregate Crushing
+ 2.8 0.75
P 12 Soil Loosening
+ 0.6
P 13 Soil Layer Mixing
+ 0.35
P 34 Change Standing Biomass Fall Rate
+ 7 3.0 2.5 2.0 1.5 1.0
+ 0.5 0.6 0.7 0.8 1.0
G 02 Biomass Manipulation
+ 1.0
P 24 Flatten Standing Biomass
+ 0 .3 .25 .2 0.1 1.0
P 25 Bury Flat Biomass
+ 1 .0525 0.0375 .03 .015 .03
P 26 Resurface Buried Biomass
+ .01 .01 .01 .02 .01
G 03 Crop Name
+ Corn, silage
P 51 Seeding Configuration
+ 1 0.0 2
+ 6.0 1.0 1 23 1.0 1.0 2
+ ton/ac
+ 65.0 4.465 4 1.0 0.65 0.8
+ 2.5 0.05 1.5240185 10.0 30.0 0 100 1700.0
+ -5.0 -15.0 0.01 0.05 0.0 40.0
+ 0.0031 0.9233 0.3266 -0.044 0.0 0.976 0.511 0.0287
+ 0.3266 -0.044 0.22259772 0.72 17.4 0.05 0 0.9
+ 333.33334 333.33334 3.0 0.03 0.0 0.0 0.0 3
+ 0.016 0.016 0.016 0.01 0.153 0.01 20.0 3.3812115
+ -1.20379 0.604887 0.3081 0.21615593 0.0 0.0 0.0 0.0
T corn silage 23 ton yield, 30" rows  Columbia, Mo DTL
T
T This record was cloned from ARS records and the revenant data adjusted to RUSLE values.
T The Biomass Conv Factor was changed from 40 to 47 based on runs made in Clovis, NM with full irrigation.
T MAS 9-27-07
T
T R2 Note - Rev residue : yield ratio 091108 DTL with 35% dry matter content. rev biomass-yield ratio 032012 DTL
T
T Added the Yield intercept and Res:Yield ratio. 
T If a cover crop is inter planted into Corn, silage users must use a harvest that call in a growing
T cover crop.  Only one crop can be grown at a time in WEPS. 4-3-12 MAS
#------------
D 22/09/03
O 04 Harvest, silage, release cover crop
+ 8.886228 .15
T This record cuts and removes a crop to a height, kills the crop, then calls in another crop file to start or continue the growth of
T an existing cover crop.  It cuts to a 5 in ht. MAS 6-30-08
T
T This harvest record specifies the actual cut height dependent upon the height
T of the crop.  The cut height is specified as a fraction of the crop height.
T Added 0.2 for the flatting of the combine and tire trafic for haulling grain.
T MAS 1-18-07
T
T ARS record - filename is:  Harvest Wheat - grain (combine cutterbar header).oprn
T This operation record is designed to represent actual field harvesting operation
T of removing the grain from small grain crops with a cutterbar head on a combine.
T This harvesting operation record removes all the reproductive component of a crop above the
T cutting height.  Typically this is specified as the "yield" component in the crop record.
T The non-harvested crop plant material above the specified cut height becomes flat residue.
T The remaining above ground crop material below the specified cut height becomes standing residue.
T Nov 02, 2005	Created - Larry Wagner
T Detailed info regarding this operation record:
T
T The harvesting operation could also have an effect on the "standing stalk"
T fall rate and fall threshold values.  The default "biomass pool" flag parameter
T is set to "No adjustments applied" so that no "stalk residue decay rate change" will occur.
T However, this flag value can be changed along with the default parameter values
T to change the "stalk residue decay processes".
+
G 02 Biomass Manipulation
+ 1.0
P 31 Kill or Defoliate Growing Crop
+ 2
P 42 Cut/Remove Biomass to Height (flags)
+ 1 1 0 1 0 127.00025 1 1 1
P 34 Change Standing Biomass Fall Rate
+ 0 1.0 1.0 1.0 1.0 1.0
+ 1.0 1.0 1.0 1.0 1.0
P 40 End crop Biomass Manipulation
P 24 Flatten Standing Biomass
+ 0 0.2 0.2 0.2 0.2 1
G 03 Crop Name
+ Ryegrass, annual, forage
P 51 Seeding Configuration
+ 1 0.0 0
+ 400.0 1 0 2000 1.0 1.0 2
+ lbs/ac
+ 0 8930.0 4 1.0 0.6 0.8
+ 1.2 0.025 1.2192148 0.0 25.0 1 100 1800.0
+ -5.0 -15.0 0.005 0.05 0.035 30.0
+ 0.013 0.8013 0.4293 -0.086 -0.018 0.932 0.556 0.0736
+ 0.3293 -0.086 2.87 1.0 20.0 0.05 0 0.3
+ 28.571428 335.0 1.4 0.012 0.1 0.1 0.0 2
+ 0.0133 0.0133 0.0133 0.0133 0.12 0.0050 17.1 5.227942
+ -2.08165 0.548606 0 0.0 0.0 0.0 0.0 0.0
T Rusle Notes: Winter wheat cover.   Drilled in 7 inch rows.   Chemically killed  in late boot stage.  Not harvested for grain.
T Base location Columbia, MO. REV 61901 DTL
T
T Not calibrated grown on heat units.
T
T Cloned from WW cover file. 12-26-07 MAS
#------------
D 08/05/04
O 03 Manure spreader, solid and semi-solid
+ 11.505327 .20 1.7881091 0.0 1.7881091 1.3410819 3.5762181
T Created from RUSLE file MAS 9/19/06.
T This assumes a defult residue type of  manure solid significant bedding and the RUSLE may contain some bedding.
T User may need to change to the correct manure type, make a calulation on the dry matter applied, and change the application rate in MCREW.
T This opn is built for an application of 10 ton/ac 60% dry matter surface applied manure.
T 10 tons x 2000 lbs/ac = 20,000 lbs/ac x 0.6 = 12,000 lbs/ac applied.
T MAS 12-5-07
+
G 01 Tillage
+ 0.0 0 1 0.0 0.0 0.0
P 24 Flatten Standing Biomass
+ 14 .1 .1 .1 .1 1.0
G 03 Crop Name
+ manure, solid, signif. bedding
P 66 Add Manure Residue Amount
+ 0.0 0.0 0.0 0.0 1
+ 0.0 0.0 0.0 0.0
+ 1.34502 0.0
+ .017 .017 .017 .017 0.169 0.0050 1 5.227942
+ -2.08165 0.548606
T Enter crop notes here.
#------------
D 11/05/04
O 03 Disk, tandem heavy primary op
+ 7.0154433 39 2.2351363 0.0 2.2351363 1.3410819 2.6821637
T 11-12in. Spacing, Front and Rear
T Recommended for primary tillage in medium to heavy soils
T Excellent residue-handling capability. MAS 10-26-06
+
G 01 Tillage
+ 152.4003 1.0 1.0 152.4003 101.600204 177.80035
P 01 Break Crust
P 02 Random Roughness
+ 1 38.100075
P 05 Ridges and Dikes
+ 1 101.600204 279.40057 0.0 0.0 0.0
P 11 Aggregate Crushing
+ 2.8 0.75
P 12 Soil Loosening
+ 0.9
P 13 Soil Layer Mixing
+ 0.4
P 31 Kill or Defoliate Growing Crop
+ 2
P 40 End crop Biomass Manipulation
P 24 Flatten Standing Biomass
+ 0 1.0 0.9 0.8 0.5 1.0
P 25 Bury Flat Biomass
+ 1 0.95 0.85 0.8 0.6 0.95
P 26 Resurface Buried Biomass
+ 0.05 0.06 0.07 0.08 0.05
P 34 Change Standing Biomass Fall Rate
+ 7 3.0 2.5 2.0 1.5 1.0
+ 0.5 0.6 0.7 0.8 1.0
#------------
D 16/05/04
O 03 Disk, tandem light finishing
+ 3.7415698 19.5 2.2351363 0.0 2.2351363 1.3410819 2.6821637
T 6/8/01 DTL RUSLE.  7in sp.  This is tool used to finish a seedbed.  MAS 10-26-06
+
G 01 Tillage
+ 101.600204 0.5 1.0 101.600204 76.20015 127.00026
P 01 Break Crust
P 02 Random Roughness
+ 1 15.240031
P 05 Ridges and Dikes
+ 1 12.700026 177.80035 0.0 0.0 0.0
P 11 Aggregate Crushing
+ 2.8 0.75
P 12 Soil Loosening
+ 0.75
P 13 Soil Layer Mixing
+ 0.35
P 31 Kill or Defoliate Growing Crop
+ 2
P 40 End crop Biomass Manipulation
P 24 Flatten Standing Biomass
+ 0 0.85 0.7 0.6 0.5 1.0
P 25 Bury Flat Biomass
+ 1 0.73 0.63 0.55 0.4 0.73
P 26 Resurface Buried Biomass
+ 0.02 0.04 0.02 0.05 0.02
P 34 Change Standing Biomass Fall Rate
+ 7 3.0 2.5 2.0 1.5 1.0
+ 0.5 0.6 0.7 0.8 1.0
#------------
D 16/05/04
O 03 Fert applic. shank low disturbance, 12 in
+ 8.418531 3.25 2.2351363 0.0 2.2351363 1.5645955 2.9056773
T Minimum disturbance fertilizer injector shank.012904 DTL RUSLE MAS 10-26-06
T G2 was added into file in front of the flattening (P24), burial (P25), and resurfacing (P26) factors because the area affected is less than 1.0 and
T the RUSLE values were normalized to 1.0.  This change will imulate the correct residue changes based on the method set forth in RUSLE.
T RUSLE's factors have been redused to based on the area affected.
T The stalk fall rate factor (P34) was moved ahead of the new (G2) factor to set the fall rate to the less than 1.0 area affected.  8/7/07 MAS
+ 
G 01 Tillage
+ 101.600204 0.8 0.25 101.600204 76.20015 152.4003
P 01 Break Crust
P 02 Random Roughness
+ 1 15.240031
P 05 Ridges and Dikes
+ 1 50.800102 304.8006 25.400051 0.0 0.0
P 11 Aggregate Crushing
+ 2.4 2.0
P 12 Soil Loosening
+ 0.7
P 13 Soil Layer Mixing
+ 0.2
P 40 End crop Biomass Manipulation
P 34 Change Standing Biomass Fall Rate
+ 7 3.0 2.5 2.0 1.5 1.0
+ 0.5 0.6 0.7 0.8 1.0
P 24 Flatten Standing Biomass
+ 0 0.5 0.45 0.4 0.4 1.0
P 25 Bury Flat Biomass
+ 4 0.2 .15 .1 0.08 0.14
P 26 Resurface Buried Biomass
+ 0.06 0.06 0.06 0.1 0.06
#------------
D 16/05/04
O 03 Planter, double disk opnr
+ 4.1157265 2.4375 2.2351363 0.0 2.2351363 1.5645955 2.9056773
T This is a standard planter on 30 in sp with a 1 in ridge.  Created in RUSLE 6/7/01.  MAS 8/7/07
T G2 was added into file in front of the flattening (P24), burial (P25), and resurfacing (P26) factors because the area affected is less than 1.0 and
T the RUSLE values were normalized to 1.0.  This change will imulate the correct residue changes based on the method set forth in RUSLE.
T RUSLE's factors have been redused to based on the area affected.
T The stalk fall rate factor (P34) was moved ahead of the new (G2) factor to set the fall rate to the less than 1.0 area affected.  8/7/07 MAS
+
G 01 Tillage
+ 63.500126 0.5 .15 63.500126 50.800102 101.600204
P 01 Break Crust
P 02 Random Roughness
+ 1 10.160021
P 05 Ridges and Dikes
+ 1 50.800102 762.0015 635.0013 0.0 0.0
P 11 Aggregate Crushing
+ 2.8 0.75
P 12 Soil Loosening
+ 0.6
P 13 Soil Layer Mixing
+ 0.35
P 34 Change Standing Biomass Fall Rate
+ 7 3.0 2.5 2.0 1.5 1.0
+ 0.5 0.6 0.7 0.8 1.0
G 02 Biomass Manipulation
+ 1.0
P 24 Flatten Standing Biomass
+ 0 .3 .25 .2 0.1 1.0
P 25 Bury Flat Biomass
+ 1 .0525 0.0375 .03 .015 .03
P 26 Resurface Buried Biomass
+ .01 .01 .01 .02 .01
G 03 Crop Name
+ Corn, silage
P 51 Seeding Configuration
+ 1 0.0 2
+ 6.0 1.0 1 23 1.0 1.0 2
+ ton/ac
+ 65.0 4.465 4 1.0 0.65 0.8
+ 2.5 0.05 1.5240185 10.0 30.0 0 100 1700.0
+ -5.0 -15.0 0.01 0.05 0.0 40.0
+ 0.0031 0.9233 0.3266 -0.044 0.0 0.976 0.511 0.0287
+ 0.3266 -0.044 0.22259772 0.72 17.4 0.05 0 0.9
+ 333.33334 333.33334 3.0 0.03 0.0 0.0 0.0 3
+ 0.016 0.016 0.016 0.01 0.153 0.01 20.0 3.3812115
+ -1.20379 0.604887 0.3081 0.21615593 0.0 0.0 0.0 0.0
T corn silage 23 ton yield, 30" rows  Columbia, Mo DTL
T
T This record was cloned from ARS records and the revenant data adjusted to RUSLE values.
T The Biomass Conv Factor was changed from 40 to 47 based on runs made in Clovis, NM with full irrigation.
T MAS 9-27-07
T
T R2 Note - Rev residue : yield ratio 091108 DTL with 35% dry matter content. rev biomass-yield ratio 032012 DTL
T
T Added the Yield intercept and Res:Yield ratio. 
T If a cover crop is inter planted into Corn, silage users must use a harvest that call in a growing
T cover crop.  Only one crop can be grown at a time in WEPS. 4-3-12 MAS
#------------
D 22/09/04
O 04 Harvest, silage, release cover crop
+ 8.886228 .15
T This record cuts and removes a crop to a height, kills the crop, then calls in another crop file to start or continue the growth of
T an existing cover crop.  It cuts to a 5 in ht. MAS 6-30-08
T
T This harvest record specifies the actual cut height dependent upon the height
T of the crop.  The cut height is specified as a fraction of the crop height.
T Added 0.2 for the flatting of the combine and tire trafic for haulling grain.
T MAS 1-18-07
T
T ARS record - filename is:  Harvest Wheat - grain (combine cutterbar header).oprn
T This operation record is designed to represent actual field harvesting operation
T of removing the grain from small grain crops with a cutterbar head on a combine.
T This harvesting operation record removes all the reproductive component of a crop above the
T cutting height.  Typically this is specified as the "yield" component in the crop record.
T The non-harvested crop plant material above the specified cut height becomes flat residue.
T The remaining above ground crop material below the specified cut height becomes standing residue.
T Nov 02, 2005	Created - Larry Wagner
T Detailed info regarding this operation record:
T
T The harvesting operation could also have an effect on the "standing stalk"
T fall rate and fall threshold values.  The default "biomass pool" flag parameter
T is set to "No adjustments applied" so that no "stalk residue decay rate change" will occur.
T However, this flag value can be changed along with the default parameter values
T to change the "stalk residue decay processes".
+
G 02 Biomass Manipulation
+ 1.0
P 31 Kill or Defoliate Growing Crop
+ 2
P 42 Cut/Remove Biomass to Height (flags)
+ 1 1 0 1 0 127.00025 1 1 1
P 34 Change Standing Biomass Fall Rate
+ 0 1.0 1.0 1.0 1.0 1.0
+ 1.0 1.0 1.0 1.0 1.0
P 40 End crop Biomass Manipulation
P 24 Flatten Standing Biomass
+ 0 0.2 0.2 0.2 0.2 1
G 03 Crop Name
+ Ryegrass, annual, forage
P 51 Seeding Configuration
+ 1 0.0 0
+ 400.0 1 0 2000 1.0 1.0 2
+ lbs/ac
+ 0 8930.0 4 1.0 0.6 0.8
+ 1.2 0.025 1.2192148 0.0 25.0 1 100 1800.0
+ -5.0 -15.0 0.005 0.05 0.035 30.0
+ 0.013 0.8013 0.4293 -0.086 -0.018 0.932 0.556 0.0736
+ 0.3293 -0.086 2.87 1.0 20.0 0.05 0 0.3
+ 28.571428 335.0 1.4 0.012 0.1 0.1 0.0 2
+ 0.0133 0.0133 0.0133 0.0133 0.12 0.0050 17.1 5.227942
+ -2.08165 0.548606 0 0.0 0.0 0.0 0.0 0.0
T Rusle Notes: Winter wheat cover.   Drilled in 7 inch rows.   Chemically killed  in late boot stage.  Not harvested for grain.
T Base location Columbia, MO. REV 61901 DTL
T
T Not calibrated grown on heat units.
T
T Cloned from WW cover file. 12-26-07 MAS
#------------
D 08/05/05
O 03 Manure spreader, solid and semi-solid
+ 11.505327 .20 1.7881091 0.0 1.7881091 1.3410819 3.5762181
T Created from RUSLE file MAS 9/19/06.
T This assumes a defult residue type of  manure solid significant bedding and the RUSLE may contain some bedding.
T User may need to change to the correct manure type, make a calulation on the dry matter applied, and change the application rate in MCREW.
T This opn is built for an application of 10 ton/ac 60% dry matter surface applied manure.
T 10 tons x 2000 lbs/ac = 20,000 lbs/ac x 0.6 = 12,000 lbs/ac applied.
T MAS 12-5-07
+
G 01 Tillage
+ 0.0 0 1 0.0 0.0 0.0
P 24 Flatten Standing Biomass
+ 14 .1 .1 .1 .1 1.0
G 03 Crop Name
+ manure, solid, signif. bedding
P 66 Add Manure Residue Amount
+ 0.0 0.0 0.0 0.0 1
+ 0.0 0.0 0.0 0.0
+ 1.34502 0.0
+ .017 .017 .017 .017 0.169 0.0050 1 5.227942
+ -2.08165 0.548606
T Enter crop notes here.
#------------
D 11/05/05
O 03 Disk, tandem heavy primary op
+ 7.0154433 39 2.2351363 0.0 2.2351363 1.3410819 2.6821637
T 11-12in. Spacing, Front and Rear
T Recommended for primary tillage in medium to heavy soils
T Excellent residue-handling capability. MAS 10-26-06
+
G 01 Tillage
+ 152.4003 1.0 1.0 152.4003 101.600204 177.80035
P 01 Break Crust
P 02 Random Roughness
+ 1 38.100075
P 05 Ridges and Dikes
+ 1 101.600204 279.40057 0.0 0.0 0.0
P 11 Aggregate Crushing
+ 2.8 0.75
P 12 Soil Loosening
+ 0.9
P 13 Soil Layer Mixing
+ 0.4
P 31 Kill or Defoliate Growing Crop
+ 2
P 40 End crop Biomass Manipulation
P 24 Flatten Standing Biomass
+ 0 1.0 0.9 0.8 0.5 1.0
P 25 Bury Flat Biomass
+ 1 0.95 0.85 0.8 0.6 0.95
P 26 Resurface Buried Biomass
+ 0.05 0.06 0.07 0.08 0.05
P 34 Change Standing Biomass Fall Rate
+ 7 3.0 2.5 2.0 1.5 1.0
+ 0.5 0.6 0.7 0.8 1.0
#------------
D 16/05/05
O 03 Disk, tandem light finishing
+ 3.7415698 19.5 2.2351363 0.0 2.2351363 1.3410819 2.6821637
T 6/8/01 DTL RUSLE.  7in sp.  This is tool used to finish a seedbed.  MAS 10-26-06
+
G 01 Tillage
+ 101.600204 0.5 1.0 101.600204 76.20015 127.00026
P 01 Break Crust
P 02 Random Roughness
+ 1 15.240031
P 05 Ridges and Dikes
+ 1 12.700026 177.80035 0.0 0.0 0.0
P 11 Aggregate Crushing
+ 2.8 0.75
P 12 Soil Loosening
+ 0.75
P 13 Soil Layer Mixing
+ 0.35
P 31 Kill or Defoliate Growing Crop
+ 2
P 40 End crop Biomass Manipulation
P 24 Flatten Standing Biomass
+ 0 0.85 0.7 0.6 0.5 1.0
P 25 Bury Flat Biomass
+ 1 0.73 0.63 0.55 0.4 0.73
P 26 Resurface Buried Biomass
+ 0.02 0.04 0.02 0.05 0.02
P 34 Change Standing Biomass Fall Rate
+ 7 3.0 2.5 2.0 1.5 1.0
+ 0.5 0.6 0.7 0.8 1.0
#------------
D 16/05/05
O 03 Fert applic. shank low disturbance, 12 in
+ 8.418531 3.25 2.2351363 0.0 2.2351363 1.5645955 2.9056773
T Minimum disturbance fertilizer injector shank.012904 DTL RUSLE MAS 10-26-06
T G2 was added into file in front of the flattening (P24), burial (P25), and resurfacing (P26) factors because the area affected is less than 1.0 and
T the RUSLE values were normalized to 1.0.  This change will imulate the correct residue changes based on the method set forth in RUSLE.
T RUSLE's factors have been redused to based on the area affected.
T The stalk fall rate factor (P34) was moved ahead of the new (G2) factor to set the fall rate to the less than 1.0 area affected.  8/7/07 MAS
+ 
G 01 Tillage
+ 101.600204 0.8 0.25 101.600204 76.20015 152.4003
P 01 Break Crust
P 02 Random Roughness
+ 1 15.240031
P 05 Ridges and Dikes
+ 1 50.800102 304.8006 25.400051 0.0 0.0
P 11 Aggregate Crushing
+ 2.4 2.0
P 12 Soil Loosening
+ 0.7
P 13 Soil Layer Mixing
+ 0.2
P 40 End crop Biomass Manipulation
P 34 Change Standing Biomass Fall Rate
+ 7 3.0 2.5 2.0 1.5 1.0
+ 0.5 0.6 0.7 0.8 1.0
P 24 Flatten Standing Biomass
+ 0 0.5 0.45 0.4 0.4 1.0
P 25 Bury Flat Biomass
+ 4 0.2 .15 .1 0.08 0.14
P 26 Resurface Buried Biomass
+ 0.06 0.06 0.06 0.1 0.06
#------------
D 16/05/05
O 03 Planter, double disk opnr
+ 4.1157265 2.4375 2.2351363 0.0 2.2351363 1.5645955 2.9056773
T This is a standard planter on 30 in sp with a 1 in ridge.  Created in RUSLE 6/7/01.  MAS 8/7/07
T G2 was added into file in front of the flattening (P24), burial (P25), and resurfacing (P26) factors because the area affected is less than 1.0 and
T the RUSLE values were normalized to 1.0.  This change will imulate the correct residue changes based on the method set forth in RUSLE.
T RUSLE's factors have been redused to based on the area affected.
T The stalk fall rate factor (P34) was moved ahead of the new (G2) factor to set the fall rate to the less than 1.0 area affected.  8/7/07 MAS
+
G 01 Tillage
+ 63.500126 0.5 .15 63.500126 50.800102 101.600204
P 01 Break Crust
P 02 Random Roughness
+ 1 10.160021
P 05 Ridges and Dikes
+ 1 50.800102 762.0015 635.0013 0.0 0.0
P 11 Aggregate Crushing
+ 2.8 0.75
P 12 Soil Loosening
+ 0.6
P 13 Soil Layer Mixing
+ 0.35
P 34 Change Standing Biomass Fall Rate
+ 7 3.0 2.5 2.0 1.5 1.0
+ 0.5 0.6 0.7 0.8 1.0
G 02 Biomass Manipulation
+ 1.0
P 24 Flatten Standing Biomass
+ 0 .3 .25 .2 0.1 1.0
P 25 Bury Flat Biomass
+ 1 .0525 0.0375 .03 .015 .03
P 26 Resurface Buried Biomass
+ .01 .01 .01 .02 .01
G 03 Crop Name
+ Corn, silage
P 51 Seeding Configuration
+ 1 0.0 2
+ 6.0 1.0 1 23 1.0 1.0 2
+ ton/ac
+ 65.0 4.465 4 1.0 0.65 0.8
+ 2.5 0.05 1.5240185 10.0 30.0 0 100 1700.0
+ -5.0 -15.0 0.01 0.05 0.0 40.0
+ 0.0031 0.9233 0.3266 -0.044 0.0 0.976 0.511 0.0287
+ 0.3266 -0.044 0.22259772 0.72 17.4 0.05 0 0.9
+ 333.33334 333.33334 3.0 0.03 0.0 0.0 0.0 3
+ 0.016 0.016 0.016 0.01 0.153 0.01 20.0 3.3812115
+ -1.20379 0.604887 0.3081 0.21615593 0.0 0.0 0.0 0.0
T corn silage 23 ton yield, 30" rows  Columbia, Mo DTL
T
T This record was cloned from ARS records and the revenant data adjusted to RUSLE values.
T The Biomass Conv Factor was changed from 40 to 47 based on runs made in Clovis, NM with full irrigation.
T MAS 9-27-07
T
T R2 Note - Rev residue : yield ratio 091108 DTL with 35% dry matter content. rev biomass-yield ratio 032012 DTL
T
T Added the Yield intercept and Res:Yield ratio. 
T If a cover crop is inter planted into Corn, silage users must use a harvest that call in a growing
T cover crop.  Only one crop can be grown at a time in WEPS. 4-3-12 MAS
#------------
D 22/09/05
O 04 Harvest, silage, release cover crop
+ 8.886228 .15
T This record cuts and removes a crop to a height, kills the crop, then calls in another crop file to start or continue the growth of
T an existing cover crop.  It cuts to a 5 in ht. MAS 6-30-08
T
T This harvest record specifies the actual cut height dependent upon the height
T of the crop.  The cut height is specified as a fraction of the crop height.
T Added 0.2 for the flatting of the combine and tire trafic for haulling grain.
T MAS 1-18-07
T
T ARS record - filename is:  Harvest Wheat - grain (combine cutterbar header).oprn
T This operation record is designed to represent actual field harvesting operation
T of removing the grain from small grain crops with a cutterbar head on a combine.
T This harvesting operation record removes all the reproductive component of a crop above the
T cutting height.  Typically this is specified as the "yield" component in the crop record.
T The non-harvested crop plant material above the specified cut height becomes flat residue.
T The remaining above ground crop material below the specified cut height becomes standing residue.
T Nov 02, 2005	Created - Larry Wagner
T Detailed info regarding this operation record:
T
T The harvesting operation could also have an effect on the "standing stalk"
T fall rate and fall threshold values.  The default "biomass pool" flag parameter
T is set to "No adjustments applied" so that no "stalk residue decay rate change" will occur.
T However, this flag value can be changed along with the default parameter values
T to change the "stalk residue decay processes".
+
G 02 Biomass Manipulation
+ 1.0
P 31 Kill or Defoliate Growing Crop
+ 2
P 42 Cut/Remove Biomass to Height (flags)
+ 1 1 0 1 0 127.00025 1 1 1
P 34 Change Standing Biomass Fall Rate
+ 0 1.0 1.0 1.0 1.0 1.0
+ 1.0 1.0 1.0 1.0 1.0
P 40 End crop Biomass Manipulation
P 24 Flatten Standing Biomass
+ 0 0.2 0.2 0.2 0.2 1
G 03 Crop Name
+ Ryegrass, annual, forage
P 51 Seeding Configuration
+ 1 0.0 0
+ 400.0 1 0 2000 1.0 1.0 2
+ lbs/ac
+ 0 8930.0 4 1.0 0.6 0.8
+ 1.2 0.025 1.2192148 0.0 25.0 1 100 1800.0
+ -5.0 -15.0 0.005 0.05 0.035 30.0
+ 0.013 0.8013 0.4293 -0.086 -0.018 0.932 0.556 0.0736
+ 0.3293 -0.086 2.87 1.0 20.0 0.05 0 0.3
+ 28.571428 335.0 1.4 0.012 0.1 0.1 0.0 2
+ 0.0133 0.0133 0.0133 0.0133 0.12 0.0050 17.1 5.227942
+ -2.08165 0.548606 0 0.0 0.0 0.0 0.0 0.0
T Rusle Notes: Winter wheat cover.   Drilled in 7 inch rows.   Chemically killed  in late boot stage.  Not harvested for grain.
T Base location Columbia, MO. REV 61901 DTL
T
T Not calibrated grown on heat units.
T
T Cloned from WW cover file. 12-26-07 MAS
#------------
D 24/05/06
O 03 Disk, tandem heavy primary op
+ 7.0154433 39 2.2351363 0.0 2.2351363 1.3410819 2.6821637
T 11-12in. Spacing, Front and Rear
T Recommended for primary tillage in medium to heavy soils
T Excellent residue-handling capability. MAS 10-26-06
+
G 01 Tillage
+ 152.4003 1.0 1.0 152.4003 101.600204 177.80035
P 01 Break Crust
P 02 Random Roughness
+ 1 38.100075
P 05 Ridges and Dikes
+ 1 101.600204 279.40057 0.0 0.0 0.0
P 11 Aggregate Crushing
+ 2.8 0.75
P 12 Soil Loosening
+ 0.9
P 13 Soil Layer Mixing
+ 0.4
P 31 Kill or Defoliate Growing Crop
+ 2
P 40 End crop Biomass Manipulation
P 24 Flatten Standing Biomass
+ 0 1.0 0.9 0.8 0.5 1.0
P 25 Bury Flat Biomass
+ 1 0.95 0.85 0.8 0.6 0.95
P 26 Resurface Buried Biomass
+ 0.05 0.06 0.07 0.08 0.05
P 34 Change Standing Biomass Fall Rate
+ 7 3.0 2.5 2.0 1.5 1.0
+ 0.5 0.6 0.7 0.8 1.0
#------------
D 29/05/06
O 03 Manure spreader, slurry
+ 11.505327 .29 1.7881091 0.0 1.7881091 1.3410819 3.5762181
T Created from RUSLE file MAS 9/19/06.
T This assumes a defult residue type of  manure slurry using a solid spread with a liquid end gate spreader.
T User needs to change to the correct manure type, make a calulation on the dry matter applied, and change the value in MCREW.
T This opn is built for an application of 10 ton/ac 10% dry matter surface applied manure.
T 10 tons x 2000 lbs/ac = 20,000 lbs/ac x 0.1 = 2,000 lbs/ac applied.
T MAS 12-5-07
+
G 01 Tillage
+ 0.0 0 1 0.0 0.0 0.0
P 24 Flatten Standing Biomass
+ 14 .1 .1 .1 .1 1.0
G 03 Crop Name
+ manure, slurry
P 66 Add Manure Residue Amount
+ 0.0 0.0 0.0 0.0 1
+ 0.0 0.0 0.0 0.0
+ 0.22417001 0.0
+ .06 .06 .06 .06 0.169 0.0050 1 0.6500045
+ -2.08165 0.548606
T Enter crop notes here.
#------------
D 29/05/06
O 03 Harrow, coiled tine
+ 4.1157265 15.6 2.6821637 0.0 2.6821637 1.3410819 3.129191
T This oprn is from a RUSLE record created 6/7/01.  10-25-06 MAS
T
T Corrected ridge height and spacing to match RUSLE2. 10-26-11 LOS
T
T Changed spacing from 0 to 1 in. The 0 caused the operation to fail.  12-12-11 MAS
+
G 01 Tillage
+ 50.800102 0.25 1.0 50.800102 25.400051 76.20015
P 01 Break Crust
P 02 Random Roughness
+ 1 10.160021
P 05 Ridges and Dikes
+ 1 25.400051 101.600204 0.0 0.0 0.0
P 11 Aggregate Crushing
+ 3.0 -0.22
P 12 Soil Loosening
+ 0.6
P 13 Soil Layer Mixing
+ 0.2
P 31 Kill or Defoliate Growing Crop
+ 2
P 40 End crop Biomass Manipulation
P 24 Flatten Standing Biomass
+ 0 0.5 0.3 0.2 0.1 1.0
P 25 Bury Flat Biomass
+ 1 0.25 0.2 0.15 0.1 0.25
P 26 Resurface Buried Biomass
+ 0.01 0.01 0.01 0.02 0.01
P 34 Change Standing Biomass Fall Rate
+ 7 3.0 2.5 2.0 1.5 1.0
+ 0.5 0.6 0.7 0.8 1.0
#------------
D 01/06/06
O 03 Drill or air seeder, hoe or chisel openers 6-12 in spac
+ 6.921904 23.4 2.2351363 0 2.2351363 1.5645955 2.9056773
T Drill or Airseeder, hoe or chisel openers and 3 in. wide presswheels.   From RUSLE 1 MAS 10-19-06
T G2 was added into file in front of the flattening (P24), burial (P25), and resurfacing (P26) factors because the area affected is less than 1.0 and
T the RUSLE values were normalized to 1.0.  This change will imulate the correct residue changes based on the method set forth in RUSLE.
T RUSLE's factors have been redused to based on the area affected.
T The stalk fall rate factor (P34) was moved ahead of the new (G2) factor to set the fall rate to the  less than 1.0 area affected.  8/7/07 MAS
+
G 01 Tillage
+ 101.600204 0.75 0.9 101.600204 76.20015 152.4003
P 01 Break Crust
P 02 Random Roughness
+ 1 12.700026
P 05 Ridges and Dikes
+ 1 76.20015 203.2004064008128 50.800102 0 0
P 11 Aggregate Crushing
+ 2.4 -2.0
P 12 Soil Loosening
+ 0.7
P 13 Soil Layer Mixing
+ 0.5
P 31 Kill or Defoliate Growing Crop
+ 2
P 40 End crop Biomass Manipulation
P 34 Change Standing Biomass Fall Rate
+ 7 3.0 2.5 2.0 1.5 1.0
+ 0.5 0.6 0.7 0.8 1.0
G 02 Biomass Manipulation
+ 1.0
P 24 Flatten Standing Biomass
+ 0 0.6 0.4 0.3 0.3 1.0
P 25 Bury Flat Biomass
+ 1 0.45 0.36 0.27 0.23 0.34
P 26 Resurface Buried Biomass
+ 0.01 0.01 0.01 0.03 0.01
G 03 Crop Name
+ Clover, red, seed
P 51 Seeding Configuration
+ 1 0.0 0
+ 120.0 5.0 1 1500.0 1.0 1.0 0
+ lb/ac
+ 12.0 8930.0 3 0.5 0.65 0.8
+ 0.8 0.01 2.0 1.0 25.0 0 120 1800.0
+ -5.0 -15.0 0.005 0.05 0.0 25.0
+ 0.023 0.8063 0.4146 -0.061 -0.024 0.9911 0.6435 0.0494
+ 0.4146 -0.061 3.9 1.0 20.6 0.05 0 0.1442091
+ 1.6666666 120.0 0.6 0.013 0.1 0.1 0.0 1
+ 0.02 0.02 0.02 0.02 0.2 0.0050 20.0 4.933536
+ -1.20379 0.604887 18 0.067251004 0.0 0.0 0.0 0.0
T Adjusted the Harvest fraction of the Plant Compoent from 0.2 to 0.5.  MAS 3-10-09
#------------
D 01/09/06
O 04 Harvest, hay, grass
+ 17.959534 .15
T Harvest legume hay crops such as Alfalfa and Red clover and grass-legume mixed hay such as Alfalfa-Bromegrass.
T Use Harvest, grass hay" for pure grass hay. Rev 11/17/01 DTL"  MAS 11-29-06
T
T Reset the fuel use to 1.92 gal/ac MAS 10-21-11
+
G 02 Biomass Manipulation
+ 1.0
P 31 Kill or Defoliate Growing Crop
+ 0
P 42 Cut/Remove Biomass to Height (flags)
+ 1 0 0 0 0 101.600204 .85 .85 1
P 34 Change Standing Biomass Fall Rate
+ 0 1.1 1.08 1.06 1.04 1.0
+ 0.9 0.92 0.93 0.95 1.0
P 40 End crop Biomass Manipulation
P 24 Flatten Standing Biomass
+ 14 .6 .5 .4 .5 .5
#------------
D 10/05/07
O 03 Manure spreader, slurry
+ 11.505327 .29 1.7881091 0.0 1.7881091 1.3410819 3.5762181
T Created from RUSLE file MAS 9/19/06.
T This assumes a defult residue type of  manure slurry using a solid spread with a liquid end gate spreader.
T User needs to change to the correct manure type, make a calulation on the dry matter applied, and change the value in MCREW.
T This opn is built for an application of 10 ton/ac 10% dry matter surface applied manure.
T 10 tons x 2000 lbs/ac = 20,000 lbs/ac x 0.1 = 2,000 lbs/ac applied.
T MAS 12-5-07
+
G 01 Tillage
+ 0.0 0 1 0.0 0.0 0.0
P 24 Flatten Standing Biomass
+ 14 .1 .1 .1 .1 1.0
G 03 Crop Name
+ manure, slurry
P 66 Add Manure Residue Amount
+ 0.0 0.0 0.0 0.0 1
+ 0.0 0.0 0.0 0.0
+ 0.22417001 0.0
+ .06 .06 .06 .06 0.169 0.0050 1 0.6500045
+ -2.08165 0.548606
T Enter crop notes here.
#------------
D 16/06/07
O 04 Harvest, hay, grass
+ 17.959534 .15
T Harvest legume hay crops such as Alfalfa and Red clover and grass-legume mixed hay such as Alfalfa-Bromegrass.
T Use Harvest, grass hay" for pure grass hay. Rev 11/17/01 DTL"  MAS 11-29-06
T
T Reset the fuel use to 1.92 gal/ac MAS 10-21-11
+
G 02 Biomass Manipulation
+ 1.0
P 31 Kill or Defoliate Growing Crop
+ 0
P 42 Cut/Remove Biomass to Height (flags)
+ 1 0 0 0 0 101.600204 .85 .85 1
P 34 Change Standing Biomass Fall Rate
+ 0 1.1 1.08 1.06 1.04 1.0
+ 0.9 0.92 0.93 0.95 1.0
P 40 End crop Biomass Manipulation
P 24 Flatten Standing Biomass
+ 14 .6 .5 .4 .5 .5
#------------
D 16/06/07
O 03 Manure spreader, slurry
+ 11.505327 .29 1.7881091 0.0 1.7881091 1.3410819 3.5762181
T Created from RUSLE file MAS 9/19/06.
T This assumes a defult residue type of  manure slurry using a solid spread with a liquid end gate spreader.
T User needs to change to the correct manure type, make a calulation on the dry matter applied, and change the value in MCREW.
T This opn is built for an application of 10 ton/ac 10% dry matter surface applied manure.
T 10 tons x 2000 lbs/ac = 20,000 lbs/ac x 0.1 = 2,000 lbs/ac applied.
T MAS 12-5-07
+
G 01 Tillage
+ 0.0 0 1 0.0 0.0 0.0
P 24 Flatten Standing Biomass
+ 14 .1 .1 .1 .1 1.0
G 03 Crop Name
+ manure, slurry
P 66 Add Manure Residue Amount
+ 0.0 0.0 0.0 0.0 1
+ 0.0 0.0 0.0 0.0
+ 0.22417001 0.0
+ .06 .06 .06 .06 0.169 0.0050 1 0.6500045
+ -2.08165 0.548606
T Enter crop notes here.
#------------
D 01/08/07
O 04 Harvest, hay, grass
+ 17.959534 .15
T Harvest legume hay crops such as Alfalfa and Red clover and grass-legume mixed hay such as Alfalfa-Bromegrass.
T Use Harvest, grass hay" for pure grass hay. Rev 11/17/01 DTL"  MAS 11-29-06
T
T Reset the fuel use to 1.92 gal/ac MAS 10-21-11
+
G 02 Biomass Manipulation
+ 1.0
P 31 Kill or Defoliate Growing Crop
+ 0
P 42 Cut/Remove Biomass to Height (flags)
+ 1 0 0 0 0 101.600204 .85 .85 1
P 34 Change Standing Biomass Fall Rate
+ 0 1.1 1.08 1.06 1.04 1.0
+ 0.9 0.92 0.93 0.95 1.0
P 40 End crop Biomass Manipulation
P 24 Flatten Standing Biomass
+ 14 .6 .5 .4 .5 .5
#------------
D 05/08/07
O 03 Manure spreader, slurry
+ 11.505327 .29 1.7881091 0.0 1.7881091 1.3410819 3.5762181
T Created from RUSLE file MAS 9/19/06.
T This assumes a defult residue type of  manure slurry using a solid spread with a liquid end gate spreader.
T User needs to change to the correct manure type, make a calulation on the dry matter applied, and change the value in MCREW.
T This opn is built for an application of 10 ton/ac 10% dry matter surface applied manure.
T 10 tons x 2000 lbs/ac = 20,000 lbs/ac x 0.1 = 2,000 lbs/ac applied.
T MAS 12-5-07
+
G 01 Tillage
+ 0.0 0 1 0.0 0.0 0.0
P 24 Flatten Standing Biomass
+ 14 .1 .1 .1 .1 1.0
G 03 Crop Name
+ manure, slurry
P 66 Add Manure Residue Amount
+ 0.0 0.0 0.0 0.0 1
+ 0.0 0.0 0.0 0.0
+ 0.22417001 0.0
+ .06 .06 .06 .06 0.169 0.0050 1 0.6500045
+ -2.08165 0.548606
T Enter crop notes here.
#------------
D 10/05/08
O 03 Manure spreader, slurry
+ 11.505327 .29 1.7881091 0.0 1.7881091 1.3410819 3.5762181
T Created from RUSLE file MAS 9/19/06.
T This assumes a defult residue type of  manure slurry using a solid spread with a liquid end gate spreader.
T User needs to change to the correct manure type, make a calulation on the dry matter applied, and change the value in MCREW.
T This opn is built for an application of 10 ton/ac 10% dry matter surface applied manure.
T 10 tons x 2000 lbs/ac = 20,000 lbs/ac x 0.1 = 2,000 lbs/ac applied.
T MAS 12-5-07
+
G 01 Tillage
+ 0.0 0 1 0.0 0.0 0.0
P 24 Flatten Standing Biomass
+ 14 .1 .1 .1 .1 1.0
G 03 Crop Name
+ manure, slurry
P 66 Add Manure Residue Amount
+ 0.0 0.0 0.0 0.0 1
+ 0.0 0.0 0.0 0.0
+ 0.22417001 0.0
+ .06 .06 .06 .06 0.169 0.0050 1 0.6500045
+ -2.08165 0.548606
T Enter crop notes here.
#------------
D 16/06/08
O 04 Harvest, hay, grass
+ 17.959534 .15
T Harvest legume hay crops such as Alfalfa and Red clover and grass-legume mixed hay such as Alfalfa-Bromegrass.
T Use Harvest, grass hay" for pure grass hay. Rev 11/17/01 DTL"  MAS 11-29-06
T
T Reset the fuel use to 1.92 gal/ac MAS 10-21-11
+
G 02 Biomass Manipulation
+ 1.0
P 31 Kill or Defoliate Growing Crop
+ 0
P 42 Cut/Remove Biomass to Height (flags)
+ 1 0 0 0 0 101.600204 .85 .85 1
P 34 Change Standing Biomass Fall Rate
+ 0 1.1 1.08 1.06 1.04 1.0
+ 0.9 0.92 0.93 0.95 1.0
P 40 End crop Biomass Manipulation
P 24 Flatten Standing Biomass
+ 14 .6 .5 .4 .5 .5
#------------
D 20/06/08
O 03 Manure spreader, slurry
+ 11.505327 .29 1.7881091 0.0 1.7881091 1.3410819 3.5762181
T Created from RUSLE file MAS 9/19/06.
T This assumes a defult residue type of  manure slurry using a solid spread with a liquid end gate spreader.
T User needs to change to the correct manure type, make a calulation on the dry matter applied, and change the value in MCREW.
T This opn is built for an application of 10 ton/ac 10% dry matter surface applied manure.
T 10 tons x 2000 lbs/ac = 20,000 lbs/ac x 0.1 = 2,000 lbs/ac applied.
T MAS 12-5-07
+
G 01 Tillage
+ 0.0 0 1 0.0 0.0 0.0
P 24 Flatten Standing Biomass
+ 14 .1 .1 .1 .1 1.0
G 03 Crop Name
+ manure, slurry
P 66 Add Manure Residue Amount
+ 0.0 0.0 0.0 0.0 1
+ 0.0 0.0 0.0 0.0
+ 0.22417001 0.0
+ .06 .06 .06 .06 0.169 0.0050 1 0.6500045
+ -2.08165 0.548606
T Enter crop notes here.
#------------
D 01/08/08
O 04 Harvest, hay, grass
+ 17.959534 .15
T Harvest legume hay crops such as Alfalfa and Red clover and grass-legume mixed hay such as Alfalfa-Bromegrass.
T Use Harvest, grass hay" for pure grass hay. Rev 11/17/01 DTL"  MAS 11-29-06
T
T Reset the fuel use to 1.92 gal/ac MAS 10-21-11
+
G 02 Biomass Manipulation
+ 1.0
P 31 Kill or Defoliate Growing Crop
+ 0
P 42 Cut/Remove Biomass to Height (flags)
+ 1 0 0 0 0 101.600204 .85 .85 1
P 34 Change Standing Biomass Fall Rate
+ 0 1.1 1.08 1.06 1.04 1.0
+ 0.9 0.92 0.93 0.95 1.0
P 40 End crop Biomass Manipulation
P 24 Flatten Standing Biomass
+ 14 .6 .5 .4 .5 .5
#------------
D 05/08/08
O 03 Manure spreader, slurry
+ 11.505327 .29 1.7881091 0.0 1.7881091 1.3410819 3.5762181
T Created from RUSLE file MAS 9/19/06.
T This assumes a defult residue type of  manure slurry using a solid spread with a liquid end gate spreader.
T User needs to change to the correct manure type, make a calulation on the dry matter applied, and change the value in MCREW.
T This opn is built for an application of 10 ton/ac 10% dry matter surface applied manure.
T 10 tons x 2000 lbs/ac = 20,000 lbs/ac x 0.1 = 2,000 lbs/ac applied.
T MAS 12-5-07
+
G 01 Tillage
+ 0.0 0 1 0.0 0.0 0.0
P 24 Flatten Standing Biomass
+ 14 .1 .1 .1 .1 1.0
G 03 Crop Name
+ manure, slurry
P 66 Add Manure Residue Amount
+ 0.0 0.0 0.0 0.0 1
+ 0.0 0.0 0.0 0.0
+ 0.22417001 0.0
+ .06 .06 .06 .06 0.169 0.0050 1 0.6500045
+ -2.08165 0.548606
T Enter crop notes here.
#------------
D 10/05/09
O 03 Manure spreader, slurry
+ 11.505327 .29 1.7881091 0.0 1.7881091 1.3410819 3.5762181
T Created from RUSLE file MAS 9/19/06.
T This assumes a defult residue type of  manure slurry using a solid spread with a liquid end gate spreader.
T User needs to change to the correct manure type, make a calulation on the dry matter applied, and change the value in MCREW.
T This opn is built for an application of 10 ton/ac 10% dry matter surface applied manure.
T 10 tons x 2000 lbs/ac = 20,000 lbs/ac x 0.1 = 2,000 lbs/ac applied.
T MAS 12-5-07
+
G 01 Tillage
+ 0.0 0 1 0.0 0.0 0.0
P 24 Flatten Standing Biomass
+ 14 .1 .1 .1 .1 1.0
G 03 Crop Name
+ manure, slurry
P 66 Add Manure Residue Amount
+ 0.0 0.0 0.0 0.0 1
+ 0.0 0.0 0.0 0.0
+ 0.22417001 0.0
+ .06 .06 .06 .06 0.169 0.0050 1 0.6500045
+ -2.08165 0.548606
T Enter crop notes here.
#------------
D 16/06/09
O 04 Harvest, hay, grass
+ 17.959534 .15
T Harvest legume hay crops such as Alfalfa and Red clover and grass-legume mixed hay such as Alfalfa-Bromegrass.
T Use Harvest, grass hay" for pure grass hay. Rev 11/17/01 DTL"  MAS 11-29-06
T
T Reset the fuel use to 1.92 gal/ac MAS 10-21-11
+
G 02 Biomass Manipulation
+ 1.0
P 31 Kill or Defoliate Growing Crop
+ 0
P 42 Cut/Remove Biomass to Height (flags)
+ 1 0 0 0 0 101.600204 .85 .85 1
P 34 Change Standing Biomass Fall Rate
+ 0 1.1 1.08 1.06 1.04 1.0
+ 0.9 0.92 0.93 0.95 1.0
P 40 End crop Biomass Manipulation
P 24 Flatten Standing Biomass
+ 14 .6 .5 .4 .5 .5
#------------
D 20/06/09
O 03 Manure spreader, slurry
+ 11.505327 .29 1.7881091 0.0 1.7881091 1.3410819 3.5762181
T Created from RUSLE file MAS 9/19/06.
T This assumes a defult residue type of  manure slurry using a solid spread with a liquid end gate spreader.
T User needs to change to the correct manure type, make a calulation on the dry matter applied, and change the value in MCREW.
T This opn is built for an application of 10 ton/ac 10% dry matter surface applied manure.
T 10 tons x 2000 lbs/ac = 20,000 lbs/ac x 0.1 = 2,000 lbs/ac applied.
T MAS 12-5-07
+
G 01 Tillage
+ 0.0 0 1 0.0 0.0 0.0
P 24 Flatten Standing Biomass
+ 14 .1 .1 .1 .1 1.0
G 03 Crop Name
+ manure, slurry
P 66 Add Manure Residue Amount
+ 0.0 0.0 0.0 0.0 1
+ 0.0 0.0 0.0 0.0
+ 0.22417001 0.0
+ .06 .06 .06 .06 0.169 0.0050 1 0.6500045
+ -2.08165 0.548606
T Enter crop notes here.
#------------
D 01/08/09
O 04 Harvest, hay, grass
+ 17.959534 .15
T Harvest legume hay crops such as Alfalfa and Red clover and grass-legume mixed hay such as Alfalfa-Bromegrass.
T Use Harvest, grass hay" for pure grass hay. Rev 11/17/01 DTL"  MAS 11-29-06
T
T Reset the fuel use to 1.92 gal/ac MAS 10-21-11
+
G 02 Biomass Manipulation
+ 1.0
P 31 Kill or Defoliate Growing Crop
+ 0
P 42 Cut/Remove Biomass to Height (flags)
+ 1 0 0 0 0 101.600204 .85 .85 1
P 34 Change Standing Biomass Fall Rate
+ 0 1.1 1.08 1.06 1.04 1.0
+ 0.9 0.92 0.93 0.95 1.0
P 40 End crop Biomass Manipulation
P 24 Flatten Standing Biomass
+ 14 .6 .5 .4 .5 .5
#------------
D 05/08/09
O 03 Manure spreader, slurry
+ 11.505327 .29 1.7881091 0.0 1.7881091 1.3410819 3.5762181
T Created from RUSLE file MAS 9/19/06.
T This assumes a defult residue type of  manure slurry using a solid spread with a liquid end gate spreader.
T User needs to change to the correct manure type, make a calulation on the dry matter applied, and change the value in MCREW.
T This opn is built for an application of 10 ton/ac 10% dry matter surface applied manure.
T 10 tons x 2000 lbs/ac = 20,000 lbs/ac x 0.1 = 2,000 lbs/ac applied.
T MAS 12-5-07
+
G 01 Tillage
+ 0.0 0 1 0.0 0.0 0.0
P 24 Flatten Standing Biomass
+ 14 .1 .1 .1 .1 1.0
G 03 Crop Name
+ manure, slurry
P 66 Add Manure Residue Amount
+ 0.0 0.0 0.0 0.0 1
+ 0.0 0.0 0.0 0.0
+ 0.22417001 0.0
+ .06 .06 .06 .06 0.169 0.0050 1 0.6500045
+ -2.08165 0.548606
T Enter crop notes here.
#------------
D 10/05/10
O 03 Manure spreader, slurry
+ 11.505327 .29 1.7881091 0.0 1.7881091 1.3410819 3.5762181
T Created from RUSLE file MAS 9/19/06.
T This assumes a defult residue type of  manure slurry using a solid spread with a liquid end gate spreader.
T User needs to change to the correct manure type, make a calulation on the dry matter applied, and change the value in MCREW.
T This opn is built for an application of 10 ton/ac 10% dry matter surface applied manure.
T 10 tons x 2000 lbs/ac = 20,000 lbs/ac x 0.1 = 2,000 lbs/ac applied.
T MAS 12-5-07
+
G 01 Tillage
+ 0.0 0 1 0.0 0.0 0.0
P 24 Flatten Standing Biomass
+ 14 .1 .1 .1 .1 1.0
G 03 Crop Name
+ manure, slurry
P 66 Add Manure Residue Amount
+ 0.0 0.0 0.0 0.0 1
+ 0.0 0.0 0.0 0.0
+ 0.22417001 0.0
+ .06 .06 .06 .06 0.169 0.0050 1 0.6500045
+ -2.08165 0.548606
T Enter crop notes here.
#------------
D 16/06/10
O 04 Harvest, hay, grass
+ 17.959534 .15
T Harvest legume hay crops such as Alfalfa and Red clover and grass-legume mixed hay such as Alfalfa-Bromegrass.
T Use Harvest, grass hay" for pure grass hay. Rev 11/17/01 DTL"  MAS 11-29-06
T
T Reset the fuel use to 1.92 gal/ac MAS 10-21-11
+
G 02 Biomass Manipulation
+ 1.0
P 31 Kill or Defoliate Growing Crop
+ 0
P 42 Cut/Remove Biomass to Height (flags)
+ 1 0 0 0 0 101.600204 .85 .85 1
P 34 Change Standing Biomass Fall Rate
+ 0 1.1 1.08 1.06 1.04 1.0
+ 0.9 0.92 0.93 0.95 1.0
P 40 End crop Biomass Manipulation
P 24 Flatten Standing Biomass
+ 14 .6 .5 .4 .5 .5
#------------
D 20/06/10
O 03 Manure spreader, slurry
+ 11.505327 .29 1.7881091 0.0 1.7881091 1.3410819 3.5762181
T Created from RUSLE file MAS 9/19/06.
T This assumes a defult residue type of  manure slurry using a solid spread with a liquid end gate spreader.
T User needs to change to the correct manure type, make a calulation on the dry matter applied, and change the value in MCREW.
T This opn is built for an application of 10 ton/ac 10% dry matter surface applied manure.
T 10 tons x 2000 lbs/ac = 20,000 lbs/ac x 0.1 = 2,000 lbs/ac applied.
T MAS 12-5-07
+
G 01 Tillage
+ 0.0 0 1 0.0 0.0 0.0
P 24 Flatten Standing Biomass
+ 14 .1 .1 .1 .1 1.0
G 03 Crop Name
+ manure, slurry
P 66 Add Manure Residue Amount
+ 0.0 0.0 0.0 0.0 1
+ 0.0 0.0 0.0 0.0
+ 0.22417001 0.0
+ .06 .06 .06 .06 0.169 0.0050 1 0.6500045
+ -2.08165 0.548606
T Enter crop notes here.
#------------
D 01/08/10
O 04 Harvest, hay, grass
+ 17.959534 .15
T Harvest legume hay crops such as Alfalfa and Red clover and grass-legume mixed hay such as Alfalfa-Bromegrass.
T Use Harvest, grass hay" for pure grass hay. Rev 11/17/01 DTL"  MAS 11-29-06
T
T Reset the fuel use to 1.92 gal/ac MAS 10-21-11
+
G 02 Biomass Manipulation
+ 1.0
P 31 Kill or Defoliate Growing Crop
+ 0
P 42 Cut/Remove Biomass to Height (flags)
+ 1 0 0 0 0 101.600204 .85 .85 1
P 34 Change Standing Biomass Fall Rate
+ 0 1.1 1.08 1.06 1.04 1.0
+ 0.9 0.92 0.93 0.95 1.0
P 40 End crop Biomass Manipulation
P 24 Flatten Standing Biomass
+ 14 .6 .5 .4 .5 .5
#------------
D 05/08/10
O 03 Manure spreader, slurry
+ 11.505327 .29 1.7881091 0.0 1.7881091 1.3410819 3.5762181
T Created from RUSLE file MAS 9/19/06.
T This assumes a defult residue type of  manure slurry using a solid spread with a liquid end gate spreader.
T User needs to change to the correct manure type, make a calulation on the dry matter applied, and change the value in MCREW.
T This opn is built for an application of 10 ton/ac 10% dry matter surface applied manure.
T 10 tons x 2000 lbs/ac = 20,000 lbs/ac x 0.1 = 2,000 lbs/ac applied.
T MAS 12-5-07
+
G 01 Tillage
+ 0.0 0 1 0.0 0.0 0.0
P 24 Flatten Standing Biomass
+ 14 .1 .1 .1 .1 1.0
G 03 Crop Name
+ manure, slurry
P 66 Add Manure Residue Amount
+ 0.0 0.0 0.0 0.0 1
+ 0.0 0.0 0.0 0.0
+ 0.22417001 0.0
+ .06 .06 .06 .06 0.169 0.0050 1 0.6500045
+ -2.08165 0.548606
T Enter crop notes here.
#------------
*END
*EOF
