Version: 1.5
*START 4
N Originating Program: RUSLE2
N Skel Format Version: 1.1
N This management file was originally converted from the NRCS standard XML format on - Thu Jun 28 14:03:09 PDT 2012
N This management file was updated to contain the most current crop and operation records for WEPS on - Tue Dec 17 19:09:10 CST 2013
#------------
D 05/05/01
O 03 Disk, tandem heavy primary op
+ 7.0154433 39 2.2351363 0.0 2.2351363 1.3410819 2.6821637
T 11-12in. Spacing, Front and Rear
T Recommended for primary tillage in medium to heavy soils
T Excellent residue-handling capability. MAS 10-26-06
+
G 01 Tillage
+ 152.4003 1.0 1.0 152.4003 101.600204 177.80035
P 01 Break Crust
P 02 Random Roughness
+ 1 38.100075
P 05 Ridges and Dikes
+ 1 101.600204 279.40057 0.0 0.0 0.0
P 11 Aggregate Crushing
+ 2.8 0.75
P 12 Soil Loosening
+ 0.9
P 13 Soil Layer Mixing
+ 0.4
P 31 Kill or Defoliate Growing Crop
+ 2
P 40 End crop Biomass Manipulation
P 24 Flatten Standing Biomass
+ 0 1.0 0.9 0.8 0.5 1.0
P 25 Bury Flat Biomass
+ 1 0.95 0.85 0.8 0.6 0.95
P 26 Resurface Buried Biomass
+ 0.05 0.06 0.07 0.08 0.05
P 34 Change Standing Biomass Fall Rate
+ 7 3.0 2.5 2.0 1.5 1.0
+ 0.5 0.6 0.7 0.8 1.0
#------------
D 10/05/01
O 03 Disk, tandem light finishing
+ 3.7415698 19.5 2.2351363 0.0 2.2351363 1.3410819 2.6821637
T 6/8/01 DTL RUSLE.  7in sp.  This is tool used to finish a seedbed.  MAS 10-26-06
+
G 01 Tillage
+ 101.600204 0.5 1.0 101.600204 76.20015 127.00026
P 01 Break Crust
P 02 Random Roughness
+ 1 15.240031
P 05 Ridges and Dikes
+ 1 12.700026 177.80035 0.0 0.0 0.0
P 11 Aggregate Crushing
+ 2.8 0.75
P 12 Soil Loosening
+ 0.75
P 13 Soil Layer Mixing
+ 0.35
P 31 Kill or Defoliate Growing Crop
+ 2
P 40 End crop Biomass Manipulation
P 24 Flatten Standing Biomass
+ 0 0.85 0.7 0.6 0.5 1.0
P 25 Bury Flat Biomass
+ 1 0.73 0.63 0.55 0.4 0.73
P 26 Resurface Buried Biomass
+ 0.02 0.04 0.02 0.05 0.02
P 34 Change Standing Biomass Fall Rate
+ 7 3.0 2.5 2.0 1.5 1.0
+ 0.5 0.6 0.7 0.8 1.0
#------------
D 15/05/01
O 03 Fert applic. shank low disturbance, 12 in
+ 8.418531 3.25 2.2351363 0.0 2.2351363 1.5645955 2.9056773
T Minimum disturbance fertilizer injector shank.012904 DTL RUSLE MAS 10-26-06
T G2 was added into file in front of the flattening (P24), burial (P25), and resurfacing (P26) factors because the area affected is less than 1.0 and
T the RUSLE values were normalized to 1.0.  This change will imulate the correct residue changes based on the method set forth in RUSLE.
T RUSLE's factors have been redused to based on the area affected.
T The stalk fall rate factor (P34) was moved ahead of the new (G2) factor to set the fall rate to the less than 1.0 area affected.  8/7/07 MAS
+ 
G 01 Tillage
+ 101.600204 0.8 0.25 101.600204 76.20015 152.4003
P 01 Break Crust
P 02 Random Roughness
+ 1 15.240031
P 05 Ridges and Dikes
+ 1 50.800102 304.8006 25.400051 0.0 0.0
P 11 Aggregate Crushing
+ 2.4 2.0
P 12 Soil Loosening
+ 0.7
P 13 Soil Layer Mixing
+ 0.2
P 40 End crop Biomass Manipulation
P 34 Change Standing Biomass Fall Rate
+ 7 3.0 2.5 2.0 1.5 1.0
+ 0.5 0.6 0.7 0.8 1.0
P 24 Flatten Standing Biomass
+ 0 0.5 0.45 0.4 0.4 1.0
P 25 Bury Flat Biomass
+ 4 0.2 .15 .1 0.08 0.14
P 26 Resurface Buried Biomass
+ 0.06 0.06 0.06 0.1 0.06
#------------
D 15/05/01
O 03 Planter, double disk opnr
+ 4.1157265 2.4375 2.2351363 0.0 2.2351363 1.5645955 2.9056773
T This is a standard planter on 30 in sp with a 1 in ridge.  Created in RUSLE 6/7/01.  MAS 8/7/07
T G2 was added into file in front of the flattening (P24), burial (P25), and resurfacing (P26) factors because the area affected is less than 1.0 and
T the RUSLE values were normalized to 1.0.  This change will imulate the correct residue changes based on the method set forth in RUSLE.
T RUSLE's factors have been redused to based on the area affected.
T The stalk fall rate factor (P34) was moved ahead of the new (G2) factor to set the fall rate to the less than 1.0 area affected.  8/7/07 MAS
+
G 01 Tillage
+ 63.500126 0.5 .15 63.500126 50.800102 101.600204
P 01 Break Crust
P 02 Random Roughness
+ 1 10.160021
P 05 Ridges and Dikes
+ 1 50.800102 762.0015 635.0013 0.0 0.0
P 11 Aggregate Crushing
+ 2.8 0.75
P 12 Soil Loosening
+ 0.6
P 13 Soil Layer Mixing
+ 0.35
P 34 Change Standing Biomass Fall Rate
+ 7 3.0 2.5 2.0 1.5 1.0
+ 0.5 0.6 0.7 0.8 1.0
G 02 Biomass Manipulation
+ 1.0
P 24 Flatten Standing Biomass
+ 0 .3 .25 .2 0.1 1.0
P 25 Bury Flat Biomass
+ 1 .0525 0.0375 .03 .015 .03
P 26 Resurface Buried Biomass
+ .01 .01 .01 .02 .01
G 03 Crop Name
+ Potato, late, harvest
P 51 Seeding Configuration
+ 1 0.0 2
+ 5.0 4.0 1 600 1.0 1.0 5
+ cwt/ac
+ 79.0 89.3 7 1.0 0.65 0.8
+ 0.8 0.05 0.6096074 2.0 25.0 0 120 1600.0
+ -5.0 -15.0 0.01 0.95 0.0 32
+ 0.0 0.6553 0.3159 -0.061 -3.0E-4 0.9911 0.3415 0.0494
+ 0.4163 -0.061 2.6 1.0 30.0 0.05 0 1.0
+ 12000.0 2700.0 3.0 0.03 0.0 0.0 0.9 1
+ 0.02 0.02 0.02 0.02 0.2 0.0050 20.0 5.227942
+ -1.20379 0.604887 0.0313 0.024658702 0.0 0.0 0.0 0.0
T Represents high yielding typically irrigated Potatoes - white, russet, red (all but sweet). 60,000 lb (600 cwt), 30 ton/ac yield .  36" rows.
T Residue at harvest includes mass before chemical kill.  Base location ID, WA, NM.
T
T File was tested in Grant Co. WA and Bingham Co. ID.  Biomas Conv Eff factor was at 32.  Yields were low.
T At 40 the yields were 553 cwt/ac in WA and 485 cwt/ac in ID.  I have made the change to get the yields closer
T to the actual field values.  MAS 9-26-07
T
T Harvest biomass ratio is set using two studies.  One from the PNW irrigated and the other in MN.
T Both sites are were sandy soils with irrigation.  Yields were 600 cwt/ac.  MAS 7-3-08
#------------
D 31/05/01
O 04 Sprayer, post emergence
+ 1.2160101 .15
T Spray pest control chemicals on growing crop.  Crop is not killed.
T In the MCREW management screen the user must select the kind of weeds killed in the growing crop as external residue.   080404 DTL
T Cloned from Defoliate (spray) crop.oprn, Changed the P31 to No crop kill and added G4 to add material to field MAS 9-28-06
T DO NOT LEAVE CROP COLUMN SET TO "no crop".  User must select the crop and then drill into the operation and specify the amount of weed
T mass that will be killed and turned into residue.
+
G 03 Crop Name
+ weed residue; 0-3 mo
P 65 Add Crop Residue Amounts
+ 0.0 0.0 0.0 0.028021252 1
+ 0.0 0.0 0.0056042504 152.4003
+ 0.025 0.025 0.025 0.025 0.169 0.0050 17.1 5.227942
+ -1.20379 0.604887
T Enter crop notes here.
#------------
D 15/06/01
O 03 Bed shaper
+ 3.554491 19.5 2.2351363 0.0 2.2351363 1.5645955 2.9056773
T RUSLE Notes: Bed shaping operation on existing beds.  May include drip tape installation. 10/28/01 DTL
T Cloned 2-15-07 MAS
T G2 was added into file in front of the flattening (P24), burial (P25), and resurfacing (P26) factors because the area affected is less than 1.0 and
T the RUSLE values were normalized to 1.0.  This change will imulate the correct residue changes based on the method set forth in RUSLE.
T RUSLE's factors have been redused to based on the area affected.
T The stalk fall rate factor (P34) was moved ahead of the new (G2) factor to set the fall rate to the  less than 1.0 area affected.  8/8/07 MAS
+
G 01 Tillage
+ 101.600204 .6 .75 101.600204 76.20015 152.4003
P 01 Break Crust
P 02 Random Roughness
+ 1 15.240031
P 11 Aggregate Crushing
+ 3.0 -0.22
P 12 Soil Loosening
+ 0.75
P 13 Soil Layer Mixing
+ 0.05
P 05 Ridges and Dikes
+ 1 203.20041 760.0 381.00076 0.0 0.0
P 34 Change Standing Biomass Fall Rate
+ 7 3.0 2.5 2.0 1.5 1.0
+ 0.5 0.6 0.7 0.8 1.0
G 02 Biomass Manipulation
+ 1.0
P 24 Flatten Standing Biomass
+ 0 0.5 0.45 0.4 0.3 1.00
P 25 Bury Flat Biomass
+ 1 0.38 0.3 0.23 0.2 0.28
P 26 Resurface Buried Biomass
+ 0.02 0.02 0.02 0.02 0.02
#------------
D 16/06/01
O 04 Sprayer, fungicide
+ 1.2160101 0.15
T Spray fungicide on growing crop.   Crop is not killed.  11/17/01 DTL Revised Sprayer,
T insecticide for fungicide application 82211 LOS
T
T Added to DB 3-1-12 MAS
+ 
#------------
D 10/07/01
O 04 Sprayer, fungicide
+ 1.2160101 0.15
T Spray fungicide on growing crop.   Crop is not killed.  11/17/01 DTL Revised Sprayer,
T insecticide for fungicide application 82211 LOS
T
T Added to DB 3-1-12 MAS
+ 
#------------
D 15/07/01
O 03 Bed shaper
+ 3.554491 19.5 2.2351363 0.0 2.2351363 1.5645955 2.9056773
T RUSLE Notes: Bed shaping operation on existing beds.  May include drip tape installation. 10/28/01 DTL
T Cloned 2-15-07 MAS
T G2 was added into file in front of the flattening (P24), burial (P25), and resurfacing (P26) factors because the area affected is less than 1.0 and
T the RUSLE values were normalized to 1.0.  This change will imulate the correct residue changes based on the method set forth in RUSLE.
T RUSLE's factors have been redused to based on the area affected.
T The stalk fall rate factor (P34) was moved ahead of the new (G2) factor to set the fall rate to the  less than 1.0 area affected.  8/8/07 MAS
+
G 01 Tillage
+ 101.600204 .6 .75 101.600204 76.20015 152.4003
P 01 Break Crust
P 02 Random Roughness
+ 1 15.240031
P 11 Aggregate Crushing
+ 3.0 -0.22
P 12 Soil Loosening
+ 0.75
P 13 Soil Layer Mixing
+ 0.05
P 05 Ridges and Dikes
+ 1 203.20041 760.0 381.00076 0.0 0.0
P 34 Change Standing Biomass Fall Rate
+ 7 3.0 2.5 2.0 1.5 1.0
+ 0.5 0.6 0.7 0.8 1.0
G 02 Biomass Manipulation
+ 1.0
P 24 Flatten Standing Biomass
+ 0 0.5 0.45 0.4 0.3 1.00
P 25 Bury Flat Biomass
+ 1 0.38 0.3 0.23 0.2 0.28
P 26 Resurface Buried Biomass
+ 0.02 0.02 0.02 0.02 0.02
#------------
D 25/07/01
O 04 Sprayer, fungicide
+ 1.2160101 0.15
T Spray fungicide on growing crop.   Crop is not killed.  11/17/01 DTL Revised Sprayer,
T insecticide for fungicide application 82211 LOS
T
T Added to DB 3-1-12 MAS
+ 
#------------
D 10/08/01
O 04 Sprayer, fungicide
+ 1.2160101 0.15
T Spray fungicide on growing crop.   Crop is not killed.  11/17/01 DTL Revised Sprayer,
T insecticide for fungicide application 82211 LOS
T
T Added to DB 3-1-12 MAS
+ 
#------------
D 21/09/01
O 03 Harvest, dig root crops res. buried
+ 17.491838 27.378 1.3410819 0.0 1.5645955 1.3410819 2.9056773
T Harvest, root crops like potatoes, sugar beets, carrots, and onions.
T Surface is rough with 4 ridges and much of the residue is buried.
T Rev 11-18-04 DTL RUSLE MAS 10-26-06
T
T P24 was changed to show that all residue types are flattened.
T This havest now flattens all residue types 100%.  MAS 1-18-11
+
G 01 Tillage
+ 177.80035 1.0 1.0 177.80035 152.4003 203.20041
P 01 Break Crust
P 02 Random Roughness
+ 1 16.510033
P 05 Ridges and Dikes
+ 1 101.600204 3657.6072 3048.006 0.0 0.0
P 11 Aggregate Crushing
+ 1.4 -1.2
P 12 Soil Loosening
+ 0.7
P 13 Soil Layer Mixing
+ 0.9
P 31 Kill or Defoliate Growing Crop
+ 2
G 02 Biomass Manipulation
+ 1.0
P 62 Remove (by age pool) Plant/Residue Material
+ 1 1 0 1 1 3 2 0.0 0.0 0.0 1.0 0.0
P 40 End crop Biomass Manipulation
P 24 Flatten Standing Biomass
+ 0 1.0 1.0 1.0 1.0 1.0
P 25 Bury Flat Biomass
+ 2 .95 .95 .95 .95 1
P 26 Resurface Buried Biomass
+ 0.01 0.01 0.03 0.01 0.01
#------------
D 05/05/02
O 03 Disk, tandem heavy primary op
+ 7.0154433 39 2.2351363 0.0 2.2351363 1.3410819 2.6821637
T 11-12in. Spacing, Front and Rear
T Recommended for primary tillage in medium to heavy soils
T Excellent residue-handling capability. MAS 10-26-06
+
G 01 Tillage
+ 152.4003 1.0 1.0 152.4003 101.600204 177.80035
P 01 Break Crust
P 02 Random Roughness
+ 1 38.100075
P 05 Ridges and Dikes
+ 1 101.600204 279.40057 0.0 0.0 0.0
P 11 Aggregate Crushing
+ 2.8 0.75
P 12 Soil Loosening
+ 0.9
P 13 Soil Layer Mixing
+ 0.4
P 31 Kill or Defoliate Growing Crop
+ 2
P 40 End crop Biomass Manipulation
P 24 Flatten Standing Biomass
+ 0 1.0 0.9 0.8 0.5 1.0
P 25 Bury Flat Biomass
+ 1 0.95 0.85 0.8 0.6 0.95
P 26 Resurface Buried Biomass
+ 0.05 0.06 0.07 0.08 0.05
P 34 Change Standing Biomass Fall Rate
+ 7 3.0 2.5 2.0 1.5 1.0
+ 0.5 0.6 0.7 0.8 1.0
#------------
D 10/05/02
O 03 Disk, tandem light finishing
+ 3.7415698 19.5 2.2351363 0.0 2.2351363 1.3410819 2.6821637
T 6/8/01 DTL RUSLE.  7in sp.  This is tool used to finish a seedbed.  MAS 10-26-06
+
G 01 Tillage
+ 101.600204 0.5 1.0 101.600204 76.20015 127.00026
P 01 Break Crust
P 02 Random Roughness
+ 1 15.240031
P 05 Ridges and Dikes
+ 1 12.700026 177.80035 0.0 0.0 0.0
P 11 Aggregate Crushing
+ 2.8 0.75
P 12 Soil Loosening
+ 0.75
P 13 Soil Layer Mixing
+ 0.35
P 31 Kill or Defoliate Growing Crop
+ 2
P 40 End crop Biomass Manipulation
P 24 Flatten Standing Biomass
+ 0 0.85 0.7 0.6 0.5 1.0
P 25 Bury Flat Biomass
+ 1 0.73 0.63 0.55 0.4 0.73
P 26 Resurface Buried Biomass
+ 0.02 0.04 0.02 0.05 0.02
P 34 Change Standing Biomass Fall Rate
+ 7 3.0 2.5 2.0 1.5 1.0
+ 0.5 0.6 0.7 0.8 1.0
#------------
D 15/05/02
O 03 Fert applic. shank low disturbance, 12 in
+ 8.418531 3.25 2.2351363 0.0 2.2351363 1.5645955 2.9056773
T Minimum disturbance fertilizer injector shank.012904 DTL RUSLE MAS 10-26-06
T G2 was added into file in front of the flattening (P24), burial (P25), and resurfacing (P26) factors because the area affected is less than 1.0 and
T the RUSLE values were normalized to 1.0.  This change will imulate the correct residue changes based on the method set forth in RUSLE.
T RUSLE's factors have been redused to based on the area affected.
T The stalk fall rate factor (P34) was moved ahead of the new (G2) factor to set the fall rate to the less than 1.0 area affected.  8/7/07 MAS
+ 
G 01 Tillage
+ 101.600204 0.8 0.25 101.600204 76.20015 152.4003
P 01 Break Crust
P 02 Random Roughness
+ 1 15.240031
P 05 Ridges and Dikes
+ 1 50.800102 304.8006 25.400051 0.0 0.0
P 11 Aggregate Crushing
+ 2.4 2.0
P 12 Soil Loosening
+ 0.7
P 13 Soil Layer Mixing
+ 0.2
P 40 End crop Biomass Manipulation
P 34 Change Standing Biomass Fall Rate
+ 7 3.0 2.5 2.0 1.5 1.0
+ 0.5 0.6 0.7 0.8 1.0
P 24 Flatten Standing Biomass
+ 0 0.5 0.45 0.4 0.4 1.0
P 25 Bury Flat Biomass
+ 4 0.2 .15 .1 0.08 0.14
P 26 Resurface Buried Biomass
+ 0.06 0.06 0.06 0.1 0.06
#------------
D 15/05/02
O 03 Planter, double disk opnr
+ 4.1157265 2.4375 2.2351363 0.0 2.2351363 1.5645955 2.9056773
T This is a standard planter on 30 in sp with a 1 in ridge.  Created in RUSLE 6/7/01.  MAS 8/7/07
T G2 was added into file in front of the flattening (P24), burial (P25), and resurfacing (P26) factors because the area affected is less than 1.0 and
T the RUSLE values were normalized to 1.0.  This change will imulate the correct residue changes based on the method set forth in RUSLE.
T RUSLE's factors have been redused to based on the area affected.
T The stalk fall rate factor (P34) was moved ahead of the new (G2) factor to set the fall rate to the less than 1.0 area affected.  8/7/07 MAS
+
G 01 Tillage
+ 63.500126 0.5 .15 63.500126 50.800102 101.600204
P 01 Break Crust
P 02 Random Roughness
+ 1 10.160021
P 05 Ridges and Dikes
+ 1 50.800102 762.0015 635.0013 0.0 0.0
P 11 Aggregate Crushing
+ 2.8 0.75
P 12 Soil Loosening
+ 0.6
P 13 Soil Layer Mixing
+ 0.35
P 34 Change Standing Biomass Fall Rate
+ 7 3.0 2.5 2.0 1.5 1.0
+ 0.5 0.6 0.7 0.8 1.0
G 02 Biomass Manipulation
+ 1.0
P 24 Flatten Standing Biomass
+ 0 .3 .25 .2 0.1 1.0
P 25 Bury Flat Biomass
+ 1 .0525 0.0375 .03 .015 .03
P 26 Resurface Buried Biomass
+ .01 .01 .01 .02 .01
G 03 Crop Name
+ Potato, late, harvest
P 51 Seeding Configuration
+ 1 0.0 2
+ 5.0 4.0 1 600 1.0 1.0 5
+ cwt/ac
+ 79.0 89.3 7 1.0 0.65 0.8
+ 0.8 0.05 0.6096074 2.0 25.0 0 120 1600.0
+ -5.0 -15.0 0.01 0.95 0.0 32
+ 0.0 0.6553 0.3159 -0.061 -3.0E-4 0.9911 0.3415 0.0494
+ 0.4163 -0.061 2.6 1.0 30.0 0.05 0 1.0
+ 12000.0 2700.0 3.0 0.03 0.0 0.0 0.9 1
+ 0.02 0.02 0.02 0.02 0.2 0.0050 20.0 5.227942
+ -1.20379 0.604887 0.0313 0.024658702 0.0 0.0 0.0 0.0
T Represents high yielding typically irrigated Potatoes - white, russet, red (all but sweet). 60,000 lb (600 cwt), 30 ton/ac yield .  36" rows.
T Residue at harvest includes mass before chemical kill.  Base location ID, WA, NM.
T
T File was tested in Grant Co. WA and Bingham Co. ID.  Biomas Conv Eff factor was at 32.  Yields were low.
T At 40 the yields were 553 cwt/ac in WA and 485 cwt/ac in ID.  I have made the change to get the yields closer
T to the actual field values.  MAS 9-26-07
T
T Harvest biomass ratio is set using two studies.  One from the PNW irrigated and the other in MN.
T Both sites are were sandy soils with irrigation.  Yields were 600 cwt/ac.  MAS 7-3-08
#------------
D 31/05/02
O 04 Sprayer, post emergence
+ 1.2160101 .15
T Spray pest control chemicals on growing crop.  Crop is not killed.
T In the MCREW management screen the user must select the kind of weeds killed in the growing crop as external residue.   080404 DTL
T Cloned from Defoliate (spray) crop.oprn, Changed the P31 to No crop kill and added G4 to add material to field MAS 9-28-06
T DO NOT LEAVE CROP COLUMN SET TO "no crop".  User must select the crop and then drill into the operation and specify the amount of weed
T mass that will be killed and turned into residue.
+
G 03 Crop Name
+ weed residue; 0-3 mo
P 65 Add Crop Residue Amounts
+ 0.0 0.0 0.0 0.028021252 1
+ 0.0 0.0 0.0056042504 152.4003
+ 0.025 0.025 0.025 0.025 0.169 0.0050 17.1 5.227942
+ -1.20379 0.604887
T Enter crop notes here.
#------------
D 15/06/02
O 03 Bed shaper
+ 3.554491 19.5 2.2351363 0.0 2.2351363 1.5645955 2.9056773
T RUSLE Notes: Bed shaping operation on existing beds.  May include drip tape installation. 10/28/01 DTL
T Cloned 2-15-07 MAS
T G2 was added into file in front of the flattening (P24), burial (P25), and resurfacing (P26) factors because the area affected is less than 1.0 and
T the RUSLE values were normalized to 1.0.  This change will imulate the correct residue changes based on the method set forth in RUSLE.
T RUSLE's factors have been redused to based on the area affected.
T The stalk fall rate factor (P34) was moved ahead of the new (G2) factor to set the fall rate to the  less than 1.0 area affected.  8/8/07 MAS
+
G 01 Tillage
+ 101.600204 .6 .75 101.600204 76.20015 152.4003
P 01 Break Crust
P 02 Random Roughness
+ 1 15.240031
P 11 Aggregate Crushing
+ 3.0 -0.22
P 12 Soil Loosening
+ 0.75
P 13 Soil Layer Mixing
+ 0.05
P 05 Ridges and Dikes
+ 1 203.20041 760.0 381.00076 0.0 0.0
P 34 Change Standing Biomass Fall Rate
+ 7 3.0 2.5 2.0 1.5 1.0
+ 0.5 0.6 0.7 0.8 1.0
G 02 Biomass Manipulation
+ 1.0
P 24 Flatten Standing Biomass
+ 0 0.5 0.45 0.4 0.3 1.00
P 25 Bury Flat Biomass
+ 1 0.38 0.3 0.23 0.2 0.28
P 26 Resurface Buried Biomass
+ 0.02 0.02 0.02 0.02 0.02
#------------
D 16/06/02
O 04 Sprayer, fungicide
+ 1.2160101 0.15
T Spray fungicide on growing crop.   Crop is not killed.  11/17/01 DTL Revised Sprayer,
T insecticide for fungicide application 82211 LOS
T
T Added to DB 3-1-12 MAS
+ 
#------------
D 10/07/02
O 04 Sprayer, fungicide
+ 1.2160101 0.15
T Spray fungicide on growing crop.   Crop is not killed.  11/17/01 DTL Revised Sprayer,
T insecticide for fungicide application 82211 LOS
T
T Added to DB 3-1-12 MAS
+ 
#------------
D 15/07/02
O 03 Bed shaper
+ 3.554491 19.5 2.2351363 0.0 2.2351363 1.5645955 2.9056773
T RUSLE Notes: Bed shaping operation on existing beds.  May include drip tape installation. 10/28/01 DTL
T Cloned 2-15-07 MAS
T G2 was added into file in front of the flattening (P24), burial (P25), and resurfacing (P26) factors because the area affected is less than 1.0 and
T the RUSLE values were normalized to 1.0.  This change will imulate the correct residue changes based on the method set forth in RUSLE.
T RUSLE's factors have been redused to based on the area affected.
T The stalk fall rate factor (P34) was moved ahead of the new (G2) factor to set the fall rate to the  less than 1.0 area affected.  8/8/07 MAS
+
G 01 Tillage
+ 101.600204 .6 .75 101.600204 76.20015 152.4003
P 01 Break Crust
P 02 Random Roughness
+ 1 15.240031
P 11 Aggregate Crushing
+ 3.0 -0.22
P 12 Soil Loosening
+ 0.75
P 13 Soil Layer Mixing
+ 0.05
P 05 Ridges and Dikes
+ 1 203.20041 760.0 381.00076 0.0 0.0
P 34 Change Standing Biomass Fall Rate
+ 7 3.0 2.5 2.0 1.5 1.0
+ 0.5 0.6 0.7 0.8 1.0
G 02 Biomass Manipulation
+ 1.0
P 24 Flatten Standing Biomass
+ 0 0.5 0.45 0.4 0.3 1.00
P 25 Bury Flat Biomass
+ 1 0.38 0.3 0.23 0.2 0.28
P 26 Resurface Buried Biomass
+ 0.02 0.02 0.02 0.02 0.02
#------------
D 25/07/02
O 04 Sprayer, fungicide
+ 1.2160101 0.15
T Spray fungicide on growing crop.   Crop is not killed.  11/17/01 DTL Revised Sprayer,
T insecticide for fungicide application 82211 LOS
T
T Added to DB 3-1-12 MAS
+ 
#------------
D 10/08/02
O 04 Sprayer, fungicide
+ 1.2160101 0.15
T Spray fungicide on growing crop.   Crop is not killed.  11/17/01 DTL Revised Sprayer,
T insecticide for fungicide application 82211 LOS
T
T Added to DB 3-1-12 MAS
+ 
#------------
D 21/09/02
O 03 Harvest, dig root crops res. buried
+ 17.491838 27.378 1.3410819 0.0 1.5645955 1.3410819 2.9056773
T Harvest, root crops like potatoes, sugar beets, carrots, and onions.
T Surface is rough with 4 ridges and much of the residue is buried.
T Rev 11-18-04 DTL RUSLE MAS 10-26-06
T
T P24 was changed to show that all residue types are flattened.
T This havest now flattens all residue types 100%.  MAS 1-18-11
+
G 01 Tillage
+ 177.80035 1.0 1.0 177.80035 152.4003 203.20041
P 01 Break Crust
P 02 Random Roughness
+ 1 16.510033
P 05 Ridges and Dikes
+ 1 101.600204 3657.6072 3048.006 0.0 0.0
P 11 Aggregate Crushing
+ 1.4 -1.2
P 12 Soil Loosening
+ 0.7
P 13 Soil Layer Mixing
+ 0.9
P 31 Kill or Defoliate Growing Crop
+ 2
G 02 Biomass Manipulation
+ 1.0
P 62 Remove (by age pool) Plant/Residue Material
+ 1 1 0 1 1 3 2 0.0 0.0 0.0 1.0 0.0
P 40 End crop Biomass Manipulation
P 24 Flatten Standing Biomass
+ 0 1.0 1.0 1.0 1.0 1.0
P 25 Bury Flat Biomass
+ 2 .95 .95 .95 .95 1
P 26 Resurface Buried Biomass
+ 0.01 0.01 0.03 0.01 0.01
#------------
D 05/05/03
O 03 Disk, tandem heavy primary op
+ 7.0154433 39 2.2351363 0.0 2.2351363 1.3410819 2.6821637
T 11-12in. Spacing, Front and Rear
T Recommended for primary tillage in medium to heavy soils
T Excellent residue-handling capability. MAS 10-26-06
+
G 01 Tillage
+ 152.4003 1.0 1.0 152.4003 101.600204 177.80035
P 01 Break Crust
P 02 Random Roughness
+ 1 38.100075
P 05 Ridges and Dikes
+ 1 101.600204 279.40057 0.0 0.0 0.0
P 11 Aggregate Crushing
+ 2.8 0.75
P 12 Soil Loosening
+ 0.9
P 13 Soil Layer Mixing
+ 0.4
P 31 Kill or Defoliate Growing Crop
+ 2
P 40 End crop Biomass Manipulation
P 24 Flatten Standing Biomass
+ 0 1.0 0.9 0.8 0.5 1.0
P 25 Bury Flat Biomass
+ 1 0.95 0.85 0.8 0.6 0.95
P 26 Resurface Buried Biomass
+ 0.05 0.06 0.07 0.08 0.05
P 34 Change Standing Biomass Fall Rate
+ 7 3.0 2.5 2.0 1.5 1.0
+ 0.5 0.6 0.7 0.8 1.0
#------------
D 10/05/03
O 03 Disk, tandem light finishing
+ 3.7415698 19.5 2.2351363 0.0 2.2351363 1.3410819 2.6821637
T 6/8/01 DTL RUSLE.  7in sp.  This is tool used to finish a seedbed.  MAS 10-26-06
+
G 01 Tillage
+ 101.600204 0.5 1.0 101.600204 76.20015 127.00026
P 01 Break Crust
P 02 Random Roughness
+ 1 15.240031
P 05 Ridges and Dikes
+ 1 12.700026 177.80035 0.0 0.0 0.0
P 11 Aggregate Crushing
+ 2.8 0.75
P 12 Soil Loosening
+ 0.75
P 13 Soil Layer Mixing
+ 0.35
P 31 Kill or Defoliate Growing Crop
+ 2
P 40 End crop Biomass Manipulation
P 24 Flatten Standing Biomass
+ 0 0.85 0.7 0.6 0.5 1.0
P 25 Bury Flat Biomass
+ 1 0.73 0.63 0.55 0.4 0.73
P 26 Resurface Buried Biomass
+ 0.02 0.04 0.02 0.05 0.02
P 34 Change Standing Biomass Fall Rate
+ 7 3.0 2.5 2.0 1.5 1.0
+ 0.5 0.6 0.7 0.8 1.0
#------------
D 15/05/03
O 03 Fert applic. shank low disturbance, 12 in
+ 8.418531 3.25 2.2351363 0.0 2.2351363 1.5645955 2.9056773
T Minimum disturbance fertilizer injector shank.012904 DTL RUSLE MAS 10-26-06
T G2 was added into file in front of the flattening (P24), burial (P25), and resurfacing (P26) factors because the area affected is less than 1.0 and
T the RUSLE values were normalized to 1.0.  This change will imulate the correct residue changes based on the method set forth in RUSLE.
T RUSLE's factors have been redused to based on the area affected.
T The stalk fall rate factor (P34) was moved ahead of the new (G2) factor to set the fall rate to the less than 1.0 area affected.  8/7/07 MAS
+ 
G 01 Tillage
+ 101.600204 0.8 0.25 101.600204 76.20015 152.4003
P 01 Break Crust
P 02 Random Roughness
+ 1 15.240031
P 05 Ridges and Dikes
+ 1 50.800102 304.8006 25.400051 0.0 0.0
P 11 Aggregate Crushing
+ 2.4 2.0
P 12 Soil Loosening
+ 0.7
P 13 Soil Layer Mixing
+ 0.2
P 40 End crop Biomass Manipulation
P 34 Change Standing Biomass Fall Rate
+ 7 3.0 2.5 2.0 1.5 1.0
+ 0.5 0.6 0.7 0.8 1.0
P 24 Flatten Standing Biomass
+ 0 0.5 0.45 0.4 0.4 1.0
P 25 Bury Flat Biomass
+ 4 0.2 .15 .1 0.08 0.14
P 26 Resurface Buried Biomass
+ 0.06 0.06 0.06 0.1 0.06
#------------
D 15/05/03
O 03 Planter, double disk opnr
+ 4.1157265 2.4375 2.2351363 0.0 2.2351363 1.5645955 2.9056773
T This is a standard planter on 30 in sp with a 1 in ridge.  Created in RUSLE 6/7/01.  MAS 8/7/07
T G2 was added into file in front of the flattening (P24), burial (P25), and resurfacing (P26) factors because the area affected is less than 1.0 and
T the RUSLE values were normalized to 1.0.  This change will imulate the correct residue changes based on the method set forth in RUSLE.
T RUSLE's factors have been redused to based on the area affected.
T The stalk fall rate factor (P34) was moved ahead of the new (G2) factor to set the fall rate to the less than 1.0 area affected.  8/7/07 MAS
+
G 01 Tillage
+ 63.500126 0.5 .15 63.500126 50.800102 101.600204
P 01 Break Crust
P 02 Random Roughness
+ 1 10.160021
P 05 Ridges and Dikes
+ 1 50.800102 762.0015 635.0013 0.0 0.0
P 11 Aggregate Crushing
+ 2.8 0.75
P 12 Soil Loosening
+ 0.6
P 13 Soil Layer Mixing
+ 0.35
P 34 Change Standing Biomass Fall Rate
+ 7 3.0 2.5 2.0 1.5 1.0
+ 0.5 0.6 0.7 0.8 1.0
G 02 Biomass Manipulation
+ 1.0
P 24 Flatten Standing Biomass
+ 0 .3 .25 .2 0.1 1.0
P 25 Bury Flat Biomass
+ 1 .0525 0.0375 .03 .015 .03
P 26 Resurface Buried Biomass
+ .01 .01 .01 .02 .01
G 03 Crop Name
+ Potato, late, harvest
P 51 Seeding Configuration
+ 1 0.0 2
+ 5.0 4.0 1 600 1.0 1.0 5
+ cwt/ac
+ 79.0 89.3 7 1.0 0.65 0.8
+ 0.8 0.05 0.6096074 2.0 25.0 0 120 1600.0
+ -5.0 -15.0 0.01 0.95 0.0 32
+ 0.0 0.6553 0.3159 -0.061 -3.0E-4 0.9911 0.3415 0.0494
+ 0.4163 -0.061 2.6 1.0 30.0 0.05 0 1.0
+ 12000.0 2700.0 3.0 0.03 0.0 0.0 0.9 1
+ 0.02 0.02 0.02 0.02 0.2 0.0050 20.0 5.227942
+ -1.20379 0.604887 0.0313 0.024658702 0.0 0.0 0.0 0.0
T Represents high yielding typically irrigated Potatoes - white, russet, red (all but sweet). 60,000 lb (600 cwt), 30 ton/ac yield .  36" rows.
T Residue at harvest includes mass before chemical kill.  Base location ID, WA, NM.
T
T File was tested in Grant Co. WA and Bingham Co. ID.  Biomas Conv Eff factor was at 32.  Yields were low.
T At 40 the yields were 553 cwt/ac in WA and 485 cwt/ac in ID.  I have made the change to get the yields closer
T to the actual field values.  MAS 9-26-07
T
T Harvest biomass ratio is set using two studies.  One from the PNW irrigated and the other in MN.
T Both sites are were sandy soils with irrigation.  Yields were 600 cwt/ac.  MAS 7-3-08
#------------
D 31/05/03
O 04 Sprayer, post emergence
+ 1.2160101 .15
T Spray pest control chemicals on growing crop.  Crop is not killed.
T In the MCREW management screen the user must select the kind of weeds killed in the growing crop as external residue.   080404 DTL
T Cloned from Defoliate (spray) crop.oprn, Changed the P31 to No crop kill and added G4 to add material to field MAS 9-28-06
T DO NOT LEAVE CROP COLUMN SET TO "no crop".  User must select the crop and then drill into the operation and specify the amount of weed
T mass that will be killed and turned into residue.
+
G 03 Crop Name
+ weed residue; 0-3 mo
P 65 Add Crop Residue Amounts
+ 0.0 0.0 0.0 0.028021252 1
+ 0.0 0.0 0.0056042504 152.4003
+ 0.025 0.025 0.025 0.025 0.169 0.0050 17.1 5.227942
+ -1.20379 0.604887
T Enter crop notes here.
#------------
D 15/06/03
O 03 Bed shaper
+ 3.554491 19.5 2.2351363 0.0 2.2351363 1.5645955 2.9056773
T RUSLE Notes: Bed shaping operation on existing beds.  May include drip tape installation. 10/28/01 DTL
T Cloned 2-15-07 MAS
T G2 was added into file in front of the flattening (P24), burial (P25), and resurfacing (P26) factors because the area affected is less than 1.0 and
T the RUSLE values were normalized to 1.0.  This change will imulate the correct residue changes based on the method set forth in RUSLE.
T RUSLE's factors have been redused to based on the area affected.
T The stalk fall rate factor (P34) was moved ahead of the new (G2) factor to set the fall rate to the  less than 1.0 area affected.  8/8/07 MAS
+
G 01 Tillage
+ 101.600204 .6 .75 101.600204 76.20015 152.4003
P 01 Break Crust
P 02 Random Roughness
+ 1 15.240031
P 11 Aggregate Crushing
+ 3.0 -0.22
P 12 Soil Loosening
+ 0.75
P 13 Soil Layer Mixing
+ 0.05
P 05 Ridges and Dikes
+ 1 203.20041 760.0 381.00076 0.0 0.0
P 34 Change Standing Biomass Fall Rate
+ 7 3.0 2.5 2.0 1.5 1.0
+ 0.5 0.6 0.7 0.8 1.0
G 02 Biomass Manipulation
+ 1.0
P 24 Flatten Standing Biomass
+ 0 0.5 0.45 0.4 0.3 1.00
P 25 Bury Flat Biomass
+ 1 0.38 0.3 0.23 0.2 0.28
P 26 Resurface Buried Biomass
+ 0.02 0.02 0.02 0.02 0.02
#------------
D 16/06/03
O 04 Sprayer, fungicide
+ 1.2160101 0.15
T Spray fungicide on growing crop.   Crop is not killed.  11/17/01 DTL Revised Sprayer,
T insecticide for fungicide application 82211 LOS
T
T Added to DB 3-1-12 MAS
+ 
#------------
D 10/07/03
O 04 Sprayer, fungicide
+ 1.2160101 0.15
T Spray fungicide on growing crop.   Crop is not killed.  11/17/01 DTL Revised Sprayer,
T insecticide for fungicide application 82211 LOS
T
T Added to DB 3-1-12 MAS
+ 
#------------
D 15/07/03
O 03 Bed shaper
+ 3.554491 19.5 2.2351363 0.0 2.2351363 1.5645955 2.9056773
T RUSLE Notes: Bed shaping operation on existing beds.  May include drip tape installation. 10/28/01 DTL
T Cloned 2-15-07 MAS
T G2 was added into file in front of the flattening (P24), burial (P25), and resurfacing (P26) factors because the area affected is less than 1.0 and
T the RUSLE values were normalized to 1.0.  This change will imulate the correct residue changes based on the method set forth in RUSLE.
T RUSLE's factors have been redused to based on the area affected.
T The stalk fall rate factor (P34) was moved ahead of the new (G2) factor to set the fall rate to the  less than 1.0 area affected.  8/8/07 MAS
+
G 01 Tillage
+ 101.600204 .6 .75 101.600204 76.20015 152.4003
P 01 Break Crust
P 02 Random Roughness
+ 1 15.240031
P 11 Aggregate Crushing
+ 3.0 -0.22
P 12 Soil Loosening
+ 0.75
P 13 Soil Layer Mixing
+ 0.05
P 05 Ridges and Dikes
+ 1 203.20041 760.0 381.00076 0.0 0.0
P 34 Change Standing Biomass Fall Rate
+ 7 3.0 2.5 2.0 1.5 1.0
+ 0.5 0.6 0.7 0.8 1.0
G 02 Biomass Manipulation
+ 1.0
P 24 Flatten Standing Biomass
+ 0 0.5 0.45 0.4 0.3 1.00
P 25 Bury Flat Biomass
+ 1 0.38 0.3 0.23 0.2 0.28
P 26 Resurface Buried Biomass
+ 0.02 0.02 0.02 0.02 0.02
#------------
D 25/07/03
O 04 Sprayer, fungicide
+ 1.2160101 0.15
T Spray fungicide on growing crop.   Crop is not killed.  11/17/01 DTL Revised Sprayer,
T insecticide for fungicide application 82211 LOS
T
T Added to DB 3-1-12 MAS
+ 
#------------
D 10/08/03
O 04 Sprayer, fungicide
+ 1.2160101 0.15
T Spray fungicide on growing crop.   Crop is not killed.  11/17/01 DTL Revised Sprayer,
T insecticide for fungicide application 82211 LOS
T
T Added to DB 3-1-12 MAS
+ 
#------------
D 21/09/03
O 03 Harvest, dig root crops res. buried
+ 17.491838 27.378 1.3410819 0.0 1.5645955 1.3410819 2.9056773
T Harvest, root crops like potatoes, sugar beets, carrots, and onions.
T Surface is rough with 4 ridges and much of the residue is buried.
T Rev 11-18-04 DTL RUSLE MAS 10-26-06
T
T P24 was changed to show that all residue types are flattened.
T This havest now flattens all residue types 100%.  MAS 1-18-11
+
G 01 Tillage
+ 177.80035 1.0 1.0 177.80035 152.4003 203.20041
P 01 Break Crust
P 02 Random Roughness
+ 1 16.510033
P 05 Ridges and Dikes
+ 1 101.600204 3657.6072 3048.006 0.0 0.0
P 11 Aggregate Crushing
+ 1.4 -1.2
P 12 Soil Loosening
+ 0.7
P 13 Soil Layer Mixing
+ 0.9
P 31 Kill or Defoliate Growing Crop
+ 2
G 02 Biomass Manipulation
+ 1.0
P 62 Remove (by age pool) Plant/Residue Material
+ 1 1 0 1 1 3 2 0.0 0.0 0.0 1.0 0.0
P 40 End crop Biomass Manipulation
P 24 Flatten Standing Biomass
+ 0 1.0 1.0 1.0 1.0 1.0
P 25 Bury Flat Biomass
+ 2 .95 .95 .95 .95 1
P 26 Resurface Buried Biomass
+ 0.01 0.01 0.03 0.01 0.01
#------------
D 30/04/04
O 03 Disk, tandem heavy primary op
+ 7.0154433 39 2.2351363 0.0 2.2351363 1.3410819 2.6821637
T 11-12in. Spacing, Front and Rear
T Recommended for primary tillage in medium to heavy soils
T Excellent residue-handling capability. MAS 10-26-06
+
G 01 Tillage
+ 152.4003 1.0 1.0 152.4003 101.600204 177.80035
P 01 Break Crust
P 02 Random Roughness
+ 1 38.100075
P 05 Ridges and Dikes
+ 1 101.600204 279.40057 0.0 0.0 0.0
P 11 Aggregate Crushing
+ 2.8 0.75
P 12 Soil Loosening
+ 0.9
P 13 Soil Layer Mixing
+ 0.4
P 31 Kill or Defoliate Growing Crop
+ 2
P 40 End crop Biomass Manipulation
P 24 Flatten Standing Biomass
+ 0 1.0 0.9 0.8 0.5 1.0
P 25 Bury Flat Biomass
+ 1 0.95 0.85 0.8 0.6 0.95
P 26 Resurface Buried Biomass
+ 0.05 0.06 0.07 0.08 0.05
P 34 Change Standing Biomass Fall Rate
+ 7 3.0 2.5 2.0 1.5 1.0
+ 0.5 0.6 0.7 0.8 1.0
#------------
D 05/05/04
O 03 Harrow, coiled tine
+ 4.1157265 15.6 2.6821637 0.0 2.6821637 1.3410819 3.129191
T This oprn is from a RUSLE record created 6/7/01.  10-25-06 MAS
T
T Corrected ridge height and spacing to match RUSLE2. 10-26-11 LOS
T
T Changed spacing from 0 to 1 in. The 0 caused the operation to fail.  12-12-11 MAS
+
G 01 Tillage
+ 50.800102 0.25 1.0 50.800102 25.400051 76.20015
P 01 Break Crust
P 02 Random Roughness
+ 1 10.160021
P 05 Ridges and Dikes
+ 1 25.400051 101.600204 0.0 0.0 0.0
P 11 Aggregate Crushing
+ 3.0 -0.22
P 12 Soil Loosening
+ 0.6
P 13 Soil Layer Mixing
+ 0.2
P 31 Kill or Defoliate Growing Crop
+ 2
P 40 End crop Biomass Manipulation
P 24 Flatten Standing Biomass
+ 0 0.5 0.3 0.2 0.1 1.0
P 25 Bury Flat Biomass
+ 1 0.25 0.2 0.15 0.1 0.25
P 26 Resurface Buried Biomass
+ 0.01 0.01 0.01 0.02 0.01
P 34 Change Standing Biomass Fall Rate
+ 7 3.0 2.5 2.0 1.5 1.0
+ 0.5 0.6 0.7 0.8 1.0
#------------
D 05/05/04
O 03 Fert applic. shank low disturbance, 12 in
+ 8.418531 3.25 2.2351363 0.0 2.2351363 1.5645955 2.9056773
T Minimum disturbance fertilizer injector shank.012904 DTL RUSLE MAS 10-26-06
T G2 was added into file in front of the flattening (P24), burial (P25), and resurfacing (P26) factors because the area affected is less than 1.0 and
T the RUSLE values were normalized to 1.0.  This change will imulate the correct residue changes based on the method set forth in RUSLE.
T RUSLE's factors have been redused to based on the area affected.
T The stalk fall rate factor (P34) was moved ahead of the new (G2) factor to set the fall rate to the less than 1.0 area affected.  8/7/07 MAS
+ 
G 01 Tillage
+ 101.600204 0.8 0.25 101.600204 76.20015 152.4003
P 01 Break Crust
P 02 Random Roughness
+ 1 15.240031
P 05 Ridges and Dikes
+ 1 50.800102 304.8006 25.400051 0.0 0.0
P 11 Aggregate Crushing
+ 2.4 2.0
P 12 Soil Loosening
+ 0.7
P 13 Soil Layer Mixing
+ 0.2
P 40 End crop Biomass Manipulation
P 34 Change Standing Biomass Fall Rate
+ 7 3.0 2.5 2.0 1.5 1.0
+ 0.5 0.6 0.7 0.8 1.0
P 24 Flatten Standing Biomass
+ 0 0.5 0.45 0.4 0.4 1.0
P 25 Bury Flat Biomass
+ 4 0.2 .15 .1 0.08 0.14
P 26 Resurface Buried Biomass
+ 0.06 0.06 0.06 0.1 0.06
#------------
D 05/05/04
O 03 Drill or airseeder, double disk
+ 3.3674128 6.34 2.2351363 0.0 2.2351363 1.5645955 2.9056773
T Drill or air seeder with double disk openers on 7 to 10 inch spacings.  Rev102403 DTL  RUSLE MAS 10-26-06
T G2 was added into file in front of the flattening (P24), burial (P25), and resurfacing (P26) factors because the area affected is less than 1.0 and
T the RUSLE values were normalized to 1.0.  This change will imulate the correct residue changes based on the method set forth in RUSLE.
T RUSLE's factors have been redused to based on the area affected.
T The stalk fall rate factor (P34) was moved ahead of the new (G2) factor to set the fall rate to the  less than 1.0 area affected.  8/8/07 MAS
T
T Deleted the G2 process because all process only affect 0.65 of the surface.  This is set a 0.65 with G1 process in the beginning. 5-11-11 MAS
+ 
G 01 Tillage
+ 38.100075 0.4 0.65 38.100075 25.400051 50.800102
P 01 Break Crust
P 02 Random Roughness
+ 1 7.6200156
P 05 Ridges and Dikes
+ 1 25.400051 203.20041 25.400051 0.0 0.0
P 11 Aggregate Crushing
+ 2.8 0.75
P 12 Soil Loosening
+ 0.6
P 13 Soil Layer Mixing
+ 0.3
P 34 Change Standing Biomass Fall Rate
+ 7 3.0 2.5 2.0 1.5 1.0
+ 0.5 0.6 0.7 0.8 1.0
P 24 Flatten Standing Biomass
+ 0 0.6 0.4 0.35 0.15 1.0
P 25 Bury Flat Biomass
+ 1 0.2275 0.1625 0.13 0.065 0.13
P 26 Resurface Buried Biomass
+ 0.01 0.01 0.01 0.02 0.01
G 03 Crop Name
+ Oats, spring
P 51 Seeding Configuration
+ 1 0.0 0
+ 220.0 8.0 1 60 1.0 1.0 0
+ bu/ac
+ 14 278.8 4 0.8 0.64 0.8
+ 1.0 0.025 1.3716166 0.0 21.0 0 90 1500.0
+ -5.0 -15.0 0.005 0.05 0.0 35.0
+ 0.013 0.8013 0.4293 -0.086 -0.018 0.932 0.456 0.0736
+ 0.4293 -0.086 3.14 1.0 23.1 0.05 0 0.3
+ 33.333332 310.0 1.5 0.015 0 0 0.0 2
+ 0.0185 0.0185 0.0185 0.0185 0.28 0.0050 17.1 5.227942
+ -2.08165 0.548606 1.8 0.042592302 0.0 0.0 0.0 0.0
T Enter crop notes here.
#------------
D 31/05/04
O 04 Sprayer, post emergence
+ 1.2160101 .15
T Spray pest control chemicals on growing crop.  Crop is not killed.
T In the MCREW management screen the user must select the kind of weeds killed in the growing crop as external residue.   080404 DTL
T Cloned from Defoliate (spray) crop.oprn, Changed the P31 to No crop kill and added G4 to add material to field MAS 9-28-06
T DO NOT LEAVE CROP COLUMN SET TO "no crop".  User must select the crop and then drill into the operation and specify the amount of weed
T mass that will be killed and turned into residue.
+
G 03 Crop Name
+ weed residue; 0-3 mo
P 65 Add Crop Residue Amounts
+ 0.0 0.0 0.0 0.028021252 1
+ 0.0 0.0 0.0056042504 152.4003
+ 0.025 0.025 0.025 0.025 0.169 0.0050 17.1 5.227942
+ -1.20379 0.604887
T Enter crop notes here.
#------------
D 15/08/04
O 04 Harvest, killing crop 50pct standing stubble
+ 14.311503 .15
T ARS record - filename is:  Harvest Wheat - grain (combine cutterbar header).oprn
T This operation record is designed to represent actual field harvesting operation
T of removing the grain from small grain crops with a cutterbar head on a combine.
T This harvesting operation record removes all the reproductive component of a crop above the
T cutting height.  Typically this is specified as the "yield" component in the crop record.
T The non-harvested crop plant material above the specified cut height becomes flat residue.
T The remaining above ground crop material below the specified cut height becomes standing residue.
T Nov 02, 2005	Created - Larry Wagner
T Detailed info regarding this operation record:
T This harvest record specifies the actual cut height dependent upon the height
T of the crop.  The cut height is specified as a fraction of the crop height.
T Added 0.2 for the flatting of the combine and tire trafic for haulling grain.
T MAS 1-18-07
T The harvesting operation could also have an effect on the "standing stalk"
T fall rate and fall threshold values.  The default "biomass pool" flag parameter
T is set to "No adjustments applied" so that no "stalk residue decay rate change" will occur.
T However, this flag value can be changed along with the default parameter values
T to change the "stalk residue decay processes".
+
G 02 Biomass Manipulation
+ 1.0
P 31 Kill or Defoliate Growing Crop
+ 2
P 43 Cut/Remove Biomass by Fraction (flags)
+ 1 1 0 1 0.2 1 0 0
P 34 Change Standing Biomass Fall Rate
+ 0 1.0 1.0 1.0 1.0 1.0
+ 1.0 1.0 1.0 1.0 1.0
P 40 End crop Biomass Manipulation
P 24 Flatten Standing Biomass
+ 0 0.2 0.2 0.15 0.2 1
#------------
D 01/11/04
O 03 Plow, moldboard
+ 17.491838 65 2.2351363 0.0 2.2351363 1.5645955 2.6821637
T Moldboard plow 8 inch operating depth.  060701 DTL  Modified flattening and burial per McCool and Foster 05/21/02 DTL RUSLE MAS 10-26-06
+
G 01 Tillage
+ 203.20041 1.0 1.0 203.20041 152.4003 254.0005
P 01 Break Crust
P 02 Random Roughness
+ 1 48.260098
P 05 Ridges and Dikes
+ 1 25.400051 406.40082 0.0 0.0 0.0
P 11 Aggregate Crushing
+ 2.8 1.0
P 12 Soil Loosening
+ 1.0
P 13 Soil Layer Mixing
+ 0.7
P 14 Soil Layer Inversion
P 31 Kill or Defoliate Growing Crop
+ 2
P 40 End crop Biomass Manipulation
P 24 Flatten Standing Biomass
+ 0 1 1 1 0.75 1.0
P 25 Bury Flat Biomass
+ 3 0.99 0.99 0.99 0.85 0.97
P 26 Resurface Buried Biomass
+ 0.01 0.02 0.04 0.1 0.02
P 34 Change Standing Biomass Fall Rate
+ 7 3.0 2.5 2.0 1.5 1.0
+ 0.5 0.6 0.7 0.8 1.0
#------------
*END
*EOF
