Version: 1.5
*START 6
N Originating Program: RUSLE2
N Skel Format Version: 1.1
N This management file was originally converted from the NRCS standard XML format on - Thu Jun 28 14:02:28 PDT 2012
N This management file was updated to contain the most current crop and operation records for WEPS on - Tue Dec 17 19:10:30 CST 2013
#------------
D 08/05/01
O 04 Sprayer, kill crop
+ 1.2160101 0.15
T All crop types are killed, green grow turned to residue, standing.  MAS 12-27-11
T
T Added Flattening to the operation to match R2 (P-24).  This will tend to increase erosion on systems that using
T cover crops by causing less standing residue from the crop or cover crop killed.  MAS 4-3-12
T
T After a conference call, Linda Scheffe, Dave Lightle, Mike Sporcic, and Fred Fox, we decided to change the flattening
T from 0.7-0.5 to 0.05 for all residue type due to wheel traffic only.  Plant canopy change over time is not considered.
T Normal plant senescence built into the model will handle plant changes.  MAS 4-5-12
+ 
G 02 Biomass Manipulation
+ 1.0
P 24 Flatten Standing Biomass
+ 0 0.05 0.05 0.05 0.05 0.05
P 31 Kill or Defoliate Growing Crop
+ 2
P 40 End crop Biomass Manipulation
#------------
D 11/05/01
O 03 Manure spreader, solid and semi-solid
+ 11.505327 .20 1.7881091 0.0 1.7881091 1.3410819 3.5762181
T Created from RUSLE file MAS 9/19/06.
T This assumes a defult residue type of  manure solid significant bedding and the RUSLE may contain some bedding.
T User may need to change to the correct manure type, make a calulation on the dry matter applied, and change the application rate in MCREW.
T This opn is built for an application of 10 ton/ac 60% dry matter surface applied manure.
T 10 tons x 2000 lbs/ac = 20,000 lbs/ac x 0.6 = 12,000 lbs/ac applied.
T MAS 12-5-07
+
G 01 Tillage
+ 0.0 0 1 0.0 0.0 0.0
P 24 Flatten Standing Biomass
+ 14 .1 .1 .1 .1 1.0
G 03 Crop Name
+ manure, solid, signif. bedding
P 66 Add Manure Residue Amount
+ 0.0 0.0 0.0 0.0 1
+ 0.0 0.0 0.0 0.0
+ 1.34502 0.0
+ .017 .017 .017 .017 0.169 0.0050 1 5.227942
+ -2.08165 0.548606
T Enter crop notes here.
#------------
D 16/05/01
O 03 Fert applic. shank low disturbance, 12 in
+ 8.418531 3.25 2.2351363 0.0 2.2351363 1.5645955 2.9056773
T Minimum disturbance fertilizer injector shank.012904 DTL RUSLE MAS 10-26-06
T G2 was added into file in front of the flattening (P24), burial (P25), and resurfacing (P26) factors because the area affected is less than 1.0 and
T the RUSLE values were normalized to 1.0.  This change will imulate the correct residue changes based on the method set forth in RUSLE.
T RUSLE's factors have been redused to based on the area affected.
T The stalk fall rate factor (P34) was moved ahead of the new (G2) factor to set the fall rate to the less than 1.0 area affected.  8/7/07 MAS
+ 
G 01 Tillage
+ 101.600204 0.8 0.25 101.600204 76.20015 152.4003
P 01 Break Crust
P 02 Random Roughness
+ 1 15.240031
P 05 Ridges and Dikes
+ 1 50.800102 304.8006 25.400051 0.0 0.0
P 11 Aggregate Crushing
+ 2.4 2.0
P 12 Soil Loosening
+ 0.7
P 13 Soil Layer Mixing
+ 0.2
P 40 End crop Biomass Manipulation
P 34 Change Standing Biomass Fall Rate
+ 7 3.0 2.5 2.0 1.5 1.0
+ 0.5 0.6 0.7 0.8 1.0
P 24 Flatten Standing Biomass
+ 0 0.5 0.45 0.4 0.4 1.0
P 25 Bury Flat Biomass
+ 4 0.2 .15 .1 0.08 0.14
P 26 Resurface Buried Biomass
+ 0.06 0.06 0.06 0.1 0.06
#------------
D 16/05/01
O 03 Planter, double disk opnr, fluted coulter
+ 5.0511193 2.44 2.2351363 0.0 2.2351363 1.5645955 2.9056773
T REVISED102403 DTL
T This is a standard planter on 30 in sp with a fluted coulter and a 1 in ridge ht.  MAS 8/7/07
T G2 was added into file in front of the flattening (P24), burial (P25), and resurfacing (P26) factors because the area affected is less than 1.0 and
T the RUSLE values were normalized to 1.0.  This change will imulate the correct residue changes based on the method set forth in RUSLE.
T RUSLE's factors have been redused to based on the area affected.
T The stalk fall rate factor (P34) was moved ahead of the new (G2) factor to set the fall rate to the less than 1.0 area affected.  8/7/07 MAS
+
G 01 Tillage
+ 63.500126 0.4 0.15 63.500126 50.800102 101.600204
P 01 Break Crust
P 02 Random Roughness
+ 1 10.160021
P 05 Ridges and Dikes
+ 1 25.400051 762.0015 635.0013 0.0 0.0
P 11 Aggregate Crushing
+ 2.4 2.0
P 12 Soil Loosening
+ 0.65
P 13 Soil Layer Mixing
+ 0.3
P 34 Change Standing Biomass Fall Rate
+ 7 3.0 2.5 2.0 1.5 1.0
+ 0.5 0.6 0.7 0.8 1.0
G 02 Biomass Manipulation
+ 1.0
P 24 Flatten Standing Biomass
+ 0 0.3 0.25 0.15 0.1 1.0
P 25 Bury Flat Biomass
+ 1 .0525 0.0375 .03 .015 .03
P 26 Resurface Buried Biomass
+ 0.01 0.01 0.01 0.02 0.01
G 03 Crop Name
+ Corn, silage
P 51 Seeding Configuration
+ 1 0.0 2
+ 6.0 1.0 1 23 1.0 1.0 2
+ ton/ac
+ 65.0 4.465 4 1.0 0.65 0.8
+ 2.5 0.05 1.5240185 10.0 30.0 0 100 1700.0
+ -5.0 -15.0 0.01 0.05 0.0 40.0
+ 0.0031 0.9233 0.3266 -0.044 0.0 0.976 0.511 0.0287
+ 0.3266 -0.044 0.22259772 0.72 17.4 0.05 0 0.9
+ 333.33334 333.33334 3.0 0.03 0.0 0.0 0.0 3
+ 0.016 0.016 0.016 0.01 0.153 0.01 20.0 3.3812115
+ -1.20379 0.604887 0.3081 0.21615593 0.0 0.0 0.0 0.0
T corn silage 23 ton yield, 30" rows  Columbia, Mo DTL
T
T This record was cloned from ARS records and the revenant data adjusted to RUSLE values.
T The Biomass Conv Factor was changed from 40 to 47 based on runs made in Clovis, NM with full irrigation.
T MAS 9-27-07
T
T R2 Note - Rev residue : yield ratio 091108 DTL with 35% dry matter content. rev biomass-yield ratio 032012 DTL
T
T Added the Yield intercept and Res:Yield ratio. 
T If a cover crop is inter planted into Corn, silage users must use a harvest that call in a growing
T cover crop.  Only one crop can be grown at a time in WEPS. 4-3-12 MAS
#------------
D 26/05/01
O 04 Sprayer, post emergence
+ 1.2160101 .15
T Spray pest control chemicals on growing crop.  Crop is not killed.
T In the MCREW management screen the user must select the kind of weeds killed in the growing crop as external residue.   080404 DTL
T Cloned from Defoliate (spray) crop.oprn, Changed the P31 to No crop kill and added G4 to add material to field MAS 9-28-06
T DO NOT LEAVE CROP COLUMN SET TO "no crop".  User must select the crop and then drill into the operation and specify the amount of weed
T mass that will be killed and turned into residue.
+
G 03 Crop Name
+ weed residue; 0-3 mo
P 65 Add Crop Residue Amounts
+ 0.0 0.0 0.0 0.028021252 1
+ 0.0 0.0 0.0056042504 152.4003
+ 0.025 0.025 0.025 0.025 0.169 0.0050 17.1 5.227942
+ -1.20379 0.604887
T Enter crop notes here.
#------------
D 22/09/01
O 04 Harvest, silage, kill crop
+ 8.886228 .15
T Use this operation  when the harvest will stop any regrowth.  It cuts to a 5 in ht. MAS 6-30-08
T
T ARS record - filename is:  Harvest Corn - silage (silage cutter).oprn
T This operation record is designed to represent a harvesting operation, e.g., a "silage cutter",
T that remove all of the above ground crop biomass above a specified cutting height.
T Examples would be cutting corn for silage and alfalfa for hay.
T This harvesting operation record removes all crop plant material above the specified cut height.
T The remaining above ground crop material below the specified cut height becomes standing residue
T for annual crops.  Perennial crops like alfalfa will automatically regrow.
T The default "Kill or Defoliate Growing Crop" parameter is set to kill annual crops but to allow
T regrowth of perennial crops.  Thus the default value is acceptable for perennial crops
T like alfalfa and most annual crops like corn harvested for silage.  There are situations where
T one might want to change this parameter value for specific types of crops and conditions.
T See additional info below in the "Detailed info regarding this operation record" section.
T No standing stalks (crop or residue) are flattened.  This record is assuming a row crop
T silage harvester, where the tires are tracking in between the rows.
T 200x	Created - Fred Fox
T Oct 31, 2005	Updated notes - Larry Wagner
T Detailed info regarding this operation record:
T This operation template has the "Kill or Defoliate Growing Crop" process parameter defaulting to
T "Annual crop killed, perennial crop regrows" value.  Thus the default value is acceptable for use
T with perennial crops like alfalfa and annual crops like corn harvested for silage.  However, if one
T intends to harvest (green chop) an annual crop that has the capacity to regrow after such a cutting,
T then one needs to change the value to "No crop killed" to allow the crop to regrow afterwards.
T Due to the way WEPS reports crop yields, the crop record selected for this type of harvesting
T operation should specify the "yield" component of the crop to be the "above ground stems, leaves
T and reproductive elements of  the plant".  This will ensure proper reporting of harvested yields
T by WEPS.  However, using a crop record that does not specify the "yield" component in this manner
T will not affect the erosion estimate or change any other simulation run results, except to incorrectly
T report the true "yield" component being removed from the field.  An example of a crop that may be
T harvested for two different types of "yield" components is corn.  There are corn crop records defined
T that specify the yield as the reproductive element (grain) and others that are defined for harvesting
T the crop as silage.
+
G 02 Biomass Manipulation
+ 1.0
P 31 Kill or Defoliate Growing Crop
+ 2
P 42 Cut/Remove Biomass to Height (flags)
+ 1 1 0 1 0 127.00025 1.0 1.0 1.0
P 34 Change Standing Biomass Fall Rate
+ 0 1.1 1.08 1.06 1.04 1.0
+ 1.0 1.0 1.0 1.0 1.0
P 40 End crop Biomass Manipulation
P 24 Flatten Standing Biomass
+ 0 0.0 0.0 0.0 0.0 0.0
#------------
D 08/05/02
O 04 Sprayer, kill crop
+ 1.2160101 0.15
T All crop types are killed, green grow turned to residue, standing.  MAS 12-27-11
T
T Added Flattening to the operation to match R2 (P-24).  This will tend to increase erosion on systems that using
T cover crops by causing less standing residue from the crop or cover crop killed.  MAS 4-3-12
T
T After a conference call, Linda Scheffe, Dave Lightle, Mike Sporcic, and Fred Fox, we decided to change the flattening
T from 0.7-0.5 to 0.05 for all residue type due to wheel traffic only.  Plant canopy change over time is not considered.
T Normal plant senescence built into the model will handle plant changes.  MAS 4-5-12
+ 
G 02 Biomass Manipulation
+ 1.0
P 24 Flatten Standing Biomass
+ 0 0.05 0.05 0.05 0.05 0.05
P 31 Kill or Defoliate Growing Crop
+ 2
P 40 End crop Biomass Manipulation
#------------
D 11/05/02
O 03 Manure spreader, solid and semi-solid
+ 11.505327 .20 1.7881091 0.0 1.7881091 1.3410819 3.5762181
T Created from RUSLE file MAS 9/19/06.
T This assumes a defult residue type of  manure solid significant bedding and the RUSLE may contain some bedding.
T User may need to change to the correct manure type, make a calulation on the dry matter applied, and change the application rate in MCREW.
T This opn is built for an application of 10 ton/ac 60% dry matter surface applied manure.
T 10 tons x 2000 lbs/ac = 20,000 lbs/ac x 0.6 = 12,000 lbs/ac applied.
T MAS 12-5-07
+
G 01 Tillage
+ 0.0 0 1 0.0 0.0 0.0
P 24 Flatten Standing Biomass
+ 14 .1 .1 .1 .1 1.0
G 03 Crop Name
+ manure, solid, signif. bedding
P 66 Add Manure Residue Amount
+ 0.0 0.0 0.0 0.0 1
+ 0.0 0.0 0.0 0.0
+ 1.34502 0.0
+ .017 .017 .017 .017 0.169 0.0050 1 5.227942
+ -2.08165 0.548606
T Enter crop notes here.
#------------
D 16/05/02
O 03 Fert applic. shank low disturbance, 12 in
+ 8.418531 3.25 2.2351363 0.0 2.2351363 1.5645955 2.9056773
T Minimum disturbance fertilizer injector shank.012904 DTL RUSLE MAS 10-26-06
T G2 was added into file in front of the flattening (P24), burial (P25), and resurfacing (P26) factors because the area affected is less than 1.0 and
T the RUSLE values were normalized to 1.0.  This change will imulate the correct residue changes based on the method set forth in RUSLE.
T RUSLE's factors have been redused to based on the area affected.
T The stalk fall rate factor (P34) was moved ahead of the new (G2) factor to set the fall rate to the less than 1.0 area affected.  8/7/07 MAS
+ 
G 01 Tillage
+ 101.600204 0.8 0.25 101.600204 76.20015 152.4003
P 01 Break Crust
P 02 Random Roughness
+ 1 15.240031
P 05 Ridges and Dikes
+ 1 50.800102 304.8006 25.400051 0.0 0.0
P 11 Aggregate Crushing
+ 2.4 2.0
P 12 Soil Loosening
+ 0.7
P 13 Soil Layer Mixing
+ 0.2
P 40 End crop Biomass Manipulation
P 34 Change Standing Biomass Fall Rate
+ 7 3.0 2.5 2.0 1.5 1.0
+ 0.5 0.6 0.7 0.8 1.0
P 24 Flatten Standing Biomass
+ 0 0.5 0.45 0.4 0.4 1.0
P 25 Bury Flat Biomass
+ 4 0.2 .15 .1 0.08 0.14
P 26 Resurface Buried Biomass
+ 0.06 0.06 0.06 0.1 0.06
#------------
D 16/05/02
O 03 Planter, double disk opnr, fluted coulter
+ 5.0511193 2.44 2.2351363 0.0 2.2351363 1.5645955 2.9056773
T REVISED102403 DTL
T This is a standard planter on 30 in sp with a fluted coulter and a 1 in ridge ht.  MAS 8/7/07
T G2 was added into file in front of the flattening (P24), burial (P25), and resurfacing (P26) factors because the area affected is less than 1.0 and
T the RUSLE values were normalized to 1.0.  This change will imulate the correct residue changes based on the method set forth in RUSLE.
T RUSLE's factors have been redused to based on the area affected.
T The stalk fall rate factor (P34) was moved ahead of the new (G2) factor to set the fall rate to the less than 1.0 area affected.  8/7/07 MAS
+
G 01 Tillage
+ 63.500126 0.4 0.15 63.500126 50.800102 101.600204
P 01 Break Crust
P 02 Random Roughness
+ 1 10.160021
P 05 Ridges and Dikes
+ 1 25.400051 762.0015 635.0013 0.0 0.0
P 11 Aggregate Crushing
+ 2.4 2.0
P 12 Soil Loosening
+ 0.65
P 13 Soil Layer Mixing
+ 0.3
P 34 Change Standing Biomass Fall Rate
+ 7 3.0 2.5 2.0 1.5 1.0
+ 0.5 0.6 0.7 0.8 1.0
G 02 Biomass Manipulation
+ 1.0
P 24 Flatten Standing Biomass
+ 0 0.3 0.25 0.15 0.1 1.0
P 25 Bury Flat Biomass
+ 1 .0525 0.0375 .03 .015 .03
P 26 Resurface Buried Biomass
+ 0.01 0.01 0.01 0.02 0.01
G 03 Crop Name
+ Corn, silage
P 51 Seeding Configuration
+ 1 0.0 2
+ 6.0 1.0 1 23 1.0 1.0 2
+ ton/ac
+ 65.0 4.465 4 1.0 0.65 0.8
+ 2.5 0.05 1.5240185 10.0 30.0 0 100 1700.0
+ -5.0 -15.0 0.01 0.05 0.0 40.0
+ 0.0031 0.9233 0.3266 -0.044 0.0 0.976 0.511 0.0287
+ 0.3266 -0.044 0.22259772 0.72 17.4 0.05 0 0.9
+ 333.33334 333.33334 3.0 0.03 0.0 0.0 0.0 3
+ 0.016 0.016 0.016 0.01 0.153 0.01 20.0 3.3812115
+ -1.20379 0.604887 0.3081 0.21615593 0.0 0.0 0.0 0.0
T corn silage 23 ton yield, 30" rows  Columbia, Mo DTL
T
T This record was cloned from ARS records and the revenant data adjusted to RUSLE values.
T The Biomass Conv Factor was changed from 40 to 47 based on runs made in Clovis, NM with full irrigation.
T MAS 9-27-07
T
T R2 Note - Rev residue : yield ratio 091108 DTL with 35% dry matter content. rev biomass-yield ratio 032012 DTL
T
T Added the Yield intercept and Res:Yield ratio. 
T If a cover crop is inter planted into Corn, silage users must use a harvest that call in a growing
T cover crop.  Only one crop can be grown at a time in WEPS. 4-3-12 MAS
#------------
D 26/05/02
O 04 Sprayer, post emergence
+ 1.2160101 .15
T Spray pest control chemicals on growing crop.  Crop is not killed.
T In the MCREW management screen the user must select the kind of weeds killed in the growing crop as external residue.   080404 DTL
T Cloned from Defoliate (spray) crop.oprn, Changed the P31 to No crop kill and added G4 to add material to field MAS 9-28-06
T DO NOT LEAVE CROP COLUMN SET TO "no crop".  User must select the crop and then drill into the operation and specify the amount of weed
T mass that will be killed and turned into residue.
+
G 03 Crop Name
+ weed residue; 0-3 mo
P 65 Add Crop Residue Amounts
+ 0.0 0.0 0.0 0.028021252 1
+ 0.0 0.0 0.0056042504 152.4003
+ 0.025 0.025 0.025 0.025 0.169 0.0050 17.1 5.227942
+ -1.20379 0.604887
T Enter crop notes here.
#------------
D 22/09/02
O 04 Harvest, silage, kill crop
+ 8.886228 .15
T Use this operation  when the harvest will stop any regrowth.  It cuts to a 5 in ht. MAS 6-30-08
T
T ARS record - filename is:  Harvest Corn - silage (silage cutter).oprn
T This operation record is designed to represent a harvesting operation, e.g., a "silage cutter",
T that remove all of the above ground crop biomass above a specified cutting height.
T Examples would be cutting corn for silage and alfalfa for hay.
T This harvesting operation record removes all crop plant material above the specified cut height.
T The remaining above ground crop material below the specified cut height becomes standing residue
T for annual crops.  Perennial crops like alfalfa will automatically regrow.
T The default "Kill or Defoliate Growing Crop" parameter is set to kill annual crops but to allow
T regrowth of perennial crops.  Thus the default value is acceptable for perennial crops
T like alfalfa and most annual crops like corn harvested for silage.  There are situations where
T one might want to change this parameter value for specific types of crops and conditions.
T See additional info below in the "Detailed info regarding this operation record" section.
T No standing stalks (crop or residue) are flattened.  This record is assuming a row crop
T silage harvester, where the tires are tracking in between the rows.
T 200x	Created - Fred Fox
T Oct 31, 2005	Updated notes - Larry Wagner
T Detailed info regarding this operation record:
T This operation template has the "Kill or Defoliate Growing Crop" process parameter defaulting to
T "Annual crop killed, perennial crop regrows" value.  Thus the default value is acceptable for use
T with perennial crops like alfalfa and annual crops like corn harvested for silage.  However, if one
T intends to harvest (green chop) an annual crop that has the capacity to regrow after such a cutting,
T then one needs to change the value to "No crop killed" to allow the crop to regrow afterwards.
T Due to the way WEPS reports crop yields, the crop record selected for this type of harvesting
T operation should specify the "yield" component of the crop to be the "above ground stems, leaves
T and reproductive elements of  the plant".  This will ensure proper reporting of harvested yields
T by WEPS.  However, using a crop record that does not specify the "yield" component in this manner
T will not affect the erosion estimate or change any other simulation run results, except to incorrectly
T report the true "yield" component being removed from the field.  An example of a crop that may be
T harvested for two different types of "yield" components is corn.  There are corn crop records defined
T that specify the yield as the reproductive element (grain) and others that are defined for harvesting
T the crop as silage.
+
G 02 Biomass Manipulation
+ 1.0
P 31 Kill or Defoliate Growing Crop
+ 2
P 42 Cut/Remove Biomass to Height (flags)
+ 1 1 0 1 0 127.00025 1.0 1.0 1.0
P 34 Change Standing Biomass Fall Rate
+ 0 1.1 1.08 1.06 1.04 1.0
+ 1.0 1.0 1.0 1.0 1.0
P 40 End crop Biomass Manipulation
P 24 Flatten Standing Biomass
+ 0 0.0 0.0 0.0 0.0 0.0
#------------
D 24/05/03
O 03 Disk, tandem heavy primary op
+ 7.0154433 39 2.2351363 0.0 2.2351363 1.3410819 2.6821637
T 11-12in. Spacing, Front and Rear
T Recommended for primary tillage in medium to heavy soils
T Excellent residue-handling capability. MAS 10-26-06
+
G 01 Tillage
+ 152.4003 1.0 1.0 152.4003 101.600204 177.80035
P 01 Break Crust
P 02 Random Roughness
+ 1 38.100075
P 05 Ridges and Dikes
+ 1 101.600204 279.40057 0.0 0.0 0.0
P 11 Aggregate Crushing
+ 2.8 0.75
P 12 Soil Loosening
+ 0.9
P 13 Soil Layer Mixing
+ 0.4
P 31 Kill or Defoliate Growing Crop
+ 2
P 40 End crop Biomass Manipulation
P 24 Flatten Standing Biomass
+ 0 1.0 0.9 0.8 0.5 1.0
P 25 Bury Flat Biomass
+ 1 0.95 0.85 0.8 0.6 0.95
P 26 Resurface Buried Biomass
+ 0.05 0.06 0.07 0.08 0.05
P 34 Change Standing Biomass Fall Rate
+ 7 3.0 2.5 2.0 1.5 1.0
+ 0.5 0.6 0.7 0.8 1.0
#------------
D 29/05/03
O 03 Manure spreader, slurry
+ 11.505327 .29 1.7881091 0.0 1.7881091 1.3410819 3.5762181
T Created from RUSLE file MAS 9/19/06.
T This assumes a defult residue type of  manure slurry using a solid spread with a liquid end gate spreader.
T User needs to change to the correct manure type, make a calulation on the dry matter applied, and change the value in MCREW.
T This opn is built for an application of 10 ton/ac 10% dry matter surface applied manure.
T 10 tons x 2000 lbs/ac = 20,000 lbs/ac x 0.1 = 2,000 lbs/ac applied.
T MAS 12-5-07
+
G 01 Tillage
+ 0.0 0 1 0.0 0.0 0.0
P 24 Flatten Standing Biomass
+ 14 .1 .1 .1 .1 1.0
G 03 Crop Name
+ manure, slurry
P 66 Add Manure Residue Amount
+ 0.0 0.0 0.0 0.0 1
+ 0.0 0.0 0.0 0.0
+ 0.22417001 0.0
+ .06 .06 .06 .06 0.169 0.0050 1 0.6500045
+ -2.08165 0.548606
T Enter crop notes here.
#------------
D 29/05/03
O 03 Harrow, coiled tine
+ 4.1157265 15.6 2.6821637 0.0 2.6821637 1.3410819 3.129191
T This oprn is from a RUSLE record created 6/7/01.  10-25-06 MAS
T
T Corrected ridge height and spacing to match RUSLE2. 10-26-11 LOS
T
T Changed spacing from 0 to 1 in. The 0 caused the operation to fail.  12-12-11 MAS
+
G 01 Tillage
+ 50.800102 0.25 1.0 50.800102 25.400051 76.20015
P 01 Break Crust
P 02 Random Roughness
+ 1 10.160021
P 05 Ridges and Dikes
+ 1 25.400051 101.600204 0.0 0.0 0.0
P 11 Aggregate Crushing
+ 3.0 -0.22
P 12 Soil Loosening
+ 0.6
P 13 Soil Layer Mixing
+ 0.2
P 31 Kill or Defoliate Growing Crop
+ 2
P 40 End crop Biomass Manipulation
P 24 Flatten Standing Biomass
+ 0 0.5 0.3 0.2 0.1 1.0
P 25 Bury Flat Biomass
+ 1 0.25 0.2 0.15 0.1 0.25
P 26 Resurface Buried Biomass
+ 0.01 0.01 0.01 0.02 0.01
P 34 Change Standing Biomass Fall Rate
+ 7 3.0 2.5 2.0 1.5 1.0
+ 0.5 0.6 0.7 0.8 1.0
#------------
D 01/06/03
O 03 Drill or airseeder, double disk, fluted coulters
+ 4.0221877 7.15 2.2351363 0.0 2.2351363 1.5645955 2.9056773
T Drill or airseeder with double disk openers and fluted coulters on 7 to 10 inch spacing.
T REVISED102403 DTL  RUSLE MAS 10-26-06
T G2 was added into file in front of the flattening (P24), burial (P25), and resurfacing (P26) factors because the area affected is less than 1.0 and
T the RUSLE values were normalized to 1.0.  This change will imulate the correct residue changes based on the method set forth in RUSLE.
T RUSLE's factors have been redused to based on the area affected.
T The stalk fall rate factor (P34) was moved ahead of the new (G2) factor to set the fall rate to the less than 1.0 area affected.  8/7/07 MAS
+
G 01 Tillage
+ 50.800102 0.4 0.55 50.800102 38.100075 63.500126
P 01 Break Crust
P 02 Random Roughness
+ 1 7.6200156
P 05 Ridges and Dikes
+ 1 50.800102 203.20041 50.800102 0.0 0.0
P 11 Aggregate Crushing
+ 2.6 0.75
P 12 Soil Loosening
+ 0.65
P 13 Soil Layer Mixing
+ 0.3
P 34 Change Standing Biomass Fall Rate
+ 7 3.0 2.5 2.0 1.5 1.0
+ 0.5 0.6 0.7 0.8 1.0
G 02 Biomass Manipulation
+ 1.0
P 24 Flatten Standing Biomass
+ 0 0.65 0.5 .45 0.15 1.0
P 25 Bury Flat Biomass
+ 1 0.19 0.14 0.11 0.06 0.11
P 26 Resurface Buried Biomass
+ 0.01 0.01 0.01 0.02 0.01
G 03 Crop Name
+ Alfalfa-Bromegrass, forage
P 51 Seeding Configuration
+ 1 0.0 0
+ 688.0 1.0 0 4.0 1 1.0 2
+ ton/ac
+ 15.0 4.465 3 1.0 0.69 0.9
+ 1.0 0.01 2.0 3.0 30.0 1 120 1800.0
+ -5.0 -9.444445 0.01 0.95 0.0 24
+ 0.023 0.55 0.63 -0.061 -0.024 0.9911 0.6435 0.0494
+ 0.5 -0.09 0.16108 0.5981 30 0.05 0 0.3
+ 17.009697 110.0 0.6 0.013 0.2 0.2 0.1 2
+ 0.0536 0.0536 0.0536 0.0536 0.2 0.0020 20.0 5.227942
+ -1.20379 0.604887 0.0 0.0 0.0 0.0 0.0 0.0
T This record was cloned from the Alfalfa, hay record.  It is an irrigated record calibrated in Grant Co. WA.
T It may not grow right on low rainfall dryland conditions.  Use the dryland Alfalfa record if you have trouble.
T MAS 11-17-08
T
T Size ranges
T J.J. rquez-Ortiz, J.F.S. Lamb, L.D. Johnson, D.K. Barnes and R.E. Stucker, 1999, Heritability of crown traits in alfalfa, Crop Science, Vol 39, Issue 1 pgs. 38-43
T Crown Depth (distance from the soil level to the top of the tap root) - 0.5cm to 5cm
T Crown width (just below the soil surface) - 2cm to 12cm or greater
T Number of crown stems - 2 to 10 or more
T Crown stem width - 2mm to 6mm or greater
T Number of crown buds - none to 12 or more
T
T D.K. Barnes, R.B. Pearce, G.E. Carlson, R.H. Hart, and C.H. Hanson. 1969. SPecific Leaf Weight Differences in Alfalfa Associated with Variety and
T Plant Age. Crop Science, Vol 9, pgs. 421-423.
T Values of Specific leaf weight measured in the paper varied from 2.15 to 4.3, with early season growth mostly in the area of 2.15 to 2.72 mg/cm^2
T Conversion to m^2/kg is * 10^6 mg/kg * 10^-4 m^2/cm^2 = 100 / mg/cm^2
T
T 2.15 mg/cm^2 = 100 / 2.15 m^2/kg = 46.5 m^2/kg, 100 / 2.72 = 36.8, 100 / 4.3 = 23.3
T
T M. H. Hall, C. J. Nelson, J. H. Coutts and R. C. Stout. 2004. Effect of Seeding Rate on Alfalfa Stand Longevity. Agron. J. 96:717-722
T Stem densities for the MO94 study (data not presented) were not different among seeding rates at any sampling time. There were 623 stems m–2 13 MAP
T and only 350 stems m–2 by 25 MAP. Stem density remained nearly constant at that level through 49 MAP. During the same time period, plant density
T declined from an average of 100 down to 25 plants m–2. This means that there was a fourfold increase in stems per plant from 25 to 49 MAP during
T the same time period. Thereafter, stem density continued to decline to 290 and 260 stems m–2 at 63 and 73 MAP, respectively, while plant density fell
T below 15 plants m–2 during the same time period. Crowns develop stems in response to light (Cowett and Sprague, 1962) and apparently could not
T continue to maintain high stem density with the thin stand and older plants.
T
T data as shown above.
T MAP = months after planting
T SPM2 = stems per square meter
T PPM2 = plants per square meter
T SPP = stems per plant
T
T MAP	SPM2	PPM2	 SPP
T 13	623	100	62.3
T 25	350	36	9.7
T 49	350	25	14
T 63	290	16	18
T 73	260	13	20
T
T With the critical period of alfalfa being establishment, a stem count, equals plant count of 400 stems per square meter is used to try and get early cover.
T
T Fick, G.W., D.A. Holt, D.G. Lugg. 1988. Environmental Physiology and Crop Growth. in A.A. Hanson, D.K. Barnes, R.R. Hill , Jr., eds. 1988 Alfalfa and Alfalfa
T Improvement. Agronomy Monograph Number 29. American Society of Agronomy.
T page 181. Growth temperatures: GDD base from 0 to 5 C, varies depending on time of year. GDD totals 0 C base, 700 to bud, 880 to first flower,
T 1075 to full bloom, 1900 to ripe seed stages. Suggests a GDD max temperature around 30 C
T
T Changed the cover to mass value to match Fosters finest stem curve, Small Grain and Alfalfa.  Reference pg. 179 Ag Handbook 703.
T No crop has a larger number (finer stems) than .000586.  This matches RUSLE2.  MAS 12-21-10
T
T The biomass adjustment factor has been set to 1.0 from the 0.6 that Fred had.  The biomass conversion eff factor was moved from 30 to 24 to match yield
T of the standard alfalfa run in Moses Lake, WA and now in Yuma, AZ.  The record runs a little under the 6 ton/ac yield in ML, and somewhat over the 10 t/ac for
T Yuma.  The seed weight was increased from 0.00007 to 0.0006 to increase the intial growth of the fall planting.There is about 1500 lbs of growth going into
T winter in WA and about 2400 lbs/ac at the first harvest in AZ.    Yuma will need to lower the Biomass Adjustment factor to 0.8 to get the 12 t/ac yield needed.
T MAS 7-6-11
#------------
D 01/09/03
O 04 Harvest, hay, legume
+ 17.959534 .15
T Harvest legume hay crops such as Alfalfa and Red clover and grass-legume mixed hay such as Alfalfa-Bromegrass.
T Use Harvest, grass hay" for pure grass hay. Rev 11/17/01 DTL"  MAS 11-29-06
T
T Reset the fuel use to 1.92 gal/ac MAS 10-21-11
+
G 02 Biomass Manipulation
+ 1.0
P 31 Kill or Defoliate Growing Crop
+ 0
P 42 Cut/Remove Biomass to Height (flags)
+ 1 0 0 0 0 101.600204 .9 .9 1
P 34 Change Standing Biomass Fall Rate
+ 0 1.1 1.08 1.06 1.04 1.0
+ 0.9 0.92 0.93 0.95 1.0
P 40 End crop Biomass Manipulation
P 24 Flatten Standing Biomass
+ 14 .6 .5 .4 .5 .5
#------------
D 05/09/03
O 03 Manure spreader, slurry
+ 11.505327 .29 1.7881091 0.0 1.7881091 1.3410819 3.5762181
T Created from RUSLE file MAS 9/19/06.
T This assumes a defult residue type of  manure slurry using a solid spread with a liquid end gate spreader.
T User needs to change to the correct manure type, make a calulation on the dry matter applied, and change the value in MCREW.
T This opn is built for an application of 10 ton/ac 10% dry matter surface applied manure.
T 10 tons x 2000 lbs/ac = 20,000 lbs/ac x 0.1 = 2,000 lbs/ac applied.
T MAS 12-5-07
+
G 01 Tillage
+ 0.0 0 1 0.0 0.0 0.0
P 24 Flatten Standing Biomass
+ 14 .1 .1 .1 .1 1.0
G 03 Crop Name
+ manure, slurry
P 66 Add Manure Residue Amount
+ 0.0 0.0 0.0 0.0 1
+ 0.0 0.0 0.0 0.0
+ 0.22417001 0.0
+ .06 .06 .06 .06 0.169 0.0050 1 0.6500045
+ -2.08165 0.548606
T Enter crop notes here.
#------------
D 02/06/04
O 04 Harvest, hay, legume
+ 17.959534 .15
T Harvest legume hay crops such as Alfalfa and Red clover and grass-legume mixed hay such as Alfalfa-Bromegrass.
T Use Harvest, grass hay" for pure grass hay. Rev 11/17/01 DTL"  MAS 11-29-06
T
T Reset the fuel use to 1.92 gal/ac MAS 10-21-11
+
G 02 Biomass Manipulation
+ 1.0
P 31 Kill or Defoliate Growing Crop
+ 0
P 42 Cut/Remove Biomass to Height (flags)
+ 1 0 0 0 0 101.600204 .9 .9 1
P 34 Change Standing Biomass Fall Rate
+ 0 1.1 1.08 1.06 1.04 1.0
+ 0.9 0.92 0.93 0.95 1.0
P 40 End crop Biomass Manipulation
P 24 Flatten Standing Biomass
+ 14 .6 .5 .4 .5 .5
#------------
D 06/06/04
O 03 Manure spreader, slurry
+ 11.505327 .29 1.7881091 0.0 1.7881091 1.3410819 3.5762181
T Created from RUSLE file MAS 9/19/06.
T This assumes a defult residue type of  manure slurry using a solid spread with a liquid end gate spreader.
T User needs to change to the correct manure type, make a calulation on the dry matter applied, and change the value in MCREW.
T This opn is built for an application of 10 ton/ac 10% dry matter surface applied manure.
T 10 tons x 2000 lbs/ac = 20,000 lbs/ac x 0.1 = 2,000 lbs/ac applied.
T MAS 12-5-07
+
G 01 Tillage
+ 0.0 0 1 0.0 0.0 0.0
P 24 Flatten Standing Biomass
+ 14 .1 .1 .1 .1 1.0
G 03 Crop Name
+ manure, slurry
P 66 Add Manure Residue Amount
+ 0.0 0.0 0.0 0.0 1
+ 0.0 0.0 0.0 0.0
+ 0.22417001 0.0
+ .06 .06 .06 .06 0.169 0.0050 1 0.6500045
+ -2.08165 0.548606
T Enter crop notes here.
#------------
D 15/07/04
O 04 Harvest, hay, legume
+ 17.959534 .15
T Harvest legume hay crops such as Alfalfa and Red clover and grass-legume mixed hay such as Alfalfa-Bromegrass.
T Use Harvest, grass hay" for pure grass hay. Rev 11/17/01 DTL"  MAS 11-29-06
T
T Reset the fuel use to 1.92 gal/ac MAS 10-21-11
+
G 02 Biomass Manipulation
+ 1.0
P 31 Kill or Defoliate Growing Crop
+ 0
P 42 Cut/Remove Biomass to Height (flags)
+ 1 0 0 0 0 101.600204 .9 .9 1
P 34 Change Standing Biomass Fall Rate
+ 0 1.1 1.08 1.06 1.04 1.0
+ 0.9 0.92 0.93 0.95 1.0
P 40 End crop Biomass Manipulation
P 24 Flatten Standing Biomass
+ 14 .6 .5 .4 .5 .5
#------------
D 19/07/04
O 03 Manure spreader, slurry
+ 11.505327 .29 1.7881091 0.0 1.7881091 1.3410819 3.5762181
T Created from RUSLE file MAS 9/19/06.
T This assumes a defult residue type of  manure slurry using a solid spread with a liquid end gate spreader.
T User needs to change to the correct manure type, make a calulation on the dry matter applied, and change the value in MCREW.
T This opn is built for an application of 10 ton/ac 10% dry matter surface applied manure.
T 10 tons x 2000 lbs/ac = 20,000 lbs/ac x 0.1 = 2,000 lbs/ac applied.
T MAS 12-5-07
+
G 01 Tillage
+ 0.0 0 1 0.0 0.0 0.0
P 24 Flatten Standing Biomass
+ 14 .1 .1 .1 .1 1.0
G 03 Crop Name
+ manure, slurry
P 66 Add Manure Residue Amount
+ 0.0 0.0 0.0 0.0 1
+ 0.0 0.0 0.0 0.0
+ 0.22417001 0.0
+ .06 .06 .06 .06 0.169 0.0050 1 0.6500045
+ -2.08165 0.548606
T Enter crop notes here.
#------------
D 01/09/04
O 04 Harvest, hay, legume
+ 17.959534 .15
T Harvest legume hay crops such as Alfalfa and Red clover and grass-legume mixed hay such as Alfalfa-Bromegrass.
T Use Harvest, grass hay" for pure grass hay. Rev 11/17/01 DTL"  MAS 11-29-06
T
T Reset the fuel use to 1.92 gal/ac MAS 10-21-11
+
G 02 Biomass Manipulation
+ 1.0
P 31 Kill or Defoliate Growing Crop
+ 0
P 42 Cut/Remove Biomass to Height (flags)
+ 1 0 0 0 0 101.600204 .9 .9 1
P 34 Change Standing Biomass Fall Rate
+ 0 1.1 1.08 1.06 1.04 1.0
+ 0.9 0.92 0.93 0.95 1.0
P 40 End crop Biomass Manipulation
P 24 Flatten Standing Biomass
+ 14 .6 .5 .4 .5 .5
#------------
D 05/09/04
O 03 Manure spreader, slurry
+ 11.505327 .29 1.7881091 0.0 1.7881091 1.3410819 3.5762181
T Created from RUSLE file MAS 9/19/06.
T This assumes a defult residue type of  manure slurry using a solid spread with a liquid end gate spreader.
T User needs to change to the correct manure type, make a calulation on the dry matter applied, and change the value in MCREW.
T This opn is built for an application of 10 ton/ac 10% dry matter surface applied manure.
T 10 tons x 2000 lbs/ac = 20,000 lbs/ac x 0.1 = 2,000 lbs/ac applied.
T MAS 12-5-07
+
G 01 Tillage
+ 0.0 0 1 0.0 0.0 0.0
P 24 Flatten Standing Biomass
+ 14 .1 .1 .1 .1 1.0
G 03 Crop Name
+ manure, slurry
P 66 Add Manure Residue Amount
+ 0.0 0.0 0.0 0.0 1
+ 0.0 0.0 0.0 0.0
+ 0.22417001 0.0
+ .06 .06 .06 .06 0.169 0.0050 1 0.6500045
+ -2.08165 0.548606
T Enter crop notes here.
#------------
D 02/06/05
O 04 Harvest, hay, legume
+ 17.959534 .15
T Harvest legume hay crops such as Alfalfa and Red clover and grass-legume mixed hay such as Alfalfa-Bromegrass.
T Use Harvest, grass hay" for pure grass hay. Rev 11/17/01 DTL"  MAS 11-29-06
T
T Reset the fuel use to 1.92 gal/ac MAS 10-21-11
+
G 02 Biomass Manipulation
+ 1.0
P 31 Kill or Defoliate Growing Crop
+ 0
P 42 Cut/Remove Biomass to Height (flags)
+ 1 0 0 0 0 101.600204 .9 .9 1
P 34 Change Standing Biomass Fall Rate
+ 0 1.1 1.08 1.06 1.04 1.0
+ 0.9 0.92 0.93 0.95 1.0
P 40 End crop Biomass Manipulation
P 24 Flatten Standing Biomass
+ 14 .6 .5 .4 .5 .5
#------------
D 06/06/05
O 03 Manure spreader, slurry
+ 11.505327 .29 1.7881091 0.0 1.7881091 1.3410819 3.5762181
T Created from RUSLE file MAS 9/19/06.
T This assumes a defult residue type of  manure slurry using a solid spread with a liquid end gate spreader.
T User needs to change to the correct manure type, make a calulation on the dry matter applied, and change the value in MCREW.
T This opn is built for an application of 10 ton/ac 10% dry matter surface applied manure.
T 10 tons x 2000 lbs/ac = 20,000 lbs/ac x 0.1 = 2,000 lbs/ac applied.
T MAS 12-5-07
+
G 01 Tillage
+ 0.0 0 1 0.0 0.0 0.0
P 24 Flatten Standing Biomass
+ 14 .1 .1 .1 .1 1.0
G 03 Crop Name
+ manure, slurry
P 66 Add Manure Residue Amount
+ 0.0 0.0 0.0 0.0 1
+ 0.0 0.0 0.0 0.0
+ 0.22417001 0.0
+ .06 .06 .06 .06 0.169 0.0050 1 0.6500045
+ -2.08165 0.548606
T Enter crop notes here.
#------------
D 15/07/05
O 04 Harvest, hay, legume
+ 17.959534 .15
T Harvest legume hay crops such as Alfalfa and Red clover and grass-legume mixed hay such as Alfalfa-Bromegrass.
T Use Harvest, grass hay" for pure grass hay. Rev 11/17/01 DTL"  MAS 11-29-06
T
T Reset the fuel use to 1.92 gal/ac MAS 10-21-11
+
G 02 Biomass Manipulation
+ 1.0
P 31 Kill or Defoliate Growing Crop
+ 0
P 42 Cut/Remove Biomass to Height (flags)
+ 1 0 0 0 0 101.600204 .9 .9 1
P 34 Change Standing Biomass Fall Rate
+ 0 1.1 1.08 1.06 1.04 1.0
+ 0.9 0.92 0.93 0.95 1.0
P 40 End crop Biomass Manipulation
P 24 Flatten Standing Biomass
+ 14 .6 .5 .4 .5 .5
#------------
D 19/07/05
O 03 Manure spreader, slurry
+ 11.505327 .29 1.7881091 0.0 1.7881091 1.3410819 3.5762181
T Created from RUSLE file MAS 9/19/06.
T This assumes a defult residue type of  manure slurry using a solid spread with a liquid end gate spreader.
T User needs to change to the correct manure type, make a calulation on the dry matter applied, and change the value in MCREW.
T This opn is built for an application of 10 ton/ac 10% dry matter surface applied manure.
T 10 tons x 2000 lbs/ac = 20,000 lbs/ac x 0.1 = 2,000 lbs/ac applied.
T MAS 12-5-07
+
G 01 Tillage
+ 0.0 0 1 0.0 0.0 0.0
P 24 Flatten Standing Biomass
+ 14 .1 .1 .1 .1 1.0
G 03 Crop Name
+ manure, slurry
P 66 Add Manure Residue Amount
+ 0.0 0.0 0.0 0.0 1
+ 0.0 0.0 0.0 0.0
+ 0.22417001 0.0
+ .06 .06 .06 .06 0.169 0.0050 1 0.6500045
+ -2.08165 0.548606
T Enter crop notes here.
#------------
D 01/09/05
O 04 Harvest, hay, legume
+ 17.959534 .15
T Harvest legume hay crops such as Alfalfa and Red clover and grass-legume mixed hay such as Alfalfa-Bromegrass.
T Use Harvest, grass hay" for pure grass hay. Rev 11/17/01 DTL"  MAS 11-29-06
T
T Reset the fuel use to 1.92 gal/ac MAS 10-21-11
+
G 02 Biomass Manipulation
+ 1.0
P 31 Kill or Defoliate Growing Crop
+ 0
P 42 Cut/Remove Biomass to Height (flags)
+ 1 0 0 0 0 101.600204 .9 .9 1
P 34 Change Standing Biomass Fall Rate
+ 0 1.1 1.08 1.06 1.04 1.0
+ 0.9 0.92 0.93 0.95 1.0
P 40 End crop Biomass Manipulation
P 24 Flatten Standing Biomass
+ 14 .6 .5 .4 .5 .5
#------------
D 02/09/05
O 03 Manure spreader, slurry
+ 11.505327 .29 1.7881091 0.0 1.7881091 1.3410819 3.5762181
T Created from RUSLE file MAS 9/19/06.
T This assumes a defult residue type of  manure slurry using a solid spread with a liquid end gate spreader.
T User needs to change to the correct manure type, make a calulation on the dry matter applied, and change the value in MCREW.
T This opn is built for an application of 10 ton/ac 10% dry matter surface applied manure.
T 10 tons x 2000 lbs/ac = 20,000 lbs/ac x 0.1 = 2,000 lbs/ac applied.
T MAS 12-5-07
+
G 01 Tillage
+ 0.0 0 1 0.0 0.0 0.0
P 24 Flatten Standing Biomass
+ 14 .1 .1 .1 .1 1.0
G 03 Crop Name
+ manure, slurry
P 66 Add Manure Residue Amount
+ 0.0 0.0 0.0 0.0 1
+ 0.0 0.0 0.0 0.0
+ 0.22417001 0.0
+ .06 .06 .06 .06 0.169 0.0050 1 0.6500045
+ -2.08165 0.548606
T Enter crop notes here.
#------------
D 02/06/06
O 04 Harvest, hay, legume
+ 17.959534 .15
T Harvest legume hay crops such as Alfalfa and Red clover and grass-legume mixed hay such as Alfalfa-Bromegrass.
T Use Harvest, grass hay" for pure grass hay. Rev 11/17/01 DTL"  MAS 11-29-06
T
T Reset the fuel use to 1.92 gal/ac MAS 10-21-11
+
G 02 Biomass Manipulation
+ 1.0
P 31 Kill or Defoliate Growing Crop
+ 0
P 42 Cut/Remove Biomass to Height (flags)
+ 1 0 0 0 0 101.600204 .9 .9 1
P 34 Change Standing Biomass Fall Rate
+ 0 1.1 1.08 1.06 1.04 1.0
+ 0.9 0.92 0.93 0.95 1.0
P 40 End crop Biomass Manipulation
P 24 Flatten Standing Biomass
+ 14 .6 .5 .4 .5 .5
#------------
D 06/06/06
O 03 Manure spreader, slurry
+ 11.505327 .29 1.7881091 0.0 1.7881091 1.3410819 3.5762181
T Created from RUSLE file MAS 9/19/06.
T This assumes a defult residue type of  manure slurry using a solid spread with a liquid end gate spreader.
T User needs to change to the correct manure type, make a calulation on the dry matter applied, and change the value in MCREW.
T This opn is built for an application of 10 ton/ac 10% dry matter surface applied manure.
T 10 tons x 2000 lbs/ac = 20,000 lbs/ac x 0.1 = 2,000 lbs/ac applied.
T MAS 12-5-07
+
G 01 Tillage
+ 0.0 0 1 0.0 0.0 0.0
P 24 Flatten Standing Biomass
+ 14 .1 .1 .1 .1 1.0
G 03 Crop Name
+ manure, slurry
P 66 Add Manure Residue Amount
+ 0.0 0.0 0.0 0.0 1
+ 0.0 0.0 0.0 0.0
+ 0.22417001 0.0
+ .06 .06 .06 .06 0.169 0.0050 1 0.6500045
+ -2.08165 0.548606
T Enter crop notes here.
#------------
D 15/07/06
O 04 Harvest, hay, legume
+ 17.959534 .15
T Harvest legume hay crops such as Alfalfa and Red clover and grass-legume mixed hay such as Alfalfa-Bromegrass.
T Use Harvest, grass hay" for pure grass hay. Rev 11/17/01 DTL"  MAS 11-29-06
T
T Reset the fuel use to 1.92 gal/ac MAS 10-21-11
+
G 02 Biomass Manipulation
+ 1.0
P 31 Kill or Defoliate Growing Crop
+ 0
P 42 Cut/Remove Biomass to Height (flags)
+ 1 0 0 0 0 101.600204 .9 .9 1
P 34 Change Standing Biomass Fall Rate
+ 0 1.1 1.08 1.06 1.04 1.0
+ 0.9 0.92 0.93 0.95 1.0
P 40 End crop Biomass Manipulation
P 24 Flatten Standing Biomass
+ 14 .6 .5 .4 .5 .5
#------------
D 19/07/06
O 03 Manure spreader, slurry
+ 11.505327 .29 1.7881091 0.0 1.7881091 1.3410819 3.5762181
T Created from RUSLE file MAS 9/19/06.
T This assumes a defult residue type of  manure slurry using a solid spread with a liquid end gate spreader.
T User needs to change to the correct manure type, make a calulation on the dry matter applied, and change the value in MCREW.
T This opn is built for an application of 10 ton/ac 10% dry matter surface applied manure.
T 10 tons x 2000 lbs/ac = 20,000 lbs/ac x 0.1 = 2,000 lbs/ac applied.
T MAS 12-5-07
+
G 01 Tillage
+ 0.0 0 1 0.0 0.0 0.0
P 24 Flatten Standing Biomass
+ 14 .1 .1 .1 .1 1.0
G 03 Crop Name
+ manure, slurry
P 66 Add Manure Residue Amount
+ 0.0 0.0 0.0 0.0 1
+ 0.0 0.0 0.0 0.0
+ 0.22417001 0.0
+ .06 .06 .06 .06 0.169 0.0050 1 0.6500045
+ -2.08165 0.548606
T Enter crop notes here.
#------------
D 01/09/06
O 04 Harvest, hay, legume
+ 17.959534 .15
T Harvest legume hay crops such as Alfalfa and Red clover and grass-legume mixed hay such as Alfalfa-Bromegrass.
T Use Harvest, grass hay" for pure grass hay. Rev 11/17/01 DTL"  MAS 11-29-06
T
T Reset the fuel use to 1.92 gal/ac MAS 10-21-11
+
G 02 Biomass Manipulation
+ 1.0
P 31 Kill or Defoliate Growing Crop
+ 0
P 42 Cut/Remove Biomass to Height (flags)
+ 1 0 0 0 0 101.600204 .9 .9 1
P 34 Change Standing Biomass Fall Rate
+ 0 1.1 1.08 1.06 1.04 1.0
+ 0.9 0.92 0.93 0.95 1.0
P 40 End crop Biomass Manipulation
P 24 Flatten Standing Biomass
+ 14 .6 .5 .4 .5 .5
#------------
D 02/09/06
O 03 Manure spreader, slurry
+ 11.505327 .29 1.7881091 0.0 1.7881091 1.3410819 3.5762181
T Created from RUSLE file MAS 9/19/06.
T This assumes a defult residue type of  manure slurry using a solid spread with a liquid end gate spreader.
T User needs to change to the correct manure type, make a calulation on the dry matter applied, and change the value in MCREW.
T This opn is built for an application of 10 ton/ac 10% dry matter surface applied manure.
T 10 tons x 2000 lbs/ac = 20,000 lbs/ac x 0.1 = 2,000 lbs/ac applied.
T MAS 12-5-07
+
G 01 Tillage
+ 0.0 0 1 0.0 0.0 0.0
P 24 Flatten Standing Biomass
+ 14 .1 .1 .1 .1 1.0
G 03 Crop Name
+ manure, slurry
P 66 Add Manure Residue Amount
+ 0.0 0.0 0.0 0.0 1
+ 0.0 0.0 0.0 0.0
+ 0.22417001 0.0
+ .06 .06 .06 .06 0.169 0.0050 1 0.6500045
+ -2.08165 0.548606
T Enter crop notes here.
#------------
*END
*EOF
