Version: 1.5
*START 4
N Originating Program: RUSLE2
N Skel Format Version: 1.1
N This management file was originally converted from the NRCS standard XML format on - Thu Jun 28 13:36:21 PDT 2012
N This management file was updated to contain the most current crop and operation records for WEPS on - Tue Dec 17 19:22:07 CST 2013
#------------
D 24/05/01
O 03 Disk, tandem heavy primary op
+ 7.0154433 39 2.2351363 0.0 2.2351363 1.3410819 2.6821637
T 11-12in. Spacing, Front and Rear
T Recommended for primary tillage in medium to heavy soils
T Excellent residue-handling capability. MAS 10-26-06
+
G 01 Tillage
+ 152.4003 1.0 1.0 152.4003 101.600204 177.80035
P 01 Break Crust
P 02 Random Roughness
+ 1 38.100075
P 05 Ridges and Dikes
+ 1 101.600204 279.40057 0.0 0.0 0.0
P 11 Aggregate Crushing
+ 2.8 0.75
P 12 Soil Loosening
+ 0.9
P 13 Soil Layer Mixing
+ 0.4
P 31 Kill or Defoliate Growing Crop
+ 2
P 40 End crop Biomass Manipulation
P 24 Flatten Standing Biomass
+ 0 1.0 0.9 0.8 0.5 1.0
P 25 Bury Flat Biomass
+ 1 0.95 0.85 0.8 0.6 0.95
P 26 Resurface Buried Biomass
+ 0.05 0.06 0.07 0.08 0.05
P 34 Change Standing Biomass Fall Rate
+ 7 3.0 2.5 2.0 1.5 1.0
+ 0.5 0.6 0.7 0.8 1.0
#------------
D 29/05/01
O 03 Manure spreader, slurry
+ 11.505327 .29 1.7881091 0.0 1.7881091 1.3410819 3.5762181
T Created from RUSLE file MAS 9/19/06.
T This assumes a defult residue type of  manure slurry using a solid spread with a liquid end gate spreader.
T User needs to change to the correct manure type, make a calulation on the dry matter applied, and change the value in MCREW.
T This opn is built for an application of 10 ton/ac 10% dry matter surface applied manure.
T 10 tons x 2000 lbs/ac = 20,000 lbs/ac x 0.1 = 2,000 lbs/ac applied.
T MAS 12-5-07
+
G 01 Tillage
+ 0.0 0 1 0.0 0.0 0.0
P 24 Flatten Standing Biomass
+ 14 .1 .1 .1 .1 1.0
G 03 Crop Name
+ manure, slurry
P 66 Add Manure Residue Amount
+ 0.0 0.0 0.0 0.0 1
+ 0.0 0.0 0.0 0.0
+ 0.22417001 0.0
+ .06 .06 .06 .06 0.169 0.0050 1 0.6500045
+ -2.08165 0.548606
T Enter crop notes here.
#------------
D 29/05/01
O 03 Harrow, coiled tine
+ 4.1157265 15.6 2.6821637 0.0 2.6821637 1.3410819 3.129191
T This oprn is from a RUSLE record created 6/7/01.  10-25-06 MAS
T
T Corrected ridge height and spacing to match RUSLE2. 10-26-11 LOS
T
T Changed spacing from 0 to 1 in. The 0 caused the operation to fail.  12-12-11 MAS
+
G 01 Tillage
+ 50.800102 0.25 1.0 50.800102 25.400051 76.20015
P 01 Break Crust
P 02 Random Roughness
+ 1 10.160021
P 05 Ridges and Dikes
+ 1 25.400051 101.600204 0.0 0.0 0.0
P 11 Aggregate Crushing
+ 3.0 -0.22
P 12 Soil Loosening
+ 0.6
P 13 Soil Layer Mixing
+ 0.2
P 31 Kill or Defoliate Growing Crop
+ 2
P 40 End crop Biomass Manipulation
P 24 Flatten Standing Biomass
+ 0 0.5 0.3 0.2 0.1 1.0
P 25 Bury Flat Biomass
+ 1 0.25 0.2 0.15 0.1 0.25
P 26 Resurface Buried Biomass
+ 0.01 0.01 0.01 0.02 0.01
P 34 Change Standing Biomass Fall Rate
+ 7 3.0 2.5 2.0 1.5 1.0
+ 0.5 0.6 0.7 0.8 1.0
#------------
D 01/06/01
O 03 Drill or air seeder, hoe or chisel openers 6-12 in spac
+ 6.921904 23.4 2.2351363 0 2.2351363 1.5645955 2.9056773
T Drill or Airseeder, hoe or chisel openers and 3 in. wide presswheels.   From RUSLE 1 MAS 10-19-06
T G2 was added into file in front of the flattening (P24), burial (P25), and resurfacing (P26) factors because the area affected is less than 1.0 and
T the RUSLE values were normalized to 1.0.  This change will imulate the correct residue changes based on the method set forth in RUSLE.
T RUSLE's factors have been redused to based on the area affected.
T The stalk fall rate factor (P34) was moved ahead of the new (G2) factor to set the fall rate to the  less than 1.0 area affected.  8/7/07 MAS
+
G 01 Tillage
+ 101.600204 0.75 0.9 101.600204 76.20015 152.4003
P 01 Break Crust
P 02 Random Roughness
+ 1 12.700026
P 05 Ridges and Dikes
+ 1 76.20015 203.2004064008128 50.800102 0 0
P 11 Aggregate Crushing
+ 2.4 -2.0
P 12 Soil Loosening
+ 0.7
P 13 Soil Layer Mixing
+ 0.5
P 31 Kill or Defoliate Growing Crop
+ 2
P 40 End crop Biomass Manipulation
P 34 Change Standing Biomass Fall Rate
+ 7 3.0 2.5 2.0 1.5 1.0
+ 0.5 0.6 0.7 0.8 1.0
G 02 Biomass Manipulation
+ 1.0
P 24 Flatten Standing Biomass
+ 0 0.6 0.4 0.3 0.3 1.0
P 25 Bury Flat Biomass
+ 1 0.45 0.36 0.27 0.23 0.34
P 26 Resurface Buried Biomass
+ 0.01 0.01 0.01 0.03 0.01
G 03 Crop Name
+ Clover, red, seed
P 51 Seeding Configuration
+ 1 0.0 0
+ 120.0 5.0 1 1500.0 1.0 1.0 0
+ lb/ac
+ 12.0 8930.0 3 0.5 0.65 0.8
+ 0.8 0.01 2.0 1.0 25.0 0 120 1800.0
+ -5.0 -15.0 0.005 0.05 0.0 25.0
+ 0.023 0.8063 0.4146 -0.061 -0.024 0.9911 0.6435 0.0494
+ 0.4146 -0.061 3.9 1.0 20.6 0.05 0 0.1442091
+ 1.6666666 120.0 0.6 0.013 0.1 0.1 0.0 1
+ 0.02 0.02 0.02 0.02 0.2 0.0050 20.0 4.933536
+ -1.20379 0.604887 18 0.067251004 0.0 0.0 0.0 0.0
T Adjusted the Harvest fraction of the Plant Compoent from 0.2 to 0.5.  MAS 3-10-09
#------------
D 01/09/01
O 04 Harvest, hay, grass
+ 17.959534 .15
T Harvest legume hay crops such as Alfalfa and Red clover and grass-legume mixed hay such as Alfalfa-Bromegrass.
T Use Harvest, grass hay" for pure grass hay. Rev 11/17/01 DTL"  MAS 11-29-06
T
T Reset the fuel use to 1.92 gal/ac MAS 10-21-11
+
G 02 Biomass Manipulation
+ 1.0
P 31 Kill or Defoliate Growing Crop
+ 0
P 42 Cut/Remove Biomass to Height (flags)
+ 1 0 0 0 0 101.600204 .85 .85 1
P 34 Change Standing Biomass Fall Rate
+ 0 1.1 1.08 1.06 1.04 1.0
+ 0.9 0.92 0.93 0.95 1.0
P 40 End crop Biomass Manipulation
P 24 Flatten Standing Biomass
+ 14 .6 .5 .4 .5 .5
#------------
D 10/05/02
O 03 Manure spreader, slurry
+ 11.505327 .29 1.7881091 0.0 1.7881091 1.3410819 3.5762181
T Created from RUSLE file MAS 9/19/06.
T This assumes a defult residue type of  manure slurry using a solid spread with a liquid end gate spreader.
T User needs to change to the correct manure type, make a calulation on the dry matter applied, and change the value in MCREW.
T This opn is built for an application of 10 ton/ac 10% dry matter surface applied manure.
T 10 tons x 2000 lbs/ac = 20,000 lbs/ac x 0.1 = 2,000 lbs/ac applied.
T MAS 12-5-07
+
G 01 Tillage
+ 0.0 0 1 0.0 0.0 0.0
P 24 Flatten Standing Biomass
+ 14 .1 .1 .1 .1 1.0
G 03 Crop Name
+ manure, slurry
P 66 Add Manure Residue Amount
+ 0.0 0.0 0.0 0.0 1
+ 0.0 0.0 0.0 0.0
+ 0.22417001 0.0
+ .06 .06 .06 .06 0.169 0.0050 1 0.6500045
+ -2.08165 0.548606
T Enter crop notes here.
#------------
D 01/08/02
O 04 Harvest, hay, grass
+ 17.959534 .15
T Harvest legume hay crops such as Alfalfa and Red clover and grass-legume mixed hay such as Alfalfa-Bromegrass.
T Use Harvest, grass hay" for pure grass hay. Rev 11/17/01 DTL"  MAS 11-29-06
T
T Reset the fuel use to 1.92 gal/ac MAS 10-21-11
+
G 02 Biomass Manipulation
+ 1.0
P 31 Kill or Defoliate Growing Crop
+ 0
P 42 Cut/Remove Biomass to Height (flags)
+ 1 0 0 0 0 101.600204 .85 .85 1
P 34 Change Standing Biomass Fall Rate
+ 0 1.1 1.08 1.06 1.04 1.0
+ 0.9 0.92 0.93 0.95 1.0
P 40 End crop Biomass Manipulation
P 24 Flatten Standing Biomass
+ 14 .6 .5 .4 .5 .5
#------------
D 05/08/02
O 03 Manure spreader, slurry
+ 11.505327 .29 1.7881091 0.0 1.7881091 1.3410819 3.5762181
T Created from RUSLE file MAS 9/19/06.
T This assumes a defult residue type of  manure slurry using a solid spread with a liquid end gate spreader.
T User needs to change to the correct manure type, make a calulation on the dry matter applied, and change the value in MCREW.
T This opn is built for an application of 10 ton/ac 10% dry matter surface applied manure.
T 10 tons x 2000 lbs/ac = 20,000 lbs/ac x 0.1 = 2,000 lbs/ac applied.
T MAS 12-5-07
+
G 01 Tillage
+ 0.0 0 1 0.0 0.0 0.0
P 24 Flatten Standing Biomass
+ 14 .1 .1 .1 .1 1.0
G 03 Crop Name
+ manure, slurry
P 66 Add Manure Residue Amount
+ 0.0 0.0 0.0 0.0 1
+ 0.0 0.0 0.0 0.0
+ 0.22417001 0.0
+ .06 .06 .06 .06 0.169 0.0050 1 0.6500045
+ -2.08165 0.548606
T Enter crop notes here.
#------------
D 10/05/03
O 03 Manure spreader, slurry
+ 11.505327 .29 1.7881091 0.0 1.7881091 1.3410819 3.5762181
T Created from RUSLE file MAS 9/19/06.
T This assumes a defult residue type of  manure slurry using a solid spread with a liquid end gate spreader.
T User needs to change to the correct manure type, make a calulation on the dry matter applied, and change the value in MCREW.
T This opn is built for an application of 10 ton/ac 10% dry matter surface applied manure.
T 10 tons x 2000 lbs/ac = 20,000 lbs/ac x 0.1 = 2,000 lbs/ac applied.
T MAS 12-5-07
+
G 01 Tillage
+ 0.0 0 1 0.0 0.0 0.0
P 24 Flatten Standing Biomass
+ 14 .1 .1 .1 .1 1.0
G 03 Crop Name
+ manure, slurry
P 66 Add Manure Residue Amount
+ 0.0 0.0 0.0 0.0 1
+ 0.0 0.0 0.0 0.0
+ 0.22417001 0.0
+ .06 .06 .06 .06 0.169 0.0050 1 0.6500045
+ -2.08165 0.548606
T Enter crop notes here.
#------------
D 01/08/03
O 04 Harvest, hay, grass
+ 17.959534 .15
T Harvest legume hay crops such as Alfalfa and Red clover and grass-legume mixed hay such as Alfalfa-Bromegrass.
T Use Harvest, grass hay" for pure grass hay. Rev 11/17/01 DTL"  MAS 11-29-06
T
T Reset the fuel use to 1.92 gal/ac MAS 10-21-11
+
G 02 Biomass Manipulation
+ 1.0
P 31 Kill or Defoliate Growing Crop
+ 0
P 42 Cut/Remove Biomass to Height (flags)
+ 1 0 0 0 0 101.600204 .85 .85 1
P 34 Change Standing Biomass Fall Rate
+ 0 1.1 1.08 1.06 1.04 1.0
+ 0.9 0.92 0.93 0.95 1.0
P 40 End crop Biomass Manipulation
P 24 Flatten Standing Biomass
+ 14 .6 .5 .4 .5 .5
#------------
D 05/08/03
O 03 Manure spreader, slurry
+ 11.505327 .29 1.7881091 0.0 1.7881091 1.3410819 3.5762181
T Created from RUSLE file MAS 9/19/06.
T This assumes a defult residue type of  manure slurry using a solid spread with a liquid end gate spreader.
T User needs to change to the correct manure type, make a calulation on the dry matter applied, and change the value in MCREW.
T This opn is built for an application of 10 ton/ac 10% dry matter surface applied manure.
T 10 tons x 2000 lbs/ac = 20,000 lbs/ac x 0.1 = 2,000 lbs/ac applied.
T MAS 12-5-07
+
G 01 Tillage
+ 0.0 0 1 0.0 0.0 0.0
P 24 Flatten Standing Biomass
+ 14 .1 .1 .1 .1 1.0
G 03 Crop Name
+ manure, slurry
P 66 Add Manure Residue Amount
+ 0.0 0.0 0.0 0.0 1
+ 0.0 0.0 0.0 0.0
+ 0.22417001 0.0
+ .06 .06 .06 .06 0.169 0.0050 1 0.6500045
+ -2.08165 0.548606
T Enter crop notes here.
#------------
D 10/05/04
O 03 Manure spreader, slurry
+ 11.505327 .29 1.7881091 0.0 1.7881091 1.3410819 3.5762181
T Created from RUSLE file MAS 9/19/06.
T This assumes a defult residue type of  manure slurry using a solid spread with a liquid end gate spreader.
T User needs to change to the correct manure type, make a calulation on the dry matter applied, and change the value in MCREW.
T This opn is built for an application of 10 ton/ac 10% dry matter surface applied manure.
T 10 tons x 2000 lbs/ac = 20,000 lbs/ac x 0.1 = 2,000 lbs/ac applied.
T MAS 12-5-07
+
G 01 Tillage
+ 0.0 0 1 0.0 0.0 0.0
P 24 Flatten Standing Biomass
+ 14 .1 .1 .1 .1 1.0
G 03 Crop Name
+ manure, slurry
P 66 Add Manure Residue Amount
+ 0.0 0.0 0.0 0.0 1
+ 0.0 0.0 0.0 0.0
+ 0.22417001 0.0
+ .06 .06 .06 .06 0.169 0.0050 1 0.6500045
+ -2.08165 0.548606
T Enter crop notes here.
#------------
D 01/08/04
O 04 Harvest, hay, grass
+ 17.959534 .15
T Harvest legume hay crops such as Alfalfa and Red clover and grass-legume mixed hay such as Alfalfa-Bromegrass.
T Use Harvest, grass hay" for pure grass hay. Rev 11/17/01 DTL"  MAS 11-29-06
T
T Reset the fuel use to 1.92 gal/ac MAS 10-21-11
+
G 02 Biomass Manipulation
+ 1.0
P 31 Kill or Defoliate Growing Crop
+ 0
P 42 Cut/Remove Biomass to Height (flags)
+ 1 0 0 0 0 101.600204 .85 .85 1
P 34 Change Standing Biomass Fall Rate
+ 0 1.1 1.08 1.06 1.04 1.0
+ 0.9 0.92 0.93 0.95 1.0
P 40 End crop Biomass Manipulation
P 24 Flatten Standing Biomass
+ 14 .6 .5 .4 .5 .5
#------------
D 05/08/04
O 03 Manure spreader, slurry
+ 11.505327 .29 1.7881091 0.0 1.7881091 1.3410819 3.5762181
T Created from RUSLE file MAS 9/19/06.
T This assumes a defult residue type of  manure slurry using a solid spread with a liquid end gate spreader.
T User needs to change to the correct manure type, make a calulation on the dry matter applied, and change the value in MCREW.
T This opn is built for an application of 10 ton/ac 10% dry matter surface applied manure.
T 10 tons x 2000 lbs/ac = 20,000 lbs/ac x 0.1 = 2,000 lbs/ac applied.
T MAS 12-5-07
+
G 01 Tillage
+ 0.0 0 1 0.0 0.0 0.0
P 24 Flatten Standing Biomass
+ 14 .1 .1 .1 .1 1.0
G 03 Crop Name
+ manure, slurry
P 66 Add Manure Residue Amount
+ 0.0 0.0 0.0 0.0 1
+ 0.0 0.0 0.0 0.0
+ 0.22417001 0.0
+ .06 .06 .06 .06 0.169 0.0050 1 0.6500045
+ -2.08165 0.548606
T Enter crop notes here.
#------------
*END
*EOF
