Version: 1.5
*START 1
N Originating Program: RUSLE2
N Skel Format Version: 1.1
N This management file was originally converted from the NRCS standard XML format on - Thu Jun 28 13:37:08 PDT 2012
N This management file was updated to contain the most current crop and operation records for WEPS on - Tue Dec 17 19:19:09 CST 2013
#------------
D 30/04/01
O 03 Disk, tandem heavy primary op
+ 7.0154433 39 2.2351363 0.0 2.2351363 1.3410819 2.6821637
T 11-12in. Spacing, Front and Rear
T Recommended for primary tillage in medium to heavy soils
T Excellent residue-handling capability. MAS 10-26-06
+
G 01 Tillage
+ 152.4003 1.0 1.0 152.4003 101.600204 177.80035
P 01 Break Crust
P 02 Random Roughness
+ 1 38.100075
P 05 Ridges and Dikes
+ 1 101.600204 279.40057 0.0 0.0 0.0
P 11 Aggregate Crushing
+ 2.8 0.75
P 12 Soil Loosening
+ 0.9
P 13 Soil Layer Mixing
+ 0.4
P 31 Kill or Defoliate Growing Crop
+ 2
P 40 End crop Biomass Manipulation
P 24 Flatten Standing Biomass
+ 0 1.0 0.9 0.8 0.5 1.0
P 25 Bury Flat Biomass
+ 1 0.95 0.85 0.8 0.6 0.95
P 26 Resurface Buried Biomass
+ 0.05 0.06 0.07 0.08 0.05
P 34 Change Standing Biomass Fall Rate
+ 7 3.0 2.5 2.0 1.5 1.0
+ 0.5 0.6 0.7 0.8 1.0
#------------
D 05/05/01
O 04 Fert applic. surface broadcast
+ 1.4966278 0.0609375
T R2 Notes: Broadcast fertilizer spreader.  Wheel traffic only.  rev 082107 DTL
T
T Added to DB 4-12-12 MAS
+
G 01 Tillage
+ 0.0 0 0.05 0.0 0.0 0.0
P 01 Break Crust
P 02 Random Roughness
+ 1 8.8900175
P 11 Aggregate Crushing
+ 4.3 2.0
P 24 Flatten Standing Biomass
+ 0 0.25 0.2 0.15 0.1 1.0
P 26 Resurface Buried Biomass
+ 0.07 0.08 0.1 0.12 0.07
P 34 Change Standing Biomass Fall Rate
+ 0 1.0 1.0 1.0 1.0 1.0
+ 1.0 1.0 1.0 1.0 1.0
#------------
D 05/05/01
O 03 Harrow, coiled tine
+ 4.1157265 15.6 2.6821637 0.0 2.6821637 1.3410819 3.129191
T This oprn is from a RUSLE record created 6/7/01.  10-25-06 MAS
T
T Corrected ridge height and spacing to match RUSLE2. 10-26-11 LOS
T
T Changed spacing from 0 to 1 in. The 0 caused the operation to fail.  12-12-11 MAS
+
G 01 Tillage
+ 50.800102 0.25 1.0 50.800102 25.400051 76.20015
P 01 Break Crust
P 02 Random Roughness
+ 1 10.160021
P 05 Ridges and Dikes
+ 1 25.400051 101.600204 0.0 0.0 0.0
P 11 Aggregate Crushing
+ 3.0 -0.22
P 12 Soil Loosening
+ 0.6
P 13 Soil Layer Mixing
+ 0.2
P 31 Kill or Defoliate Growing Crop
+ 2
P 40 End crop Biomass Manipulation
P 24 Flatten Standing Biomass
+ 0 0.5 0.3 0.2 0.1 1.0
P 25 Bury Flat Biomass
+ 1 0.25 0.2 0.15 0.1 0.25
P 26 Resurface Buried Biomass
+ 0.01 0.01 0.01 0.02 0.01
P 34 Change Standing Biomass Fall Rate
+ 7 3.0 2.5 2.0 1.5 1.0
+ 0.5 0.6 0.7 0.8 1.0
#------------
D 05/05/01
O 03 Drill or airseeder, double disk
+ 3.3674128 6.34 2.2351363 0.0 2.2351363 1.5645955 2.9056773
T Drill or air seeder with double disk openers on 7 to 10 inch spacings.  Rev102403 DTL  RUSLE MAS 10-26-06
T G2 was added into file in front of the flattening (P24), burial (P25), and resurfacing (P26) factors because the area affected is less than 1.0 and
T the RUSLE values were normalized to 1.0.  This change will imulate the correct residue changes based on the method set forth in RUSLE.
T RUSLE's factors have been redused to based on the area affected.
T The stalk fall rate factor (P34) was moved ahead of the new (G2) factor to set the fall rate to the  less than 1.0 area affected.  8/8/07 MAS
T
T Deleted the G2 process because all process only affect 0.65 of the surface.  This is set a 0.65 with G1 process in the beginning. 5-11-11 MAS
+ 
G 01 Tillage
+ 38.100075 0.4 0.65 38.100075 25.400051 50.800102
P 01 Break Crust
P 02 Random Roughness
+ 1 7.6200156
P 05 Ridges and Dikes
+ 1 25.400051 203.20041 25.400051 0.0 0.0
P 11 Aggregate Crushing
+ 2.8 0.75
P 12 Soil Loosening
+ 0.6
P 13 Soil Layer Mixing
+ 0.3
P 34 Change Standing Biomass Fall Rate
+ 7 3.0 2.5 2.0 1.5 1.0
+ 0.5 0.6 0.7 0.8 1.0
P 24 Flatten Standing Biomass
+ 0 0.6 0.4 0.35 0.15 1.0
P 25 Bury Flat Biomass
+ 1 0.2275 0.1625 0.13 0.065 0.13
P 26 Resurface Buried Biomass
+ 0.01 0.01 0.01 0.02 0.01
G 03 Crop Name
+ Oats, spring
P 51 Seeding Configuration
+ 1 0.0 0
+ 220.0 8.0 1 60 1.0 1.0 0
+ bu/ac
+ 14 278.8 4 0.8 0.64 0.8
+ 1.0 0.025 1.3716166 0.0 21.0 0 90 1500.0
+ -5.0 -15.0 0.005 0.05 0.0 35.0
+ 0.013 0.8013 0.4293 -0.086 -0.018 0.932 0.456 0.0736
+ 0.4293 -0.086 3.14 1.0 23.1 0.05 0 0.3
+ 33.333332 310.0 1.5 0.015 0 0 0.0 2
+ 0.0185 0.0185 0.0185 0.0185 0.28 0.0050 17.1 5.227942
+ -2.08165 0.548606 1.8 0.042592302 0.0 0.0 0.0 0.0
T Enter crop notes here.
#------------
D 15/08/01
O 04 Harvest, grain, high cut, release new crop
+ 14.311503 .15
T ARS record - filename is:  Harvest Wheat - grain (combine cutterbar header).oprn
T This operation record is designed to represent actual field harvesting operation
T of removing the grain from small grain crops with a cutterbar head on a combine.
T This harvesting operation record removes all the reproductive component of a crop above the
T cutting height.  Typically this is specified as the "yield" component in the crop record.
T The non-harvested crop plant material above the specified cut height becomes flat residue.
T The remaining above ground crop material below the specified cut height becomes standing residue.
T Nov 02, 2005	Created - Larry Wagner
T Detailed info regarding this operation record:
T This harvest record specifies the actual cut height dependent upon the height
T of the crop.  The cut height is specified as a fraction of the crop height.
T Added 0.2 for the flatting of the combine and tire trafic for haulling grain.
T MAS 1-18-07
T The harvesting operation could also have an effect on the "standing stalk"
T fall rate and fall threshold values.  The default "biomass pool" flag parameter
T is set to "No adjustments applied" so that no "stalk residue decay rate change" will occur.
T However, this flag value can be changed along with the default parameter values
T to change the "stalk residue decay processes".
+
G 02 Biomass Manipulation
+ 1.0
P 31 Kill or Defoliate Growing Crop
+ 2
P 43 Cut/Remove Biomass by Fraction (flags)
+ 1 1 0 1 0.2 1 0 0
P 34 Change Standing Biomass Fall Rate
+ 0 1.0 1.0 1.0 1.0 1.0
+ 1.0 1.0 1.0 1.0 1.0
P 40 End crop Biomass Manipulation
P 24 Flatten Standing Biomass
+ 0 0.2 0.2 0.2 0.2 1
G 03 Crop Name
+ Clover, red, released growing crop
P 51 Seeding Configuration
+ 1 0.0 0
+ 120.0 1 0 3.0 1.0 1.0 2
+ ton/ac
+ 0 4.465 3 1.0 0.65 0.8
+ 0.8 0.01 2.0 1.0 25.0 1 120 1800.0
+ -5.0 -15.0 0.005 0.05 0.0 25.0
+ 0.023 0.8063 0.4146 -0.061 -0.024 0.9911 0.6435 0.0494
+ 0.4146 -0.061 3.9 1.0 20.6 0.05 0 0.1442091
+ 850.4848 850.4848 0.6 0.013 0.1 0.1 0.0 2
+ 0.02 0.02 0.02 0.02 0.2 0.0050 20.0 4.933536
+ -1.20379 0.604887 0.0 0.0 0.0 0.0 0.0 0.0
T Enter crop notes here.
#------------
D 01/11/01
O 03 Plow, moldboard
+ 17.491838 65 2.2351363 0.0 2.2351363 1.5645955 2.6821637
T Moldboard plow 8 inch operating depth.  060701 DTL  Modified flattening and burial per McCool and Foster 05/21/02 DTL RUSLE MAS 10-26-06
+
G 01 Tillage
+ 203.20041 1.0 1.0 203.20041 152.4003 254.0005
P 01 Break Crust
P 02 Random Roughness
+ 1 48.260098
P 05 Ridges and Dikes
+ 1 25.400051 406.40082 0.0 0.0 0.0
P 11 Aggregate Crushing
+ 2.8 1.0
P 12 Soil Loosening
+ 1.0
P 13 Soil Layer Mixing
+ 0.7
P 14 Soil Layer Inversion
P 31 Kill or Defoliate Growing Crop
+ 2
P 40 End crop Biomass Manipulation
P 24 Flatten Standing Biomass
+ 0 1 1 1 0.75 1.0
P 25 Bury Flat Biomass
+ 3 0.99 0.99 0.99 0.85 0.97
P 26 Resurface Buried Biomass
+ 0.01 0.02 0.04 0.1 0.02
P 34 Change Standing Biomass Fall Rate
+ 7 3.0 2.5 2.0 1.5 1.0
+ 0.5 0.6 0.7 0.8 1.0
#------------
*END
*EOF
