Version: 1.5
*START 3
N Originating Program: RUSLE2
N Skel Format Version: 1.1
N This management file was originally converted from the NRCS standard XML format on - Thu Jul 05 09:35:33 PDT 2012
N This management file was updated to contain the most current crop and operation records for WEPS on - Tue Dec 17 21:14:16 CST 2013
#------------
D 09/05/01
O 03 Disk, tandem light finishing
+ 3.7415698 19.5 2.2351363 0.0 2.2351363 1.3410819 2.6821637
T 6/8/01 DTL RUSLE.  7in sp.  This is tool used to finish a seedbed.  MAS 10-26-06
+
G 01 Tillage
+ 101.600204 0.5 1.0 101.600204 76.20015 127.00026
P 01 Break Crust
P 02 Random Roughness
+ 1 15.240031
P 05 Ridges and Dikes
+ 1 12.700026 177.80035 0.0 0.0 0.0
P 11 Aggregate Crushing
+ 2.8 0.75
P 12 Soil Loosening
+ 0.75
P 13 Soil Layer Mixing
+ 0.35
P 31 Kill or Defoliate Growing Crop
+ 2
P 40 End crop Biomass Manipulation
P 24 Flatten Standing Biomass
+ 0 0.85 0.7 0.6 0.5 1.0
P 25 Bury Flat Biomass
+ 1 0.73 0.63 0.55 0.4 0.73
P 26 Resurface Buried Biomass
+ 0.02 0.04 0.02 0.05 0.02
P 34 Change Standing Biomass Fall Rate
+ 7 3.0 2.5 2.0 1.5 1.0
+ 0.5 0.6 0.7 0.8 1.0
#------------
D 10/05/01
O 04 Fert applic. surface broadcast
+ 1.4966278 0.0609375
T R2 Notes: Broadcast fertilizer spreader.  Wheel traffic only.  rev 082107 DTL
T
T Added to DB 4-12-12 MAS
+
G 01 Tillage
+ 0.0 0 0.05 0.0 0.0 0.0
P 01 Break Crust
P 02 Random Roughness
+ 1 8.8900175
P 11 Aggregate Crushing
+ 4.3 2.0
P 24 Flatten Standing Biomass
+ 0 0.25 0.2 0.15 0.1 1.0
P 26 Resurface Buried Biomass
+ 0.07 0.08 0.1 0.12 0.07
P 34 Change Standing Biomass Fall Rate
+ 0 1.0 1.0 1.0 1.0 1.0
+ 1.0 1.0 1.0 1.0 1.0
#------------
D 10/05/01
O 03 Disk, tandem secondary op
+ 4.4898834 32.5 2.2351363 0.0 2.2351363 1.3410819 2.6821637
T 9-in. Spacing, Front and Rear; Good for seedbed preparation/chemical incorporation in medium to heavy soils
T Works well in primary tillage in light to medium soils
T Provides good residue-handling capability.  MAS 10-26-06
+
G 01 Tillage
+ 127.00027 0.75 1.0 127.00026 76.20015 152.4003
P 01 Break Crust
P 02 Random Roughness
+ 1 15.240031
P 05 Ridges and Dikes
+ 1 50.800102 228.60046 0.0 0.0 0.0
P 11 Aggregate Crushing
+ 2.8 0.75
P 12 Soil Loosening
+ 0.85
P 13 Soil Layer Mixing
+ 0.4
P 31 Kill or Defoliate Growing Crop
+ 2
P 40 End crop Biomass Manipulation
P 24 Flatten Standing Biomass
+ 0 0.85 0.7 0.6 0.5 1.0
P 25 Bury Flat Biomass
+ 1 0.73 0.63 0.55 0.4 0.73
P 26 Resurface Buried Biomass
+ 0.02 0.04 0.02 0.05 0.02
P 34 Change Standing Biomass Fall Rate
+ 7 3.0 2.5 2.0 1.5 1.0
+ 0.5 0.6 0.7 0.8 1.0
#------------
D 11/05/01
O 03 Cultipacker, roller
+ 5.799433 35.59 2.6821637 0.0 2.6821637 1.3410819 3.5762181
T Based on RUSLE core Cultipacker Roller finishing tool.
T Consists of an inline gang of ridged rollers follow by one or more rows of staggerd
T spring culivator teeth, followed by a second row of ridged rollers.
T When the culivator teeth are raised out of the ground use the
T operation Roller, corregated packer MAS 10-18-06
+
G 01 Tillage
+ 38.100075 0.5 1.0 38.100075 25.400051 50.800102
P 01 Break Crust
P 02 Random Roughness
+ 1 10.160021
P 05 Ridges and Dikes
+ 1 25.400051 76.20015 0.0 0.0 0.0
P 11 Aggregate Crushing
+ 3.0 -0.22
P 24 Flatten Standing Biomass
+ 0 0.95 .95 .95 .95 1.0
P 25 Bury Flat Biomass
+ 1 .05 .05 .05 .05 .05
P 26 Resurface Buried Biomass
+ 0.01 0.01 0.01 .01 0.01
G 01 Tillage
+ 101.600204 .5 1.0 101.600204 50.800102 152.4003
P 01 Break Crust
P 02 Random Roughness
+ 1 20.320042
P 05 Ridges and Dikes
+ 1 50.800102 228.60045 0.0 0.0 0.0
P 11 Aggregate Crushing
+ 3.0 1.0
P 12 Soil Loosening
+ 0.5
P 13 Soil Layer Mixing
+ .4
P 31 Kill or Defoliate Growing Crop
+ 2
P 40 End crop Biomass Manipulation
P 24 Flatten Standing Biomass
+ 0 0.8 .7 .4 .3 1.0
P 25 Bury Flat Biomass
+ 1 .5 .4 .35 .2 .85
P 26 Resurface Buried Biomass
+ 0.05 0.06 0.07 .2 0.05
G 01 Tillage
+ 38.100075 0.5 1.0 38.100075 25.400051 50.800102
P 01 Break Crust
P 02 Random Roughness
+ 1 10.160021
P 05 Ridges and Dikes
+ 1 25.400051 76.20015 0.0 0.0 0.0
P 11 Aggregate Crushing
+ 3.0 -0.22
P 24 Flatten Standing Biomass
+ 0 .95 .95 .95 .95 1.0
P 25 Bury Flat Biomass
+ 1 .05 .05 .05 .05 .05
P 26 Resurface Buried Biomass
+ 0.01 0.01 0.01 .01 0.01
P 34 Change Standing Biomass Fall Rate
+ 7 3.0 2.5 2.0 1.5 1.0
+ 0.5 0.6 0.7 0.8 1.0
#------------
D 12/05/01
O 03 Planter, sprig conventional
+ 3.7415698 13 2.2351363 0.0 2.2351363 1.3410819 2.6821637
T Planter used to plant sprigs.  Similar to a light finishing disk 11-14-02 DTL
+ 
G 01 Tillage
+ 50.800102 0.4 1.0 50.800102 25.400051 76.20015
P 01 Break Crust
P 02 Random Roughness
+ 1 15.240031
P 05 Ridges and Dikes
+ 1 25.400051 609.6012 508.001 0.0 0.0
P 11 Aggregate Crushing
+ 2.4 2.0
P 12 Soil Loosening
+ 0.8
P 13 Soil Layer Mixing
+ 0.25
P 24 Flatten Standing Biomass
+ 0 0.85 0.7 0.6 0.5 1.0
P 25 Bury Flat Biomass
+ 1 .73 0.63 .55 .4 .73
P 26 Resurface Buried Biomass
+ 0.02 0.04 0.02 0.05 0.02
P 34 Change Standing Biomass Fall Rate
+ 7 3.0 2.5 2.0 1.5 1.0
+ 0.5 0.6 0.7 0.8 1.0
G 03 Crop Name
+ Grass, warm season, forage
P 51 Seeding Configuration
+ 1 0.0 2
+ 400.0 1.0 0 3000 1 1.0 2
+ lbs/ac
+ 0 8930.0 6 1.0 0.69 0.9
+ 1.0 0.01 2.0 3.0 30.0 1 120 1800.0
+ -5.0 -9.444445 0.01 0.95 0.0 45
+ 0.023 0.8063 0.4146 -0.061 -0.024 0.9911 0.6435 0.0494
+ 0.3 -0.075 3.9 1.0 30 0.05 0 0.3
+ 2.0 110.0 0.6 0.013 0.2 0.2 0.1 2
+ 0.0536 0.0536 0.0536 0.0536 0.2 0.0020 20.0 5.227942
+ -1.20379 0.604887 0.0 0.0 0.0 0.0 0.0 0.0
T This record was cloned from the Dryland Alfalfa record that Fred Fox and I worked on mid 2008.  It was the only record we could
T find that would grow biomass and regrow correctly after cutting.  All of the ARS grass records were tested and none would grow correctly.
T
T This record will grow biomass in most cases.  The amount can be adjusted using the biomass adjustment factor in the mgt editor.
T This is considered a tempoary record to use until the WERU and NRCS staff has time to refine the data.
T Do not use the growth values for grazing management.
T MAS 8-7-08
T
T See Alfalfa, hay notes.  This record was cloned from the Alfalfa file, and some of the factors changed to represent dryland alfalfa
T Yield is from and OR state crop guide and the growth trials were from MT.  Yield is set at 1.5 t/ac.
T Calibration of yield must be done manually by adding up the cuttings each year and averaging the years.
T If too high or too low use the biomass adjument factor to reduce or increase the forage produced.
T Grass is not considered in this file.  MAS 8-7-08
T
T Changed the cover to mass value to match Fosters finest stem curve, Small Grain and Alfalfa.  Reference pg. 179 Ag Handbook 703.
T No crop has a larger number (finer stems) than .000586.  This matches RUSLE2.  MAS 12-21-10
#------------
D 10/06/01
O 03 Shredder, flail or rotary
+ 6.828365 .15 2.2351363 0.0 2.2351363 1.7881091 2.6821637
T Rusle Note: Rotary mower or flail shredder used to defoliate root crops such as sugarbeets before harvest or on cotton or
T other crop residue where crop has been previously harvested and
T residue is shredded  and spread flat..   10/3/01 DTL 11/15/01
T
T P42 is used to set a height of cut and removed the flattening P24.
T The 0.90 fraction used in RUSLE is by mass.  WEPS fraction is by height.
T It is not the same as RUSLE and cannot be used.
T Set the height to 2 inches per the conversation the Dave Lightle.  He said that most
T corn shredders are set to 2 inches.  Cotton shredding is much higher, use the 6 in shredder.
T A new operation was also created for root crop defoliation where all of the green tops
T are flatten to residue without killing the crop, "Shredder, beet topper".
T Kill crop was removed because of the interference with most harvest operations
T if used before harvest.  MAS 1-5-11
+
G 02 Biomass Manipulation
+ 1.0
P 42 Cut/Remove Biomass to Height (flags)
+ 0 0 1 0 0 50.800102 0 0 0.0
P 40 End crop Biomass Manipulation
#------------
D 20/06/01
O 03 Shredder, flail or rotary
+ 6.828365 .15 2.2351363 0.0 2.2351363 1.7881091 2.6821637
T Rusle Note: Rotary mower or flail shredder used to defoliate root crops such as sugarbeets before harvest or on cotton or
T other crop residue where crop has been previously harvested and
T residue is shredded  and spread flat..   10/3/01 DTL 11/15/01
T
T P42 is used to set a height of cut and removed the flattening P24.
T The 0.90 fraction used in RUSLE is by mass.  WEPS fraction is by height.
T It is not the same as RUSLE and cannot be used.
T Set the height to 2 inches per the conversation the Dave Lightle.  He said that most
T corn shredders are set to 2 inches.  Cotton shredding is much higher, use the 6 in shredder.
T A new operation was also created for root crop defoliation where all of the green tops
T are flatten to residue without killing the crop, "Shredder, beet topper".
T Kill crop was removed because of the interference with most harvest operations
T if used before harvest.  MAS 1-5-11
+
G 02 Biomass Manipulation
+ 1.0
P 42 Cut/Remove Biomass to Height (flags)
+ 0 0 1 0 0 50.800102 0 0 0.0
P 40 End crop Biomass Manipulation
#------------
D 20/06/01
O 04 Fert applic. surface broadcast
+ 1.4966278 0.0609375
T R2 Notes: Broadcast fertilizer spreader.  Wheel traffic only.  rev 082107 DTL
T
T Added to DB 4-12-12 MAS
+
G 01 Tillage
+ 0.0 0 0.05 0.0 0.0 0.0
P 01 Break Crust
P 02 Random Roughness
+ 1 8.8900175
P 11 Aggregate Crushing
+ 4.3 2.0
P 24 Flatten Standing Biomass
+ 0 0.25 0.2 0.15 0.1 1.0
P 26 Resurface Buried Biomass
+ 0.07 0.08 0.1 0.12 0.07
P 34 Change Standing Biomass Fall Rate
+ 0 1.0 1.0 1.0 1.0 1.0
+ 1.0 1.0 1.0 1.0 1.0
#------------
D 07/07/01
O 03 Shredder, flail or rotary
+ 6.828365 .15 2.2351363 0.0 2.2351363 1.7881091 2.6821637
T Rusle Note: Rotary mower or flail shredder used to defoliate root crops such as sugarbeets before harvest or on cotton or
T other crop residue where crop has been previously harvested and
T residue is shredded  and spread flat..   10/3/01 DTL 11/15/01
T
T P42 is used to set a height of cut and removed the flattening P24.
T The 0.90 fraction used in RUSLE is by mass.  WEPS fraction is by height.
T It is not the same as RUSLE and cannot be used.
T Set the height to 2 inches per the conversation the Dave Lightle.  He said that most
T corn shredders are set to 2 inches.  Cotton shredding is much higher, use the 6 in shredder.
T A new operation was also created for root crop defoliation where all of the green tops
T are flatten to residue without killing the crop, "Shredder, beet topper".
T Kill crop was removed because of the interference with most harvest operations
T if used before harvest.  MAS 1-5-11
+
G 02 Biomass Manipulation
+ 1.0
P 42 Cut/Remove Biomass to Height (flags)
+ 0 0 1 0 0 50.800102 0 0 0.0
P 40 End crop Biomass Manipulation
#------------
D 14/07/01
O 03 Shredder, flail or rotary
+ 6.828365 .15 2.2351363 0.0 2.2351363 1.7881091 2.6821637
T Rusle Note: Rotary mower or flail shredder used to defoliate root crops such as sugarbeets before harvest or on cotton or
T other crop residue where crop has been previously harvested and
T residue is shredded  and spread flat..   10/3/01 DTL 11/15/01
T
T P42 is used to set a height of cut and removed the flattening P24.
T The 0.90 fraction used in RUSLE is by mass.  WEPS fraction is by height.
T It is not the same as RUSLE and cannot be used.
T Set the height to 2 inches per the conversation the Dave Lightle.  He said that most
T corn shredders are set to 2 inches.  Cotton shredding is much higher, use the 6 in shredder.
T A new operation was also created for root crop defoliation where all of the green tops
T are flatten to residue without killing the crop, "Shredder, beet topper".
T Kill crop was removed because of the interference with most harvest operations
T if used before harvest.  MAS 1-5-11
+
G 02 Biomass Manipulation
+ 1.0
P 42 Cut/Remove Biomass to Height (flags)
+ 0 0 1 0 0 50.800102 0 0 0.0
P 40 End crop Biomass Manipulation
#------------
D 21/07/01
O 03 Shredder, flail or rotary
+ 6.828365 .15 2.2351363 0.0 2.2351363 1.7881091 2.6821637
T Rusle Note: Rotary mower or flail shredder used to defoliate root crops such as sugarbeets before harvest or on cotton or
T other crop residue where crop has been previously harvested and
T residue is shredded  and spread flat..   10/3/01 DTL 11/15/01
T
T P42 is used to set a height of cut and removed the flattening P24.
T The 0.90 fraction used in RUSLE is by mass.  WEPS fraction is by height.
T It is not the same as RUSLE and cannot be used.
T Set the height to 2 inches per the conversation the Dave Lightle.  He said that most
T corn shredders are set to 2 inches.  Cotton shredding is much higher, use the 6 in shredder.
T A new operation was also created for root crop defoliation where all of the green tops
T are flatten to residue without killing the crop, "Shredder, beet topper".
T Kill crop was removed because of the interference with most harvest operations
T if used before harvest.  MAS 1-5-11
+
G 02 Biomass Manipulation
+ 1.0
P 42 Cut/Remove Biomass to Height (flags)
+ 0 0 1 0 0 50.800102 0 0 0.0
P 40 End crop Biomass Manipulation
#------------
D 21/07/01
O 04 Fert applic. surface broadcast
+ 1.4966278 0.0609375
T R2 Notes: Broadcast fertilizer spreader.  Wheel traffic only.  rev 082107 DTL
T
T Added to DB 4-12-12 MAS
+
G 01 Tillage
+ 0.0 0 0.05 0.0 0.0 0.0
P 01 Break Crust
P 02 Random Roughness
+ 1 8.8900175
P 11 Aggregate Crushing
+ 4.3 2.0
P 24 Flatten Standing Biomass
+ 0 0.25 0.2 0.15 0.1 1.0
P 26 Resurface Buried Biomass
+ 0.07 0.08 0.1 0.12 0.07
P 34 Change Standing Biomass Fall Rate
+ 0 1.0 1.0 1.0 1.0 1.0
+ 1.0 1.0 1.0 1.0 1.0
#------------
D 28/07/01
O 03 Shredder, flail or rotary
+ 6.828365 .15 2.2351363 0.0 2.2351363 1.7881091 2.6821637
T Rusle Note: Rotary mower or flail shredder used to defoliate root crops such as sugarbeets before harvest or on cotton or
T other crop residue where crop has been previously harvested and
T residue is shredded  and spread flat..   10/3/01 DTL 11/15/01
T
T P42 is used to set a height of cut and removed the flattening P24.
T The 0.90 fraction used in RUSLE is by mass.  WEPS fraction is by height.
T It is not the same as RUSLE and cannot be used.
T Set the height to 2 inches per the conversation the Dave Lightle.  He said that most
T corn shredders are set to 2 inches.  Cotton shredding is much higher, use the 6 in shredder.
T A new operation was also created for root crop defoliation where all of the green tops
T are flatten to residue without killing the crop, "Shredder, beet topper".
T Kill crop was removed because of the interference with most harvest operations
T if used before harvest.  MAS 1-5-11
+
G 02 Biomass Manipulation
+ 1.0
P 42 Cut/Remove Biomass to Height (flags)
+ 0 0 1 0 0 50.800102 0 0 0.0
P 40 End crop Biomass Manipulation
#------------
D 04/08/01
O 03 Shredder, flail or rotary
+ 6.828365 .15 2.2351363 0.0 2.2351363 1.7881091 2.6821637
T Rusle Note: Rotary mower or flail shredder used to defoliate root crops such as sugarbeets before harvest or on cotton or
T other crop residue where crop has been previously harvested and
T residue is shredded  and spread flat..   10/3/01 DTL 11/15/01
T
T P42 is used to set a height of cut and removed the flattening P24.
T The 0.90 fraction used in RUSLE is by mass.  WEPS fraction is by height.
T It is not the same as RUSLE and cannot be used.
T Set the height to 2 inches per the conversation the Dave Lightle.  He said that most
T corn shredders are set to 2 inches.  Cotton shredding is much higher, use the 6 in shredder.
T A new operation was also created for root crop defoliation where all of the green tops
T are flatten to residue without killing the crop, "Shredder, beet topper".
T Kill crop was removed because of the interference with most harvest operations
T if used before harvest.  MAS 1-5-11
+
G 02 Biomass Manipulation
+ 1.0
P 42 Cut/Remove Biomass to Height (flags)
+ 0 0 1 0 0 50.800102 0 0 0.0
P 40 End crop Biomass Manipulation
#------------
D 11/08/01
O 03 Shredder, flail or rotary
+ 6.828365 .15 2.2351363 0.0 2.2351363 1.7881091 2.6821637
T Rusle Note: Rotary mower or flail shredder used to defoliate root crops such as sugarbeets before harvest or on cotton or
T other crop residue where crop has been previously harvested and
T residue is shredded  and spread flat..   10/3/01 DTL 11/15/01
T
T P42 is used to set a height of cut and removed the flattening P24.
T The 0.90 fraction used in RUSLE is by mass.  WEPS fraction is by height.
T It is not the same as RUSLE and cannot be used.
T Set the height to 2 inches per the conversation the Dave Lightle.  He said that most
T corn shredders are set to 2 inches.  Cotton shredding is much higher, use the 6 in shredder.
T A new operation was also created for root crop defoliation where all of the green tops
T are flatten to residue without killing the crop, "Shredder, beet topper".
T Kill crop was removed because of the interference with most harvest operations
T if used before harvest.  MAS 1-5-11
+
G 02 Biomass Manipulation
+ 1.0
P 42 Cut/Remove Biomass to Height (flags)
+ 0 0 1 0 0 50.800102 0 0 0.0
P 40 End crop Biomass Manipulation
#------------
D 18/08/01
O 03 Shredder, flail or rotary
+ 6.828365 .15 2.2351363 0.0 2.2351363 1.7881091 2.6821637
T Rusle Note: Rotary mower or flail shredder used to defoliate root crops such as sugarbeets before harvest or on cotton or
T other crop residue where crop has been previously harvested and
T residue is shredded  and spread flat..   10/3/01 DTL 11/15/01
T
T P42 is used to set a height of cut and removed the flattening P24.
T The 0.90 fraction used in RUSLE is by mass.  WEPS fraction is by height.
T It is not the same as RUSLE and cannot be used.
T Set the height to 2 inches per the conversation the Dave Lightle.  He said that most
T corn shredders are set to 2 inches.  Cotton shredding is much higher, use the 6 in shredder.
T A new operation was also created for root crop defoliation where all of the green tops
T are flatten to residue without killing the crop, "Shredder, beet topper".
T Kill crop was removed because of the interference with most harvest operations
T if used before harvest.  MAS 1-5-11
+
G 02 Biomass Manipulation
+ 1.0
P 42 Cut/Remove Biomass to Height (flags)
+ 0 0 1 0 0 50.800102 0 0 0.0
P 40 End crop Biomass Manipulation
#------------
D 18/08/01
O 04 Fert applic. surface broadcast
+ 1.4966278 0.0609375
T R2 Notes: Broadcast fertilizer spreader.  Wheel traffic only.  rev 082107 DTL
T
T Added to DB 4-12-12 MAS
+
G 01 Tillage
+ 0.0 0 0.05 0.0 0.0 0.0
P 01 Break Crust
P 02 Random Roughness
+ 1 8.8900175
P 11 Aggregate Crushing
+ 4.3 2.0
P 24 Flatten Standing Biomass
+ 0 0.25 0.2 0.15 0.1 1.0
P 26 Resurface Buried Biomass
+ 0.07 0.08 0.1 0.12 0.07
P 34 Change Standing Biomass Fall Rate
+ 0 1.0 1.0 1.0 1.0 1.0
+ 1.0 1.0 1.0 1.0 1.0
#------------
D 25/08/01
O 03 Shredder, flail or rotary
+ 6.828365 .15 2.2351363 0.0 2.2351363 1.7881091 2.6821637
T Rusle Note: Rotary mower or flail shredder used to defoliate root crops such as sugarbeets before harvest or on cotton or
T other crop residue where crop has been previously harvested and
T residue is shredded  and spread flat..   10/3/01 DTL 11/15/01
T
T P42 is used to set a height of cut and removed the flattening P24.
T The 0.90 fraction used in RUSLE is by mass.  WEPS fraction is by height.
T It is not the same as RUSLE and cannot be used.
T Set the height to 2 inches per the conversation the Dave Lightle.  He said that most
T corn shredders are set to 2 inches.  Cotton shredding is much higher, use the 6 in shredder.
T A new operation was also created for root crop defoliation where all of the green tops
T are flatten to residue without killing the crop, "Shredder, beet topper".
T Kill crop was removed because of the interference with most harvest operations
T if used before harvest.  MAS 1-5-11
+
G 02 Biomass Manipulation
+ 1.0
P 42 Cut/Remove Biomass to Height (flags)
+ 0 0 1 0 0 50.800102 0 0 0.0
P 40 End crop Biomass Manipulation
#------------
D 10/09/01
O 03 Shredder, flail or rotary
+ 6.828365 .15 2.2351363 0.0 2.2351363 1.7881091 2.6821637
T Rusle Note: Rotary mower or flail shredder used to defoliate root crops such as sugarbeets before harvest or on cotton or
T other crop residue where crop has been previously harvested and
T residue is shredded  and spread flat..   10/3/01 DTL 11/15/01
T
T P42 is used to set a height of cut and removed the flattening P24.
T The 0.90 fraction used in RUSLE is by mass.  WEPS fraction is by height.
T It is not the same as RUSLE and cannot be used.
T Set the height to 2 inches per the conversation the Dave Lightle.  He said that most
T corn shredders are set to 2 inches.  Cotton shredding is much higher, use the 6 in shredder.
T A new operation was also created for root crop defoliation where all of the green tops
T are flatten to residue without killing the crop, "Shredder, beet topper".
T Kill crop was removed because of the interference with most harvest operations
T if used before harvest.  MAS 1-5-11
+
G 02 Biomass Manipulation
+ 1.0
P 42 Cut/Remove Biomass to Height (flags)
+ 0 0 1 0 0 50.800102 0 0 0.0
P 40 End crop Biomass Manipulation
#------------
D 15/09/01
O 04 Fert applic. surface broadcast
+ 1.4966278 0.0609375
T R2 Notes: Broadcast fertilizer spreader.  Wheel traffic only.  rev 082107 DTL
T
T Added to DB 4-12-12 MAS
+
G 01 Tillage
+ 0.0 0 0.05 0.0 0.0 0.0
P 01 Break Crust
P 02 Random Roughness
+ 1 8.8900175
P 11 Aggregate Crushing
+ 4.3 2.0
P 24 Flatten Standing Biomass
+ 0 0.25 0.2 0.15 0.1 1.0
P 26 Resurface Buried Biomass
+ 0.07 0.08 0.1 0.12 0.07
P 34 Change Standing Biomass Fall Rate
+ 0 1.0 1.0 1.0 1.0 1.0
+ 1.0 1.0 1.0 1.0 1.0
#------------
D 27/09/01
O 03 Shredder, flail or rotary
+ 6.828365 .15 2.2351363 0.0 2.2351363 1.7881091 2.6821637
T Rusle Note: Rotary mower or flail shredder used to defoliate root crops such as sugarbeets before harvest or on cotton or
T other crop residue where crop has been previously harvested and
T residue is shredded  and spread flat..   10/3/01 DTL 11/15/01
T
T P42 is used to set a height of cut and removed the flattening P24.
T The 0.90 fraction used in RUSLE is by mass.  WEPS fraction is by height.
T It is not the same as RUSLE and cannot be used.
T Set the height to 2 inches per the conversation the Dave Lightle.  He said that most
T corn shredders are set to 2 inches.  Cotton shredding is much higher, use the 6 in shredder.
T A new operation was also created for root crop defoliation where all of the green tops
T are flatten to residue without killing the crop, "Shredder, beet topper".
T Kill crop was removed because of the interference with most harvest operations
T if used before harvest.  MAS 1-5-11
+
G 02 Biomass Manipulation
+ 1.0
P 42 Cut/Remove Biomass to Height (flags)
+ 0 0 1 0 0 50.800102 0 0 0.0
P 40 End crop Biomass Manipulation
#------------
D 07/10/01
O 03 Shredder, flail or rotary
+ 6.828365 .15 2.2351363 0.0 2.2351363 1.7881091 2.6821637
T Rusle Note: Rotary mower or flail shredder used to defoliate root crops such as sugarbeets before harvest or on cotton or
T other crop residue where crop has been previously harvested and
T residue is shredded  and spread flat..   10/3/01 DTL 11/15/01
T
T P42 is used to set a height of cut and removed the flattening P24.
T The 0.90 fraction used in RUSLE is by mass.  WEPS fraction is by height.
T It is not the same as RUSLE and cannot be used.
T Set the height to 2 inches per the conversation the Dave Lightle.  He said that most
T corn shredders are set to 2 inches.  Cotton shredding is much higher, use the 6 in shredder.
T A new operation was also created for root crop defoliation where all of the green tops
T are flatten to residue without killing the crop, "Shredder, beet topper".
T Kill crop was removed because of the interference with most harvest operations
T if used before harvest.  MAS 1-5-11
+
G 02 Biomass Manipulation
+ 1.0
P 42 Cut/Remove Biomass to Height (flags)
+ 0 0 1 0 0 50.800102 0 0 0.0
P 40 End crop Biomass Manipulation
#------------
D 01/04/02
O 04 Fert applic. surface broadcast
+ 1.4966278 0.0609375
T R2 Notes: Broadcast fertilizer spreader.  Wheel traffic only.  rev 082107 DTL
T
T Added to DB 4-12-12 MAS
+
G 01 Tillage
+ 0.0 0 0.05 0.0 0.0 0.0
P 01 Break Crust
P 02 Random Roughness
+ 1 8.8900175
P 11 Aggregate Crushing
+ 4.3 2.0
P 24 Flatten Standing Biomass
+ 0 0.25 0.2 0.15 0.1 1.0
P 26 Resurface Buried Biomass
+ 0.07 0.08 0.1 0.12 0.07
P 34 Change Standing Biomass Fall Rate
+ 0 1.0 1.0 1.0 1.0 1.0
+ 1.0 1.0 1.0 1.0 1.0
#------------
D 12/04/02
O 03 Shredder, flail or rotary
+ 6.828365 .15 2.2351363 0.0 2.2351363 1.7881091 2.6821637
T Rusle Note: Rotary mower or flail shredder used to defoliate root crops such as sugarbeets before harvest or on cotton or
T other crop residue where crop has been previously harvested and
T residue is shredded  and spread flat..   10/3/01 DTL 11/15/01
T
T P42 is used to set a height of cut and removed the flattening P24.
T The 0.90 fraction used in RUSLE is by mass.  WEPS fraction is by height.
T It is not the same as RUSLE and cannot be used.
T Set the height to 2 inches per the conversation the Dave Lightle.  He said that most
T corn shredders are set to 2 inches.  Cotton shredding is much higher, use the 6 in shredder.
T A new operation was also created for root crop defoliation where all of the green tops
T are flatten to residue without killing the crop, "Shredder, beet topper".
T Kill crop was removed because of the interference with most harvest operations
T if used before harvest.  MAS 1-5-11
+
G 02 Biomass Manipulation
+ 1.0
P 42 Cut/Remove Biomass to Height (flags)
+ 0 0 1 0 0 50.800102 0 0 0.0
P 40 End crop Biomass Manipulation
#------------
D 22/04/02
O 03 Shredder, flail or rotary
+ 6.828365 .15 2.2351363 0.0 2.2351363 1.7881091 2.6821637
T Rusle Note: Rotary mower or flail shredder used to defoliate root crops such as sugarbeets before harvest or on cotton or
T other crop residue where crop has been previously harvested and
T residue is shredded  and spread flat..   10/3/01 DTL 11/15/01
T
T P42 is used to set a height of cut and removed the flattening P24.
T The 0.90 fraction used in RUSLE is by mass.  WEPS fraction is by height.
T It is not the same as RUSLE and cannot be used.
T Set the height to 2 inches per the conversation the Dave Lightle.  He said that most
T corn shredders are set to 2 inches.  Cotton shredding is much higher, use the 6 in shredder.
T A new operation was also created for root crop defoliation where all of the green tops
T are flatten to residue without killing the crop, "Shredder, beet topper".
T Kill crop was removed because of the interference with most harvest operations
T if used before harvest.  MAS 1-5-11
+
G 02 Biomass Manipulation
+ 1.0
P 42 Cut/Remove Biomass to Height (flags)
+ 0 0 1 0 0 50.800102 0 0 0.0
P 40 End crop Biomass Manipulation
#------------
D 02/05/02
O 03 Shredder, flail or rotary
+ 6.828365 .15 2.2351363 0.0 2.2351363 1.7881091 2.6821637
T Rusle Note: Rotary mower or flail shredder used to defoliate root crops such as sugarbeets before harvest or on cotton or
T other crop residue where crop has been previously harvested and
T residue is shredded  and spread flat..   10/3/01 DTL 11/15/01
T
T P42 is used to set a height of cut and removed the flattening P24.
T The 0.90 fraction used in RUSLE is by mass.  WEPS fraction is by height.
T It is not the same as RUSLE and cannot be used.
T Set the height to 2 inches per the conversation the Dave Lightle.  He said that most
T corn shredders are set to 2 inches.  Cotton shredding is much higher, use the 6 in shredder.
T A new operation was also created for root crop defoliation where all of the green tops
T are flatten to residue without killing the crop, "Shredder, beet topper".
T Kill crop was removed because of the interference with most harvest operations
T if used before harvest.  MAS 1-5-11
+
G 02 Biomass Manipulation
+ 1.0
P 42 Cut/Remove Biomass to Height (flags)
+ 0 0 1 0 0 50.800102 0 0 0.0
P 40 End crop Biomass Manipulation
#------------
D 12/05/02
O 03 Shredder, flail or rotary
+ 6.828365 .15 2.2351363 0.0 2.2351363 1.7881091 2.6821637
T Rusle Note: Rotary mower or flail shredder used to defoliate root crops such as sugarbeets before harvest or on cotton or
T other crop residue where crop has been previously harvested and
T residue is shredded  and spread flat..   10/3/01 DTL 11/15/01
T
T P42 is used to set a height of cut and removed the flattening P24.
T The 0.90 fraction used in RUSLE is by mass.  WEPS fraction is by height.
T It is not the same as RUSLE and cannot be used.
T Set the height to 2 inches per the conversation the Dave Lightle.  He said that most
T corn shredders are set to 2 inches.  Cotton shredding is much higher, use the 6 in shredder.
T A new operation was also created for root crop defoliation where all of the green tops
T are flatten to residue without killing the crop, "Shredder, beet topper".
T Kill crop was removed because of the interference with most harvest operations
T if used before harvest.  MAS 1-5-11
+
G 02 Biomass Manipulation
+ 1.0
P 42 Cut/Remove Biomass to Height (flags)
+ 0 0 1 0 0 50.800102 0 0 0.0
P 40 End crop Biomass Manipulation
#------------
D 12/05/02
O 04 Fert applic. surface broadcast
+ 1.4966278 0.0609375
T R2 Notes: Broadcast fertilizer spreader.  Wheel traffic only.  rev 082107 DTL
T
T Added to DB 4-12-12 MAS
+
G 01 Tillage
+ 0.0 0 0.05 0.0 0.0 0.0
P 01 Break Crust
P 02 Random Roughness
+ 1 8.8900175
P 11 Aggregate Crushing
+ 4.3 2.0
P 24 Flatten Standing Biomass
+ 0 0.25 0.2 0.15 0.1 1.0
P 26 Resurface Buried Biomass
+ 0.07 0.08 0.1 0.12 0.07
P 34 Change Standing Biomass Fall Rate
+ 0 1.0 1.0 1.0 1.0 1.0
+ 1.0 1.0 1.0 1.0 1.0
#------------
D 22/05/02
O 03 Shredder, flail or rotary
+ 6.828365 .15 2.2351363 0.0 2.2351363 1.7881091 2.6821637
T Rusle Note: Rotary mower or flail shredder used to defoliate root crops such as sugarbeets before harvest or on cotton or
T other crop residue where crop has been previously harvested and
T residue is shredded  and spread flat..   10/3/01 DTL 11/15/01
T
T P42 is used to set a height of cut and removed the flattening P24.
T The 0.90 fraction used in RUSLE is by mass.  WEPS fraction is by height.
T It is not the same as RUSLE and cannot be used.
T Set the height to 2 inches per the conversation the Dave Lightle.  He said that most
T corn shredders are set to 2 inches.  Cotton shredding is much higher, use the 6 in shredder.
T A new operation was also created for root crop defoliation where all of the green tops
T are flatten to residue without killing the crop, "Shredder, beet topper".
T Kill crop was removed because of the interference with most harvest operations
T if used before harvest.  MAS 1-5-11
+
G 02 Biomass Manipulation
+ 1.0
P 42 Cut/Remove Biomass to Height (flags)
+ 0 0 1 0 0 50.800102 0 0 0.0
P 40 End crop Biomass Manipulation
#------------
D 02/06/02
O 03 Shredder, flail or rotary
+ 6.828365 .15 2.2351363 0.0 2.2351363 1.7881091 2.6821637
T Rusle Note: Rotary mower or flail shredder used to defoliate root crops such as sugarbeets before harvest or on cotton or
T other crop residue where crop has been previously harvested and
T residue is shredded  and spread flat..   10/3/01 DTL 11/15/01
T
T P42 is used to set a height of cut and removed the flattening P24.
T The 0.90 fraction used in RUSLE is by mass.  WEPS fraction is by height.
T It is not the same as RUSLE and cannot be used.
T Set the height to 2 inches per the conversation the Dave Lightle.  He said that most
T corn shredders are set to 2 inches.  Cotton shredding is much higher, use the 6 in shredder.
T A new operation was also created for root crop defoliation where all of the green tops
T are flatten to residue without killing the crop, "Shredder, beet topper".
T Kill crop was removed because of the interference with most harvest operations
T if used before harvest.  MAS 1-5-11
+
G 02 Biomass Manipulation
+ 1.0
P 42 Cut/Remove Biomass to Height (flags)
+ 0 0 1 0 0 50.800102 0 0 0.0
P 40 End crop Biomass Manipulation
#------------
D 10/06/02
O 03 Sod cutter
+ 8.418531 .24 0.44702727 0.0 0.44702727 0.22351363 2.2351363
T Cut and remove grass sod,  P31 set:  annual crops killed, perennial crops regrow jkp 130910
+
G 01 Tillage
+ 25.400051 1.0 1.0 25.400051 12.700026 38.100075
P 01 Break Crust
P 02 Random Roughness
+ 1 10.160021
P 05 Ridges and Dikes
+ 1 0.0 0.0 0.0 0.0 0.0
P 11 Aggregate Crushing
+ 4.3 2.0
P 12 Soil Loosening
+ 0.65
P 13 Soil Layer Mixing
+ 0.2
G 02 Biomass Manipulation
+ 1.0
P 31 Kill or Defoliate Growing Crop
+ 1
P 62 Remove (by age pool) Plant/Residue Material
+ 1 1 0 1 7 7 0 1 1 1 1.0 .2
P 40 End crop Biomass Manipulation
P 25 Bury Flat Biomass
+ 2 0.001 0.001 0.001 0.001 0.5
P 26 Resurface Buried Biomass
+ 0.001 0.001 0.001 0.001 0.07
#------------
D 22/06/02
O 04 Fert applic. surface broadcast
+ 1.4966278 0.0609375
T R2 Notes: Broadcast fertilizer spreader.  Wheel traffic only.  rev 082107 DTL
T
T Added to DB 4-12-12 MAS
+
G 01 Tillage
+ 0.0 0 0.05 0.0 0.0 0.0
P 01 Break Crust
P 02 Random Roughness
+ 1 8.8900175
P 11 Aggregate Crushing
+ 4.3 2.0
P 24 Flatten Standing Biomass
+ 0 0.25 0.2 0.15 0.1 1.0
P 26 Resurface Buried Biomass
+ 0.07 0.08 0.1 0.12 0.07
P 34 Change Standing Biomass Fall Rate
+ 0 1.0 1.0 1.0 1.0 1.0
+ 1.0 1.0 1.0 1.0 1.0
#------------
D 30/06/02
O 03 Planter, sprig conventional
+ 3.7415698 13 2.2351363 0.0 2.2351363 1.3410819 2.6821637
T Planter used to plant sprigs.  Similar to a light finishing disk 11-14-02 DTL
+ 
G 01 Tillage
+ 50.800102 0.4 1.0 50.800102 25.400051 76.20015
P 01 Break Crust
P 02 Random Roughness
+ 1 15.240031
P 05 Ridges and Dikes
+ 1 25.400051 609.6012 508.001 0.0 0.0
P 11 Aggregate Crushing
+ 2.4 2.0
P 12 Soil Loosening
+ 0.8
P 13 Soil Layer Mixing
+ 0.25
P 24 Flatten Standing Biomass
+ 0 0.85 0.7 0.6 0.5 1.0
P 25 Bury Flat Biomass
+ 1 .73 0.63 .55 .4 .73
P 26 Resurface Buried Biomass
+ 0.02 0.04 0.02 0.05 0.02
P 34 Change Standing Biomass Fall Rate
+ 7 3.0 2.5 2.0 1.5 1.0
+ 0.5 0.6 0.7 0.8 1.0
G 03 Crop Name
+ Grass, warm season, forage
P 51 Seeding Configuration
+ 1 0.0 2
+ 400.0 1.0 0 3000 1 1.0 2
+ lbs/ac
+ 0 8930.0 6 1.0 0.69 0.9
+ 1.0 0.01 2.0 3.0 30.0 1 120 1800.0
+ -5.0 -9.444445 0.01 0.95 0.0 45
+ 0.023 0.8063 0.4146 -0.061 -0.024 0.9911 0.6435 0.0494
+ 0.3 -0.075 3.9 1.0 30 0.05 0 0.3
+ 2.0 110.0 0.6 0.013 0.2 0.2 0.1 2
+ 0.0536 0.0536 0.0536 0.0536 0.2 0.0020 20.0 5.227942
+ -1.20379 0.604887 0.0 0.0 0.0 0.0 0.0 0.0
T This record was cloned from the Dryland Alfalfa record that Fred Fox and I worked on mid 2008.  It was the only record we could
T find that would grow biomass and regrow correctly after cutting.  All of the ARS grass records were tested and none would grow correctly.
T
T This record will grow biomass in most cases.  The amount can be adjusted using the biomass adjustment factor in the mgt editor.
T This is considered a tempoary record to use until the WERU and NRCS staff has time to refine the data.
T Do not use the growth values for grazing management.
T MAS 8-7-08
T
T See Alfalfa, hay notes.  This record was cloned from the Alfalfa file, and some of the factors changed to represent dryland alfalfa
T Yield is from and OR state crop guide and the growth trials were from MT.  Yield is set at 1.5 t/ac.
T Calibration of yield must be done manually by adding up the cuttings each year and averaging the years.
T If too high or too low use the biomass adjument factor to reduce or increase the forage produced.
T Grass is not considered in this file.  MAS 8-7-08
T
T Changed the cover to mass value to match Fosters finest stem curve, Small Grain and Alfalfa.  Reference pg. 179 Ag Handbook 703.
T No crop has a larger number (finer stems) than .000586.  This matches RUSLE2.  MAS 12-21-10
#------------
D 04/07/02
O 03 Shredder, flail or rotary
+ 6.828365 .15 2.2351363 0.0 2.2351363 1.7881091 2.6821637
T Rusle Note: Rotary mower or flail shredder used to defoliate root crops such as sugarbeets before harvest or on cotton or
T other crop residue where crop has been previously harvested and
T residue is shredded  and spread flat..   10/3/01 DTL 11/15/01
T
T P42 is used to set a height of cut and removed the flattening P24.
T The 0.90 fraction used in RUSLE is by mass.  WEPS fraction is by height.
T It is not the same as RUSLE and cannot be used.
T Set the height to 2 inches per the conversation the Dave Lightle.  He said that most
T corn shredders are set to 2 inches.  Cotton shredding is much higher, use the 6 in shredder.
T A new operation was also created for root crop defoliation where all of the green tops
T are flatten to residue without killing the crop, "Shredder, beet topper".
T Kill crop was removed because of the interference with most harvest operations
T if used before harvest.  MAS 1-5-11
+
G 02 Biomass Manipulation
+ 1.0
P 42 Cut/Remove Biomass to Height (flags)
+ 0 0 1 0 0 50.800102 0 0 0.0
P 40 End crop Biomass Manipulation
#------------
D 14/07/02
O 03 Shredder, flail or rotary
+ 6.828365 .15 2.2351363 0.0 2.2351363 1.7881091 2.6821637
T Rusle Note: Rotary mower or flail shredder used to defoliate root crops such as sugarbeets before harvest or on cotton or
T other crop residue where crop has been previously harvested and
T residue is shredded  and spread flat..   10/3/01 DTL 11/15/01
T
T P42 is used to set a height of cut and removed the flattening P24.
T The 0.90 fraction used in RUSLE is by mass.  WEPS fraction is by height.
T It is not the same as RUSLE and cannot be used.
T Set the height to 2 inches per the conversation the Dave Lightle.  He said that most
T corn shredders are set to 2 inches.  Cotton shredding is much higher, use the 6 in shredder.
T A new operation was also created for root crop defoliation where all of the green tops
T are flatten to residue without killing the crop, "Shredder, beet topper".
T Kill crop was removed because of the interference with most harvest operations
T if used before harvest.  MAS 1-5-11
+
G 02 Biomass Manipulation
+ 1.0
P 42 Cut/Remove Biomass to Height (flags)
+ 0 0 1 0 0 50.800102 0 0 0.0
P 40 End crop Biomass Manipulation
#------------
D 14/07/02
O 04 Fert applic. surface broadcast
+ 1.4966278 0.0609375
T R2 Notes: Broadcast fertilizer spreader.  Wheel traffic only.  rev 082107 DTL
T
T Added to DB 4-12-12 MAS
+
G 01 Tillage
+ 0.0 0 0.05 0.0 0.0 0.0
P 01 Break Crust
P 02 Random Roughness
+ 1 8.8900175
P 11 Aggregate Crushing
+ 4.3 2.0
P 24 Flatten Standing Biomass
+ 0 0.25 0.2 0.15 0.1 1.0
P 26 Resurface Buried Biomass
+ 0.07 0.08 0.1 0.12 0.07
P 34 Change Standing Biomass Fall Rate
+ 0 1.0 1.0 1.0 1.0 1.0
+ 1.0 1.0 1.0 1.0 1.0
#------------
D 24/07/02
O 03 Shredder, flail or rotary
+ 6.828365 .15 2.2351363 0.0 2.2351363 1.7881091 2.6821637
T Rusle Note: Rotary mower or flail shredder used to defoliate root crops such as sugarbeets before harvest or on cotton or
T other crop residue where crop has been previously harvested and
T residue is shredded  and spread flat..   10/3/01 DTL 11/15/01
T
T P42 is used to set a height of cut and removed the flattening P24.
T The 0.90 fraction used in RUSLE is by mass.  WEPS fraction is by height.
T It is not the same as RUSLE and cannot be used.
T Set the height to 2 inches per the conversation the Dave Lightle.  He said that most
T corn shredders are set to 2 inches.  Cotton shredding is much higher, use the 6 in shredder.
T A new operation was also created for root crop defoliation where all of the green tops
T are flatten to residue without killing the crop, "Shredder, beet topper".
T Kill crop was removed because of the interference with most harvest operations
T if used before harvest.  MAS 1-5-11
+
G 02 Biomass Manipulation
+ 1.0
P 42 Cut/Remove Biomass to Height (flags)
+ 0 0 1 0 0 50.800102 0 0 0.0
P 40 End crop Biomass Manipulation
#------------
D 04/08/02
O 03 Shredder, flail or rotary
+ 6.828365 .15 2.2351363 0.0 2.2351363 1.7881091 2.6821637
T Rusle Note: Rotary mower or flail shredder used to defoliate root crops such as sugarbeets before harvest or on cotton or
T other crop residue where crop has been previously harvested and
T residue is shredded  and spread flat..   10/3/01 DTL 11/15/01
T
T P42 is used to set a height of cut and removed the flattening P24.
T The 0.90 fraction used in RUSLE is by mass.  WEPS fraction is by height.
T It is not the same as RUSLE and cannot be used.
T Set the height to 2 inches per the conversation the Dave Lightle.  He said that most
T corn shredders are set to 2 inches.  Cotton shredding is much higher, use the 6 in shredder.
T A new operation was also created for root crop defoliation where all of the green tops
T are flatten to residue without killing the crop, "Shredder, beet topper".
T Kill crop was removed because of the interference with most harvest operations
T if used before harvest.  MAS 1-5-11
+
G 02 Biomass Manipulation
+ 1.0
P 42 Cut/Remove Biomass to Height (flags)
+ 0 0 1 0 0 50.800102 0 0 0.0
P 40 End crop Biomass Manipulation
#------------
D 11/08/02
O 03 Shredder, flail or rotary
+ 6.828365 .15 2.2351363 0.0 2.2351363 1.7881091 2.6821637
T Rusle Note: Rotary mower or flail shredder used to defoliate root crops such as sugarbeets before harvest or on cotton or
T other crop residue where crop has been previously harvested and
T residue is shredded  and spread flat..   10/3/01 DTL 11/15/01
T
T P42 is used to set a height of cut and removed the flattening P24.
T The 0.90 fraction used in RUSLE is by mass.  WEPS fraction is by height.
T It is not the same as RUSLE and cannot be used.
T Set the height to 2 inches per the conversation the Dave Lightle.  He said that most
T corn shredders are set to 2 inches.  Cotton shredding is much higher, use the 6 in shredder.
T A new operation was also created for root crop defoliation where all of the green tops
T are flatten to residue without killing the crop, "Shredder, beet topper".
T Kill crop was removed because of the interference with most harvest operations
T if used before harvest.  MAS 1-5-11
+
G 02 Biomass Manipulation
+ 1.0
P 42 Cut/Remove Biomass to Height (flags)
+ 0 0 1 0 0 50.800102 0 0 0.0
P 40 End crop Biomass Manipulation
#------------
D 18/08/02
O 03 Shredder, flail or rotary
+ 6.828365 .15 2.2351363 0.0 2.2351363 1.7881091 2.6821637
T Rusle Note: Rotary mower or flail shredder used to defoliate root crops such as sugarbeets before harvest or on cotton or
T other crop residue where crop has been previously harvested and
T residue is shredded  and spread flat..   10/3/01 DTL 11/15/01
T
T P42 is used to set a height of cut and removed the flattening P24.
T The 0.90 fraction used in RUSLE is by mass.  WEPS fraction is by height.
T It is not the same as RUSLE and cannot be used.
T Set the height to 2 inches per the conversation the Dave Lightle.  He said that most
T corn shredders are set to 2 inches.  Cotton shredding is much higher, use the 6 in shredder.
T A new operation was also created for root crop defoliation where all of the green tops
T are flatten to residue without killing the crop, "Shredder, beet topper".
T Kill crop was removed because of the interference with most harvest operations
T if used before harvest.  MAS 1-5-11
+
G 02 Biomass Manipulation
+ 1.0
P 42 Cut/Remove Biomass to Height (flags)
+ 0 0 1 0 0 50.800102 0 0 0.0
P 40 End crop Biomass Manipulation
#------------
D 18/08/02
O 04 Fert applic. surface broadcast
+ 1.4966278 0.0609375
T R2 Notes: Broadcast fertilizer spreader.  Wheel traffic only.  rev 082107 DTL
T
T Added to DB 4-12-12 MAS
+
G 01 Tillage
+ 0.0 0 0.05 0.0 0.0 0.0
P 01 Break Crust
P 02 Random Roughness
+ 1 8.8900175
P 11 Aggregate Crushing
+ 4.3 2.0
P 24 Flatten Standing Biomass
+ 0 0.25 0.2 0.15 0.1 1.0
P 26 Resurface Buried Biomass
+ 0.07 0.08 0.1 0.12 0.07
P 34 Change Standing Biomass Fall Rate
+ 0 1.0 1.0 1.0 1.0 1.0
+ 1.0 1.0 1.0 1.0 1.0
#------------
D 30/08/02
O 03 Shredder, flail or rotary
+ 6.828365 .15 2.2351363 0.0 2.2351363 1.7881091 2.6821637
T Rusle Note: Rotary mower or flail shredder used to defoliate root crops such as sugarbeets before harvest or on cotton or
T other crop residue where crop has been previously harvested and
T residue is shredded  and spread flat..   10/3/01 DTL 11/15/01
T
T P42 is used to set a height of cut and removed the flattening P24.
T The 0.90 fraction used in RUSLE is by mass.  WEPS fraction is by height.
T It is not the same as RUSLE and cannot be used.
T Set the height to 2 inches per the conversation the Dave Lightle.  He said that most
T corn shredders are set to 2 inches.  Cotton shredding is much higher, use the 6 in shredder.
T A new operation was also created for root crop defoliation where all of the green tops
T are flatten to residue without killing the crop, "Shredder, beet topper".
T Kill crop was removed because of the interference with most harvest operations
T if used before harvest.  MAS 1-5-11
+
G 02 Biomass Manipulation
+ 1.0
P 42 Cut/Remove Biomass to Height (flags)
+ 0 0 1 0 0 50.800102 0 0 0.0
P 40 End crop Biomass Manipulation
#------------
D 01/09/02
O 03 Shredder, flail or rotary
+ 6.828365 .15 2.2351363 0.0 2.2351363 1.7881091 2.6821637
T Rusle Note: Rotary mower or flail shredder used to defoliate root crops such as sugarbeets before harvest or on cotton or
T other crop residue where crop has been previously harvested and
T residue is shredded  and spread flat..   10/3/01 DTL 11/15/01
T
T P42 is used to set a height of cut and removed the flattening P24.
T The 0.90 fraction used in RUSLE is by mass.  WEPS fraction is by height.
T It is not the same as RUSLE and cannot be used.
T Set the height to 2 inches per the conversation the Dave Lightle.  He said that most
T corn shredders are set to 2 inches.  Cotton shredding is much higher, use the 6 in shredder.
T A new operation was also created for root crop defoliation where all of the green tops
T are flatten to residue without killing the crop, "Shredder, beet topper".
T Kill crop was removed because of the interference with most harvest operations
T if used before harvest.  MAS 1-5-11
+
G 02 Biomass Manipulation
+ 1.0
P 42 Cut/Remove Biomass to Height (flags)
+ 0 0 1 0 0 50.800102 0 0 0.0
P 40 End crop Biomass Manipulation
#------------
D 02/09/02
O 04 Fert applic. surface broadcast
+ 1.4966278 0.0609375
T R2 Notes: Broadcast fertilizer spreader.  Wheel traffic only.  rev 082107 DTL
T
T Added to DB 4-12-12 MAS
+
G 01 Tillage
+ 0.0 0 0.05 0.0 0.0 0.0
P 01 Break Crust
P 02 Random Roughness
+ 1 8.8900175
P 11 Aggregate Crushing
+ 4.3 2.0
P 24 Flatten Standing Biomass
+ 0 0.25 0.2 0.15 0.1 1.0
P 26 Resurface Buried Biomass
+ 0.07 0.08 0.1 0.12 0.07
P 34 Change Standing Biomass Fall Rate
+ 0 1.0 1.0 1.0 1.0 1.0
+ 1.0 1.0 1.0 1.0 1.0
#------------
D 15/09/02
O 03 Shredder, flail or rotary
+ 6.828365 .15 2.2351363 0.0 2.2351363 1.7881091 2.6821637
T Rusle Note: Rotary mower or flail shredder used to defoliate root crops such as sugarbeets before harvest or on cotton or
T other crop residue where crop has been previously harvested and
T residue is shredded  and spread flat..   10/3/01 DTL 11/15/01
T
T P42 is used to set a height of cut and removed the flattening P24.
T The 0.90 fraction used in RUSLE is by mass.  WEPS fraction is by height.
T It is not the same as RUSLE and cannot be used.
T Set the height to 2 inches per the conversation the Dave Lightle.  He said that most
T corn shredders are set to 2 inches.  Cotton shredding is much higher, use the 6 in shredder.
T A new operation was also created for root crop defoliation where all of the green tops
T are flatten to residue without killing the crop, "Shredder, beet topper".
T Kill crop was removed because of the interference with most harvest operations
T if used before harvest.  MAS 1-5-11
+
G 02 Biomass Manipulation
+ 1.0
P 42 Cut/Remove Biomass to Height (flags)
+ 0 0 1 0 0 50.800102 0 0 0.0
P 40 End crop Biomass Manipulation
#------------
D 01/04/03
O 04 Fert applic. surface broadcast
+ 1.4966278 0.0609375
T R2 Notes: Broadcast fertilizer spreader.  Wheel traffic only.  rev 082107 DTL
T
T Added to DB 4-12-12 MAS
+
G 01 Tillage
+ 0.0 0 0.05 0.0 0.0 0.0
P 01 Break Crust
P 02 Random Roughness
+ 1 8.8900175
P 11 Aggregate Crushing
+ 4.3 2.0
P 24 Flatten Standing Biomass
+ 0 0.25 0.2 0.15 0.1 1.0
P 26 Resurface Buried Biomass
+ 0.07 0.08 0.1 0.12 0.07
P 34 Change Standing Biomass Fall Rate
+ 0 1.0 1.0 1.0 1.0 1.0
+ 1.0 1.0 1.0 1.0 1.0
#------------
D 12/04/03
O 03 Shredder, flail or rotary
+ 6.828365 .15 2.2351363 0.0 2.2351363 1.7881091 2.6821637
T Rusle Note: Rotary mower or flail shredder used to defoliate root crops such as sugarbeets before harvest or on cotton or
T other crop residue where crop has been previously harvested and
T residue is shredded  and spread flat..   10/3/01 DTL 11/15/01
T
T P42 is used to set a height of cut and removed the flattening P24.
T The 0.90 fraction used in RUSLE is by mass.  WEPS fraction is by height.
T It is not the same as RUSLE and cannot be used.
T Set the height to 2 inches per the conversation the Dave Lightle.  He said that most
T corn shredders are set to 2 inches.  Cotton shredding is much higher, use the 6 in shredder.
T A new operation was also created for root crop defoliation where all of the green tops
T are flatten to residue without killing the crop, "Shredder, beet topper".
T Kill crop was removed because of the interference with most harvest operations
T if used before harvest.  MAS 1-5-11
+
G 02 Biomass Manipulation
+ 1.0
P 42 Cut/Remove Biomass to Height (flags)
+ 0 0 1 0 0 50.800102 0 0 0.0
P 40 End crop Biomass Manipulation
#------------
D 19/04/03
O 03 Shredder, flail or rotary
+ 6.828365 .15 2.2351363 0.0 2.2351363 1.7881091 2.6821637
T Rusle Note: Rotary mower or flail shredder used to defoliate root crops such as sugarbeets before harvest or on cotton or
T other crop residue where crop has been previously harvested and
T residue is shredded  and spread flat..   10/3/01 DTL 11/15/01
T
T P42 is used to set a height of cut and removed the flattening P24.
T The 0.90 fraction used in RUSLE is by mass.  WEPS fraction is by height.
T It is not the same as RUSLE and cannot be used.
T Set the height to 2 inches per the conversation the Dave Lightle.  He said that most
T corn shredders are set to 2 inches.  Cotton shredding is much higher, use the 6 in shredder.
T A new operation was also created for root crop defoliation where all of the green tops
T are flatten to residue without killing the crop, "Shredder, beet topper".
T Kill crop was removed because of the interference with most harvest operations
T if used before harvest.  MAS 1-5-11
+
G 02 Biomass Manipulation
+ 1.0
P 42 Cut/Remove Biomass to Height (flags)
+ 0 0 1 0 0 50.800102 0 0 0.0
P 40 End crop Biomass Manipulation
#------------
D 26/04/03
O 03 Shredder, flail or rotary
+ 6.828365 .15 2.2351363 0.0 2.2351363 1.7881091 2.6821637
T Rusle Note: Rotary mower or flail shredder used to defoliate root crops such as sugarbeets before harvest or on cotton or
T other crop residue where crop has been previously harvested and
T residue is shredded  and spread flat..   10/3/01 DTL 11/15/01
T
T P42 is used to set a height of cut and removed the flattening P24.
T The 0.90 fraction used in RUSLE is by mass.  WEPS fraction is by height.
T It is not the same as RUSLE and cannot be used.
T Set the height to 2 inches per the conversation the Dave Lightle.  He said that most
T corn shredders are set to 2 inches.  Cotton shredding is much higher, use the 6 in shredder.
T A new operation was also created for root crop defoliation where all of the green tops
T are flatten to residue without killing the crop, "Shredder, beet topper".
T Kill crop was removed because of the interference with most harvest operations
T if used before harvest.  MAS 1-5-11
+
G 02 Biomass Manipulation
+ 1.0
P 42 Cut/Remove Biomass to Height (flags)
+ 0 0 1 0 0 50.800102 0 0 0.0
P 40 End crop Biomass Manipulation
#------------
D 26/04/03
O 04 Fert applic. surface broadcast
+ 1.4966278 0.0609375
T R2 Notes: Broadcast fertilizer spreader.  Wheel traffic only.  rev 082107 DTL
T
T Added to DB 4-12-12 MAS
+
G 01 Tillage
+ 0.0 0 0.05 0.0 0.0 0.0
P 01 Break Crust
P 02 Random Roughness
+ 1 8.8900175
P 11 Aggregate Crushing
+ 4.3 2.0
P 24 Flatten Standing Biomass
+ 0 0.25 0.2 0.15 0.1 1.0
P 26 Resurface Buried Biomass
+ 0.07 0.08 0.1 0.12 0.07
P 34 Change Standing Biomass Fall Rate
+ 0 1.0 1.0 1.0 1.0 1.0
+ 1.0 1.0 1.0 1.0 1.0
#------------
D 07/05/03
O 03 Shredder, flail or rotary
+ 6.828365 .15 2.2351363 0.0 2.2351363 1.7881091 2.6821637
T Rusle Note: Rotary mower or flail shredder used to defoliate root crops such as sugarbeets before harvest or on cotton or
T other crop residue where crop has been previously harvested and
T residue is shredded  and spread flat..   10/3/01 DTL 11/15/01
T
T P42 is used to set a height of cut and removed the flattening P24.
T The 0.90 fraction used in RUSLE is by mass.  WEPS fraction is by height.
T It is not the same as RUSLE and cannot be used.
T Set the height to 2 inches per the conversation the Dave Lightle.  He said that most
T corn shredders are set to 2 inches.  Cotton shredding is much higher, use the 6 in shredder.
T A new operation was also created for root crop defoliation where all of the green tops
T are flatten to residue without killing the crop, "Shredder, beet topper".
T Kill crop was removed because of the interference with most harvest operations
T if used before harvest.  MAS 1-5-11
+
G 02 Biomass Manipulation
+ 1.0
P 42 Cut/Remove Biomass to Height (flags)
+ 0 0 1 0 0 50.800102 0 0 0.0
P 40 End crop Biomass Manipulation
#------------
D 14/05/03
O 03 Shredder, flail or rotary
+ 6.828365 .15 2.2351363 0.0 2.2351363 1.7881091 2.6821637
T Rusle Note: Rotary mower or flail shredder used to defoliate root crops such as sugarbeets before harvest or on cotton or
T other crop residue where crop has been previously harvested and
T residue is shredded  and spread flat..   10/3/01 DTL 11/15/01
T
T P42 is used to set a height of cut and removed the flattening P24.
T The 0.90 fraction used in RUSLE is by mass.  WEPS fraction is by height.
T It is not the same as RUSLE and cannot be used.
T Set the height to 2 inches per the conversation the Dave Lightle.  He said that most
T corn shredders are set to 2 inches.  Cotton shredding is much higher, use the 6 in shredder.
T A new operation was also created for root crop defoliation where all of the green tops
T are flatten to residue without killing the crop, "Shredder, beet topper".
T Kill crop was removed because of the interference with most harvest operations
T if used before harvest.  MAS 1-5-11
+
G 02 Biomass Manipulation
+ 1.0
P 42 Cut/Remove Biomass to Height (flags)
+ 0 0 1 0 0 50.800102 0 0 0.0
P 40 End crop Biomass Manipulation
#------------
D 21/05/03
O 03 Shredder, flail or rotary
+ 6.828365 .15 2.2351363 0.0 2.2351363 1.7881091 2.6821637
T Rusle Note: Rotary mower or flail shredder used to defoliate root crops such as sugarbeets before harvest or on cotton or
T other crop residue where crop has been previously harvested and
T residue is shredded  and spread flat..   10/3/01 DTL 11/15/01
T
T P42 is used to set a height of cut and removed the flattening P24.
T The 0.90 fraction used in RUSLE is by mass.  WEPS fraction is by height.
T It is not the same as RUSLE and cannot be used.
T Set the height to 2 inches per the conversation the Dave Lightle.  He said that most
T corn shredders are set to 2 inches.  Cotton shredding is much higher, use the 6 in shredder.
T A new operation was also created for root crop defoliation where all of the green tops
T are flatten to residue without killing the crop, "Shredder, beet topper".
T Kill crop was removed because of the interference with most harvest operations
T if used before harvest.  MAS 1-5-11
+
G 02 Biomass Manipulation
+ 1.0
P 42 Cut/Remove Biomass to Height (flags)
+ 0 0 1 0 0 50.800102 0 0 0.0
P 40 End crop Biomass Manipulation
#------------
D 21/05/03
O 04 Fert applic. surface broadcast
+ 1.4966278 0.0609375
T R2 Notes: Broadcast fertilizer spreader.  Wheel traffic only.  rev 082107 DTL
T
T Added to DB 4-12-12 MAS
+
G 01 Tillage
+ 0.0 0 0.05 0.0 0.0 0.0
P 01 Break Crust
P 02 Random Roughness
+ 1 8.8900175
P 11 Aggregate Crushing
+ 4.3 2.0
P 24 Flatten Standing Biomass
+ 0 0.25 0.2 0.15 0.1 1.0
P 26 Resurface Buried Biomass
+ 0.07 0.08 0.1 0.12 0.07
P 34 Change Standing Biomass Fall Rate
+ 0 1.0 1.0 1.0 1.0 1.0
+ 1.0 1.0 1.0 1.0 1.0
#------------
D 30/05/03
O 03 Shredder, flail or rotary
+ 6.828365 .15 2.2351363 0.0 2.2351363 1.7881091 2.6821637
T Rusle Note: Rotary mower or flail shredder used to defoliate root crops such as sugarbeets before harvest or on cotton or
T other crop residue where crop has been previously harvested and
T residue is shredded  and spread flat..   10/3/01 DTL 11/15/01
T
T P42 is used to set a height of cut and removed the flattening P24.
T The 0.90 fraction used in RUSLE is by mass.  WEPS fraction is by height.
T It is not the same as RUSLE and cannot be used.
T Set the height to 2 inches per the conversation the Dave Lightle.  He said that most
T corn shredders are set to 2 inches.  Cotton shredding is much higher, use the 6 in shredder.
T A new operation was also created for root crop defoliation where all of the green tops
T are flatten to residue without killing the crop, "Shredder, beet topper".
T Kill crop was removed because of the interference with most harvest operations
T if used before harvest.  MAS 1-5-11
+
G 02 Biomass Manipulation
+ 1.0
P 42 Cut/Remove Biomass to Height (flags)
+ 0 0 1 0 0 50.800102 0 0 0.0
P 40 End crop Biomass Manipulation
#------------
D 10/06/03
O 03 Shredder, flail or rotary
+ 6.828365 .15 2.2351363 0.0 2.2351363 1.7881091 2.6821637
T Rusle Note: Rotary mower or flail shredder used to defoliate root crops such as sugarbeets before harvest or on cotton or
T other crop residue where crop has been previously harvested and
T residue is shredded  and spread flat..   10/3/01 DTL 11/15/01
T
T P42 is used to set a height of cut and removed the flattening P24.
T The 0.90 fraction used in RUSLE is by mass.  WEPS fraction is by height.
T It is not the same as RUSLE and cannot be used.
T Set the height to 2 inches per the conversation the Dave Lightle.  He said that most
T corn shredders are set to 2 inches.  Cotton shredding is much higher, use the 6 in shredder.
T A new operation was also created for root crop defoliation where all of the green tops
T are flatten to residue without killing the crop, "Shredder, beet topper".
T Kill crop was removed because of the interference with most harvest operations
T if used before harvest.  MAS 1-5-11
+
G 02 Biomass Manipulation
+ 1.0
P 42 Cut/Remove Biomass to Height (flags)
+ 0 0 1 0 0 50.800102 0 0 0.0
P 40 End crop Biomass Manipulation
#------------
D 20/06/03
O 03 Shredder, flail or rotary
+ 6.828365 .15 2.2351363 0.0 2.2351363 1.7881091 2.6821637
T Rusle Note: Rotary mower or flail shredder used to defoliate root crops such as sugarbeets before harvest or on cotton or
T other crop residue where crop has been previously harvested and
T residue is shredded  and spread flat..   10/3/01 DTL 11/15/01
T
T P42 is used to set a height of cut and removed the flattening P24.
T The 0.90 fraction used in RUSLE is by mass.  WEPS fraction is by height.
T It is not the same as RUSLE and cannot be used.
T Set the height to 2 inches per the conversation the Dave Lightle.  He said that most
T corn shredders are set to 2 inches.  Cotton shredding is much higher, use the 6 in shredder.
T A new operation was also created for root crop defoliation where all of the green tops
T are flatten to residue without killing the crop, "Shredder, beet topper".
T Kill crop was removed because of the interference with most harvest operations
T if used before harvest.  MAS 1-5-11
+
G 02 Biomass Manipulation
+ 1.0
P 42 Cut/Remove Biomass to Height (flags)
+ 0 0 1 0 0 50.800102 0 0 0.0
P 40 End crop Biomass Manipulation
#------------
D 20/06/03
O 04 Fert applic. surface broadcast
+ 1.4966278 0.0609375
T R2 Notes: Broadcast fertilizer spreader.  Wheel traffic only.  rev 082107 DTL
T
T Added to DB 4-12-12 MAS
+
G 01 Tillage
+ 0.0 0 0.05 0.0 0.0 0.0
P 01 Break Crust
P 02 Random Roughness
+ 1 8.8900175
P 11 Aggregate Crushing
+ 4.3 2.0
P 24 Flatten Standing Biomass
+ 0 0.25 0.2 0.15 0.1 1.0
P 26 Resurface Buried Biomass
+ 0.07 0.08 0.1 0.12 0.07
P 34 Change Standing Biomass Fall Rate
+ 0 1.0 1.0 1.0 1.0 1.0
+ 1.0 1.0 1.0 1.0 1.0
#------------
D 07/07/03
O 03 Shredder, flail or rotary
+ 6.828365 .15 2.2351363 0.0 2.2351363 1.7881091 2.6821637
T Rusle Note: Rotary mower or flail shredder used to defoliate root crops such as sugarbeets before harvest or on cotton or
T other crop residue where crop has been previously harvested and
T residue is shredded  and spread flat..   10/3/01 DTL 11/15/01
T
T P42 is used to set a height of cut and removed the flattening P24.
T The 0.90 fraction used in RUSLE is by mass.  WEPS fraction is by height.
T It is not the same as RUSLE and cannot be used.
T Set the height to 2 inches per the conversation the Dave Lightle.  He said that most
T corn shredders are set to 2 inches.  Cotton shredding is much higher, use the 6 in shredder.
T A new operation was also created for root crop defoliation where all of the green tops
T are flatten to residue without killing the crop, "Shredder, beet topper".
T Kill crop was removed because of the interference with most harvest operations
T if used before harvest.  MAS 1-5-11
+
G 02 Biomass Manipulation
+ 1.0
P 42 Cut/Remove Biomass to Height (flags)
+ 0 0 1 0 0 50.800102 0 0 0.0
P 40 End crop Biomass Manipulation
#------------
D 21/07/03
O 03 Shredder, flail or rotary
+ 6.828365 .15 2.2351363 0.0 2.2351363 1.7881091 2.6821637
T Rusle Note: Rotary mower or flail shredder used to defoliate root crops such as sugarbeets before harvest or on cotton or
T other crop residue where crop has been previously harvested and
T residue is shredded  and spread flat..   10/3/01 DTL 11/15/01
T
T P42 is used to set a height of cut and removed the flattening P24.
T The 0.90 fraction used in RUSLE is by mass.  WEPS fraction is by height.
T It is not the same as RUSLE and cannot be used.
T Set the height to 2 inches per the conversation the Dave Lightle.  He said that most
T corn shredders are set to 2 inches.  Cotton shredding is much higher, use the 6 in shredder.
T A new operation was also created for root crop defoliation where all of the green tops
T are flatten to residue without killing the crop, "Shredder, beet topper".
T Kill crop was removed because of the interference with most harvest operations
T if used before harvest.  MAS 1-5-11
+
G 02 Biomass Manipulation
+ 1.0
P 42 Cut/Remove Biomass to Height (flags)
+ 0 0 1 0 0 50.800102 0 0 0.0
P 40 End crop Biomass Manipulation
#------------
D 21/07/03
O 04 Fert applic. surface broadcast
+ 1.4966278 0.0609375
T R2 Notes: Broadcast fertilizer spreader.  Wheel traffic only.  rev 082107 DTL
T
T Added to DB 4-12-12 MAS
+
G 01 Tillage
+ 0.0 0 0.05 0.0 0.0 0.0
P 01 Break Crust
P 02 Random Roughness
+ 1 8.8900175
P 11 Aggregate Crushing
+ 4.3 2.0
P 24 Flatten Standing Biomass
+ 0 0.25 0.2 0.15 0.1 1.0
P 26 Resurface Buried Biomass
+ 0.07 0.08 0.1 0.12 0.07
P 34 Change Standing Biomass Fall Rate
+ 0 1.0 1.0 1.0 1.0 1.0
+ 1.0 1.0 1.0 1.0 1.0
#------------
D 28/07/03
O 03 Shredder, flail or rotary
+ 6.828365 .15 2.2351363 0.0 2.2351363 1.7881091 2.6821637
T Rusle Note: Rotary mower or flail shredder used to defoliate root crops such as sugarbeets before harvest or on cotton or
T other crop residue where crop has been previously harvested and
T residue is shredded  and spread flat..   10/3/01 DTL 11/15/01
T
T P42 is used to set a height of cut and removed the flattening P24.
T The 0.90 fraction used in RUSLE is by mass.  WEPS fraction is by height.
T It is not the same as RUSLE and cannot be used.
T Set the height to 2 inches per the conversation the Dave Lightle.  He said that most
T corn shredders are set to 2 inches.  Cotton shredding is much higher, use the 6 in shredder.
T A new operation was also created for root crop defoliation where all of the green tops
T are flatten to residue without killing the crop, "Shredder, beet topper".
T Kill crop was removed because of the interference with most harvest operations
T if used before harvest.  MAS 1-5-11
+
G 02 Biomass Manipulation
+ 1.0
P 42 Cut/Remove Biomass to Height (flags)
+ 0 0 1 0 0 50.800102 0 0 0.0
P 40 End crop Biomass Manipulation
#------------
D 04/08/03
O 03 Shredder, flail or rotary
+ 6.828365 .15 2.2351363 0.0 2.2351363 1.7881091 2.6821637
T Rusle Note: Rotary mower or flail shredder used to defoliate root crops such as sugarbeets before harvest or on cotton or
T other crop residue where crop has been previously harvested and
T residue is shredded  and spread flat..   10/3/01 DTL 11/15/01
T
T P42 is used to set a height of cut and removed the flattening P24.
T The 0.90 fraction used in RUSLE is by mass.  WEPS fraction is by height.
T It is not the same as RUSLE and cannot be used.
T Set the height to 2 inches per the conversation the Dave Lightle.  He said that most
T corn shredders are set to 2 inches.  Cotton shredding is much higher, use the 6 in shredder.
T A new operation was also created for root crop defoliation where all of the green tops
T are flatten to residue without killing the crop, "Shredder, beet topper".
T Kill crop was removed because of the interference with most harvest operations
T if used before harvest.  MAS 1-5-11
+
G 02 Biomass Manipulation
+ 1.0
P 42 Cut/Remove Biomass to Height (flags)
+ 0 0 1 0 0 50.800102 0 0 0.0
P 40 End crop Biomass Manipulation
#------------
D 11/08/03
O 03 Shredder, flail or rotary
+ 6.828365 .15 2.2351363 0.0 2.2351363 1.7881091 2.6821637
T Rusle Note: Rotary mower or flail shredder used to defoliate root crops such as sugarbeets before harvest or on cotton or
T other crop residue where crop has been previously harvested and
T residue is shredded  and spread flat..   10/3/01 DTL 11/15/01
T
T P42 is used to set a height of cut and removed the flattening P24.
T The 0.90 fraction used in RUSLE is by mass.  WEPS fraction is by height.
T It is not the same as RUSLE and cannot be used.
T Set the height to 2 inches per the conversation the Dave Lightle.  He said that most
T corn shredders are set to 2 inches.  Cotton shredding is much higher, use the 6 in shredder.
T A new operation was also created for root crop defoliation where all of the green tops
T are flatten to residue without killing the crop, "Shredder, beet topper".
T Kill crop was removed because of the interference with most harvest operations
T if used before harvest.  MAS 1-5-11
+
G 02 Biomass Manipulation
+ 1.0
P 42 Cut/Remove Biomass to Height (flags)
+ 0 0 1 0 0 50.800102 0 0 0.0
P 40 End crop Biomass Manipulation
#------------
D 18/08/03
O 03 Shredder, flail or rotary
+ 6.828365 .15 2.2351363 0.0 2.2351363 1.7881091 2.6821637
T Rusle Note: Rotary mower or flail shredder used to defoliate root crops such as sugarbeets before harvest or on cotton or
T other crop residue where crop has been previously harvested and
T residue is shredded  and spread flat..   10/3/01 DTL 11/15/01
T
T P42 is used to set a height of cut and removed the flattening P24.
T The 0.90 fraction used in RUSLE is by mass.  WEPS fraction is by height.
T It is not the same as RUSLE and cannot be used.
T Set the height to 2 inches per the conversation the Dave Lightle.  He said that most
T corn shredders are set to 2 inches.  Cotton shredding is much higher, use the 6 in shredder.
T A new operation was also created for root crop defoliation where all of the green tops
T are flatten to residue without killing the crop, "Shredder, beet topper".
T Kill crop was removed because of the interference with most harvest operations
T if used before harvest.  MAS 1-5-11
+
G 02 Biomass Manipulation
+ 1.0
P 42 Cut/Remove Biomass to Height (flags)
+ 0 0 1 0 0 50.800102 0 0 0.0
P 40 End crop Biomass Manipulation
#------------
D 18/08/03
O 04 Fert applic. surface broadcast
+ 1.4966278 0.0609375
T R2 Notes: Broadcast fertilizer spreader.  Wheel traffic only.  rev 082107 DTL
T
T Added to DB 4-12-12 MAS
+
G 01 Tillage
+ 0.0 0 0.05 0.0 0.0 0.0
P 01 Break Crust
P 02 Random Roughness
+ 1 8.8900175
P 11 Aggregate Crushing
+ 4.3 2.0
P 24 Flatten Standing Biomass
+ 0 0.25 0.2 0.15 0.1 1.0
P 26 Resurface Buried Biomass
+ 0.07 0.08 0.1 0.12 0.07
P 34 Change Standing Biomass Fall Rate
+ 0 1.0 1.0 1.0 1.0 1.0
+ 1.0 1.0 1.0 1.0 1.0
#------------
D 25/08/03
O 03 Shredder, flail or rotary
+ 6.828365 .15 2.2351363 0.0 2.2351363 1.7881091 2.6821637
T Rusle Note: Rotary mower or flail shredder used to defoliate root crops such as sugarbeets before harvest or on cotton or
T other crop residue where crop has been previously harvested and
T residue is shredded  and spread flat..   10/3/01 DTL 11/15/01
T
T P42 is used to set a height of cut and removed the flattening P24.
T The 0.90 fraction used in RUSLE is by mass.  WEPS fraction is by height.
T It is not the same as RUSLE and cannot be used.
T Set the height to 2 inches per the conversation the Dave Lightle.  He said that most
T corn shredders are set to 2 inches.  Cotton shredding is much higher, use the 6 in shredder.
T A new operation was also created for root crop defoliation where all of the green tops
T are flatten to residue without killing the crop, "Shredder, beet topper".
T Kill crop was removed because of the interference with most harvest operations
T if used before harvest.  MAS 1-5-11
+
G 02 Biomass Manipulation
+ 1.0
P 42 Cut/Remove Biomass to Height (flags)
+ 0 0 1 0 0 50.800102 0 0 0.0
P 40 End crop Biomass Manipulation
#------------
D 01/09/03
O 03 Shredder, flail or rotary
+ 6.828365 .15 2.2351363 0.0 2.2351363 1.7881091 2.6821637
T Rusle Note: Rotary mower or flail shredder used to defoliate root crops such as sugarbeets before harvest or on cotton or
T other crop residue where crop has been previously harvested and
T residue is shredded  and spread flat..   10/3/01 DTL 11/15/01
T
T P42 is used to set a height of cut and removed the flattening P24.
T The 0.90 fraction used in RUSLE is by mass.  WEPS fraction is by height.
T It is not the same as RUSLE and cannot be used.
T Set the height to 2 inches per the conversation the Dave Lightle.  He said that most
T corn shredders are set to 2 inches.  Cotton shredding is much higher, use the 6 in shredder.
T A new operation was also created for root crop defoliation where all of the green tops
T are flatten to residue without killing the crop, "Shredder, beet topper".
T Kill crop was removed because of the interference with most harvest operations
T if used before harvest.  MAS 1-5-11
+
G 02 Biomass Manipulation
+ 1.0
P 42 Cut/Remove Biomass to Height (flags)
+ 0 0 1 0 0 50.800102 0 0 0.0
P 40 End crop Biomass Manipulation
#------------
D 15/09/03
O 03 Shredder, flail or rotary
+ 6.828365 .15 2.2351363 0.0 2.2351363 1.7881091 2.6821637
T Rusle Note: Rotary mower or flail shredder used to defoliate root crops such as sugarbeets before harvest or on cotton or
T other crop residue where crop has been previously harvested and
T residue is shredded  and spread flat..   10/3/01 DTL 11/15/01
T
T P42 is used to set a height of cut and removed the flattening P24.
T The 0.90 fraction used in RUSLE is by mass.  WEPS fraction is by height.
T It is not the same as RUSLE and cannot be used.
T Set the height to 2 inches per the conversation the Dave Lightle.  He said that most
T corn shredders are set to 2 inches.  Cotton shredding is much higher, use the 6 in shredder.
T A new operation was also created for root crop defoliation where all of the green tops
T are flatten to residue without killing the crop, "Shredder, beet topper".
T Kill crop was removed because of the interference with most harvest operations
T if used before harvest.  MAS 1-5-11
+
G 02 Biomass Manipulation
+ 1.0
P 42 Cut/Remove Biomass to Height (flags)
+ 0 0 1 0 0 50.800102 0 0 0.0
P 40 End crop Biomass Manipulation
#------------
D 20/09/03
O 03 Sod cutter
+ 8.418531 .24 0.44702727 0.0 0.44702727 0.22351363 2.2351363
T Cut and remove grass sod,  P31 set:  annual crops killed, perennial crops regrow jkp 130910
+
G 01 Tillage
+ 25.400051 1.0 1.0 25.400051 12.700026 38.100075
P 01 Break Crust
P 02 Random Roughness
+ 1 10.160021
P 05 Ridges and Dikes
+ 1 0.0 0.0 0.0 0.0 0.0
P 11 Aggregate Crushing
+ 4.3 2.0
P 12 Soil Loosening
+ 0.65
P 13 Soil Layer Mixing
+ 0.2
G 02 Biomass Manipulation
+ 1.0
P 31 Kill or Defoliate Growing Crop
+ 1
P 62 Remove (by age pool) Plant/Residue Material
+ 1 1 0 1 7 7 0 1 1 1 1.0 .2
P 40 End crop Biomass Manipulation
P 25 Bury Flat Biomass
+ 2 0.001 0.001 0.001 0.001 0.5
P 26 Resurface Buried Biomass
+ 0.001 0.001 0.001 0.001 0.07
#------------
*END
*EOF
