Version: 1.5
*START 2
N Originating Program: RUSLE2
N Skel Format Version: 1.1
N This management file was originally converted from the NRCS standard XML format on - Thu Jun 21 09:32:27 PDT 2012
N This management file was updated to contain the most current crop and operation records for WEPS on - Tue Jun 26 16:04:52 PDT 2012
#------------
D 01/11/01
O 03 Plow, moldboard
+ 17.491838 65 2.2351363 0.0 2.2351363 1.5645955 2.6821637
T Moldboard plow 8 inch operating depth.  060701 DTL  Modified flattening and burial per McCool and Foster 05/21/02 DTL RUSLE MAS 10-26-06
+
G 01 Tillage
+ 203.20041 1.0 1.0 203.20041 152.4003 254.0005
P 01 Break Crust
P 02 Random Roughness
+ 1 48.260098
P 05 Ridges and Dikes
+ 1 25.400051 406.40082 0.0 0.0 0.0
P 11 Aggregate Crushing
+ 2.8 1.0
P 12 Soil Loosening
+ 1.0
P 13 Soil Layer Mixing
+ 0.7
P 14 Soil Layer Inversion
P 31 Kill or Defoliate Growing Crop
+ 2
P 40 End crop Biomass Manipulation
P 24 Flatten Standing Biomass
+ 0 1 1 1 0.75 1.0
P 25 Bury Flat Biomass
+ 3 0.99 0.99 0.99 0.85 0.97
P 26 Resurface Buried Biomass
+ 0.01 0.02 0.04 0.1 0.02
P 34 Change Standing Biomass Fall Rate
+ 7 3.0 2.5 2.0 1.5 1.0
+ 0.5 0.6 0.7 0.8 1.0
#------------
D 01/05/02
O 03 Disk, tandem secondary op
+ 4.4898834 32.5 2.2351363 0.0 2.2351363 1.3410819 2.6821637
T 9-in. Spacing, Front and Rear; Good for seedbed preparation/chemical incorporation in medium to heavy soils
T Works well in primary tillage in light to medium soils
T Provides good residue-handling capability.  MAS 10-26-06
+
G 01 Tillage
+ 127.00027 0.75 1.0 127.00026 76.20015 152.4003
P 01 Break Crust
P 02 Random Roughness
+ 1 15.240031
P 05 Ridges and Dikes
+ 1 50.800102 228.60046 0.0 0.0 0.0
P 11 Aggregate Crushing
+ 2.8 0.75
P 12 Soil Loosening
+ 0.85
P 13 Soil Layer Mixing
+ 0.4
P 31 Kill or Defoliate Growing Crop
+ 2
P 40 End crop Biomass Manipulation
P 24 Flatten Standing Biomass
+ 0 0.85 0.7 0.6 0.5 1.0
P 25 Bury Flat Biomass
+ 1 0.73 0.63 0.55 0.4 0.73
P 26 Resurface Buried Biomass
+ 0.02 0.04 0.02 0.05 0.02
P 34 Change Standing Biomass Fall Rate
+ 7 3.0 2.5 2.0 1.5 1.0
+ 0.5 0.6 0.7 0.8 1.0
#------------
D 10/05/02
O 03 Cultivator, field 6-12 in sweeps
+ 6.921904 26 2.2351363 0.0 2.2351363 1.5645955 2.9056773
T Corrected Speed of operation numbers 11-1-11 MAS
+
G 01 Tillage
+ 101.600204 0.4 1.0 101.600204 50.800102 152.4003
P 01 Break Crust
P 02 Random Roughness
+ 1 15.240031
P 05 Ridges and Dikes
+ 1 50.800102 228.60045 0.0 0.0 0.0
P 11 Aggregate Crushing
+ 3.0 1.0
P 12 Soil Loosening
+ 0.65
P 13 Soil Layer Mixing
+ 0.3
P 31 Kill or Defoliate Growing Crop
+ 2
P 40 End crop Biomass Manipulation
P 24 Flatten Standing Biomass
+ 0 0.7 0.4 0.3 0.2 1.0
P 25 Bury Flat Biomass
+ 1 0.4 0.35 0.3 0.2 0.85
P 26 Resurface Buried Biomass
+ 0.05 0.06 0.07 0.2 0.05
P 34 Change Standing Biomass Fall Rate
+ 7 3.0 2.5 2.0 1.5 1.0
+ 0.5 0.6 0.7 0.8 1.0
#------------
D 15/05/02
O 03 Drill or airseeder, double disk
+ 3.3674128 6.34 2.2351363 0.0 2.2351363 1.5645955 2.9056773
T Drill or air seeder with double disk openers on 7 to 10 inch spacings.  Rev102403 DTL  RUSLE MAS 10-26-06
T G2 was added into file in front of the flattening (P24), burial (P25), and resurfacing (P26) factors because the area affected is less than 1.0 and
T the RUSLE values were normalized to 1.0.  This change will imulate the correct residue changes based on the method set forth in RUSLE.
T RUSLE's factors have been redused to based on the area affected.
T The stalk fall rate factor (P34) was moved ahead of the new (G2) factor to set the fall rate to the  less than 1.0 area affected.  8/8/07 MAS
T
T Deleted the G2 process because all process only affect 0.65 of the surface.  This is set a 0.65 with G1 process in the beginning. 5-11-11 MAS
+ 
G 01 Tillage
+ 38.100075 0.4 0.65 38.100075 25.400051 50.800102
P 01 Break Crust
P 02 Random Roughness
+ 1 7.6200156
P 05 Ridges and Dikes
+ 1 25.400051 203.20041 25.400051 0.0 0.0
P 11 Aggregate Crushing
+ 2.8 0.75
P 12 Soil Loosening
+ 0.6
P 13 Soil Layer Mixing
+ 0.3
P 34 Change Standing Biomass Fall Rate
+ 7 3.0 2.5 2.0 1.5 1.0
+ 0.5 0.6 0.7 0.8 1.0
P 24 Flatten Standing Biomass
+ 0 0.6 0.4 0.35 0.15 1.0
P 25 Bury Flat Biomass
+ 1 0.2275 0.1625 0.13 0.065 0.13
P 26 Resurface Buried Biomass
+ 0.01 0.01 0.01 0.02 0.01
G 03 Crop Name
+ Sorghum, forage
P 51 Seeding Configuration
+ 1 0.0 0
+ 62.0 5.0 0 10 1.0 1.0 2
+ ton/ac
+ 0 4.465 4 1.0 0.46 0.8
+ 1.9812241 0.025 2.0 10.0 27.5 1 110 1500.0
+ -5.0 -15.0 0.01 0.95 0.0 40
+ -0.0302 0.9263 0.3728 -0.065 -0.018 1.015 0.7224 0.039
+ 0.3728 -0.065 0.03985145 0.42 19.2 0.05 0 0.7
+ 8.333333 13.0 3.0 0.03 0.1 0.1 0.0 3
+ 0.01 0.01 0.01 0.01 0.153 0.01 20.0 3.0
+ -1.20379 0.604887 0.0 0.0 0.0 0.0 0.0 0.0
T This file is most like  forage sorghum silage 20 ton  30" row spacing.  Base location Columbia, MO REV 61801 DTL
T
T The residue ratio is set to Sorghum, silage from RUSLE.  If you need a hay file use Sorghum, hay.
T MAS 4-27-08
T
T Changed the flag to not selectect for calabration from calabration  MAS 9-2-09
T Changed the flag from day maturity to heat units.  MAS 9-2-09
#------------
D 01/07/02
O 04 Graze, rotational 50 pct removal
+ 9.353924E-8 0.4875
T Rotational Grazing system with 50% of growth removed with each grazing cycle.12-20-01 DTL
T Created 11-27-07 MAS
T
T Restructured processes.  Moved all grazing to O4 for energy and stir cal.
T
T Crop removal (green standing) is cal by using Rusle factors
T Port of Tt biomas affected (%)-(Port of Tt biomas affected (%))x(Portion of affected left on surface (%)
T Graze, continous Example: 0.3-(0.3 x 0.5) = 0.15
T
T Flattening Residue is cal by using Rusle Factors
T Port of Tt biomas affected (%) x Portion of affected left on surface (%)
T Graze, continous Example 0.3 x 0.5 = 0.15
T This value was used for the Mod residue (Wheat) values were reduced by 10% or increased by 10% of the value for each residue class.
T MAS 4-2-08
T Changed stem removal from 0.5 to 0 to prevent the stand from thining.  MAS 1-6-11
T Changed reports to include only the current green crop biomass.  Multiple report values are confusing users.  MAS 6-21-11
+
G 02 Biomass Manipulation
+ 1
P 62 Remove (by age pool) Plant/Residue Material
+ 1 0 1 0 1 1 0 0.5 0.5 0.0 0.0 0.0
P 62 Remove (by age pool) Plant/Residue Material
+ 0 0 1 0 2 4 2 .05 .05 .05 0.0 0.0
P 62 Remove (by age pool) Plant/Residue Material
+ 0 0 1 0 1 4 2 0.1 .1 0.1 0 0
P 24 Flatten Standing Biomass
+ 1 0.08 0.075 0.07 0.01 0.01
#------------
D 15/08/02
O 04 Graze, rotational 50 pct removal
+ 9.353924E-8 0.4875
T Rotational Grazing system with 50% of growth removed with each grazing cycle.12-20-01 DTL
T Created 11-27-07 MAS
T
T Restructured processes.  Moved all grazing to O4 for energy and stir cal.
T
T Crop removal (green standing) is cal by using Rusle factors
T Port of Tt biomas affected (%)-(Port of Tt biomas affected (%))x(Portion of affected left on surface (%)
T Graze, continous Example: 0.3-(0.3 x 0.5) = 0.15
T
T Flattening Residue is cal by using Rusle Factors
T Port of Tt biomas affected (%) x Portion of affected left on surface (%)
T Graze, continous Example 0.3 x 0.5 = 0.15
T This value was used for the Mod residue (Wheat) values were reduced by 10% or increased by 10% of the value for each residue class.
T MAS 4-2-08
T Changed stem removal from 0.5 to 0 to prevent the stand from thining.  MAS 1-6-11
T Changed reports to include only the current green crop biomass.  Multiple report values are confusing users.  MAS 6-21-11
+
G 02 Biomass Manipulation
+ 1
P 62 Remove (by age pool) Plant/Residue Material
+ 1 0 1 0 1 1 0 0.5 0.5 0.0 0.0 0.0
P 62 Remove (by age pool) Plant/Residue Material
+ 0 0 1 0 2 4 2 .05 .05 .05 0.0 0.0
P 62 Remove (by age pool) Plant/Residue Material
+ 0 0 1 0 1 4 2 0.1 .1 0.1 0 0
P 24 Flatten Standing Biomass
+ 1 0.08 0.075 0.07 0.01 0.01
#------------
D 20/10/02
O 04 Kill crop
+ 0.0 0
T Enter Operation notes here
+
G 02 Biomass Manipulation
+ 1.0
P 31 Kill or Defoliate Growing Crop
+ 2
P 40 End crop Biomass Manipulation
#------------
D 01/11/02
O 04 Graze, stubble or residue
+ 9.353924E-8 0.4875
T Grazing of crop residue such as corn stalks or cotton.  10/26/01 DTL
T Created 11-27-07  This can be used as it is in RUSLE.  MAS
T
T Restructured processes.  Moved all grazing to O4 for energy and stir cal. MAS 4-2-08
T
T Adjusted total reduction of residue to match RUSLE values.
T Standing and Flat values may vary slightly.  MAS 4-10-08
T Changed report harvest to "no report" to better work with the crop yr interval MAS 7-26-11
+
G 02 Biomass Manipulation
+ 1.0
P 62 Remove (by age pool) Plant/Residue Material
+ 1 0 1 0 1 4 2 0.11 0.11 0.11 0.0 0.0
P 62 Remove (by age pool) Plant/Residue Material
+ 1 0 1 0 2 4 2 0.11 0.11 0.11 0.0 0.0
P 24 Flatten Standing Biomass
+ 0 .2 0.15 .1 .01 .01
#------------
*END
*EOF
