Version: 1.5
*START 4
N Originating Program: RUSLE2
N Skel Format Version: 1.1
N This management file was originally converted from the NRCS standard XML format on - Thu Jun 21 11:13:50 PDT 2012
N This management file was updated to contain the most current crop and operation records for WEPS on - Tue Jun 26 15:42:53 PDT 2012
N This management file was updated to contain the most current crop and operation records for WEPS on - Tue Dec 17 19:25:55 CST 2013
#------------
D 18/04/01
O 03 Chisel, twisted shovel
+ 10.289317 65 2.9056773 0.0 2.9056773 1.5645955 2.9056773
T This is a stanard 3 inch twisted point chisel plow.  This is a 12 in sp machine placed staggered on three tool bars. MAS 6-4-09
+
G 01 Tillage
+ 165.10033 0.9 1.0 165.10033 101.600204 203.20041
P 01 Break Crust
P 02 Random Roughness
+ 1 48.260098
P 05 Ridges and Dikes
+ 1 152.4003 304.8006 101.600204 0.0 0.0
P 11 Aggregate Crushing
+ 2.4 -2.0
P 12 Soil Loosening
+ 0.85
P 13 Soil Layer Mixing
+ 0.42
P 31 Kill or Defoliate Growing Crop
+ 2
P 40 End crop Biomass Manipulation
P 24 Flatten Standing Biomass
+ 0 0.85 0.8 0.7 0.6 1.0
P 25 Bury Flat Biomass
+ 1 0.9 0.8 0.75 0.6 0.93
P 26 Resurface Buried Biomass
+ 0.05 0.06 0.07 0.15 0.05
P 34 Change Standing Biomass Fall Rate
+ 7 3.0 2.5 2.0 1.5 1.0
+ 0.5 0.6 0.7 0.8 1.0
#------------
D 03/05/01
O 03 Disk, tandem secondary op
+ 4.4898834 32.5 2.2351363 0.0 2.2351363 1.3410819 2.6821637
T 9-in. Spacing, Front and Rear; Good for seedbed preparation/chemical incorporation in medium to heavy soils
T Works well in primary tillage in light to medium soils
T Provides good residue-handling capability.  MAS 10-26-06
+
G 01 Tillage
+ 127.00027 0.75 1.0 127.00026 76.20015 152.4003
P 01 Break Crust
P 02 Random Roughness
+ 1 15.240031
P 05 Ridges and Dikes
+ 1 50.800102 228.60046 0.0 0.0 0.0
P 11 Aggregate Crushing
+ 2.8 0.75
P 12 Soil Loosening
+ 0.85
P 13 Soil Layer Mixing
+ 0.4
P 31 Kill or Defoliate Growing Crop
+ 2
P 40 End crop Biomass Manipulation
P 24 Flatten Standing Biomass
+ 0 0.85 0.7 0.6 0.5 1.0
P 25 Bury Flat Biomass
+ 1 0.73 0.63 0.55 0.4 0.73
P 26 Resurface Buried Biomass
+ 0.02 0.04 0.02 0.05 0.02
P 34 Change Standing Biomass Fall Rate
+ 7 3.0 2.5 2.0 1.5 1.0
+ 0.5 0.6 0.7 0.8 1.0
#------------
D 22/05/01
O 03 Disk, tandem secondary op
+ 4.4898834 32.5 2.2351363 0.0 2.2351363 1.3410819 2.6821637
T 9-in. Spacing, Front and Rear; Good for seedbed preparation/chemical incorporation in medium to heavy soils
T Works well in primary tillage in light to medium soils
T Provides good residue-handling capability.  MAS 10-26-06
+
G 01 Tillage
+ 127.00027 0.75 1.0 127.00026 76.20015 152.4003
P 01 Break Crust
P 02 Random Roughness
+ 1 15.240031
P 05 Ridges and Dikes
+ 1 50.800102 228.60046 0.0 0.0 0.0
P 11 Aggregate Crushing
+ 2.8 0.75
P 12 Soil Loosening
+ 0.85
P 13 Soil Layer Mixing
+ 0.4
P 31 Kill or Defoliate Growing Crop
+ 2
P 40 End crop Biomass Manipulation
P 24 Flatten Standing Biomass
+ 0 0.85 0.7 0.6 0.5 1.0
P 25 Bury Flat Biomass
+ 1 0.73 0.63 0.55 0.4 0.73
P 26 Resurface Buried Biomass
+ 0.02 0.04 0.02 0.05 0.02
P 34 Change Standing Biomass Fall Rate
+ 7 3.0 2.5 2.0 1.5 1.0
+ 0.5 0.6 0.7 0.8 1.0
#------------
D 23/05/01
O 03 Drill or air seeder single disk openers 7-10 in spac
+ 3.2738733 2.44 2.2351363 0.0 2.2351363 1.5645955 2.9056773
T Drill or Air seeder with single disk no-till openers  JD 750 or similar openers. (No-till air drill)
T Based on Drill, no-till single disk 7-10 spacing. 102403 DTL. RUSLE MAS 10-26-06
T G2 was added into file in front of the flattening (P24), burial (P25), and resurfacing (P26) factors because the area affected is less than 1.0 and
T the RUSLE values were normalized to 1.0.  This change will imulate the correct residue changes based on the method set forth in RUSLE.
T RUSLE's factors have been redused to based on the area affected.
T The stalk fall rate factor (P34) was moved ahead of the new (G2) factor to set the fall rate to the less than 1.0 area affected.  8/7/07 MAS
+
G 01 Tillage
+ 63.500134 0.4 0.15 63.50013 50.800102 101.600204
P 01 Break Crust
P 02 Random Roughness
+ 1 7.6200156
P 05 Ridges and Dikes
+ 1 25.400051 203.20041 0.0 0.0 0.0
P 11 Aggregate Crushing
+ 2.8 0.75
P 12 Soil Loosening
+ 0.4
P 13 Soil Layer Mixing
+ 0.20
P 34 Change Standing Biomass Fall Rate
+ 7 3.0 2.5 2.0 1.5 1.0
+ 0.5 0.6 0.7 0.8 1.0
G 02 Biomass Manipulation
+ 1.0
P 24 Flatten Standing Biomass
+ 0 0.6 0.4 0.35 0.15 1.0
P 25 Bury Flat Biomass
+ 1 0.05 0.04 0.03 0.02 0.03
P 26 Resurface Buried Biomass
+ 0.01 0.01 0.01 0.05 0.01
G 03 Crop Name
+ Grass seed, cool season
P 51 Seeding Configuration
+ 1 0.0 0
+ 1902.7849852966615 1 0 1200 1 1 1
+ lbs/ac
+ 0 8930 6 0.8 0.69 0.9
+ 1 0.0050 2 1.6666666666666665 21.11111111111111 1 120 1833.3333333333335
+ -5 -15 0.0050 0.05 0.04 10
+ 0.023 0.975 0.6 -0.08 -0.024 0.9911 0.8 0.08
+ 0.45 -0.095 3.9 1 30 0.05 0 0.3
+ 7.9378586 110 0.6 0.0070 0 0.1 0.1 2
+ 0.0536 0.0536 0.0536 0.0536 0.2 0.0020 20 5.227942
+ -1.20379 0.604887 5.312 0 0 0.0 0.0 0.0
T This record has been completely revised.  It has been calibrated to simulate Blue grass seed
T planted Aug to Late Sept in three counties in the PNW, Umatilla, OR, Benton, WA, and Adams, WA.
T It will give reasonable fall growth after planting in those counties.  Issues with unpredictable re-growth and
T low establishment grow were corrected.  There is still a problem with the Res to Grain ratios.  Users will see high seed yield.
T DO NOT try to hand calibrate down to the 1000 lbs/ac average seed yield for the PNW.  Hand calibration
T (adjusting the biomass adjustment factor) can be done to get the needed fall growth.
T This crop should only be grown in the northern cool regions of the US.
T
T Dr. Fred Fox from the USDA ARS in Manhattan, KS has made most of the changes to the file.
T MAS 3-29-12.
#------------
D 16/07/01
O 03 Shredder, flail or rotary
+ 6.828365 .15 2.2351363 0.0 2.2351363 1.7881091 2.6821637
T Rusle Note: Rotary mower or flail shredder used to defoliate root crops such as sugarbeets before harvest or on cotton or
T other crop residue where crop has been previously harvested and
T residue is shredded  and spread flat..   10/3/01 DTL 11/15/01
T
T P42 is used to set a height of cut and removed the flattening P24.
T The 0.90 fraction used in RUSLE is by mass.  WEPS fraction is by height.
T It is not the same as RUSLE and cannot be used.
T Set the height to 2 inches per the conversation the Dave Lightle.  He said that most
T corn shredders are set to 2 inches.  Cotton shredding is much higher, use the 6 in shredder.
T A new operation was also created for root crop defoliation where all of the green tops
T are flatten to residue without killing the crop, "Shredder, beet topper".
T Kill crop was removed because of the interference with most harvest operations
T if used before harvest.  MAS 1-5-11
+
G 02 Biomass Manipulation
+ 1.0
P 42 Cut/Remove Biomass to Height (flags)
+ 0 0 1 0 0 50.800102 0 0 0.0
P 40 End crop Biomass Manipulation
#------------
D 30/07/02
O 04 Graze, rotational 50 pct removal
+ 9.353924E-8 0.4875
T Rotational Grazing system with 50% of growth removed with each grazing cycle.12-20-01 DTL
T Created 11-27-07 MAS
T
T Restructured processes.  Moved all grazing to O4 for energy and stir cal.
T
T Crop removal (green standing) is cal by using Rusle factors
T Port of Tt biomas affected (%)-(Port of Tt biomas affected (%))x(Portion of affected left on surface (%)
T Graze, continous Example: 0.3-(0.3 x 0.5) = 0.15
T
T Flattening Residue is cal by using Rusle Factors
T Port of Tt biomas affected (%) x Portion of affected left on surface (%)
T Graze, continous Example 0.3 x 0.5 = 0.15
T This value was used for the Mod residue (Wheat) values were reduced by 10% or increased by 10% of the value for each residue class.
T MAS 4-2-08
T Changed stem removal from 0.5 to 0 to prevent the stand from thining.  MAS 1-6-11
T Changed reports to include only the current green crop biomass.  Multiple report values are confusing users.  MAS 6-21-11
+
G 02 Biomass Manipulation
+ 1
P 62 Remove (by age pool) Plant/Residue Material
+ 1 0 1 0 1 1 0 0.5 0.5 0.0 0.0 0.0
P 62 Remove (by age pool) Plant/Residue Material
+ 0 0 1 0 2 4 2 .05 .05 .05 0.0 0.0
P 62 Remove (by age pool) Plant/Residue Material
+ 0 0 1 0 1 4 2 0.1 .1 0.1 0 0
P 24 Flatten Standing Biomass
+ 1 0.08 0.075 0.07 0.01 0.01
#------------
D 07/08/03
O 04 Graze, rotational 50 pct removal
+ 9.353924E-8 0.4875
T Rotational Grazing system with 50% of growth removed with each grazing cycle.12-20-01 DTL
T Created 11-27-07 MAS
T
T Restructured processes.  Moved all grazing to O4 for energy and stir cal.
T
T Crop removal (green standing) is cal by using Rusle factors
T Port of Tt biomas affected (%)-(Port of Tt biomas affected (%))x(Portion of affected left on surface (%)
T Graze, continous Example: 0.3-(0.3 x 0.5) = 0.15
T
T Flattening Residue is cal by using Rusle Factors
T Port of Tt biomas affected (%) x Portion of affected left on surface (%)
T Graze, continous Example 0.3 x 0.5 = 0.15
T This value was used for the Mod residue (Wheat) values were reduced by 10% or increased by 10% of the value for each residue class.
T MAS 4-2-08
T Changed stem removal from 0.5 to 0 to prevent the stand from thining.  MAS 1-6-11
T Changed reports to include only the current green crop biomass.  Multiple report values are confusing users.  MAS 6-21-11
+
G 02 Biomass Manipulation
+ 1
P 62 Remove (by age pool) Plant/Residue Material
+ 1 0 1 0 1 1 0 0.5 0.5 0.0 0.0 0.0
P 62 Remove (by age pool) Plant/Residue Material
+ 0 0 1 0 2 4 2 .05 .05 .05 0.0 0.0
P 62 Remove (by age pool) Plant/Residue Material
+ 0 0 1 0 1 4 2 0.1 .1 0.1 0 0
P 24 Flatten Standing Biomass
+ 1 0.08 0.075 0.07 0.01 0.01
#------------
D 30/09/03
O 04 Graze, rotational 50 pct removal
+ 9.353924E-8 0.4875
T Rotational Grazing system with 50% of growth removed with each grazing cycle.12-20-01 DTL
T Created 11-27-07 MAS
T
T Restructured processes.  Moved all grazing to O4 for energy and stir cal.
T
T Crop removal (green standing) is cal by using Rusle factors
T Port of Tt biomas affected (%)-(Port of Tt biomas affected (%))x(Portion of affected left on surface (%)
T Graze, continous Example: 0.3-(0.3 x 0.5) = 0.15
T
T Flattening Residue is cal by using Rusle Factors
T Port of Tt biomas affected (%) x Portion of affected left on surface (%)
T Graze, continous Example 0.3 x 0.5 = 0.15
T This value was used for the Mod residue (Wheat) values were reduced by 10% or increased by 10% of the value for each residue class.
T MAS 4-2-08
T Changed stem removal from 0.5 to 0 to prevent the stand from thining.  MAS 1-6-11
T Changed reports to include only the current green crop biomass.  Multiple report values are confusing users.  MAS 6-21-11
+
G 02 Biomass Manipulation
+ 1
P 62 Remove (by age pool) Plant/Residue Material
+ 1 0 1 0 1 1 0 0.5 0.5 0.0 0.0 0.0
P 62 Remove (by age pool) Plant/Residue Material
+ 0 0 1 0 2 4 2 .05 .05 .05 0.0 0.0
P 62 Remove (by age pool) Plant/Residue Material
+ 0 0 1 0 1 4 2 0.1 .1 0.1 0 0
P 24 Flatten Standing Biomass
+ 1 0.08 0.075 0.07 0.01 0.01
#------------
D 18/05/04
O 04 Graze, rotational 50 pct removal
+ 9.353924E-8 0.4875
T Rotational Grazing system with 50% of growth removed with each grazing cycle.12-20-01 DTL
T Created 11-27-07 MAS
T
T Restructured processes.  Moved all grazing to O4 for energy and stir cal.
T
T Crop removal (green standing) is cal by using Rusle factors
T Port of Tt biomas affected (%)-(Port of Tt biomas affected (%))x(Portion of affected left on surface (%)
T Graze, continous Example: 0.3-(0.3 x 0.5) = 0.15
T
T Flattening Residue is cal by using Rusle Factors
T Port of Tt biomas affected (%) x Portion of affected left on surface (%)
T Graze, continous Example 0.3 x 0.5 = 0.15
T This value was used for the Mod residue (Wheat) values were reduced by 10% or increased by 10% of the value for each residue class.
T MAS 4-2-08
T Changed stem removal from 0.5 to 0 to prevent the stand from thining.  MAS 1-6-11
T Changed reports to include only the current green crop biomass.  Multiple report values are confusing users.  MAS 6-21-11
+
G 02 Biomass Manipulation
+ 1
P 62 Remove (by age pool) Plant/Residue Material
+ 1 0 1 0 1 1 0 0.5 0.5 0.0 0.0 0.0
P 62 Remove (by age pool) Plant/Residue Material
+ 0 0 1 0 2 4 2 .05 .05 .05 0.0 0.0
P 62 Remove (by age pool) Plant/Residue Material
+ 0 0 1 0 1 4 2 0.1 .1 0.1 0 0
P 24 Flatten Standing Biomass
+ 1 0.08 0.075 0.07 0.01 0.01
#------------
D 23/07/04
O 04 Graze, rotational 50 pct removal
+ 9.353924E-8 0.4875
T Rotational Grazing system with 50% of growth removed with each grazing cycle.12-20-01 DTL
T Created 11-27-07 MAS
T
T Restructured processes.  Moved all grazing to O4 for energy and stir cal.
T
T Crop removal (green standing) is cal by using Rusle factors
T Port of Tt biomas affected (%)-(Port of Tt biomas affected (%))x(Portion of affected left on surface (%)
T Graze, continous Example: 0.3-(0.3 x 0.5) = 0.15
T
T Flattening Residue is cal by using Rusle Factors
T Port of Tt biomas affected (%) x Portion of affected left on surface (%)
T Graze, continous Example 0.3 x 0.5 = 0.15
T This value was used for the Mod residue (Wheat) values were reduced by 10% or increased by 10% of the value for each residue class.
T MAS 4-2-08
T Changed stem removal from 0.5 to 0 to prevent the stand from thining.  MAS 1-6-11
T Changed reports to include only the current green crop biomass.  Multiple report values are confusing users.  MAS 6-21-11
+
G 02 Biomass Manipulation
+ 1
P 62 Remove (by age pool) Plant/Residue Material
+ 1 0 1 0 1 1 0 0.5 0.5 0.0 0.0 0.0
P 62 Remove (by age pool) Plant/Residue Material
+ 0 0 1 0 2 4 2 .05 .05 .05 0.0 0.0
P 62 Remove (by age pool) Plant/Residue Material
+ 0 0 1 0 1 4 2 0.1 .1 0.1 0 0
P 24 Flatten Standing Biomass
+ 1 0.08 0.075 0.07 0.01 0.01
#------------
D 23/09/04
O 04 Graze, rotational 50 pct removal
+ 9.353924E-8 0.4875
T Rotational Grazing system with 50% of growth removed with each grazing cycle.12-20-01 DTL
T Created 11-27-07 MAS
T
T Restructured processes.  Moved all grazing to O4 for energy and stir cal.
T
T Crop removal (green standing) is cal by using Rusle factors
T Port of Tt biomas affected (%)-(Port of Tt biomas affected (%))x(Portion of affected left on surface (%)
T Graze, continous Example: 0.3-(0.3 x 0.5) = 0.15
T
T Flattening Residue is cal by using Rusle Factors
T Port of Tt biomas affected (%) x Portion of affected left on surface (%)
T Graze, continous Example 0.3 x 0.5 = 0.15
T This value was used for the Mod residue (Wheat) values were reduced by 10% or increased by 10% of the value for each residue class.
T MAS 4-2-08
T Changed stem removal from 0.5 to 0 to prevent the stand from thining.  MAS 1-6-11
T Changed reports to include only the current green crop biomass.  Multiple report values are confusing users.  MAS 6-21-11
+
G 02 Biomass Manipulation
+ 1
P 62 Remove (by age pool) Plant/Residue Material
+ 1 0 1 0 1 1 0 0.5 0.5 0.0 0.0 0.0
P 62 Remove (by age pool) Plant/Residue Material
+ 0 0 1 0 2 4 2 .05 .05 .05 0.0 0.0
P 62 Remove (by age pool) Plant/Residue Material
+ 0 0 1 0 1 4 2 0.1 .1 0.1 0 0
P 24 Flatten Standing Biomass
+ 1 0.08 0.075 0.07 0.01 0.01
#------------
*END
*EOF
