Version: 1.5
*START 1
N Originating Program: RUSLE2
N Skel Format Version: 1.1
N This management file was originally converted from the NRCS standard XML format on - Thu Jun 21 11:13:36 PDT 2012
N This management file was updated to contain the most current crop and operation records for WEPS on - Tue Jun 26 15:43:35 PDT 2012
N This management file was updated to contain the most current crop and operation records for WEPS on - Tue Dec 17 19:26:37 CST 2013
#------------
D 10/04/01
O 03 Chisel, twisted shovel
+ 10.289317 65 2.9056773 0.0 2.9056773 1.5645955 2.9056773
T This is a stanard 3 inch twisted point chisel plow.  This is a 12 in sp machine placed staggered on three tool bars. MAS 6-4-09
+
G 01 Tillage
+ 165.10033 0.9 1.0 165.10033 101.600204 203.20041
P 01 Break Crust
P 02 Random Roughness
+ 1 48.260098
P 05 Ridges and Dikes
+ 1 152.4003 304.8006 101.600204 0.0 0.0
P 11 Aggregate Crushing
+ 2.4 -2.0
P 12 Soil Loosening
+ 0.85
P 13 Soil Layer Mixing
+ 0.42
P 31 Kill or Defoliate Growing Crop
+ 2
P 40 End crop Biomass Manipulation
P 24 Flatten Standing Biomass
+ 0 0.85 0.8 0.7 0.6 1.0
P 25 Bury Flat Biomass
+ 1 0.9 0.8 0.75 0.6 0.93
P 26 Resurface Buried Biomass
+ 0.05 0.06 0.07 0.15 0.05
P 34 Change Standing Biomass Fall Rate
+ 7 3.0 2.5 2.0 1.5 1.0
+ 0.5 0.6 0.7 0.8 1.0
#------------
D 20/04/01
O 04 Fert applic. surface broadcast
+ 1.4966278 0.0609375
T R2 Notes: Broadcast fertilizer spreader.  Wheel traffic only.  rev 082107 DTL
T
T Added to DB 4-12-12 MAS
+
G 01 Tillage
+ 0.0 0 0.05 0.0 0.0 0.0
P 01 Break Crust
P 02 Random Roughness
+ 1 8.8900175
P 11 Aggregate Crushing
+ 4.3 2.0
P 24 Flatten Standing Biomass
+ 0 0.25 0.2 0.15 0.1 1.0
P 26 Resurface Buried Biomass
+ 0.07 0.08 0.1 0.12 0.07
P 34 Change Standing Biomass Fall Rate
+ 0 1.0 1.0 1.0 1.0 1.0
+ 1.0 1.0 1.0 1.0 1.0
#------------
D 20/04/01
O 03 Disk, tandem heavy primary op
+ 7.0154433 39 2.2351363 0.0 2.2351363 1.3410819 2.6821637
T 11-12in. Spacing, Front and Rear
T Recommended for primary tillage in medium to heavy soils
T Excellent residue-handling capability. MAS 10-26-06
+
G 01 Tillage
+ 152.4003 1.0 1.0 152.4003 101.600204 177.80035
P 01 Break Crust
P 02 Random Roughness
+ 1 38.100075
P 05 Ridges and Dikes
+ 1 101.600204 279.40057 0.0 0.0 0.0
P 11 Aggregate Crushing
+ 2.8 0.75
P 12 Soil Loosening
+ 0.9
P 13 Soil Layer Mixing
+ 0.4
P 31 Kill or Defoliate Growing Crop
+ 2
P 40 End crop Biomass Manipulation
P 24 Flatten Standing Biomass
+ 0 1.0 0.9 0.8 0.5 1.0
P 25 Bury Flat Biomass
+ 1 0.95 0.85 0.8 0.6 0.95
P 26 Resurface Buried Biomass
+ 0.05 0.06 0.07 0.08 0.05
P 34 Change Standing Biomass Fall Rate
+ 7 3.0 2.5 2.0 1.5 1.0
+ 0.5 0.6 0.7 0.8 1.0
#------------
D 25/04/01
O 03 Bedder, hipper, disk hiller
+ 4.2092657 26 2.0116227 0.0 2.0116227 1.5645955 2.2351363
T This is an 8 in high tool to reform beds from RUSLE 6-7-01 DTL
T
T Corrected the tillage depths and other residue values 11-1-11
+
G 01 Tillage
+ 101.600204 0.9 1.0 101.600204 50.800102 127.00025
P 01 Break Crust
P 02 Random Roughness
+ 1 15.240031
P 11 Aggregate Crushing
+ 3.0 2.0
P 12 Soil Loosening
+ 0.75
P 13 Soil Layer Mixing
+ 0.75
P 05 Ridges and Dikes
+ 1 203.20041 760.0 381.00076 0.0 0.0
P 31 Kill or Defoliate Growing Crop
+ 2
P 40 End crop Biomass Manipulation
P 24 Flatten Standing Biomass
+ 0 1 0.90 0.9 0.5 1.00
P 25 Bury Flat Biomass
+ 1 0.95 0.92 0.85 0.5 0.6
P 26 Resurface Buried Biomass
+ 0.02 0.02 0.02 0.05 0.03
P 34 Change Standing Biomass Fall Rate
+ 7 3.0 2.5 2.0 1.5 1.0
+ 0.5 0.6 0.7 0.8 1.0
#------------
D 25/04/01
O 03 Bed shaper
+ 3.554491 19.5 2.2351363 0.0 2.2351363 1.5645955 2.9056773
T RUSLE Notes: Bed shaping operation on existing beds.  May include drip tape installation. 10/28/01 DTL
T Cloned 2-15-07 MAS
T G2 was added into file in front of the flattening (P24), burial (P25), and resurfacing (P26) factors because the area affected is less than 1.0 and
T the RUSLE values were normalized to 1.0.  This change will imulate the correct residue changes based on the method set forth in RUSLE.
T RUSLE's factors have been redused to based on the area affected.
T The stalk fall rate factor (P34) was moved ahead of the new (G2) factor to set the fall rate to the  less than 1.0 area affected.  8/8/07 MAS
+
G 01 Tillage
+ 101.600204 .6 .75 101.600204 76.20015 152.4003
P 01 Break Crust
P 02 Random Roughness
+ 1 15.240031
P 11 Aggregate Crushing
+ 3.0 -0.22
P 12 Soil Loosening
+ 0.75
P 13 Soil Layer Mixing
+ 0.05
P 05 Ridges and Dikes
+ 1 203.20041 760.0 381.00076 0.0 0.0
P 34 Change Standing Biomass Fall Rate
+ 7 3.0 2.5 2.0 1.5 1.0
+ 0.5 0.6 0.7 0.8 1.0
G 02 Biomass Manipulation
+ 1.0
P 24 Flatten Standing Biomass
+ 0 0.5 0.45 0.4 0.3 1.00
P 25 Bury Flat Biomass
+ 1 0.38 0.3 0.23 0.2 0.28
P 26 Resurface Buried Biomass
+ 0.02 0.02 0.02 0.02 0.02
#------------
D 28/04/01
O 03 Plastic mulch applicator
+ 2.5255597 1.56 0.89405453 0.0 0.89405453 0.44702727 1.7881091
T Plastic mulch application covering 100% of the surface.  May include drip tape installation. 11/08/01 DTL
T
T This operation follows tillage  for crops such as strawberries and green pepers.
T Uses crop names with small letter to indicate mulch type and high mass weights of woody mulch type.
T MAS 6-9-09
+
G 01 Tillage
+ 76.20015 .1 .2 76.20015 50.800102 101.600204
P 01 Break Crust
P 02 Random Roughness
+ 1 15.240031
P 05 Ridges and Dikes
+ 1 50.800102 1422.4028 1016.002 0.0 0.0
P 11 Aggregate Crushing
+ 3.0 -0.22
P 25 Bury Flat Biomass
+ 1 0.1 0.08 0.06 0.052 0.076
P 26 Resurface Buried Biomass
+ 0.02 0.02 0.02 0.05 0.03
P 34 Change Standing Biomass Fall Rate
+ 7 3.0 2.5 2.0 1.5 1.0
+ 0.5 0.6 0.7 0.8 1.0
G 03 Crop Name
+ plastic mulch
P 65 Add Crop Residue Amounts
+ 0.0 0.0 0.0 0.22417001 4
+ 0.0 0.0 0.0 0.0
+ .0001 .0001 .0001 .001 0.169 0.0050 17.1 6.244982
+ -0.604267 0.711259
T Enter crop notes here.
#------------
D 28/04/01
O 03 Planting, manual
+ 0.0 .78 0.44702727 0.0 0.44702727 0.44702727 0.44702727
T Manual planting with hoe or shovel.  11/16/05 DTL
T G2 was added into file in front of the flattening (P24), burial (P25), and resurfacing (P26) factors because the area affected is less than 1.0 and
T the RUSLE values were normalized to 1.0.  This change will imulate the correct residue changes based on the method set forth in RUSLE.
T RUSLE's factors have been redused to based on the area affected.
T The stalk fall rate factor (P34) was moved ahead of the new (G2) factor to set the fall rate to the less than 1.0 area affected.  8/7/07 MAS
+
G 01 Tillage
+ 50.800102 .5 .3 50.800102 25.400051 76.20015
P 01 Break Crust
P 02 Random Roughness
+ 1 22.860044
P 05 Ridges and Dikes
+ 1 25.400051 762.0015 609.6012 0.0 0.0
P 11 Aggregate Crushing
+ 2.8 2
P 12 Soil Loosening
+ .3
P 13 Soil Layer Mixing
+ .3
P 34 Change Standing Biomass Fall Rate
+ 7 3.0 2.5 2.0 1.5 1.0
+ 0.5 0.6 0.7 0.8 1.0
G 02 Biomass Manipulation
+ 1.0
P 25 Bury Flat Biomass
+ 1 0.15 0.12 0.09 0.078 0.01
P 26 Resurface Buried Biomass
+ .007 .008 .01 .12 0.01
G 03 Crop Name
+ Tomato, fresh mkt
P 51 Seeding Configuration
+ 1 0.0 2
+ 2.0 1.0 1 300 1.0 1.0 0
+ cwt/ac
+ 94.0 89.3 4 1.0 0.65 0.95
+ 0.8 0.025 1.5 10.0 27.0 0 70 750.0
+ -1.0 -4.0 0.15 0.95 0.0 30.0
+ -0.0198 0.6575 0.4807 -0.1453 -0.336 1.3726 0.5408 0.1081
+ 0.4807 -0.1453 3.08 1.0 31.1 0.01 1 1.1170388
+ 1700.0 1700.0 3.0 0.03 0.0 0.0 0.0 1
+ 0.02 0.02 0.02 0.02 0.2 0.0050 20.0 2.7
+ -1.20379 0.604887 0.0767 0.012329351 0.0 0.0 0.0 0.0
T This records comes from ARS tomato transplant record and has the yield,
T Residue yield ration and the yield intercept changed to RUSLE values MAS 3-6-07
T Made changes as Fred instructed, mass of planting MAS 3/15/07
#------------
D 20/05/01
O 04 Sprayer, insecticide post emergence
+ 1.2160101 0.15
T Spray pest control chemicals on growing crop.   Crop is not killed.  11/17/01 DTL
T
T Added to the DB.  This assumes no crop flattening.  4-5-12 MAS
+
#------------
D 15/06/01
O 04 Sprayer, insecticide post emergence
+ 1.2160101 0.15
T Spray pest control chemicals on growing crop.   Crop is not killed.  11/17/01 DTL
T
T Added to the DB.  This assumes no crop flattening.  4-5-12 MAS
+
#------------
D 15/07/01
O 04 Harvest, hand pick
+ 3.2738733 0.15
T Hand pick lettuce or similar crops or to represent one final picking of fruit or berry crops.
T Do not use for multiple pickings of fruit or berry crops unless a regrowth vegetation file representing
T regrowth between pickings is available in the database to be called in.
T This is not the case for strawberries.  12132011 DTL
T Added 3/29/07 MAS
T Reworked the values MAS 2-24-09
T Added the change to flat on the crop type.  8-27-10
T This operation takes all of the yield, and can be used to calibrate the yield. 12-27-11 MAS
T Adjusted the Energy use to 0.000000010 gal/ac  2-23-12
T
T Changed the fuel use from 0.000000010 to 0.36 g/ac 4-17-12 MAS
+
G 02 Biomass Manipulation
+ 1.0
P 31 Kill or Defoliate Growing Crop
+ 0
P 62 Remove (by age pool) Plant/Residue Material
+ 1 1 0 1 3 3 2 1.0 0.0 0.0 0.0 0.0
P 40 End crop Biomass Manipulation
#------------
D 30/07/01
O 04 Harvest, hand pick
+ 3.2738733 0.15
T Hand pick lettuce or similar crops or to represent one final picking of fruit or berry crops.
T Do not use for multiple pickings of fruit or berry crops unless a regrowth vegetation file representing
T regrowth between pickings is available in the database to be called in.
T This is not the case for strawberries.  12132011 DTL
T Added 3/29/07 MAS
T Reworked the values MAS 2-24-09
T Added the change to flat on the crop type.  8-27-10
T This operation takes all of the yield, and can be used to calibrate the yield. 12-27-11 MAS
T Adjusted the Energy use to 0.000000010 gal/ac  2-23-12
T
T Changed the fuel use from 0.000000010 to 0.36 g/ac 4-17-12 MAS
+
G 02 Biomass Manipulation
+ 1.0
P 31 Kill or Defoliate Growing Crop
+ 0
P 62 Remove (by age pool) Plant/Residue Material
+ 1 1 0 1 3 3 2 1.0 0.0 0.0 0.0 0.0
P 40 End crop Biomass Manipulation
#------------
D 01/10/01
O 04 Harvest, hand pick
+ 3.2738733 0.15
T Hand pick lettuce or similar crops or to represent one final picking of fruit or berry crops.
T Do not use for multiple pickings of fruit or berry crops unless a regrowth vegetation file representing
T regrowth between pickings is available in the database to be called in.
T This is not the case for strawberries.  12132011 DTL
T Added 3/29/07 MAS
T Reworked the values MAS 2-24-09
T Added the change to flat on the crop type.  8-27-10
T This operation takes all of the yield, and can be used to calibrate the yield. 12-27-11 MAS
T Adjusted the Energy use to 0.000000010 gal/ac  2-23-12
T
T Changed the fuel use from 0.000000010 to 0.36 g/ac 4-17-12 MAS
+
G 02 Biomass Manipulation
+ 1.0
P 31 Kill or Defoliate Growing Crop
+ 0
P 62 Remove (by age pool) Plant/Residue Material
+ 1 1 0 1 3 3 2 1.0 0.0 0.0 0.0 0.0
P 40 End crop Biomass Manipulation
#------------
D 05/10/01
O 04 Plastic mulch, remove
+ 3.6480303 .52
T Added a kill crop process to cause the crop residue to be changed after the picking operations  MAS 1-22-08
+
G 02 Biomass Manipulation
+ 1
P 62 Remove (by age pool) Plant/Residue Material
+ 0 0 1 0 2 4 2 1 1 1 0 0
P 31 Kill or Defoliate Growing Crop
+ 2
P 40 End crop Biomass Manipulation
#------------
D 01/11/01
O 04 Begin weed growth
+ 9.353924E-8 0
T Enter Operation notes here
+
G 03 Crop Name
+ Weeds, less than 3 mo growth
P 51 Seeding Configuration
+ 0 0.0 0
+ 9 1 0 500 1 1 2
+ lbs/ac
+ 0 8930.0 4 1 0.65 0.95
+ 0.3048037 0.025 0.8 0 18.199999999999996 0 75 1100
+ -5 -15 0.01 0.95 0 19
+ 0.3128 0.576 0.6898 -0.1533 0 1 1.1 0.01
+ 0.4995 -0.0944 0.1 1 30 0.05 0 0.2562663
+ 500 500 1.5 0.01 0 0 0 1
+ 0.02 0.02 0.02 0.02 0.2 0.0050 20 5.227942
+ -1.20379 0.604887 0 0 0 0.0 0.0 0.0
T This record was replaced by Collard, greens.  The old record using winter peas did not grow in the south.
T The collard green produce 1400 lbs of biomass in the N part of N Dakota and 2356 lbs S FL.
T Edits were made to show just biomass above ground produced.  MAS 11-16-10
#------------
*END
*EOF
