Version: 1.5
*START 1
N Originating Program: RUSLE2
N Skel Format Version: 1.1
N This management file was originally converted from the NRCS standard XML format on - Thu Jun 21 11:11:55 PDT 2012
N This management file was updated to contain the most current crop and operation records for WEPS on - Tue Jun 26 15:45:43 PDT 2012
N This management file was updated to contain the most current crop and operation records for WEPS on - Tue Dec 17 19:28:58 CST 2013
#------------
D 10/04/01
O 03 Cultivator, field 6-12 in sweeps
+ 6.921904 26 2.2351363 0.0 2.2351363 1.5645955 2.9056773
T Corrected Speed of operation numbers 11-1-11 MAS
+
G 01 Tillage
+ 101.600204 0.4 1.0 101.600204 50.800102 152.4003
P 01 Break Crust
P 02 Random Roughness
+ 1 15.240031
P 05 Ridges and Dikes
+ 1 50.800102 228.60045 0.0 0.0 0.0
P 11 Aggregate Crushing
+ 3.0 1.0
P 12 Soil Loosening
+ 0.65
P 13 Soil Layer Mixing
+ 0.3
P 31 Kill or Defoliate Growing Crop
+ 2
P 40 End crop Biomass Manipulation
P 24 Flatten Standing Biomass
+ 0 0.7 0.4 0.3 0.2 1.0
P 25 Bury Flat Biomass
+ 1 0.4 0.35 0.3 0.2 0.85
P 26 Resurface Buried Biomass
+ 0.05 0.06 0.07 0.2 0.05
P 34 Change Standing Biomass Fall Rate
+ 7 3.0 2.5 2.0 1.5 1.0
+ 0.5 0.6 0.7 0.8 1.0
#------------
D 10/04/01
O 03 Disk, tandem light finishing
+ 3.7415698 19.5 2.2351363 0.0 2.2351363 1.3410819 2.6821637
T 6/8/01 DTL RUSLE.  7in sp.  This is tool used to finish a seedbed.  MAS 10-26-06
+
G 01 Tillage
+ 101.600204 0.5 1.0 101.600204 76.20015 127.00026
P 01 Break Crust
P 02 Random Roughness
+ 1 15.240031
P 05 Ridges and Dikes
+ 1 12.700026 177.80035 0.0 0.0 0.0
P 11 Aggregate Crushing
+ 2.8 0.75
P 12 Soil Loosening
+ 0.75
P 13 Soil Layer Mixing
+ 0.35
P 31 Kill or Defoliate Growing Crop
+ 2
P 40 End crop Biomass Manipulation
P 24 Flatten Standing Biomass
+ 0 0.85 0.7 0.6 0.5 1.0
P 25 Bury Flat Biomass
+ 1 0.73 0.63 0.55 0.4 0.73
P 26 Resurface Buried Biomass
+ 0.02 0.04 0.02 0.05 0.02
P 34 Change Standing Biomass Fall Rate
+ 7 3.0 2.5 2.0 1.5 1.0
+ 0.5 0.6 0.7 0.8 1.0
#------------
D 25/04/01
O 03 Planter, double disk opnr
+ 4.1157265 2.4375 2.2351363 0.0 2.2351363 1.5645955 2.9056773
T This is a standard planter on 30 in sp with a 1 in ridge.  Created in RUSLE 6/7/01.  MAS 8/7/07
T G2 was added into file in front of the flattening (P24), burial (P25), and resurfacing (P26) factors because the area affected is less than 1.0 and
T the RUSLE values were normalized to 1.0.  This change will imulate the correct residue changes based on the method set forth in RUSLE.
T RUSLE's factors have been redused to based on the area affected.
T The stalk fall rate factor (P34) was moved ahead of the new (G2) factor to set the fall rate to the less than 1.0 area affected.  8/7/07 MAS
+
G 01 Tillage
+ 63.500126 0.5 .15 63.500126 50.800102 101.600204
P 01 Break Crust
P 02 Random Roughness
+ 1 10.160021
P 05 Ridges and Dikes
+ 1 50.800102 762.0015 635.0013 0.0 0.0
P 11 Aggregate Crushing
+ 2.8 0.75
P 12 Soil Loosening
+ 0.6
P 13 Soil Layer Mixing
+ 0.35
P 34 Change Standing Biomass Fall Rate
+ 7 3.0 2.5 2.0 1.5 1.0
+ 0.5 0.6 0.7 0.8 1.0
G 02 Biomass Manipulation
+ 1.0
P 24 Flatten Standing Biomass
+ 0 .3 .25 .2 0.1 1.0
P 25 Bury Flat Biomass
+ 1 .0525 0.0375 .03 .015 .03
P 26 Resurface Buried Biomass
+ .01 .01 .01 .02 .01
G 03 Crop Name
+ Corn, silage
P 51 Seeding Configuration
+ 1 0.0 2
+ 6.0 1.0 1 23 1.0 1.0 2
+ ton/ac
+ 65.0 4.465 4 1.0 0.65 0.8
+ 2.5 0.05 1.5240185 10.0 30.0 0 100 1700.0
+ -5.0 -15.0 0.01 0.05 0.0 40.0
+ 0.0031 0.9233 0.3266 -0.044 0.0 0.976 0.511 0.0287
+ 0.3266 -0.044 0.22259772 0.72 17.4 0.05 0 0.9
+ 333.33334 333.33334 3.0 0.03 0.0 0.0 0.0 3
+ 0.016 0.016 0.016 0.01 0.153 0.01 20.0 3.3812115
+ -1.20379 0.604887 0.3081 0.21615593 0.0 0.0 0.0 0.0
T corn silage 23 ton yield, 30" rows  Columbia, Mo DTL
T
T This record was cloned from ARS records and the revenant data adjusted to RUSLE values.
T The Biomass Conv Factor was changed from 40 to 47 based on runs made in Clovis, NM with full irrigation.
T MAS 9-27-07
T
T R2 Note - Rev residue : yield ratio 091108 DTL with 35% dry matter content. rev biomass-yield ratio 032012 DTL
T
T Added the Yield intercept and Res:Yield ratio. 
T If a cover crop is inter planted into Corn, silage users must use a harvest that call in a growing
T cover crop.  Only one crop can be grown at a time in WEPS. 4-3-12 MAS
#------------
D 25/04/01
O 04 Sprayer, pre-emergence
+ 1.2160101 .15
T Spray pest control chemicals on growing crop.  Crop is not killed.
T In the MCREW management screen the user must select the kind of weeds killed in the growing crop as external residue.   080404 DTL
T Cloned from Defoliate (spray) crop.oprn, Changed the P31 to No crop kill and added G4 to add material to field MAS 9-28-06
+
G 03 Crop Name
+ weed residue; 0-3 mo
P 65 Add Crop Residue Amounts
+ 0.0 0.0 0.0 0.0 1
+ 0.0 0.0 0.0056042504 152.4003
+ 0.025 0.025 0.025 0.025 0.169 0.0050 17.1 5.227942
+ -1.20379 0.604887
T Enter crop notes here.
#------------
D 20/05/01
O 03 Cultivator, row 1 in ridge
+ 5.799433 14.63 2.2351363 0.0 2.2351363 0.89405453 2.4586499
T RUSLE:Row crop cultivator w/ sweeps leaving a 1" ridge 05-14-02 DTL
T G2 was added into file in front of the flattening (P24), burial (P25), and resurfacing (P26) factors because the area affected is less than 1.0 and
T the RUSLE values were normalized to 1.0.  This change will imulate the correct residue changes based on the method set forth in RUSLE.
T RUSLE's factors have been redused to based on the area affected.
T The stalk fall rate factor (P34) was moved ahead of the new (G2) factor to set the fall rate to the less than 1.0 area affected.  8/8/07 MAS
+
G 01 Tillage
+ 76.20015 0.5 .75 76.20015 50.800102 101.600204
P 01 Break Crust
P 02 Random Roughness
+ 1 7.6200156
P 05 Ridges and Dikes
+ 1 25.400051 762.0015 0.0 0.0 0.0
P 11 Aggregate Crushing
+ 3.0 1.0
P 12 Soil Loosening
+ 0.75
P 13 Soil Layer Mixing
+ 0.35
P 34 Change Standing Biomass Fall Rate
+ 4 3.0 2.5 2.0 1.5 1.0
+ 0.5 0.6 0.7 0.8 1.0
G 02 Biomass Manipulation
+ 1.0
P 24 Flatten Standing Biomass
+ 14 0.7 0.3 0.3 0.1 1.0
P 25 Bury Flat Biomass
+ 1 .57 0.5 0.44 0.32 0.64
P 26 Resurface Buried Biomass
+ 0.01 0.01 0.01 0.01 0.01
#------------
D 20/06/01
O 04 Fert applic. side-dress, liquid
+ 1.2160101 0.15
T Spray or dribble side-dress application of fertilizer into row crop.   Crop is not affected.
T Created from DTL's Sprayer, insecticide post emergence" record.  04/13/11 GGF
T
T Added to WEPS 3-1-12
+ 
#------------
D 20/06/01
O 03 Cultivator, row 1 in ridge
+ 5.799433 14.63 2.2351363 0.0 2.2351363 0.89405453 2.4586499
T RUSLE:Row crop cultivator w/ sweeps leaving a 1" ridge 05-14-02 DTL
T G2 was added into file in front of the flattening (P24), burial (P25), and resurfacing (P26) factors because the area affected is less than 1.0 and
T the RUSLE values were normalized to 1.0.  This change will imulate the correct residue changes based on the method set forth in RUSLE.
T RUSLE's factors have been redused to based on the area affected.
T The stalk fall rate factor (P34) was moved ahead of the new (G2) factor to set the fall rate to the less than 1.0 area affected.  8/8/07 MAS
+
G 01 Tillage
+ 76.20015 0.5 .75 76.20015 50.800102 101.600204
P 01 Break Crust
P 02 Random Roughness
+ 1 7.6200156
P 05 Ridges and Dikes
+ 1 25.400051 762.0015 0.0 0.0 0.0
P 11 Aggregate Crushing
+ 3.0 1.0
P 12 Soil Loosening
+ 0.75
P 13 Soil Layer Mixing
+ 0.35
P 34 Change Standing Biomass Fall Rate
+ 4 3.0 2.5 2.0 1.5 1.0
+ 0.5 0.6 0.7 0.8 1.0
G 02 Biomass Manipulation
+ 1.0
P 24 Flatten Standing Biomass
+ 14 0.7 0.3 0.3 0.1 1.0
P 25 Bury Flat Biomass
+ 1 .57 0.5 0.44 0.32 0.64
P 26 Resurface Buried Biomass
+ 0.01 0.01 0.01 0.01 0.01
#------------
D 20/08/01
O 04 Sprayer, post emergence
+ 1.2160101 .15
T Spray pest control chemicals on growing crop.  Crop is not killed.
T In the MCREW management screen the user must select the kind of weeds killed in the growing crop as external residue.   080404 DTL
T Cloned from Defoliate (spray) crop.oprn, Changed the P31 to No crop kill and added G4 to add material to field MAS 9-28-06
T DO NOT LEAVE CROP COLUMN SET TO "no crop".  User must select the crop and then drill into the operation and specify the amount of weed
T mass that will be killed and turned into residue.
+
G 03 Crop Name
+ weed residue; 0-3 mo
P 65 Add Crop Residue Amounts
+ 0.0 0.0 0.0 0.028021252 1
+ 0.0 0.0 0.0056042504 152.4003
+ 0.025 0.025 0.025 0.025 0.169 0.0050 17.1 5.227942
+ -1.20379 0.604887
T Enter crop notes here.
#------------
D 05/09/01
O 04 Harvest, silage, kill crop
+ 8.886228 .15
T Use this operation  when the harvest will stop any regrowth.  It cuts to a 5 in ht. MAS 6-30-08
T
T ARS record - filename is:  Harvest Corn - silage (silage cutter).oprn
T This operation record is designed to represent a harvesting operation, e.g., a "silage cutter",
T that remove all of the above ground crop biomass above a specified cutting height.
T Examples would be cutting corn for silage and alfalfa for hay.
T This harvesting operation record removes all crop plant material above the specified cut height.
T The remaining above ground crop material below the specified cut height becomes standing residue
T for annual crops.  Perennial crops like alfalfa will automatically regrow.
T The default "Kill or Defoliate Growing Crop" parameter is set to kill annual crops but to allow
T regrowth of perennial crops.  Thus the default value is acceptable for perennial crops
T like alfalfa and most annual crops like corn harvested for silage.  There are situations where
T one might want to change this parameter value for specific types of crops and conditions.
T See additional info below in the "Detailed info regarding this operation record" section.
T No standing stalks (crop or residue) are flattened.  This record is assuming a row crop
T silage harvester, where the tires are tracking in between the rows.
T 200x	Created - Fred Fox
T Oct 31, 2005	Updated notes - Larry Wagner
T Detailed info regarding this operation record:
T This operation template has the "Kill or Defoliate Growing Crop" process parameter defaulting to
T "Annual crop killed, perennial crop regrows" value.  Thus the default value is acceptable for use
T with perennial crops like alfalfa and annual crops like corn harvested for silage.  However, if one
T intends to harvest (green chop) an annual crop that has the capacity to regrow after such a cutting,
T then one needs to change the value to "No crop killed" to allow the crop to regrow afterwards.
T Due to the way WEPS reports crop yields, the crop record selected for this type of harvesting
T operation should specify the "yield" component of the crop to be the "above ground stems, leaves
T and reproductive elements of  the plant".  This will ensure proper reporting of harvested yields
T by WEPS.  However, using a crop record that does not specify the "yield" component in this manner
T will not affect the erosion estimate or change any other simulation run results, except to incorrectly
T report the true "yield" component being removed from the field.  An example of a crop that may be
T harvested for two different types of "yield" components is corn.  There are corn crop records defined
T that specify the yield as the reproductive element (grain) and others that are defined for harvesting
T the crop as silage.
+
G 02 Biomass Manipulation
+ 1.0
P 31 Kill or Defoliate Growing Crop
+ 2
P 42 Cut/Remove Biomass to Height (flags)
+ 1 1 0 1 0 127.00025 1.0 1.0 1.0
P 34 Change Standing Biomass Fall Rate
+ 0 1.1 1.08 1.06 1.04 1.0
+ 1.0 1.0 1.0 1.0 1.0
P 40 End crop Biomass Manipulation
P 24 Flatten Standing Biomass
+ 0 0.0 0.0 0.0 0.0 0.0
#------------
D 15/10/01
O 03 Chisel, sweep shovel
+ 10.289317 45.5 2.2351363 0.0 2.2351363 1.5645955 2.9056773
T Enter Operation notes here
+
G 01 Tillage
+ 127.00026 0.85 1.0 127.00026 76.20015 177.80035
P 01 Break Crust
P 02 Random Roughness
+ 1 30.480062
P 05 Ridges and Dikes
+ 1 76.20015 381.00076 0.0 0.0 0.0
P 11 Aggregate Crushing
+ 2.4 -2.0
P 12 Soil Loosening
+ 0.75
P 13 Soil Layer Mixing
+ 0.33
P 31 Kill or Defoliate Growing Crop
+ 2
P 40 End crop Biomass Manipulation
P 24 Flatten Standing Biomass
+ 0 0.5 0.3 0.2 0.3 1.0
P 25 Bury Flat Biomass
+ 1 0.6 0.45 0.3 0.5 0.92
P 26 Resurface Buried Biomass
+ 0.05 0.06 0.07 0.2 0.05
P 34 Change Standing Biomass Fall Rate
+ 7 3.0 2.5 2.0 1.5 1.0
+ 0.5 0.6 0.7 0.8 1.0
#------------
D 16/10/01
O 04 Begin weed growth
+ 9.353924E-8 0
T Enter Operation notes here
+
G 03 Crop Name
+ Weeds, winter, Central
P 51 Seeding Configuration
+ 0 0.0 0
+ 9 1 0 1000 1 1 2
+ lbs/ac
+ 0 8930.0 4 1 0.65 0.95
+ 0.3048037 0.025 0.8 0 18.199999999999996 0 75 1100
+ -5 -15 0.01 0.95 0 19
+ 0.3128 0.576 0.6898 -0.1533 0 1 1.1 0.01
+ 0.4995 -0.0944 0.1 1 30 0.05 0 0.2562663
+ 500 500 1.5 0.01 0 0 0 1
+ 0.02 0.02 0.02 0.02 0.2 0.0050 20 5.227942
+ -1.20379 0.604887 0 0 0 0.0 0.0 0.0
T This record was replaced by Collard, greens.  The old record using winter peas did not grow in the south.
T The collard green produce 1400 lbs of biomass in the N part of N Dakota and 2356 lbs S FL.
T Edits were made to show just biomass above ground produced.  MAS 11-16-10
#------------
*END
*EOF
