Version: 1.5
*START 1
N Originating Program: RUSLE2
N Skel Format Version: 1.1
N This management file was originally converted from the NRCS standard XML format on - Thu Jun 21 11:15:46 PDT 2012
N This management file was updated to contain the most current crop and operation records for WEPS on - Tue Jun 26 15:41:26 PDT 2012
N This management file was updated to contain the most current crop and operation records for WEPS on - Tue Dec 17 19:24:31 CST 2013
#------------
D 20/03/01
O 04 Kill crop
+ 0.0 0
T Enter Operation notes here
+
G 02 Biomass Manipulation
+ 1.0
P 31 Kill or Defoliate Growing Crop
+ 2
P 40 End crop Biomass Manipulation
#------------
D 25/03/01
O 03 Chisel, twisted shovel
+ 10.289317 65 2.9056773 0.0 2.9056773 1.5645955 2.9056773
T This is a stanard 3 inch twisted point chisel plow.  This is a 12 in sp machine placed staggered on three tool bars. MAS 6-4-09
+
G 01 Tillage
+ 165.10033 0.9 1.0 165.10033 101.600204 203.20041
P 01 Break Crust
P 02 Random Roughness
+ 1 48.260098
P 05 Ridges and Dikes
+ 1 152.4003 304.8006 101.600204 0.0 0.0
P 11 Aggregate Crushing
+ 2.4 -2.0
P 12 Soil Loosening
+ 0.85
P 13 Soil Layer Mixing
+ 0.42
P 31 Kill or Defoliate Growing Crop
+ 2
P 40 End crop Biomass Manipulation
P 24 Flatten Standing Biomass
+ 0 0.85 0.8 0.7 0.6 1.0
P 25 Bury Flat Biomass
+ 1 0.9 0.8 0.75 0.6 0.93
P 26 Resurface Buried Biomass
+ 0.05 0.06 0.07 0.15 0.05
P 34 Change Standing Biomass Fall Rate
+ 7 3.0 2.5 2.0 1.5 1.0
+ 0.5 0.6 0.7 0.8 1.0
#------------
D 05/04/01
O 03 Disk, tandem secondary op
+ 4.4898834 32.5 2.2351363 0.0 2.2351363 1.3410819 2.6821637
T 9-in. Spacing, Front and Rear; Good for seedbed preparation/chemical incorporation in medium to heavy soils
T Works well in primary tillage in light to medium soils
T Provides good residue-handling capability.  MAS 10-26-06
+
G 01 Tillage
+ 127.00027 0.75 1.0 127.00026 76.20015 152.4003
P 01 Break Crust
P 02 Random Roughness
+ 1 15.240031
P 05 Ridges and Dikes
+ 1 50.800102 228.60046 0.0 0.0 0.0
P 11 Aggregate Crushing
+ 2.8 0.75
P 12 Soil Loosening
+ 0.85
P 13 Soil Layer Mixing
+ 0.4
P 31 Kill or Defoliate Growing Crop
+ 2
P 40 End crop Biomass Manipulation
P 24 Flatten Standing Biomass
+ 0 0.85 0.7 0.6 0.5 1.0
P 25 Bury Flat Biomass
+ 1 0.73 0.63 0.55 0.4 0.73
P 26 Resurface Buried Biomass
+ 0.02 0.04 0.02 0.05 0.02
P 34 Change Standing Biomass Fall Rate
+ 7 3.0 2.5 2.0 1.5 1.0
+ 0.5 0.6 0.7 0.8 1.0
#------------
D 10/04/01
O 04 Fert applic. surface broadcast
+ 1.4966278 0.0609375
T R2 Notes: Broadcast fertilizer spreader.  Wheel traffic only.  rev 082107 DTL
T
T Added to DB 4-12-12 MAS
+
G 01 Tillage
+ 0.0 0 0.05 0.0 0.0 0.0
P 01 Break Crust
P 02 Random Roughness
+ 1 8.8900175
P 11 Aggregate Crushing
+ 4.3 2.0
P 24 Flatten Standing Biomass
+ 0 0.25 0.2 0.15 0.1 1.0
P 26 Resurface Buried Biomass
+ 0.07 0.08 0.1 0.12 0.07
P 34 Change Standing Biomass Fall Rate
+ 0 1.0 1.0 1.0 1.0 1.0
+ 1.0 1.0 1.0 1.0 1.0
#------------
D 10/04/01
O 03 Disk, tandem light finishing
+ 3.7415698 19.5 2.2351363 0.0 2.2351363 1.3410819 2.6821637
T 6/8/01 DTL RUSLE.  7in sp.  This is tool used to finish a seedbed.  MAS 10-26-06
+
G 01 Tillage
+ 101.600204 0.5 1.0 101.600204 76.20015 127.00026
P 01 Break Crust
P 02 Random Roughness
+ 1 15.240031
P 05 Ridges and Dikes
+ 1 12.700026 177.80035 0.0 0.0 0.0
P 11 Aggregate Crushing
+ 2.8 0.75
P 12 Soil Loosening
+ 0.75
P 13 Soil Layer Mixing
+ 0.35
P 31 Kill or Defoliate Growing Crop
+ 2
P 40 End crop Biomass Manipulation
P 24 Flatten Standing Biomass
+ 0 0.85 0.7 0.6 0.5 1.0
P 25 Bury Flat Biomass
+ 1 0.73 0.63 0.55 0.4 0.73
P 26 Resurface Buried Biomass
+ 0.02 0.04 0.02 0.05 0.02
P 34 Change Standing Biomass Fall Rate
+ 7 3.0 2.5 2.0 1.5 1.0
+ 0.5 0.6 0.7 0.8 1.0
#------------
D 23/04/01
O 03 Harrow, spike tooth
+ 3.1803343 15.6 2.6821637 0.0 2.6821637 1.3410819 3.129191
T 6/7/01 DTL RUSLE MAS 10-26-06
+
G 01 Tillage
+ 50.800102 0.50 1.0 50.800102 25.400051 76.20015
P 01 Break Crust
P 02 Random Roughness
+ 1 10.160021
P 05 Ridges and Dikes
+ 1 25.400051 101.600204 6.350013 0.0 0.0
P 11 Aggregate Crushing
+ 3.0 -0.22
P 12 Soil Loosening
+ 0.6
P 13 Soil Layer Mixing
+ 0.2
P 31 Kill or Defoliate Growing Crop
+ 2
P 40 End crop Biomass Manipulation
P 24 Flatten Standing Biomass
+ 0 0.6 0.4 0.25 0.1 1.0
P 25 Bury Flat Biomass
+ 1 0.3 0.25 0.2 0.1 0.3
P 26 Resurface Buried Biomass
+ .01 0.01 .01 0.02 0.01
P 34 Change Standing Biomass Fall Rate
+ 7 3.0 2.5 2.0 1.5 1.0
+ 0.5 0.6 0.7 0.8 1.0
#------------
D 25/04/01
O 03 Planter, transplanter, vegetable
+ 7.4831395 3.12 0.89405453 0.0 0.89405453 0.44702727 1.3410819
T G2 was added into file in front of the flattening (P24), burial (P25), and resurfacing (P26) factors because the area affected is less than 1.0 and
T the RUSLE values were normalized to 1.0.  This change will imulate the correct residue changes based on the method set forth in RUSLE.
T RUSLE's factors have been redused to based on the area affected.
T The stalk fall rate factor (P34) was moved ahead of the new (G2) factor to set the fall rate to theless than 1.0 area affected.  8/7/07 MAS
T
T Changed the P5 to allow the preexisting ridges and furrows to set the ridge roughness.  MAS  12-30-2010
+
G 01 Tillage
+ 152.4003 0.4 0.2 152.4003 101.600204 203.20041
P 01 Break Crust
P 02 Random Roughness
+ 1 10.160021
P 05 Ridges and Dikes
+ 0 50.800102 762.0015 635.0013 0.0 0.0
P 11 Aggregate Crushing
+ 2.4 2.0
P 12 Soil Loosening
+ 0.6
P 13 Soil Layer Mixing
+ 0.3
P 34 Change Standing Biomass Fall Rate
+ 7 3.0 2.5 2.0 1.5 1.0
+ 0.5 0.6 0.7 0.8 1.0
G 02 Biomass Manipulation
+ 1.0
P 24 Flatten Standing Biomass
+ 0 0.3 0.25 0.2 0.1 1.0
P 25 Bury Flat Biomass
+ 1 .07 0.05 .04 .02 .03
P 26 Resurface Buried Biomass
+ 0.01 0.01 0.01 0.02 0.01
G 03 Crop Name
+ Tomato, processing
P 51 Seeding Configuration
+ 1 0.0 2
+ 2.0 1.0 1 25 1.0 1.0 0
+ ton/ac
+ 94.0 4.465 4 1.0 0.65 0.95
+ 0.8 0.025 1.5 10.0 27.0 0 70 750.0
+ -1.0 -4.0 0.15 0.95 0.0 30.0
+ -0.0198 0.6575 0.4807 -0.1453 -0.336 1.3726 0.5408 0.1081
+ 0.4807 -0.1453 3.08 1.0 31.1 0.01 1 1.1170388
+ 1700.0 1700.0 3.0 0.03 0.0 0.0 0.0 1
+ 0.02 0.02 0.02 0.02 0.2 0.0050 20.0 2.7
+ -1.20379 0.604887 .0415 0.025006166 0.0 0.0 0.0 0.0
T This records comes from ARS tomato transplant record and has the yield,
T Residue yield ration and the yield intercept changed to RUSLE values MAS 3-6-07
T Made changes to file as Fred insturctioned, mass of the plant MAS 3/15/07
T Fred Fox sent this back to me today with some changes and it appears to run in SC
#------------
D 15/05/01
O 03 Cultivator, row 1 in ridge
+ 5.799433 14.63 2.2351363 0.0 2.2351363 0.89405453 2.4586499
T RUSLE:Row crop cultivator w/ sweeps leaving a 1" ridge 05-14-02 DTL
T G2 was added into file in front of the flattening (P24), burial (P25), and resurfacing (P26) factors because the area affected is less than 1.0 and
T the RUSLE values were normalized to 1.0.  This change will imulate the correct residue changes based on the method set forth in RUSLE.
T RUSLE's factors have been redused to based on the area affected.
T The stalk fall rate factor (P34) was moved ahead of the new (G2) factor to set the fall rate to the less than 1.0 area affected.  8/8/07 MAS
+
G 01 Tillage
+ 76.20015 0.5 .75 76.20015 50.800102 101.600204
P 01 Break Crust
P 02 Random Roughness
+ 1 7.6200156
P 05 Ridges and Dikes
+ 1 25.400051 762.0015 0.0 0.0 0.0
P 11 Aggregate Crushing
+ 3.0 1.0
P 12 Soil Loosening
+ 0.75
P 13 Soil Layer Mixing
+ 0.35
P 34 Change Standing Biomass Fall Rate
+ 4 3.0 2.5 2.0 1.5 1.0
+ 0.5 0.6 0.7 0.8 1.0
G 02 Biomass Manipulation
+ 1.0
P 24 Flatten Standing Biomass
+ 14 0.7 0.3 0.3 0.1 1.0
P 25 Bury Flat Biomass
+ 1 .57 0.5 0.44 0.32 0.64
P 26 Resurface Buried Biomass
+ 0.01 0.01 0.01 0.01 0.01
#------------
D 05/06/01
O 04 Sprayer, insecticide post emergence
+ 1.2160101 0.15
T Spray pest control chemicals on growing crop.   Crop is not killed.  11/17/01 DTL
T
T Added to the DB.  This assumes no crop flattening.  4-5-12 MAS
+
#------------
D 05/06/01
O 03 Cultivator, row 1 in ridge
+ 5.799433 14.63 2.2351363 0.0 2.2351363 0.89405453 2.4586499
T RUSLE:Row crop cultivator w/ sweeps leaving a 1" ridge 05-14-02 DTL
T G2 was added into file in front of the flattening (P24), burial (P25), and resurfacing (P26) factors because the area affected is less than 1.0 and
T the RUSLE values were normalized to 1.0.  This change will imulate the correct residue changes based on the method set forth in RUSLE.
T RUSLE's factors have been redused to based on the area affected.
T The stalk fall rate factor (P34) was moved ahead of the new (G2) factor to set the fall rate to the less than 1.0 area affected.  8/8/07 MAS
+
G 01 Tillage
+ 76.20015 0.5 .75 76.20015 50.800102 101.600204
P 01 Break Crust
P 02 Random Roughness
+ 1 7.6200156
P 05 Ridges and Dikes
+ 1 25.400051 762.0015 0.0 0.0 0.0
P 11 Aggregate Crushing
+ 3.0 1.0
P 12 Soil Loosening
+ 0.75
P 13 Soil Layer Mixing
+ 0.35
P 34 Change Standing Biomass Fall Rate
+ 4 3.0 2.5 2.0 1.5 1.0
+ 0.5 0.6 0.7 0.8 1.0
G 02 Biomass Manipulation
+ 1.0
P 24 Flatten Standing Biomass
+ 14 0.7 0.3 0.3 0.1 1.0
P 25 Bury Flat Biomass
+ 1 .57 0.5 0.44 0.32 0.64
P 26 Resurface Buried Biomass
+ 0.01 0.01 0.01 0.01 0.01
#------------
D 05/07/01
O 04 Harvest, hand pick vegetables
+ 3.2738733 0.15
T Hand pick tomato, artichoke, peppers, strawberries or similar crops
T with multiple harvests from the same plants.  12-13-2011 DTL
T This is a partial harvest only 50% of the yield is taken with this harvest.
T This operation MUST be followed by a final harvest operation.
T Crops that use multiple harvests must be manually calibrated.
T Added 12-27-11 MAS
+
G 02 Biomass Manipulation
+ 1.0
P 31 Kill or Defoliate Growing Crop
+ 0
P 62 Remove (by age pool) Plant/Residue Material
+ 1 0 0 0 3 3 2 0.5 0.0 0.0 0.0 0.0
P 40 End crop Biomass Manipulation
#------------
D 07/07/01
O 03 Disk, offset, heavy
+ 8.418531 39.0 2.2351363 0.0 2.2351363 1.3410819 2.6821637
T 6/8/01 DTL
T MAS 10-26-06
T Corrected the Burial values MAS 11-21-11
+
G 01 Tillage
+ 152.4003 1.0 1.0 152.4003 101.600204 177.80035
P 01 Break Crust
P 02 Random Roughness
+ 1 38.100075
P 05 Ridges and Dikes
+ 1 101.600204 254.0005 0.0 0.0 0.0
P 11 Aggregate Crushing
+ 2.8 0.75
P 12 Soil Loosening
+ 0.9
P 13 Soil Layer Mixing
+ 0.5
P 31 Kill or Defoliate Growing Crop
+ 2
P 40 End crop Biomass Manipulation
P 24 Flatten Standing Biomass
+ 0 1.0 0.9 0.8 0.5 1.0
P 25 Bury Flat Biomass
+ 1 0.95 0.9 0.85 0.6 0.95
P 26 Resurface Buried Biomass
+ 0.05 0.06 0.07 0.08 0.05
P 34 Change Standing Biomass Fall Rate
+ 7 3.0 2.5 2.0 1.5 1.0
+ 0.5 0.6 0.7 0.8 1.0
#------------
D 25/07/01
O 03 Disk, tandem secondary op
+ 4.4898834 32.5 2.2351363 0.0 2.2351363 1.3410819 2.6821637
T 9-in. Spacing, Front and Rear; Good for seedbed preparation/chemical incorporation in medium to heavy soils
T Works well in primary tillage in light to medium soils
T Provides good residue-handling capability.  MAS 10-26-06
+
G 01 Tillage
+ 127.00027 0.75 1.0 127.00026 76.20015 152.4003
P 01 Break Crust
P 02 Random Roughness
+ 1 15.240031
P 05 Ridges and Dikes
+ 1 50.800102 228.60046 0.0 0.0 0.0
P 11 Aggregate Crushing
+ 2.8 0.75
P 12 Soil Loosening
+ 0.85
P 13 Soil Layer Mixing
+ 0.4
P 31 Kill or Defoliate Growing Crop
+ 2
P 40 End crop Biomass Manipulation
P 24 Flatten Standing Biomass
+ 0 0.85 0.7 0.6 0.5 1.0
P 25 Bury Flat Biomass
+ 1 0.73 0.63 0.55 0.4 0.73
P 26 Resurface Buried Biomass
+ 0.02 0.04 0.02 0.05 0.02
P 34 Change Standing Biomass Fall Rate
+ 7 3.0 2.5 2.0 1.5 1.0
+ 0.5 0.6 0.7 0.8 1.0
#------------
D 30/07/01
O 03 Drill or air seeder single disk openers 7-10 in spac
+ 3.2738733 2.44 2.2351363 0.0 2.2351363 1.5645955 2.9056773
T Drill or Air seeder with single disk no-till openers  JD 750 or similar openers. (No-till air drill)
T Based on Drill, no-till single disk 7-10 spacing. 102403 DTL. RUSLE MAS 10-26-06
T G2 was added into file in front of the flattening (P24), burial (P25), and resurfacing (P26) factors because the area affected is less than 1.0 and
T the RUSLE values were normalized to 1.0.  This change will imulate the correct residue changes based on the method set forth in RUSLE.
T RUSLE's factors have been redused to based on the area affected.
T The stalk fall rate factor (P34) was moved ahead of the new (G2) factor to set the fall rate to the less than 1.0 area affected.  8/7/07 MAS
+
G 01 Tillage
+ 63.500134 0.4 0.15 63.50013 50.800102 101.600204
P 01 Break Crust
P 02 Random Roughness
+ 1 7.6200156
P 05 Ridges and Dikes
+ 1 25.400051 203.20041 0.0 0.0 0.0
P 11 Aggregate Crushing
+ 2.8 0.75
P 12 Soil Loosening
+ 0.4
P 13 Soil Layer Mixing
+ 0.20
P 34 Change Standing Biomass Fall Rate
+ 7 3.0 2.5 2.0 1.5 1.0
+ 0.5 0.6 0.7 0.8 1.0
G 02 Biomass Manipulation
+ 1.0
P 24 Flatten Standing Biomass
+ 0 0.6 0.4 0.35 0.15 1.0
P 25 Bury Flat Biomass
+ 1 0.05 0.04 0.03 0.02 0.03
P 26 Resurface Buried Biomass
+ 0.01 0.01 0.01 0.05 0.01
G 03 Crop Name
+ Sorghum, forage
P 51 Seeding Configuration
+ 1 0.0 0
+ 62.0 5.0 0 10 1.0 1.0 2
+ ton/ac
+ 0 4.465 4 1.0 0.46 0.8
+ 1.9812241 0.025 2.0 10.0 27.5 1 110 1500.0
+ -5.0 -15.0 0.01 0.95 0.0 40
+ -0.0302 0.9263 0.3728 -0.065 -0.018 1.015 0.7224 0.039
+ 0.3728 -0.065 0.03985145 0.42 19.2 0.05 0 0.7
+ 8.333333 13.0 3.0 0.03 0.1 0.1 0.0 3
+ 0.01 0.01 0.01 0.01 0.153 0.01 20.0 3.0
+ -1.20379 0.604887 0.0 0.0 0.0 0.0 0.0 0.0
T This file is most like  forage sorghum silage 20 ton  30" row spacing.  Base location Columbia, MO REV 61801 DTL
T
T The residue ratio is set to Sorghum, silage from RUSLE.  If you need a hay file use Sorghum, hay.
T MAS 4-27-08
T
T Changed the flag to not selectect for calabration from calabration  MAS 9-2-09
T Changed the flag from day maturity to heat units.  MAS 9-2-09
#------------
D 12/09/01
O 03 Disk, offset, heavy
+ 8.418531 39.0 2.2351363 0.0 2.2351363 1.3410819 2.6821637
T 6/8/01 DTL
T MAS 10-26-06
T Corrected the Burial values MAS 11-21-11
+
G 01 Tillage
+ 152.4003 1.0 1.0 152.4003 101.600204 177.80035
P 01 Break Crust
P 02 Random Roughness
+ 1 38.100075
P 05 Ridges and Dikes
+ 1 101.600204 254.0005 0.0 0.0 0.0
P 11 Aggregate Crushing
+ 2.8 0.75
P 12 Soil Loosening
+ 0.9
P 13 Soil Layer Mixing
+ 0.5
P 31 Kill or Defoliate Growing Crop
+ 2
P 40 End crop Biomass Manipulation
P 24 Flatten Standing Biomass
+ 0 1.0 0.9 0.8 0.5 1.0
P 25 Bury Flat Biomass
+ 1 0.95 0.9 0.85 0.6 0.95
P 26 Resurface Buried Biomass
+ 0.05 0.06 0.07 0.08 0.05
P 34 Change Standing Biomass Fall Rate
+ 7 3.0 2.5 2.0 1.5 1.0
+ 0.5 0.6 0.7 0.8 1.0
#------------
D 15/09/01
O 03 Disk, tandem secondary op
+ 4.4898834 32.5 2.2351363 0.0 2.2351363 1.3410819 2.6821637
T 9-in. Spacing, Front and Rear; Good for seedbed preparation/chemical incorporation in medium to heavy soils
T Works well in primary tillage in light to medium soils
T Provides good residue-handling capability.  MAS 10-26-06
+
G 01 Tillage
+ 127.00027 0.75 1.0 127.00026 76.20015 152.4003
P 01 Break Crust
P 02 Random Roughness
+ 1 15.240031
P 05 Ridges and Dikes
+ 1 50.800102 228.60046 0.0 0.0 0.0
P 11 Aggregate Crushing
+ 2.8 0.75
P 12 Soil Loosening
+ 0.85
P 13 Soil Layer Mixing
+ 0.4
P 31 Kill or Defoliate Growing Crop
+ 2
P 40 End crop Biomass Manipulation
P 24 Flatten Standing Biomass
+ 0 0.85 0.7 0.6 0.5 1.0
P 25 Bury Flat Biomass
+ 1 0.73 0.63 0.55 0.4 0.73
P 26 Resurface Buried Biomass
+ 0.02 0.04 0.02 0.05 0.02
P 34 Change Standing Biomass Fall Rate
+ 7 3.0 2.5 2.0 1.5 1.0
+ 0.5 0.6 0.7 0.8 1.0
#------------
D 30/09/01
O 03 Drill or air seeder single disk openers 7-10 in spac
+ 3.2738733 2.44 2.2351363 0.0 2.2351363 1.5645955 2.9056773
T Drill or Air seeder with single disk no-till openers  JD 750 or similar openers. (No-till air drill)
T Based on Drill, no-till single disk 7-10 spacing. 102403 DTL. RUSLE MAS 10-26-06
T G2 was added into file in front of the flattening (P24), burial (P25), and resurfacing (P26) factors because the area affected is less than 1.0 and
T the RUSLE values were normalized to 1.0.  This change will imulate the correct residue changes based on the method set forth in RUSLE.
T RUSLE's factors have been redused to based on the area affected.
T The stalk fall rate factor (P34) was moved ahead of the new (G2) factor to set the fall rate to the less than 1.0 area affected.  8/7/07 MAS
+
G 01 Tillage
+ 63.500134 0.4 0.15 63.50013 50.800102 101.600204
P 01 Break Crust
P 02 Random Roughness
+ 1 7.6200156
P 05 Ridges and Dikes
+ 1 25.400051 203.20041 0.0 0.0 0.0
P 11 Aggregate Crushing
+ 2.8 0.75
P 12 Soil Loosening
+ 0.4
P 13 Soil Layer Mixing
+ 0.20
P 34 Change Standing Biomass Fall Rate
+ 7 3.0 2.5 2.0 1.5 1.0
+ 0.5 0.6 0.7 0.8 1.0
G 02 Biomass Manipulation
+ 1.0
P 24 Flatten Standing Biomass
+ 0 0.6 0.4 0.35 0.15 1.0
P 25 Bury Flat Biomass
+ 1 0.05 0.04 0.03 0.02 0.03
P 26 Resurface Buried Biomass
+ 0.01 0.01 0.01 0.05 0.01
G 03 Crop Name
+ Rye, winter cover
P 51 Seeding Configuration
+ 1 0.0 0
+ 220.0 8.0 0 2240 1.0 1.0 2
+ lbs/ac
+ 0 8930 5 1.0 0.6 0.8
+ 1.2 0.025 1.2192148 0.0 25.0 1 60 1472.2223
+ -5.0 -15.0 0.005 0.05 0.035 30.0
+ 0.013 0.8013 0.4293 -0.086 -0.018 0.932 0.556 0.0736
+ 0.3293 -0.086 2.87 1.0 20.0 0.05 0 0.3
+ 28.571428 335.0 1.4 0.012 0.1 0.1 0.0 2
+ 0.0133 0.0133 0.0133 0.0133 0.12 0.0050 17.1 5.227942
+ -2.08165 0.548606 0 0.0 0.0 0.0 0.0 0.0
T RUSLE Notes: Rye, as winter cover. Killed in vegetative stage the following spring.
T Decomposition  0.017 like grass forages. Rev 021705 DTL
T
T Cloned 2-16-07 MAS
T Lowered the heat units from 3600 to 2650 to match the core crop runs for OK  MAS 10-29-08
#------------
*END
*EOF
