Version: 1.5
*START 4
N Originating Program: RUSLE2
N Skel Format Version: 1.1
N This management file was originally converted from the NRCS standard XML format on - Thu Jun 28 13:37:02 PDT 2012
N This management file was updated to contain the most current crop and operation records for WEPS on - Tue Dec 17 19:19:28 CST 2013
#------------
D 01/07/01
O 04 Harvest, hand pick
+ 3.2738733 0.15
T Hand pick lettuce or similar crops or to represent one final picking of fruit or berry crops.
T Do not use for multiple pickings of fruit or berry crops unless a regrowth vegetation file representing
T regrowth between pickings is available in the database to be called in.
T This is not the case for strawberries.  12132011 DTL
T Added 3/29/07 MAS
T Reworked the values MAS 2-24-09
T Added the change to flat on the crop type.  8-27-10
T This operation takes all of the yield, and can be used to calibrate the yield. 12-27-11 MAS
T Adjusted the Energy use to 0.000000010 gal/ac  2-23-12
T
T Changed the fuel use from 0.000000010 to 0.36 g/ac 4-17-12 MAS
+
G 02 Biomass Manipulation
+ 1.0
P 31 Kill or Defoliate Growing Crop
+ 0
P 62 Remove (by age pool) Plant/Residue Material
+ 1 1 0 1 3 3 2 1.0 0.0 0.0 0.0 0.0
P 40 End crop Biomass Manipulation
#------------
D 15/08/01
O 04 Kill crop
+ 0.0 0
T Enter Operation notes here
+
G 02 Biomass Manipulation
+ 1.0
P 31 Kill or Defoliate Growing Crop
+ 2
P 40 End crop Biomass Manipulation
#------------
D 01/10/01
O 04 Sprayer, kill crop
+ 1.2160101 0.15
T All crop types are killed, green grow turned to residue, standing.  MAS 12-27-11
T
T Added Flattening to the operation to match R2 (P-24).  This will tend to increase erosion on systems that using
T cover crops by causing less standing residue from the crop or cover crop killed.  MAS 4-3-12
T
T After a conference call, Linda Scheffe, Dave Lightle, Mike Sporcic, and Fred Fox, we decided to change the flattening
T from 0.7-0.5 to 0.05 for all residue type due to wheel traffic only.  Plant canopy change over time is not considered.
T Normal plant senescence built into the model will handle plant changes.  MAS 4-5-12
+ 
G 02 Biomass Manipulation
+ 1.0
P 24 Flatten Standing Biomass
+ 0 0.05 0.05 0.05 0.05 0.05
P 31 Kill or Defoliate Growing Crop
+ 2
P 40 End crop Biomass Manipulation
#------------
D 15/10/01
O 03 Plow, moldboard
+ 17.491838 65 2.2351363 0.0 2.2351363 1.5645955 2.6821637
T Moldboard plow 8 inch operating depth.  060701 DTL  Modified flattening and burial per McCool and Foster 05/21/02 DTL RUSLE MAS 10-26-06
+
G 01 Tillage
+ 203.20041 1.0 1.0 203.20041 152.4003 254.0005
P 01 Break Crust
P 02 Random Roughness
+ 1 48.260098
P 05 Ridges and Dikes
+ 1 25.400051 406.40082 0.0 0.0 0.0
P 11 Aggregate Crushing
+ 2.8 1.0
P 12 Soil Loosening
+ 1.0
P 13 Soil Layer Mixing
+ 0.7
P 14 Soil Layer Inversion
P 31 Kill or Defoliate Growing Crop
+ 2
P 40 End crop Biomass Manipulation
P 24 Flatten Standing Biomass
+ 0 1 1 1 0.75 1.0
P 25 Bury Flat Biomass
+ 3 0.99 0.99 0.99 0.85 0.97
P 26 Resurface Buried Biomass
+ 0.01 0.02 0.04 0.1 0.02
P 34 Change Standing Biomass Fall Rate
+ 7 3.0 2.5 2.0 1.5 1.0
+ 0.5 0.6 0.7 0.8 1.0
#------------
D 25/04/02
O 03 Disk, tandem secondary op
+ 4.4898834 32.5 2.2351363 0.0 2.2351363 1.3410819 2.6821637
T 9-in. Spacing, Front and Rear; Good for seedbed preparation/chemical incorporation in medium to heavy soils
T Works well in primary tillage in light to medium soils
T Provides good residue-handling capability.  MAS 10-26-06
+
G 01 Tillage
+ 127.00027 0.75 1.0 127.00026 76.20015 152.4003
P 01 Break Crust
P 02 Random Roughness
+ 1 15.240031
P 05 Ridges and Dikes
+ 1 50.800102 228.60046 0.0 0.0 0.0
P 11 Aggregate Crushing
+ 2.8 0.75
P 12 Soil Loosening
+ 0.85
P 13 Soil Layer Mixing
+ 0.4
P 31 Kill or Defoliate Growing Crop
+ 2
P 40 End crop Biomass Manipulation
P 24 Flatten Standing Biomass
+ 0 0.85 0.7 0.6 0.5 1.0
P 25 Bury Flat Biomass
+ 1 0.73 0.63 0.55 0.4 0.73
P 26 Resurface Buried Biomass
+ 0.02 0.04 0.02 0.05 0.02
P 34 Change Standing Biomass Fall Rate
+ 7 3.0 2.5 2.0 1.5 1.0
+ 0.5 0.6 0.7 0.8 1.0
#------------
D 01/05/02
O 03 Harrow, coiled tine
+ 4.1157265 15.6 2.6821637 0.0 2.6821637 1.3410819 3.129191
T This oprn is from a RUSLE record created 6/7/01.  10-25-06 MAS
T
T Corrected ridge height and spacing to match RUSLE2. 10-26-11 LOS
T
T Changed spacing from 0 to 1 in. The 0 caused the operation to fail.  12-12-11 MAS
+
G 01 Tillage
+ 50.800102 0.25 1.0 50.800102 25.400051 76.20015
P 01 Break Crust
P 02 Random Roughness
+ 1 10.160021
P 05 Ridges and Dikes
+ 1 25.400051 101.600204 0.0 0.0 0.0
P 11 Aggregate Crushing
+ 3.0 -0.22
P 12 Soil Loosening
+ 0.6
P 13 Soil Layer Mixing
+ 0.2
P 31 Kill or Defoliate Growing Crop
+ 2
P 40 End crop Biomass Manipulation
P 24 Flatten Standing Biomass
+ 0 0.5 0.3 0.2 0.1 1.0
P 25 Bury Flat Biomass
+ 1 0.25 0.2 0.15 0.1 0.25
P 26 Resurface Buried Biomass
+ 0.01 0.01 0.01 0.02 0.01
P 34 Change Standing Biomass Fall Rate
+ 7 3.0 2.5 2.0 1.5 1.0
+ 0.5 0.6 0.7 0.8 1.0
#------------
D 01/05/02
O 04 Fert applic. surface broadcast
+ 1.4966278 0.0609375
T R2 Notes: Broadcast fertilizer spreader.  Wheel traffic only.  rev 082107 DTL
T
T Added to DB 4-12-12 MAS
+
G 01 Tillage
+ 0.0 0 0.05 0.0 0.0 0.0
P 01 Break Crust
P 02 Random Roughness
+ 1 8.8900175
P 11 Aggregate Crushing
+ 4.3 2.0
P 24 Flatten Standing Biomass
+ 0 0.25 0.2 0.15 0.1 1.0
P 26 Resurface Buried Biomass
+ 0.07 0.08 0.1 0.12 0.07
P 34 Change Standing Biomass Fall Rate
+ 0 1.0 1.0 1.0 1.0 1.0
+ 1.0 1.0 1.0 1.0 1.0
#------------
D 01/05/02
O 03 Planter, double disk opnr
+ 4.1157265 2.4375 2.2351363 0.0 2.2351363 1.5645955 2.9056773
T This is a standard planter on 30 in sp with a 1 in ridge.  Created in RUSLE 6/7/01.  MAS 8/7/07
T G2 was added into file in front of the flattening (P24), burial (P25), and resurfacing (P26) factors because the area affected is less than 1.0 and
T the RUSLE values were normalized to 1.0.  This change will imulate the correct residue changes based on the method set forth in RUSLE.
T RUSLE's factors have been redused to based on the area affected.
T The stalk fall rate factor (P34) was moved ahead of the new (G2) factor to set the fall rate to the less than 1.0 area affected.  8/7/07 MAS
+
G 01 Tillage
+ 63.500126 0.5 .15 63.500126 50.800102 101.600204
P 01 Break Crust
P 02 Random Roughness
+ 1 10.160021
P 05 Ridges and Dikes
+ 1 50.800102 762.0015 635.0013 0.0 0.0
P 11 Aggregate Crushing
+ 2.8 0.75
P 12 Soil Loosening
+ 0.6
P 13 Soil Layer Mixing
+ 0.35
P 34 Change Standing Biomass Fall Rate
+ 7 3.0 2.5 2.0 1.5 1.0
+ 0.5 0.6 0.7 0.8 1.0
G 02 Biomass Manipulation
+ 1.0
P 24 Flatten Standing Biomass
+ 0 .3 .25 .2 0.1 1.0
P 25 Bury Flat Biomass
+ 1 .0525 0.0375 .03 .015 .03
P 26 Resurface Buried Biomass
+ .01 .01 .01 .02 .01
G 03 Crop Name
+ Strawberry
P 51 Seeding Configuration
+ 1 0.0 2
+ 13.8 1.0 0 20000 1.0 1.0 0
+ lbs/ac
+ 90.0 8930 6 0.9 0.65 0.8
+ 0.3048037 0.025 0.4 7.0 22.0 0 365 3600.0
+ -5.0 -15.0 0.01 0.95 0.0 30.0
+ 0.1685 0.2125 0.6321 -0.0599 -0.0161 0.2118 0.6328 0.0822
+ 0.5321 -0.0599 1.2 1.0 12.2 0.01 0 0.5
+ 2000.0 4400.0 3.0 0.03 0.1 0.1 0.0 1
+ 0.02 0.02 0.02 0.02 0.2 0.0050 20.0 3.479347
+ -1.20379 0.604887 .1350 0.033625502 0.0 0.0 0.0 0.0
T Cloned from ARS Strawberry, short-day, or day-neutral, mult yr.  11-9-07 MAS
#------------
D 15/05/02
O 03 Cultivator, row 1 in ridge
+ 5.799433 14.63 2.2351363 0.0 2.2351363 0.89405453 2.4586499
T RUSLE:Row crop cultivator w/ sweeps leaving a 1" ridge 05-14-02 DTL
T G2 was added into file in front of the flattening (P24), burial (P25), and resurfacing (P26) factors because the area affected is less than 1.0 and
T the RUSLE values were normalized to 1.0.  This change will imulate the correct residue changes based on the method set forth in RUSLE.
T RUSLE's factors have been redused to based on the area affected.
T The stalk fall rate factor (P34) was moved ahead of the new (G2) factor to set the fall rate to the less than 1.0 area affected.  8/8/07 MAS
+
G 01 Tillage
+ 76.20015 0.5 .75 76.20015 50.800102 101.600204
P 01 Break Crust
P 02 Random Roughness
+ 1 7.6200156
P 05 Ridges and Dikes
+ 1 25.400051 762.0015 0.0 0.0 0.0
P 11 Aggregate Crushing
+ 3.0 1.0
P 12 Soil Loosening
+ 0.75
P 13 Soil Layer Mixing
+ 0.35
P 34 Change Standing Biomass Fall Rate
+ 4 3.0 2.5 2.0 1.5 1.0
+ 0.5 0.6 0.7 0.8 1.0
G 02 Biomass Manipulation
+ 1.0
P 24 Flatten Standing Biomass
+ 14 0.7 0.3 0.3 0.1 1.0
P 25 Bury Flat Biomass
+ 1 .57 0.5 0.44 0.32 0.64
P 26 Resurface Buried Biomass
+ 0.01 0.01 0.01 0.01 0.01
#------------
D 01/06/02
O 03 Cultivator, row 1 in ridge
+ 5.799433 14.63 2.2351363 0.0 2.2351363 0.89405453 2.4586499
T RUSLE:Row crop cultivator w/ sweeps leaving a 1" ridge 05-14-02 DTL
T G2 was added into file in front of the flattening (P24), burial (P25), and resurfacing (P26) factors because the area affected is less than 1.0 and
T the RUSLE values were normalized to 1.0.  This change will imulate the correct residue changes based on the method set forth in RUSLE.
T RUSLE's factors have been redused to based on the area affected.
T The stalk fall rate factor (P34) was moved ahead of the new (G2) factor to set the fall rate to the less than 1.0 area affected.  8/8/07 MAS
+
G 01 Tillage
+ 76.20015 0.5 .75 76.20015 50.800102 101.600204
P 01 Break Crust
P 02 Random Roughness
+ 1 7.6200156
P 05 Ridges and Dikes
+ 1 25.400051 762.0015 0.0 0.0 0.0
P 11 Aggregate Crushing
+ 3.0 1.0
P 12 Soil Loosening
+ 0.75
P 13 Soil Layer Mixing
+ 0.35
P 34 Change Standing Biomass Fall Rate
+ 4 3.0 2.5 2.0 1.5 1.0
+ 0.5 0.6 0.7 0.8 1.0
G 02 Biomass Manipulation
+ 1.0
P 24 Flatten Standing Biomass
+ 14 0.7 0.3 0.3 0.1 1.0
P 25 Bury Flat Biomass
+ 1 .57 0.5 0.44 0.32 0.64
P 26 Resurface Buried Biomass
+ 0.01 0.01 0.01 0.01 0.01
#------------
D 01/07/02
O 03 Cultivator, row 1 in ridge
+ 5.799433 14.63 2.2351363 0.0 2.2351363 0.89405453 2.4586499
T RUSLE:Row crop cultivator w/ sweeps leaving a 1" ridge 05-14-02 DTL
T G2 was added into file in front of the flattening (P24), burial (P25), and resurfacing (P26) factors because the area affected is less than 1.0 and
T the RUSLE values were normalized to 1.0.  This change will imulate the correct residue changes based on the method set forth in RUSLE.
T RUSLE's factors have been redused to based on the area affected.
T The stalk fall rate factor (P34) was moved ahead of the new (G2) factor to set the fall rate to the less than 1.0 area affected.  8/8/07 MAS
+
G 01 Tillage
+ 76.20015 0.5 .75 76.20015 50.800102 101.600204
P 01 Break Crust
P 02 Random Roughness
+ 1 7.6200156
P 05 Ridges and Dikes
+ 1 25.400051 762.0015 0.0 0.0 0.0
P 11 Aggregate Crushing
+ 3.0 1.0
P 12 Soil Loosening
+ 0.75
P 13 Soil Layer Mixing
+ 0.35
P 34 Change Standing Biomass Fall Rate
+ 4 3.0 2.5 2.0 1.5 1.0
+ 0.5 0.6 0.7 0.8 1.0
G 02 Biomass Manipulation
+ 1.0
P 24 Flatten Standing Biomass
+ 14 0.7 0.3 0.3 0.1 1.0
P 25 Bury Flat Biomass
+ 1 .57 0.5 0.44 0.32 0.64
P 26 Resurface Buried Biomass
+ 0.01 0.01 0.01 0.01 0.01
#------------
D 01/08/02
O 03 Cultivator, row 1 in ridge
+ 5.799433 14.63 2.2351363 0.0 2.2351363 0.89405453 2.4586499
T RUSLE:Row crop cultivator w/ sweeps leaving a 1" ridge 05-14-02 DTL
T G2 was added into file in front of the flattening (P24), burial (P25), and resurfacing (P26) factors because the area affected is less than 1.0 and
T the RUSLE values were normalized to 1.0.  This change will imulate the correct residue changes based on the method set forth in RUSLE.
T RUSLE's factors have been redused to based on the area affected.
T The stalk fall rate factor (P34) was moved ahead of the new (G2) factor to set the fall rate to the less than 1.0 area affected.  8/8/07 MAS
+
G 01 Tillage
+ 76.20015 0.5 .75 76.20015 50.800102 101.600204
P 01 Break Crust
P 02 Random Roughness
+ 1 7.6200156
P 05 Ridges and Dikes
+ 1 25.400051 762.0015 0.0 0.0 0.0
P 11 Aggregate Crushing
+ 3.0 1.0
P 12 Soil Loosening
+ 0.75
P 13 Soil Layer Mixing
+ 0.35
P 34 Change Standing Biomass Fall Rate
+ 4 3.0 2.5 2.0 1.5 1.0
+ 0.5 0.6 0.7 0.8 1.0
G 02 Biomass Manipulation
+ 1.0
P 24 Flatten Standing Biomass
+ 14 0.7 0.3 0.3 0.1 1.0
P 25 Bury Flat Biomass
+ 1 .57 0.5 0.44 0.32 0.64
P 26 Resurface Buried Biomass
+ 0.01 0.01 0.01 0.01 0.01
#------------
D 01/09/02
O 03 Cultivator, row 1 in ridge
+ 5.799433 14.63 2.2351363 0.0 2.2351363 0.89405453 2.4586499
T RUSLE:Row crop cultivator w/ sweeps leaving a 1" ridge 05-14-02 DTL
T G2 was added into file in front of the flattening (P24), burial (P25), and resurfacing (P26) factors because the area affected is less than 1.0 and
T the RUSLE values were normalized to 1.0.  This change will imulate the correct residue changes based on the method set forth in RUSLE.
T RUSLE's factors have been redused to based on the area affected.
T The stalk fall rate factor (P34) was moved ahead of the new (G2) factor to set the fall rate to the less than 1.0 area affected.  8/8/07 MAS
+
G 01 Tillage
+ 76.20015 0.5 .75 76.20015 50.800102 101.600204
P 01 Break Crust
P 02 Random Roughness
+ 1 7.6200156
P 05 Ridges and Dikes
+ 1 25.400051 762.0015 0.0 0.0 0.0
P 11 Aggregate Crushing
+ 3.0 1.0
P 12 Soil Loosening
+ 0.75
P 13 Soil Layer Mixing
+ 0.35
P 34 Change Standing Biomass Fall Rate
+ 4 3.0 2.5 2.0 1.5 1.0
+ 0.5 0.6 0.7 0.8 1.0
G 02 Biomass Manipulation
+ 1.0
P 24 Flatten Standing Biomass
+ 14 0.7 0.3 0.3 0.1 1.0
P 25 Bury Flat Biomass
+ 1 .57 0.5 0.44 0.32 0.64
P 26 Resurface Buried Biomass
+ 0.01 0.01 0.01 0.01 0.01
#------------
D 01/10/02
O 03 Cultivator, row 1 in ridge
+ 5.799433 14.63 2.2351363 0.0 2.2351363 0.89405453 2.4586499
T RUSLE:Row crop cultivator w/ sweeps leaving a 1" ridge 05-14-02 DTL
T G2 was added into file in front of the flattening (P24), burial (P25), and resurfacing (P26) factors because the area affected is less than 1.0 and
T the RUSLE values were normalized to 1.0.  This change will imulate the correct residue changes based on the method set forth in RUSLE.
T RUSLE's factors have been redused to based on the area affected.
T The stalk fall rate factor (P34) was moved ahead of the new (G2) factor to set the fall rate to the less than 1.0 area affected.  8/8/07 MAS
+
G 01 Tillage
+ 76.20015 0.5 .75 76.20015 50.800102 101.600204
P 01 Break Crust
P 02 Random Roughness
+ 1 7.6200156
P 05 Ridges and Dikes
+ 1 25.400051 762.0015 0.0 0.0 0.0
P 11 Aggregate Crushing
+ 3.0 1.0
P 12 Soil Loosening
+ 0.75
P 13 Soil Layer Mixing
+ 0.35
P 34 Change Standing Biomass Fall Rate
+ 4 3.0 2.5 2.0 1.5 1.0
+ 0.5 0.6 0.7 0.8 1.0
G 02 Biomass Manipulation
+ 1.0
P 24 Flatten Standing Biomass
+ 14 0.7 0.3 0.3 0.1 1.0
P 25 Bury Flat Biomass
+ 1 .57 0.5 0.44 0.32 0.64
P 26 Resurface Buried Biomass
+ 0.01 0.01 0.01 0.01 0.01
#------------
D 01/11/02
O 04 Add mulch
+ 9.353924E-8 0
T Enter Operation notes here
+
G 03 Crop Name
+ small grain straw
P 65 Add Crop Residue Amounts
+ 0.0 0.0 0.0 0.22417001 2
+ 0.0 0.0 0.0 0.0
+ .008 .008 .008 .008 0.169 0.0050 17.1 5.227942
+ -2.08165 0.548606
T Enter crop notes here.
#------------
D 01/07/03
O 04 Harvest, hand pick
+ 3.2738733 0.15
T Hand pick lettuce or similar crops or to represent one final picking of fruit or berry crops.
T Do not use for multiple pickings of fruit or berry crops unless a regrowth vegetation file representing
T regrowth between pickings is available in the database to be called in.
T This is not the case for strawberries.  12132011 DTL
T Added 3/29/07 MAS
T Reworked the values MAS 2-24-09
T Added the change to flat on the crop type.  8-27-10
T This operation takes all of the yield, and can be used to calibrate the yield. 12-27-11 MAS
T Adjusted the Energy use to 0.000000010 gal/ac  2-23-12
T
T Changed the fuel use from 0.000000010 to 0.36 g/ac 4-17-12 MAS
+
G 02 Biomass Manipulation
+ 1.0
P 31 Kill or Defoliate Growing Crop
+ 0
P 62 Remove (by age pool) Plant/Residue Material
+ 1 1 0 1 3 3 2 1.0 0.0 0.0 0.0 0.0
P 40 End crop Biomass Manipulation
#------------
D 25/07/03
O 03 Rotary hoe
+ 2.338481 16.58 4.4702725 0 4.4702725 2.6821637 6.705409
+
G 01 Tillage
+ 38.100075 0.5 1.0 38.100075 25.400051 63.50013
P 01 Break Crust
P 02 Random Roughness
+ 1 10.160021
P 05 Ridges and Dikes
+ 1 0.0 0.0 0.0 0.0 0.0
P 11 Aggregate Crushing
+ 3.0 -0.22
P 12 Soil Loosening
+ .4
P 13 Soil Layer Mixing
+ 0.1
P 24 Flatten Standing Biomass
+ 14 0.25 0.2 0.15 0.1 1.0
P 25 Bury Flat Biomass
+ 1 0.2 0.2 0.15 0.1 0.2
P 26 Resurface Buried Biomass
+ 0.05 0.05 0.05 0.07 0.05
P 34 Change Standing Biomass Fall Rate
+ 7 3.0 2.5 2.0 1.5 1.0
+ 0.5 0.6 0.7 0.8 1.0
#------------
D 01/11/03
O 04 Add mulch
+ 9.353924E-8 0
T Enter Operation notes here
+
G 03 Crop Name
+ small grain straw
P 65 Add Crop Residue Amounts
+ 0.0 0.0 0.0 0.22417001 2
+ 0.0 0.0 0.0 0.0
+ .008 .008 .008 .008 0.169 0.0050 17.1 5.227942
+ -2.08165 0.548606
T Enter crop notes here.
#------------
D 01/07/04
O 04 Harvest, hand pick
+ 3.2738733 0.15
T Hand pick lettuce or similar crops or to represent one final picking of fruit or berry crops.
T Do not use for multiple pickings of fruit or berry crops unless a regrowth vegetation file representing
T regrowth between pickings is available in the database to be called in.
T This is not the case for strawberries.  12132011 DTL
T Added 3/29/07 MAS
T Reworked the values MAS 2-24-09
T Added the change to flat on the crop type.  8-27-10
T This operation takes all of the yield, and can be used to calibrate the yield. 12-27-11 MAS
T Adjusted the Energy use to 0.000000010 gal/ac  2-23-12
T
T Changed the fuel use from 0.000000010 to 0.36 g/ac 4-17-12 MAS
+
G 02 Biomass Manipulation
+ 1.0
P 31 Kill or Defoliate Growing Crop
+ 0
P 62 Remove (by age pool) Plant/Residue Material
+ 1 1 0 1 3 3 2 1.0 0.0 0.0 0.0 0.0
P 40 End crop Biomass Manipulation
#------------
D 25/07/04
O 03 Rotary hoe
+ 2.338481 16.58 4.4702725 0 4.4702725 2.6821637 6.705409
+
G 01 Tillage
+ 38.100075 0.5 1.0 38.100075 25.400051 63.50013
P 01 Break Crust
P 02 Random Roughness
+ 1 10.160021
P 05 Ridges and Dikes
+ 1 0.0 0.0 0.0 0.0 0.0
P 11 Aggregate Crushing
+ 3.0 -0.22
P 12 Soil Loosening
+ .4
P 13 Soil Layer Mixing
+ 0.1
P 24 Flatten Standing Biomass
+ 14 0.25 0.2 0.15 0.1 1.0
P 25 Bury Flat Biomass
+ 1 0.2 0.2 0.15 0.1 0.2
P 26 Resurface Buried Biomass
+ 0.05 0.05 0.05 0.07 0.05
P 34 Change Standing Biomass Fall Rate
+ 7 3.0 2.5 2.0 1.5 1.0
+ 0.5 0.6 0.7 0.8 1.0
#------------
D 01/11/04
O 04 Add mulch
+ 9.353924E-8 0
T Enter Operation notes here
+
G 03 Crop Name
+ small grain straw
P 65 Add Crop Residue Amounts
+ 0.0 0.0 0.0 0.22417001 2
+ 0.0 0.0 0.0 0.0
+ .008 .008 .008 .008 0.169 0.0050 17.1 5.227942
+ -2.08165 0.548606
T Enter crop notes here.
#------------
*END
*EOF
