Version: 1.5
*START 1
N Originating Program: RUSLE2
N Skel Format Version: 1.1
N This management file was originally converted from the NRCS standard XML format on - Thu Jun 28 13:37:02 PDT 2012
N This management file was updated to contain the most current crop and operation records for WEPS on - Tue Dec 17 19:19:29 CST 2013
#------------
D 10/05/01
O 03 Disk, tandem light finishing
+ 3.7415698 19.5 2.2351363 0.0 2.2351363 1.3410819 2.6821637
T 6/8/01 DTL RUSLE.  7in sp.  This is tool used to finish a seedbed.  MAS 10-26-06
+
G 01 Tillage
+ 101.600204 0.5 1.0 101.600204 76.20015 127.00026
P 01 Break Crust
P 02 Random Roughness
+ 1 15.240031
P 05 Ridges and Dikes
+ 1 12.700026 177.80035 0.0 0.0 0.0
P 11 Aggregate Crushing
+ 2.8 0.75
P 12 Soil Loosening
+ 0.75
P 13 Soil Layer Mixing
+ 0.35
P 31 Kill or Defoliate Growing Crop
+ 2
P 40 End crop Biomass Manipulation
P 24 Flatten Standing Biomass
+ 0 0.85 0.7 0.6 0.5 1.0
P 25 Bury Flat Biomass
+ 1 0.73 0.63 0.55 0.4 0.73
P 26 Resurface Buried Biomass
+ 0.02 0.04 0.02 0.05 0.02
P 34 Change Standing Biomass Fall Rate
+ 7 3.0 2.5 2.0 1.5 1.0
+ 0.5 0.6 0.7 0.8 1.0
#------------
D 15/05/01
O 03 Planter, double disk opnr
+ 4.1157265 2.4375 2.2351363 0.0 2.2351363 1.5645955 2.9056773
T This is a standard planter on 30 in sp with a 1 in ridge.  Created in RUSLE 6/7/01.  MAS 8/7/07
T G2 was added into file in front of the flattening (P24), burial (P25), and resurfacing (P26) factors because the area affected is less than 1.0 and
T the RUSLE values were normalized to 1.0.  This change will imulate the correct residue changes based on the method set forth in RUSLE.
T RUSLE's factors have been redused to based on the area affected.
T The stalk fall rate factor (P34) was moved ahead of the new (G2) factor to set the fall rate to the less than 1.0 area affected.  8/7/07 MAS
+
G 01 Tillage
+ 63.500126 0.5 .15 63.500126 50.800102 101.600204
P 01 Break Crust
P 02 Random Roughness
+ 1 10.160021
P 05 Ridges and Dikes
+ 1 50.800102 762.0015 635.0013 0.0 0.0
P 11 Aggregate Crushing
+ 2.8 0.75
P 12 Soil Loosening
+ 0.6
P 13 Soil Layer Mixing
+ 0.35
P 34 Change Standing Biomass Fall Rate
+ 7 3.0 2.5 2.0 1.5 1.0
+ 0.5 0.6 0.7 0.8 1.0
G 02 Biomass Manipulation
+ 1.0
P 24 Flatten Standing Biomass
+ 0 .3 .25 .2 0.1 1.0
P 25 Bury Flat Biomass
+ 1 .0525 0.0375 .03 .015 .03
P 26 Resurface Buried Biomass
+ .01 .01 .01 .02 .01
G 03 Crop Name
+ Potato, late, harvest
P 51 Seeding Configuration
+ 1 0.0 2
+ 5.0 4.0 1 600 1.0 1.0 5
+ cwt/ac
+ 79.0 89.3 7 1.0 0.65 0.8
+ 0.8 0.05 0.6096074 2.0 25.0 0 120 1600.0
+ -5.0 -15.0 0.01 0.95 0.0 32
+ 0.0 0.6553 0.3159 -0.061 -3.0E-4 0.9911 0.3415 0.0494
+ 0.4163 -0.061 2.6 1.0 30.0 0.05 0 1.0
+ 12000.0 2700.0 3.0 0.03 0.0 0.0 0.9 1
+ 0.02 0.02 0.02 0.02 0.2 0.0050 20.0 5.227942
+ -1.20379 0.604887 0.0313 0.024658702 0.0 0.0 0.0 0.0
T Represents high yielding typically irrigated Potatoes - white, russet, red (all but sweet). 60,000 lb (600 cwt), 30 ton/ac yield .  36" rows.
T Residue at harvest includes mass before chemical kill.  Base location ID, WA, NM.
T
T File was tested in Grant Co. WA and Bingham Co. ID.  Biomas Conv Eff factor was at 32.  Yields were low.
T At 40 the yields were 553 cwt/ac in WA and 485 cwt/ac in ID.  I have made the change to get the yields closer
T to the actual field values.  MAS 9-26-07
T
T Harvest biomass ratio is set using two studies.  One from the PNW irrigated and the other in MN.
T Both sites are were sandy soils with irrigation.  Yields were 600 cwt/ac.  MAS 7-3-08
#------------
D 16/05/01
O 04 Sprayer, pre-emergence
+ 1.2160101 .15
T Spray pest control chemicals on growing crop.  Crop is not killed.
T In the MCREW management screen the user must select the kind of weeds killed in the growing crop as external residue.   080404 DTL
T Cloned from Defoliate (spray) crop.oprn, Changed the P31 to No crop kill and added G4 to add material to field MAS 9-28-06
+
G 03 Crop Name
+ weed residue; 0-3 mo
P 65 Add Crop Residue Amounts
+ 0.0 0.0 0.0 0.0 1
+ 0.0 0.0 0.0056042504 152.4003
+ 0.025 0.025 0.025 0.025 0.169 0.0050 17.1 5.227942
+ -1.20379 0.604887
T Enter crop notes here.
#------------
D 15/06/01
O 03 Bed shaper
+ 3.554491 19.5 2.2351363 0.0 2.2351363 1.5645955 2.9056773
T RUSLE Notes: Bed shaping operation on existing beds.  May include drip tape installation. 10/28/01 DTL
T Cloned 2-15-07 MAS
T G2 was added into file in front of the flattening (P24), burial (P25), and resurfacing (P26) factors because the area affected is less than 1.0 and
T the RUSLE values were normalized to 1.0.  This change will imulate the correct residue changes based on the method set forth in RUSLE.
T RUSLE's factors have been redused to based on the area affected.
T The stalk fall rate factor (P34) was moved ahead of the new (G2) factor to set the fall rate to the  less than 1.0 area affected.  8/8/07 MAS
+
G 01 Tillage
+ 101.600204 .6 .75 101.600204 76.20015 152.4003
P 01 Break Crust
P 02 Random Roughness
+ 1 15.240031
P 11 Aggregate Crushing
+ 3.0 -0.22
P 12 Soil Loosening
+ 0.75
P 13 Soil Layer Mixing
+ 0.05
P 05 Ridges and Dikes
+ 1 203.20041 760.0 381.00076 0.0 0.0
P 34 Change Standing Biomass Fall Rate
+ 7 3.0 2.5 2.0 1.5 1.0
+ 0.5 0.6 0.7 0.8 1.0
G 02 Biomass Manipulation
+ 1.0
P 24 Flatten Standing Biomass
+ 0 0.5 0.45 0.4 0.3 1.00
P 25 Bury Flat Biomass
+ 1 0.38 0.3 0.23 0.2 0.28
P 26 Resurface Buried Biomass
+ 0.02 0.02 0.02 0.02 0.02
#------------
D 15/06/01
O 04 Sprayer, fungicide
+ 1.2160101 0.15
T Spray fungicide on growing crop.   Crop is not killed.  11/17/01 DTL Revised Sprayer,
T insecticide for fungicide application 82211 LOS
T
T Added to DB 3-1-12 MAS
+ 
#------------
D 22/06/01
O 04 Sprayer, fungicide
+ 1.2160101 0.15
T Spray fungicide on growing crop.   Crop is not killed.  11/17/01 DTL Revised Sprayer,
T insecticide for fungicide application 82211 LOS
T
T Added to DB 3-1-12 MAS
+ 
#------------
D 02/07/01
O 04 Sprayer, fungicide
+ 1.2160101 0.15
T Spray fungicide on growing crop.   Crop is not killed.  11/17/01 DTL Revised Sprayer,
T insecticide for fungicide application 82211 LOS
T
T Added to DB 3-1-12 MAS
+ 
#------------
D 15/07/01
O 03 Bed shaper
+ 3.554491 19.5 2.2351363 0.0 2.2351363 1.5645955 2.9056773
T RUSLE Notes: Bed shaping operation on existing beds.  May include drip tape installation. 10/28/01 DTL
T Cloned 2-15-07 MAS
T G2 was added into file in front of the flattening (P24), burial (P25), and resurfacing (P26) factors because the area affected is less than 1.0 and
T the RUSLE values were normalized to 1.0.  This change will imulate the correct residue changes based on the method set forth in RUSLE.
T RUSLE's factors have been redused to based on the area affected.
T The stalk fall rate factor (P34) was moved ahead of the new (G2) factor to set the fall rate to the  less than 1.0 area affected.  8/8/07 MAS
+
G 01 Tillage
+ 101.600204 .6 .75 101.600204 76.20015 152.4003
P 01 Break Crust
P 02 Random Roughness
+ 1 15.240031
P 11 Aggregate Crushing
+ 3.0 -0.22
P 12 Soil Loosening
+ 0.75
P 13 Soil Layer Mixing
+ 0.05
P 05 Ridges and Dikes
+ 1 203.20041 760.0 381.00076 0.0 0.0
P 34 Change Standing Biomass Fall Rate
+ 7 3.0 2.5 2.0 1.5 1.0
+ 0.5 0.6 0.7 0.8 1.0
G 02 Biomass Manipulation
+ 1.0
P 24 Flatten Standing Biomass
+ 0 0.5 0.45 0.4 0.3 1.00
P 25 Bury Flat Biomass
+ 1 0.38 0.3 0.23 0.2 0.28
P 26 Resurface Buried Biomass
+ 0.02 0.02 0.02 0.02 0.02
#------------
D 18/07/01
O 04 Sprayer, fungicide
+ 1.2160101 0.15
T Spray fungicide on growing crop.   Crop is not killed.  11/17/01 DTL Revised Sprayer,
T insecticide for fungicide application 82211 LOS
T
T Added to DB 3-1-12 MAS
+ 
#------------
D 31/07/01
O 04 Sprayer, fungicide
+ 1.2160101 0.15
T Spray fungicide on growing crop.   Crop is not killed.  11/17/01 DTL Revised Sprayer,
T insecticide for fungicide application 82211 LOS
T
T Added to DB 3-1-12 MAS
+ 
#------------
D 10/08/01
O 04 Sprayer, fungicide
+ 1.2160101 0.15
T Spray fungicide on growing crop.   Crop is not killed.  11/17/01 DTL Revised Sprayer,
T insecticide for fungicide application 82211 LOS
T
T Added to DB 3-1-12 MAS
+ 
#------------
D 30/08/01
O 04 Sprayer, defoliant
+ 1.2160101 .15
T Sprayer, defoliant as used on cotton or other crops.  082806 DTL
T
T Stops all plant crop growth.  10-27-06 MAS
T
T Moves leaves from plant to flat residue.
T There seems to be a drop in yield since the leaves are gone for the last 2 week period.
T May need to adjust calibration (bioadjustement) when using this operation.  MAS 4-11-08
+
G 02 Biomass Manipulation
+ 1.0
P 31 Kill or Defoliate Growing Crop
+ 3
#------------
D 21/09/01
O 03 Harvest, dig root crops res. buried
+ 17.491838 27.378 1.3410819 0.0 1.5645955 1.3410819 2.9056773
T Harvest, root crops like potatoes, sugar beets, carrots, and onions.
T Surface is rough with 4 ridges and much of the residue is buried.
T Rev 11-18-04 DTL RUSLE MAS 10-26-06
T
T P24 was changed to show that all residue types are flattened.
T This havest now flattens all residue types 100%.  MAS 1-18-11
+
G 01 Tillage
+ 177.80035 1.0 1.0 177.80035 152.4003 203.20041
P 01 Break Crust
P 02 Random Roughness
+ 1 16.510033
P 05 Ridges and Dikes
+ 1 101.600204 3657.6072 3048.006 0.0 0.0
P 11 Aggregate Crushing
+ 1.4 -1.2
P 12 Soil Loosening
+ 0.7
P 13 Soil Layer Mixing
+ 0.9
P 31 Kill or Defoliate Growing Crop
+ 2
G 02 Biomass Manipulation
+ 1.0
P 62 Remove (by age pool) Plant/Residue Material
+ 1 1 0 1 1 3 2 0.0 0.0 0.0 1.0 0.0
P 40 End crop Biomass Manipulation
P 24 Flatten Standing Biomass
+ 0 1.0 1.0 1.0 1.0 1.0
P 25 Bury Flat Biomass
+ 2 .95 .95 .95 .95 1
P 26 Resurface Buried Biomass
+ 0.01 0.01 0.03 0.01 0.01
#------------
D 25/09/01
O 03 Chisel, st. pt
+ 9.353924 45.5 2.2351363 0.0 2.2351363 1.5645955 2.9056773
T Enter Operation notes here
+
G 01 Tillage
+ 177.80035 0.75 1.0 177.80035 101.600204 203.20041
P 01 Break Crust
P 02 Random Roughness
+ 1 38.100075
P 05 Ridges and Dikes
+ 1 76.20015 381.00076 101.600204 0.0 0.0
P 11 Aggregate Crushing
+ 2.4 -2.0
P 12 Soil Loosening
+ 0.85
P 13 Soil Layer Mixing
+ 0.37
P 31 Kill or Defoliate Growing Crop
+ 2
P 40 End crop Biomass Manipulation
P 24 Flatten Standing Biomass
+ 0 0.6 0.4 0.25 0.1 1.0
P 25 Bury Flat Biomass
+ 1 0.76 0.68 0.58 0.5 0.9
P 26 Resurface Buried Biomass
+ 0.05 0.06 0.07 0.2 0.05
P 34 Change Standing Biomass Fall Rate
+ 7 3.0 2.5 2.0 1.5 1.0
+ 0.5 0.6 0.7 0.8 1.0
#------------
D 25/09/01
O 03 Disk, tandem light finishing
+ 3.7415698 19.5 2.2351363 0.0 2.2351363 1.3410819 2.6821637
T 6/8/01 DTL RUSLE.  7in sp.  This is tool used to finish a seedbed.  MAS 10-26-06
+
G 01 Tillage
+ 101.600204 0.5 1.0 101.600204 76.20015 127.00026
P 01 Break Crust
P 02 Random Roughness
+ 1 15.240031
P 05 Ridges and Dikes
+ 1 12.700026 177.80035 0.0 0.0 0.0
P 11 Aggregate Crushing
+ 2.8 0.75
P 12 Soil Loosening
+ 0.75
P 13 Soil Layer Mixing
+ 0.35
P 31 Kill or Defoliate Growing Crop
+ 2
P 40 End crop Biomass Manipulation
P 24 Flatten Standing Biomass
+ 0 0.85 0.7 0.6 0.5 1.0
P 25 Bury Flat Biomass
+ 1 0.73 0.63 0.55 0.4 0.73
P 26 Resurface Buried Biomass
+ 0.02 0.04 0.02 0.05 0.02
P 34 Change Standing Biomass Fall Rate
+ 7 3.0 2.5 2.0 1.5 1.0
+ 0.5 0.6 0.7 0.8 1.0
#------------
D 25/09/01
O 04 Planting, broadcast seeder
+ 1.2160101 .15
T Broadcast seeding. Begins growth .    11/30/01 DTL
T No tillage processes added. MAS 3-28-07
+
G 03 Crop Name
+ Rye, winter cover
P 51 Seeding Configuration
+ 1 0.0 0
+ 220.0 8.0 0 2240 1.0 1.0 2
+ lbs/ac
+ 0 8930 5 1.0 0.6 0.8
+ 1.2 0.025 1.2192148 0.0 25.0 1 60 1472.2223
+ -5.0 -15.0 0.005 0.05 0.035 30.0
+ 0.013 0.8013 0.4293 -0.086 -0.018 0.932 0.556 0.0736
+ 0.3293 -0.086 2.87 1.0 20.0 0.05 0 0.3
+ 28.571428 335.0 1.4 0.012 0.1 0.1 0.0 2
+ 0.0133 0.0133 0.0133 0.0133 0.12 0.0050 17.1 5.227942
+ -2.08165 0.548606 0 0.0 0.0 0.0 0.0 0.0
T RUSLE Notes: Rye, as winter cover. Killed in vegetative stage the following spring.
T Decomposition  0.017 like grass forages. Rev 021705 DTL
T
T Cloned 2-16-07 MAS
T Lowered the heat units from 3600 to 2650 to match the core crop runs for OK  MAS 10-29-08
#------------
*END
*EOF
