Version: 1.5
*START 1
N Originating Program: RUSLE2
N Skel Format Version: 1.1
N This management file was originally converted from the NRCS standard XML format on - Thu Jun 28 13:35:31 PDT 2012
N This management file was updated to contain the most current crop and operation records for WEPS on - Tue Dec 17 19:23:05 CST 2013
#------------
D 01/08/01
O 03 Shredder, flail or rotary
+ 6.828365 .15 2.2351363 0.0 2.2351363 1.7881091 2.6821637
T Rusle Note: Rotary mower or flail shredder used to defoliate root crops such as sugarbeets before harvest or on cotton or
T other crop residue where crop has been previously harvested and
T residue is shredded  and spread flat..   10/3/01 DTL 11/15/01
T
T P42 is used to set a height of cut and removed the flattening P24.
T The 0.90 fraction used in RUSLE is by mass.  WEPS fraction is by height.
T It is not the same as RUSLE and cannot be used.
T Set the height to 2 inches per the conversation the Dave Lightle.  He said that most
T corn shredders are set to 2 inches.  Cotton shredding is much higher, use the 6 in shredder.
T A new operation was also created for root crop defoliation where all of the green tops
T are flatten to residue without killing the crop, "Shredder, beet topper".
T Kill crop was removed because of the interference with most harvest operations
T if used before harvest.  MAS 1-5-11
+
G 02 Biomass Manipulation
+ 1.0
P 42 Cut/Remove Biomass to Height (flags)
+ 0 0 1 0 0 50.800102 0 0 0.0
P 40 End crop Biomass Manipulation
#------------
*END
*EOF
