Version: 1.5
*START 1
N Originating Program: RUSLE2
N Skel Format Version: 1.1
N This management file was originally converted from the NRCS standard XML format on - Thu Jun 28 13:35:01 PDT 2012
N This management file was updated to contain the most current crop and operation records for WEPS on - Tue Dec 17 19:23:08 CST 2013
#------------
D 15/05/01
O 03 Manure spreader, solid and semi-solid
+ 11.505327 .20 1.7881091 0.0 1.7881091 1.3410819 3.5762181
T Created from RUSLE file MAS 9/19/06.
T This assumes a defult residue type of  manure solid significant bedding and the RUSLE may contain some bedding.
T User may need to change to the correct manure type, make a calulation on the dry matter applied, and change the application rate in MCREW.
T This opn is built for an application of 10 ton/ac 60% dry matter surface applied manure.
T 10 tons x 2000 lbs/ac = 20,000 lbs/ac x 0.6 = 12,000 lbs/ac applied.
T MAS 12-5-07
+
G 01 Tillage
+ 0.0 0 1 0.0 0.0 0.0
P 24 Flatten Standing Biomass
+ 14 .1 .1 .1 .1 1.0
G 03 Crop Name
+ manure, solid, signif. bedding
P 66 Add Manure Residue Amount
+ 0.0 0.0 0.0 0.0 1
+ 0.0 0.0 0.0 0.0
+ 1.34502 0.0
+ .017 .017 .017 .017 0.169 0.0050 1 5.227942
+ -2.08165 0.548606
T Enter crop notes here.
#------------
D 15/05/01
O 04 Add mulch
+ 9.353924E-8 0
T Enter Operation notes here
+
G 03 Crop Name
+ small grain straw
P 65 Add Crop Residue Amounts
+ 0.0 0.0 0.0 0.22417001 2
+ 0.0 0.0 0.0 0.0
+ .008 .008 .008 .008 0.169 0.0050 17.1 5.227942
+ -2.08165 0.548606
T Enter crop notes here.
#------------
D 31/08/01
O 04 Harvest, hand pick
+ 3.2738733 0.15
T Hand pick lettuce or similar crops or to represent one final picking of fruit or berry crops.
T Do not use for multiple pickings of fruit or berry crops unless a regrowth vegetation file representing
T regrowth between pickings is available in the database to be called in.
T This is not the case for strawberries.  12132011 DTL
T Added 3/29/07 MAS
T Reworked the values MAS 2-24-09
T Added the change to flat on the crop type.  8-27-10
T This operation takes all of the yield, and can be used to calibrate the yield. 12-27-11 MAS
T Adjusted the Energy use to 0.000000010 gal/ac  2-23-12
T
T Changed the fuel use from 0.000000010 to 0.36 g/ac 4-17-12 MAS
+
G 02 Biomass Manipulation
+ 1.0
P 31 Kill or Defoliate Growing Crop
+ 0
P 62 Remove (by age pool) Plant/Residue Material
+ 1 1 0 1 3 3 2 1.0 0.0 0.0 0.0 0.0
P 40 End crop Biomass Manipulation
#------------
*END
*EOF
