Version: 1.5
*START 1
N Originating Program: RUSLE2
N Skel Format Version: 1.1
N This management file was originally converted from the NRCS standard XML format on - Thu Jun 28 13:58:22 PDT 2012
N This management file was updated to contain the most current crop and operation records for WEPS on - Tue Dec 17 19:17:02 CST 2013
#------------
D 15/05/01
O 03 Plow, moldboard
+ 17.491838 65 2.2351363 0.0 2.2351363 1.5645955 2.6821637
T Moldboard plow 8 inch operating depth.  060701 DTL  Modified flattening and burial per McCool and Foster 05/21/02 DTL RUSLE MAS 10-26-06
+
G 01 Tillage
+ 203.20041 1.0 1.0 203.20041 152.4003 254.0005
P 01 Break Crust
P 02 Random Roughness
+ 1 48.260098
P 05 Ridges and Dikes
+ 1 25.400051 406.40082 0.0 0.0 0.0
P 11 Aggregate Crushing
+ 2.8 1.0
P 12 Soil Loosening
+ 1.0
P 13 Soil Layer Mixing
+ 0.7
P 14 Soil Layer Inversion
P 31 Kill or Defoliate Growing Crop
+ 2
P 40 End crop Biomass Manipulation
P 24 Flatten Standing Biomass
+ 0 1 1 1 0.75 1.0
P 25 Bury Flat Biomass
+ 3 0.99 0.99 0.99 0.85 0.97
P 26 Resurface Buried Biomass
+ 0.01 0.02 0.04 0.1 0.02
P 34 Change Standing Biomass Fall Rate
+ 7 3.0 2.5 2.0 1.5 1.0
+ 0.5 0.6 0.7 0.8 1.0
#------------
D 25/05/01
O 03 Harrow, coiled tine
+ 4.1157265 15.6 2.6821637 0.0 2.6821637 1.3410819 3.129191
T This oprn is from a RUSLE record created 6/7/01.  10-25-06 MAS
T
T Corrected ridge height and spacing to match RUSLE2. 10-26-11 LOS
T
T Changed spacing from 0 to 1 in. The 0 caused the operation to fail.  12-12-11 MAS
+
G 01 Tillage
+ 50.800102 0.25 1.0 50.800102 25.400051 76.20015
P 01 Break Crust
P 02 Random Roughness
+ 1 10.160021
P 05 Ridges and Dikes
+ 1 25.400051 101.600204 0.0 0.0 0.0
P 11 Aggregate Crushing
+ 3.0 -0.22
P 12 Soil Loosening
+ 0.6
P 13 Soil Layer Mixing
+ 0.2
P 31 Kill or Defoliate Growing Crop
+ 2
P 40 End crop Biomass Manipulation
P 24 Flatten Standing Biomass
+ 0 0.5 0.3 0.2 0.1 1.0
P 25 Bury Flat Biomass
+ 1 0.25 0.2 0.15 0.1 0.25
P 26 Resurface Buried Biomass
+ 0.01 0.01 0.01 0.02 0.01
P 34 Change Standing Biomass Fall Rate
+ 7 3.0 2.5 2.0 1.5 1.0
+ 0.5 0.6 0.7 0.8 1.0
#------------
D 25/05/01
O 03 Planter, small veg seed
+ 3.3674128 .59 0.89405453 0.0 0.89405453 0.44702727 1.3410819
T Small seed planter like used in planting small seeded vegetables in 25 to 30" rows.
T Shallow depth and minimal disturbance in fine seedbed.  Like Planet Junior.  12-10-01 DTL
T G2 was added into file in front of the flattening (P24), burial (P25), and resurfacing (P26) factors because the area affected is less than 1.0 and
T the RUSLE values were normalized to 1.0.  This change will imulate the correct residue changes based on the method set forth in RUSLE.
T RUSLE's factors have been redused to based on the area affected.
T The stalk fall rate factor (P34) was moved ahead of the new (G2) factor to set the fall rate to theless than 1.0 area affected.  8/7/07 MAS
T
T Changed the P5 to allow the preexisting ridges and furrows to set the ridge roughness.  MAS  12-30-2010
+
G 01 Tillage
+ 25.400051 0.5 .15 25.400051 12.700026 50.800102
P 01 Break Crust
P 02 Random Roughness
+ 1 7.6200156
P 05 Ridges and Dikes
+ 0 25.400051 762.0015 711.2014 0.0 0.0
P 11 Aggregate Crushing
+ 2.8 0.75
P 12 Soil Loosening
+ 0.6
P 13 Soil Layer Mixing
+ 0.35
P 34 Change Standing Biomass Fall Rate
+ 7 3.0 2.5 2.0 1.5 1.0
+ 0.5 0.6 0.7 0.8 1.0
G 02 Biomass Manipulation
+ 1.0
P 24 Flatten Standing Biomass
+ 0 .3 .25 .2 0.1 1.0
P 25 Bury Flat Biomass
+ 1 .0525 .0375 .03 .015 .03
P 26 Resurface Buried Biomass
+ 0.01 .01 .01 0.05 .01
G 03 Crop Name
+ Cantaloupe, Muskmelon, Honeydew
P 51 Seeding Configuration
+ 1 0.0 2
+ 0.7 1.0 1 25000 1.0 1.0 0
+ lbs/ac
+ 89.8 8930 4 0.8 0.65 0.9
+ 0.6096074 0.025 1.3 10.0 32.0 0 75 650.0
+ -5.0 -15.0 0.15 0.95 0.0 30.0
+ -0.0062 0.8478 0.4633 -0.0721 -0.0083 1.005 0.7292 0.0562
+ 0.3633 -0.0721 2.0 1.0 20.0 0.02 1 6.0957026
+ 23.809525 23.809525 1.5 0.01 0.0 0.0 0.0 1
+ 0.02 0.02 0.02 0.02 0.2 0.0050 20.0 5.227942
+ -1.20379 0.604887 .2025 0.0201753 0.0 0.0 0.0 0.0
T This file has ARS tranplants as its orgin.
T
T 1/30/92 ljo, rev 5/23/93 & 5/21/01 gaw
T Based primarily on  Alcorn St. Univ. data
T Plant date = mid-May.  Harvest date = mid-Aug. Transplants.
T
T Yield and harvest index are from RUSLE
T MAS 10-24-07
#------------
D 10/06/01
O 03 Cultivator, row 1 in ridge
+ 5.799433 14.63 2.2351363 0.0 2.2351363 0.89405453 2.4586499
T RUSLE:Row crop cultivator w/ sweeps leaving a 1" ridge 05-14-02 DTL
T G2 was added into file in front of the flattening (P24), burial (P25), and resurfacing (P26) factors because the area affected is less than 1.0 and
T the RUSLE values were normalized to 1.0.  This change will imulate the correct residue changes based on the method set forth in RUSLE.
T RUSLE's factors have been redused to based on the area affected.
T The stalk fall rate factor (P34) was moved ahead of the new (G2) factor to set the fall rate to the less than 1.0 area affected.  8/8/07 MAS
+
G 01 Tillage
+ 76.20015 0.5 .75 76.20015 50.800102 101.600204
P 01 Break Crust
P 02 Random Roughness
+ 1 7.6200156
P 05 Ridges and Dikes
+ 1 25.400051 762.0015 0.0 0.0 0.0
P 11 Aggregate Crushing
+ 3.0 1.0
P 12 Soil Loosening
+ 0.75
P 13 Soil Layer Mixing
+ 0.35
P 34 Change Standing Biomass Fall Rate
+ 4 3.0 2.5 2.0 1.5 1.0
+ 0.5 0.6 0.7 0.8 1.0
G 02 Biomass Manipulation
+ 1.0
P 24 Flatten Standing Biomass
+ 14 0.7 0.3 0.3 0.1 1.0
P 25 Bury Flat Biomass
+ 1 .57 0.5 0.44 0.32 0.64
P 26 Resurface Buried Biomass
+ 0.01 0.01 0.01 0.01 0.01
#------------
D 20/06/01
O 03 Cultivator, row 1 in ridge
+ 5.799433 14.63 2.2351363 0.0 2.2351363 0.89405453 2.4586499
T RUSLE:Row crop cultivator w/ sweeps leaving a 1" ridge 05-14-02 DTL
T G2 was added into file in front of the flattening (P24), burial (P25), and resurfacing (P26) factors because the area affected is less than 1.0 and
T the RUSLE values were normalized to 1.0.  This change will imulate the correct residue changes based on the method set forth in RUSLE.
T RUSLE's factors have been redused to based on the area affected.
T The stalk fall rate factor (P34) was moved ahead of the new (G2) factor to set the fall rate to the less than 1.0 area affected.  8/8/07 MAS
+
G 01 Tillage
+ 76.20015 0.5 .75 76.20015 50.800102 101.600204
P 01 Break Crust
P 02 Random Roughness
+ 1 7.6200156
P 05 Ridges and Dikes
+ 1 25.400051 762.0015 0.0 0.0 0.0
P 11 Aggregate Crushing
+ 3.0 1.0
P 12 Soil Loosening
+ 0.75
P 13 Soil Layer Mixing
+ 0.35
P 34 Change Standing Biomass Fall Rate
+ 4 3.0 2.5 2.0 1.5 1.0
+ 0.5 0.6 0.7 0.8 1.0
G 02 Biomass Manipulation
+ 1.0
P 24 Flatten Standing Biomass
+ 14 0.7 0.3 0.3 0.1 1.0
P 25 Bury Flat Biomass
+ 1 .57 0.5 0.44 0.32 0.64
P 26 Resurface Buried Biomass
+ 0.01 0.01 0.01 0.01 0.01
#------------
D 20/09/01
O 04 Harvest, vine crops
+ 3.2738733 .15
T RUSLE notes: Hand pick melons, cucumbers, pumpkins or similar crops.  03-12-02 DTL
T Build 3-16-07 MAS
T Reworked the values MAS 2-24-09
T Changed the parts harvested to include flat to correct yield-residue issue with GA run on
T watermelons.  8-27-10  MAS
T Corrected the Diesel Energy gal/ac to 0.35 12-27-11 MAS
T
T ARS template record - filename is:  Harvest  Template (pick and remove).oprn
T This operation record is designed to represent harvesting operations that
T remove the specified "yield" of a crop without cutting the crop stalks.
T However, it may flatten and/or disturb the remaining stalks
T (i.e., causing a change in the rate standing stalks decay and go flat).
T Eamples of harvesting operations that can be represented with this operation template are:
T hand harvesting corn,  hand picking of vegetable crops like peas, beans, etc. and also harvesting
T of leaf crops like tobacco (with appropriate parameter value settings).  Another example
T would be the use of a combine stripper header harvesting wheat.
T This harvesting operation record defaults to removing all the reproductive component of a crop
T (typically this is specified as the "yield" component in the crop record) and to kill the crop.
T This would be acceptable as defined for representing hand harvesting of corn for example.
T However, it may not be acceptable for a crop that is "hand picked" several times
T during the year (like peas or beans).  The default parameter values need to be
T changed to meet this type of harvest operation requirements.  Likewise for a harvest
T operation which woud remove some of the leaves instead of a "grain" yield, such as
T harvesting of tobacco leaves (yet this is the template that will often be used for developing
T such "leaf harvesting" operations).
T See the "Detailed info regarding this operation record:" section for more specific
T information regarding the use of non-default process parameter values for
T this harvest operation template.
T 
T 200x	Created - Fred Fox
T Oct 31, 2005	Updated notes - Larry Wagner
T Detailed info regarding this operation record:
T The default "Kill or Defoliate Growing Crop" parameter is set to kill all crops.
T If one doesn't want the operation to kill the crop or only annuals, then they need
T to change this value.  Examples might be where multiple harvest operations
T are necessary to remove the "yield" such as hand picking peas or beans.
T Also, the crop plant component that is harvested can be changed to be something
T other than the reproductive component (grain or fruit).  For example, a fraction of the
T leaves only could be specified, leaving the rest of the crop alone, e.g. harvesting of
T tobacco leaves.
T Some standing crop stalks could be flattened during the harvesting process,
T e.g. by the harvester's tire tracks.  Therefore, a flattening process is also a part of this
T operation record.  The default values are set to zero, assuming no flattening of standing
T stalks are occuring.  However, these can be set as necessary for the specific harvesting
T device used in the operation.
T The harvesting operation could also have an effect on the "standing stalk"
T fall rate and fall threshold values.  The default "biomass pool" flag parameter
T is set to "No adjustments applied" so that no "stalk disturbance" will occur.
T However, this flag value can be changed along with the default parameter values
T to change the "stalk residue decay processes".  An example where one might
T want to apply this effect is when simulating a "combine stripper header" where
T the physical action of pulling the wheat heads would apply a stress to the wheat
T straw such that it would be weakened enough to increase the threshold and
T fall rate values.
T If a harvest operation is expected to "cut" the crop to a prescribed height (or depth
T from the top of the canopy), then one of the "cut and remove" harvest templates should
T probably be used instead of this one.
+
G 02 Biomass Manipulation
+ 1.0
P 31 Kill or Defoliate Growing Crop
+ 0
P 62 Remove (by age pool) Plant/Residue Material
+ 1 1 0 1 3 3 2 1.0 0.0 0.0 0.0 0.0
P 40 End crop Biomass Manipulation
#------------
D 25/09/01
O 03 Disk, tandem light finishing
+ 3.7415698 19.5 2.2351363 0.0 2.2351363 1.3410819 2.6821637
T 6/8/01 DTL RUSLE.  7in sp.  This is tool used to finish a seedbed.  MAS 10-26-06
+
G 01 Tillage
+ 101.600204 0.5 1.0 101.600204 76.20015 127.00026
P 01 Break Crust
P 02 Random Roughness
+ 1 15.240031
P 05 Ridges and Dikes
+ 1 12.700026 177.80035 0.0 0.0 0.0
P 11 Aggregate Crushing
+ 2.8 0.75
P 12 Soil Loosening
+ 0.75
P 13 Soil Layer Mixing
+ 0.35
P 31 Kill or Defoliate Growing Crop
+ 2
P 40 End crop Biomass Manipulation
P 24 Flatten Standing Biomass
+ 0 0.85 0.7 0.6 0.5 1.0
P 25 Bury Flat Biomass
+ 1 0.73 0.63 0.55 0.4 0.73
P 26 Resurface Buried Biomass
+ 0.02 0.04 0.02 0.05 0.02
P 34 Change Standing Biomass Fall Rate
+ 7 3.0 2.5 2.0 1.5 1.0
+ 0.5 0.6 0.7 0.8 1.0
#------------
D 25/09/01
O 04 Planting, broadcast seeder
+ 1.2160101 .15
T Broadcast seeding. Begins growth .    11/30/01 DTL
T No tillage processes added. MAS 3-28-07
+
G 03 Crop Name
+ Rye, winter cover
P 51 Seeding Configuration
+ 1 0.0 0
+ 220.0 8.0 0 2240 1.0 1.0 2
+ lbs/ac
+ 0 8930 5 1.0 0.6 0.8
+ 1.2 0.025 1.2192148 0.0 25.0 1 60 1472.2223
+ -5.0 -15.0 0.005 0.05 0.035 30.0
+ 0.013 0.8013 0.4293 -0.086 -0.018 0.932 0.556 0.0736
+ 0.3293 -0.086 2.87 1.0 20.0 0.05 0 0.3
+ 28.571428 335.0 1.4 0.012 0.1 0.1 0.0 2
+ 0.0133 0.0133 0.0133 0.0133 0.12 0.0050 17.1 5.227942
+ -2.08165 0.548606 0 0.0 0.0 0.0 0.0 0.0
T RUSLE Notes: Rye, as winter cover. Killed in vegetative stage the following spring.
T Decomposition  0.017 like grass forages. Rev 021705 DTL
T
T Cloned 2-16-07 MAS
T Lowered the heat units from 3600 to 2650 to match the core crop runs for OK  MAS 10-29-08
#------------
*END
*EOF
