Version: 1.5
*START 1
N Originating Program: RUSLE2
N Skel Format Version: 1.1
N This management file was originally converted from the NRCS standard XML format on - Thu Jun 28 13:37:05 PDT 2012
N This management file was updated to contain the most current crop and operation records for WEPS on - Tue Dec 17 19:19:22 CST 2013
#------------
D 01/05/01
O 04 Sprayer, insecticide post emergence
+ 1.2160101 0.15
T Spray pest control chemicals on growing crop.   Crop is not killed.  11/17/01 DTL
T
T Added to the DB.  This assumes no crop flattening.  4-5-12 MAS
+
#------------
D 10/05/01
O 04 Fert applic. surface broadcast
+ 1.4966278 0.0609375
T R2 Notes: Broadcast fertilizer spreader.  Wheel traffic only.  rev 082107 DTL
T
T Added to DB 4-12-12 MAS
+
G 01 Tillage
+ 0.0 0 0.05 0.0 0.0 0.0
P 01 Break Crust
P 02 Random Roughness
+ 1 8.8900175
P 11 Aggregate Crushing
+ 4.3 2.0
P 24 Flatten Standing Biomass
+ 0 0.25 0.2 0.15 0.1 1.0
P 26 Resurface Buried Biomass
+ 0.07 0.08 0.1 0.12 0.07
P 34 Change Standing Biomass Fall Rate
+ 0 1.0 1.0 1.0 1.0 1.0
+ 1.0 1.0 1.0 1.0 1.0
#------------
D 30/06/01
O 04 Fert applic. surface broadcast
+ 1.4966278 0.0609375
T R2 Notes: Broadcast fertilizer spreader.  Wheel traffic only.  rev 082107 DTL
T
T Added to DB 4-12-12 MAS
+
G 01 Tillage
+ 0.0 0 0.05 0.0 0.0 0.0
P 01 Break Crust
P 02 Random Roughness
+ 1 8.8900175
P 11 Aggregate Crushing
+ 4.3 2.0
P 24 Flatten Standing Biomass
+ 0 0.25 0.2 0.15 0.1 1.0
P 26 Resurface Buried Biomass
+ 0.07 0.08 0.1 0.12 0.07
P 34 Change Standing Biomass Fall Rate
+ 0 1.0 1.0 1.0 1.0 1.0
+ 1.0 1.0 1.0 1.0 1.0
#------------
D 10/07/01
O 04 Sprayer, insecticide post emergence
+ 1.2160101 0.15
T Spray pest control chemicals on growing crop.   Crop is not killed.  11/17/01 DTL
T
T Added to the DB.  This assumes no crop flattening.  4-5-12 MAS
+
#------------
D 01/08/01
O 04 Harvest, hand pick
+ 3.2738733 0.15
T Hand pick lettuce or similar crops or to represent one final picking of fruit or berry crops.
T Do not use for multiple pickings of fruit or berry crops unless a regrowth vegetation file representing
T regrowth between pickings is available in the database to be called in.
T This is not the case for strawberries.  12132011 DTL
T Added 3/29/07 MAS
T Reworked the values MAS 2-24-09
T Added the change to flat on the crop type.  8-27-10
T This operation takes all of the yield, and can be used to calibrate the yield. 12-27-11 MAS
T Adjusted the Energy use to 0.000000010 gal/ac  2-23-12
T
T Changed the fuel use from 0.000000010 to 0.36 g/ac 4-17-12 MAS
+
G 02 Biomass Manipulation
+ 1.0
P 31 Kill or Defoliate Growing Crop
+ 0
P 62 Remove (by age pool) Plant/Residue Material
+ 1 1 0 1 3 3 2 1.0 0.0 0.0 0.0 0.0
P 40 End crop Biomass Manipulation
#------------
D 01/10/01
O 03 Shredder, flail or rotary
+ 6.828365 .15 2.2351363 0.0 2.2351363 1.7881091 2.6821637
T Rusle Note: Rotary mower or flail shredder used to defoliate root crops such as sugarbeets before harvest or on cotton or
T other crop residue where crop has been previously harvested and
T residue is shredded  and spread flat..   10/3/01 DTL 11/15/01
T
T P42 is used to set a height of cut and removed the flattening P24.
T The 0.90 fraction used in RUSLE is by mass.  WEPS fraction is by height.
T It is not the same as RUSLE and cannot be used.
T Set the height to 2 inches per the conversation the Dave Lightle.  He said that most
T corn shredders are set to 2 inches.  Cotton shredding is much higher, use the 6 in shredder.
T A new operation was also created for root crop defoliation where all of the green tops
T are flatten to residue without killing the crop, "Shredder, beet topper".
T Kill crop was removed because of the interference with most harvest operations
T if used before harvest.  MAS 1-5-11
+
G 02 Biomass Manipulation
+ 1.0
P 42 Cut/Remove Biomass to Height (flags)
+ 0 0 1 0 0 50.800102 0 0 0.0
P 40 End crop Biomass Manipulation
#------------
*END
*EOF
