Version: 1.5
*START 1
N Originating Program: RUSLE2
N Skel Format Version: 1.1
N This management file was originally converted from the NRCS standard XML format on - Thu Jul 05 09:35:40 PDT 2012
N This management file was updated to contain the most current crop and operation records for WEPS on - Tue Dec 17 21:13:54 CST 2013
#------------
D 15/04/01
O 04 Sprayer, kill crop
+ 1.2160101 0.15
T All crop types are killed, green grow turned to residue, standing.  MAS 12-27-11
T
T Added Flattening to the operation to match R2 (P-24).  This will tend to increase erosion on systems that using
T cover crops by causing less standing residue from the crop or cover crop killed.  MAS 4-3-12
T
T After a conference call, Linda Scheffe, Dave Lightle, Mike Sporcic, and Fred Fox, we decided to change the flattening
T from 0.7-0.5 to 0.05 for all residue type due to wheel traffic only.  Plant canopy change over time is not considered.
T Normal plant senescence built into the model will handle plant changes.  MAS 4-5-12
+ 
G 02 Biomass Manipulation
+ 1.0
P 24 Flatten Standing Biomass
+ 0 0.05 0.05 0.05 0.05 0.05
P 31 Kill or Defoliate Growing Crop
+ 2
P 40 End crop Biomass Manipulation
#------------
D 01/05/01
O 03 Fert applic. shank low disturbance, 15 in spacing
+ 8.418531 2.6 2.2351363 0.0 2.2351363 1.5645955 2.9056773
T Minimum disturbance fertilizer injector shank.on 15 inch spacing.
T Each injector typically has depth guage wheels that control the amount of disturbance and lateral soil splash.
T About 3 inch wide disturbed area per shank.  122106 DTL
T G2 was added into file in front of the flattening (P24), burial (P25), and resurfacing (P26) factors because the area affected is less than 1.0 and
T the RUSLE values were normalized to 1.0.  This change will imulate the correct residue changes based on the method set forth in RUSLE.
T RUSLE's factors have been redused to based on the area affected.
T The stalk fall rate factor (P34) was moved ahead of the new (G2) factor to set the fall rate to the less than 1.0 area affected.  8/7/07 MAS
T Created 12-11-07 MAS
+
G 01 Tillage
+ 101.600204 0.8 0.25 101.600204 76.20015 152.4003
P 01 Break Crust
P 02 Random Roughness
+ 1 15.240031
P 05 Ridges and Dikes
+ 1 50.800102 381.00076 254.0005 0.0 0.0
P 11 Aggregate Crushing
+ 2.4 2.0
P 12 Soil Loosening
+ 0.7
P 13 Soil Layer Mixing
+ 0.2
P 40 End crop Biomass Manipulation
P 34 Change Standing Biomass Fall Rate
+ 7 3.0 2.5 2.0 1.5 1.0
+ 0.5 0.6 0.7 0.8 1.0
G 02 Biomass Manipulation
+ 1.0
P 24 Flatten Standing Biomass
+ 0 0.5 0.45 0.4 0.4 1.0
P 25 Bury Flat Biomass
+ 1 0.17 .13 .099 0.086 0.14
P 26 Resurface Buried Biomass
+ 0.04 0.04 0.04 0.06 0.06
#------------
D 01/05/01
O 03 Planter, transplanter, vegetable
+ 7.4831395 3.12 0.89405453 0.0 0.89405453 0.44702727 1.3410819
T G2 was added into file in front of the flattening (P24), burial (P25), and resurfacing (P26) factors because the area affected is less than 1.0 and
T the RUSLE values were normalized to 1.0.  This change will imulate the correct residue changes based on the method set forth in RUSLE.
T RUSLE's factors have been redused to based on the area affected.
T The stalk fall rate factor (P34) was moved ahead of the new (G2) factor to set the fall rate to theless than 1.0 area affected.  8/7/07 MAS
T
T Changed the P5 to allow the preexisting ridges and furrows to set the ridge roughness.  MAS  12-30-2010
+
G 01 Tillage
+ 152.4003 0.4 0.2 152.4003 101.600204 203.20041
P 01 Break Crust
P 02 Random Roughness
+ 1 10.160021
P 05 Ridges and Dikes
+ 0 50.800102 762.0015 635.0013 0.0 0.0
P 11 Aggregate Crushing
+ 2.4 2.0
P 12 Soil Loosening
+ 0.6
P 13 Soil Layer Mixing
+ 0.3
P 34 Change Standing Biomass Fall Rate
+ 7 3.0 2.5 2.0 1.5 1.0
+ 0.5 0.6 0.7 0.8 1.0
G 02 Biomass Manipulation
+ 1.0
P 24 Flatten Standing Biomass
+ 0 0.3 0.25 0.2 0.1 1.0
P 25 Bury Flat Biomass
+ 1 .07 0.05 .04 .02 .03
P 26 Resurface Buried Biomass
+ 0.01 0.01 0.01 0.02 0.01
G 03 Crop Name
+ Tomato, fresh mkt
P 51 Seeding Configuration
+ 1 0.0 2
+ 2.0 1.0 1 300 1.0 1.0 0
+ cwt/ac
+ 94.0 89.3 4 1.0 0.65 0.95
+ 0.8 0.025 1.5 10.0 27.0 0 70 750.0
+ -1.0 -4.0 0.15 0.95 0.0 30.0
+ -0.0198 0.6575 0.4807 -0.1453 -0.336 1.3726 0.5408 0.1081
+ 0.4807 -0.1453 3.08 1.0 31.1 0.01 1 1.1170388
+ 1700.0 1700.0 3.0 0.03 0.0 0.0 0.0 1
+ 0.02 0.02 0.02 0.02 0.2 0.0050 20.0 2.7
+ -1.20379 0.604887 0.0767 0.012329351 0.0 0.0 0.0 0.0
T This records comes from ARS tomato transplant record and has the yield,
T Residue yield ration and the yield intercept changed to RUSLE values MAS 3-6-07
T Made changes as Fred instructed, mass of planting MAS 3/15/07
#------------
D 10/05/01
O 04 Sprayer, insecticide post emergence
+ 1.2160101 0.15
T Spray pest control chemicals on growing crop.   Crop is not killed.  11/17/01 DTL
T
T Added to the DB.  This assumes no crop flattening.  4-5-12 MAS
+
#------------
D 24/05/01
O 04 Sprayer, insecticide post emergence
+ 1.2160101 0.15
T Spray pest control chemicals on growing crop.   Crop is not killed.  11/17/01 DTL
T
T Added to the DB.  This assumes no crop flattening.  4-5-12 MAS
+
#------------
D 07/06/01
O 04 Sprayer, insecticide post emergence
+ 1.2160101 0.15
T Spray pest control chemicals on growing crop.   Crop is not killed.  11/17/01 DTL
T
T Added to the DB.  This assumes no crop flattening.  4-5-12 MAS
+
#------------
D 21/06/01
O 04 Sprayer, insecticide post emergence
+ 1.2160101 0.15
T Spray pest control chemicals on growing crop.   Crop is not killed.  11/17/01 DTL
T
T Added to the DB.  This assumes no crop flattening.  4-5-12 MAS
+
#------------
D 15/07/01
O 04 Harvest, hand pick vegetables
+ 3.2738733 0.15
T Hand pick tomato, artichoke, peppers, strawberries or similar crops
T with multiple harvests from the same plants.  12-13-2011 DTL
T This is a partial harvest only 50% of the yield is taken with this harvest.
T This operation MUST be followed by a final harvest operation.
T Crops that use multiple harvests must be manually calibrated.
T Added 12-27-11 MAS
+
G 02 Biomass Manipulation
+ 1.0
P 31 Kill or Defoliate Growing Crop
+ 0
P 62 Remove (by age pool) Plant/Residue Material
+ 1 0 0 0 3 3 2 0.5 0.0 0.0 0.0 0.0
P 40 End crop Biomass Manipulation
#------------
*END
*EOF
