Version: 1.5
*START 7
N Originating Program: RUSLE2
N Skel Format Version: 1.1
N This management file was originally converted from the NRCS standard XML format on - Thu Jul 05 09:33:29 PDT 2012
N This management file was updated to contain the most current crop and operation records for WEPS on - Tue Dec 17 21:16:44 CST 2013
#------------
D 15/08/01
O 03 Disk, tandem secondary op
+ 4.4898834 32.5 2.2351363 0.0 2.2351363 1.3410819 2.6821637
T 9-in. Spacing, Front and Rear; Good for seedbed preparation/chemical incorporation in medium to heavy soils
T Works well in primary tillage in light to medium soils
T Provides good residue-handling capability.  MAS 10-26-06
+
G 01 Tillage
+ 127.00027 0.75 1.0 127.00026 76.20015 152.4003
P 01 Break Crust
P 02 Random Roughness
+ 1 15.240031
P 05 Ridges and Dikes
+ 1 50.800102 228.60046 0.0 0.0 0.0
P 11 Aggregate Crushing
+ 2.8 0.75
P 12 Soil Loosening
+ 0.85
P 13 Soil Layer Mixing
+ 0.4
P 31 Kill or Defoliate Growing Crop
+ 2
P 40 End crop Biomass Manipulation
P 24 Flatten Standing Biomass
+ 0 0.85 0.7 0.6 0.5 1.0
P 25 Bury Flat Biomass
+ 1 0.73 0.63 0.55 0.4 0.73
P 26 Resurface Buried Biomass
+ 0.02 0.04 0.02 0.05 0.02
P 34 Change Standing Biomass Fall Rate
+ 7 3.0 2.5 2.0 1.5 1.0
+ 0.5 0.6 0.7 0.8 1.0
#------------
D 15/08/05
O 03 Disk, tandem secondary op
+ 4.4898834 32.5 2.2351363 0.0 2.2351363 1.3410819 2.6821637
T 9-in. Spacing, Front and Rear; Good for seedbed preparation/chemical incorporation in medium to heavy soils
T Works well in primary tillage in light to medium soils
T Provides good residue-handling capability.  MAS 10-26-06
+
G 01 Tillage
+ 127.00027 0.75 1.0 127.00026 76.20015 152.4003
P 01 Break Crust
P 02 Random Roughness
+ 1 15.240031
P 05 Ridges and Dikes
+ 1 50.800102 228.60046 0.0 0.0 0.0
P 11 Aggregate Crushing
+ 2.8 0.75
P 12 Soil Loosening
+ 0.85
P 13 Soil Layer Mixing
+ 0.4
P 31 Kill or Defoliate Growing Crop
+ 2
P 40 End crop Biomass Manipulation
P 24 Flatten Standing Biomass
+ 0 0.85 0.7 0.6 0.5 1.0
P 25 Bury Flat Biomass
+ 1 0.73 0.63 0.55 0.4 0.73
P 26 Resurface Buried Biomass
+ 0.02 0.04 0.02 0.05 0.02
P 34 Change Standing Biomass Fall Rate
+ 7 3.0 2.5 2.0 1.5 1.0
+ 0.5 0.6 0.7 0.8 1.0
#------------
*END
*EOF
