Version: 1.5
*START 7
N Originating Program: RUSLE2
N Skel Format Version: 1.1
N This management file was originally converted from the NRCS standard XML format on - Thu Jul 05 09:36:45 PDT 2012
N This management file was updated to contain the most current crop and operation records for WEPS on - Tue Dec 17 21:11:00 CST 2013
#------------
D 15/03/01
O 03 Plow, moldboard 6-7 inch depth
+ 17.491838 48.75 2.2351363 0.0 2.2351363 1.5645955 2.6821637
T Moldboard plow 6-7 inch operating depth.  020904 DTL
T MAS 11-29-07
+
G 01 Tillage
+ 152.4003 1.0 1.0 152.4003 101.600204 203.20041
P 01 Break Crust
P 02 Random Roughness
+ 1 48.260098
P 05 Ridges and Dikes
+ 1 25.400051 406.40082 0.0 0.0 0.0
P 11 Aggregate Crushing
+ 2.8 1.0
P 12 Soil Loosening
+ 1.0
P 13 Soil Layer Mixing
+ 0.7
P 14 Soil Layer Inversion
P 31 Kill or Defoliate Growing Crop
+ 2
P 40 End crop Biomass Manipulation
P 24 Flatten Standing Biomass
+ 0 0.98 0.98 0.95 0.75 1.0
P 25 Bury Flat Biomass
+ 3 0.99 0.98 0.98 0.85 0.97
P 26 Resurface Buried Biomass
+ 0.01 0.02 0.04 0.1 0.02
P 34 Change Standing Biomass Fall Rate
+ 7 3.0 2.5 2.0 1.5 1.0
+ 0.5 0.6 0.7 0.8 1.0
#------------
D 15/05/01
O 03 Disk, tandem secondary op
+ 4.4898834 32.5 2.2351363 0.0 2.2351363 1.3410819 2.6821637
T 9-in. Spacing, Front and Rear; Good for seedbed preparation/chemical incorporation in medium to heavy soils
T Works well in primary tillage in light to medium soils
T Provides good residue-handling capability.  MAS 10-26-06
+
G 01 Tillage
+ 127.00027 0.75 1.0 127.00026 76.20015 152.4003
P 01 Break Crust
P 02 Random Roughness
+ 1 15.240031
P 05 Ridges and Dikes
+ 1 50.800102 228.60046 0.0 0.0 0.0
P 11 Aggregate Crushing
+ 2.8 0.75
P 12 Soil Loosening
+ 0.85
P 13 Soil Layer Mixing
+ 0.4
P 31 Kill or Defoliate Growing Crop
+ 2
P 40 End crop Biomass Manipulation
P 24 Flatten Standing Biomass
+ 0 0.85 0.7 0.6 0.5 1.0
P 25 Bury Flat Biomass
+ 1 0.73 0.63 0.55 0.4 0.73
P 26 Resurface Buried Biomass
+ 0.02 0.04 0.02 0.05 0.02
P 34 Change Standing Biomass Fall Rate
+ 7 3.0 2.5 2.0 1.5 1.0
+ 0.5 0.6 0.7 0.8 1.0
#------------
D 25/05/01
O 04 Fert applic. surface broadcast
+ 1.4966278 0.0609375
T R2 Notes: Broadcast fertilizer spreader.  Wheel traffic only.  rev 082107 DTL
T
T Added to DB 4-12-12 MAS
+
G 01 Tillage
+ 0.0 0 0.05 0.0 0.0 0.0
P 01 Break Crust
P 02 Random Roughness
+ 1 8.8900175
P 11 Aggregate Crushing
+ 4.3 2.0
P 24 Flatten Standing Biomass
+ 0 0.25 0.2 0.15 0.1 1.0
P 26 Resurface Buried Biomass
+ 0.07 0.08 0.1 0.12 0.07
P 34 Change Standing Biomass Fall Rate
+ 0 1.0 1.0 1.0 1.0 1.0
+ 1.0 1.0 1.0 1.0 1.0
#------------
D 25/05/01
O 03 Disk, tandem light finishing
+ 3.7415698 19.5 2.2351363 0.0 2.2351363 1.3410819 2.6821637
T 6/8/01 DTL RUSLE.  7in sp.  This is tool used to finish a seedbed.  MAS 10-26-06
+
G 01 Tillage
+ 101.600204 0.5 1.0 101.600204 76.20015 127.00026
P 01 Break Crust
P 02 Random Roughness
+ 1 15.240031
P 05 Ridges and Dikes
+ 1 12.700026 177.80035 0.0 0.0 0.0
P 11 Aggregate Crushing
+ 2.8 0.75
P 12 Soil Loosening
+ 0.75
P 13 Soil Layer Mixing
+ 0.35
P 31 Kill or Defoliate Growing Crop
+ 2
P 40 End crop Biomass Manipulation
P 24 Flatten Standing Biomass
+ 0 0.85 0.7 0.6 0.5 1.0
P 25 Bury Flat Biomass
+ 1 0.73 0.63 0.55 0.4 0.73
P 26 Resurface Buried Biomass
+ 0.02 0.04 0.02 0.05 0.02
P 34 Change Standing Biomass Fall Rate
+ 7 3.0 2.5 2.0 1.5 1.0
+ 0.5 0.6 0.7 0.8 1.0
#------------
D 25/05/01
O 04 Sprayer, pre-emergence
+ 1.2160101 .15
T Spray pest control chemicals on growing crop.  Crop is not killed.
T In the MCREW management screen the user must select the kind of weeds killed in the growing crop as external residue.   080404 DTL
T Cloned from Defoliate (spray) crop.oprn, Changed the P31 to No crop kill and added G4 to add material to field MAS 9-28-06
+
G 03 Crop Name
+ weed residue; 0-3 mo
P 65 Add Crop Residue Amounts
+ 0.0 0.0 0.0 0.0 1
+ 0.0 0.0 0.0056042504 152.4003
+ 0.025 0.025 0.025 0.025 0.169 0.0050 17.1 5.227942
+ -1.20379 0.604887
T Enter crop notes here.
#------------
D 26/05/01
O 03 Planter, transplanter, vegetable
+ 7.4831395 3.12 0.89405453 0.0 0.89405453 0.44702727 1.3410819
T G2 was added into file in front of the flattening (P24), burial (P25), and resurfacing (P26) factors because the area affected is less than 1.0 and
T the RUSLE values were normalized to 1.0.  This change will imulate the correct residue changes based on the method set forth in RUSLE.
T RUSLE's factors have been redused to based on the area affected.
T The stalk fall rate factor (P34) was moved ahead of the new (G2) factor to set the fall rate to theless than 1.0 area affected.  8/7/07 MAS
T
T Changed the P5 to allow the preexisting ridges and furrows to set the ridge roughness.  MAS  12-30-2010
+
G 01 Tillage
+ 152.4003 0.4 0.2 152.4003 101.600204 203.20041
P 01 Break Crust
P 02 Random Roughness
+ 1 10.160021
P 05 Ridges and Dikes
+ 0 50.800102 762.0015 635.0013 0.0 0.0
P 11 Aggregate Crushing
+ 2.4 2.0
P 12 Soil Loosening
+ 0.6
P 13 Soil Layer Mixing
+ 0.3
P 34 Change Standing Biomass Fall Rate
+ 7 3.0 2.5 2.0 1.5 1.0
+ 0.5 0.6 0.7 0.8 1.0
G 02 Biomass Manipulation
+ 1.0
P 24 Flatten Standing Biomass
+ 0 0.3 0.25 0.2 0.1 1.0
P 25 Bury Flat Biomass
+ 1 .07 0.05 .04 .02 .03
P 26 Resurface Buried Biomass
+ 0.01 0.01 0.01 0.02 0.01
G 03 Crop Name
+ Tobacco, burley
P 51 Seeding Configuration
+ 1 0.0 2
+ 2.0 1.0 1 25 1.0 1.0 3
+ ton/ac
+ 11.0 8930.0 4 0.8 0.65 0.95
+ 2.5 0.025 2.0 8.0 25.0 0 100 1400.0
+ -5.0 -15.0 0.15 0.95 0.0 30.0
+ 0.0 0.8008 0.8341 -0.0737 0.0 1.0 1.1 0.01
+ 0.3726 -0.0744 2.0 1.0 10.0 0.03 1 1.1170388
+ 500.0 500.0 2.0 0.03 0.1 0.1 0.0 3
+ 0.02 0.02 0.02 0.02 0.2 0.0050 20.0 2.9797485
+ -1.20379 0.604887 .8308 0.025006166 0.0 0.0 0.0 0.0
T Cloned from WEPS tobacco, leaf, transplants 10-19-06 MAS
#------------
D 05/06/01
O 03 Cultivator, row 1 in ridge
+ 5.799433 14.63 2.2351363 0.0 2.2351363 0.89405453 2.4586499
T RUSLE:Row crop cultivator w/ sweeps leaving a 1" ridge 05-14-02 DTL
T G2 was added into file in front of the flattening (P24), burial (P25), and resurfacing (P26) factors because the area affected is less than 1.0 and
T the RUSLE values were normalized to 1.0.  This change will imulate the correct residue changes based on the method set forth in RUSLE.
T RUSLE's factors have been redused to based on the area affected.
T The stalk fall rate factor (P34) was moved ahead of the new (G2) factor to set the fall rate to the less than 1.0 area affected.  8/8/07 MAS
+
G 01 Tillage
+ 76.20015 0.5 .75 76.20015 50.800102 101.600204
P 01 Break Crust
P 02 Random Roughness
+ 1 7.6200156
P 05 Ridges and Dikes
+ 1 25.400051 762.0015 0.0 0.0 0.0
P 11 Aggregate Crushing
+ 3.0 1.0
P 12 Soil Loosening
+ 0.75
P 13 Soil Layer Mixing
+ 0.35
P 34 Change Standing Biomass Fall Rate
+ 4 3.0 2.5 2.0 1.5 1.0
+ 0.5 0.6 0.7 0.8 1.0
G 02 Biomass Manipulation
+ 1.0
P 24 Flatten Standing Biomass
+ 14 0.7 0.3 0.3 0.1 1.0
P 25 Bury Flat Biomass
+ 1 .57 0.5 0.44 0.32 0.64
P 26 Resurface Buried Biomass
+ 0.01 0.01 0.01 0.01 0.01
#------------
D 05/06/01
O 04 Sprayer, post emergence
+ 1.2160101 .15
T Spray pest control chemicals on growing crop.  Crop is not killed.
T In the MCREW management screen the user must select the kind of weeds killed in the growing crop as external residue.   080404 DTL
T Cloned from Defoliate (spray) crop.oprn, Changed the P31 to No crop kill and added G4 to add material to field MAS 9-28-06
T DO NOT LEAVE CROP COLUMN SET TO "no crop".  User must select the crop and then drill into the operation and specify the amount of weed
T mass that will be killed and turned into residue.
+
G 03 Crop Name
+ weed residue; 0-3 mo
P 65 Add Crop Residue Amounts
+ 0.0 0.0 0.0 0.028021252 1
+ 0.0 0.0 0.0056042504 152.4003
+ 0.025 0.025 0.025 0.025 0.169 0.0050 17.1 5.227942
+ -1.20379 0.604887
T Enter crop notes here.
#------------
D 20/06/01
O 03 Cultivator, row 3 in ridge
+ 5.799433 17.55 2.2351363 0.0 2.2351363 0.89405453 2.4586499
T Row crop cultivator w/ sweeps leaving a 3" ridge 05-14-02 DTL
T G2 was added into file in front of the flattening (P24), burial (P25), and resurfacing (P26) factors because the area affected is less than 1.0 and
T the RUSLE values were normalized to 1.0.  This change will imulate the correct residue changes based on the method set forth in RUSLE.
T RUSLE's factors have been redused to based on the area affected.
T The stalk fall rate factor (P34) was moved ahead of the new (G2) factor to set the fall rate to the  less than 1.0 area affected.  8/7/07 MAS
+
G 01 Tillage
+ 76.20015 0.5 .9 76.20015 50.800102 101.600204
P 01 Break Crust
P 02 Random Roughness
+ 1 15.240031
P 05 Ridges and Dikes
+ 1 76.20015 762.0015 0.0 0.0 0.0
P 11 Aggregate Crushing
+ 3.0 1.0
P 12 Soil Loosening
+ 0.75
P 13 Soil Layer Mixing
+ 0.35
P 34 Change Standing Biomass Fall Rate
+ 4 3.0 2.5 2.0 1.5 1.0
+ 0.5 0.6 0.7 0.8 1.0
G 02 Biomass Manipulation
+ 1.0
P 24 Flatten Standing Biomass
+ 14 0.7 0.3 0.3 0.1 1.0
P 25 Bury Flat Biomass
+ 1 0.68 0.6 0.52 0.39 0.77
P 26 Resurface Buried Biomass
+ 0.04 0.04 0.04 0.06 0.04
#------------
D 20/06/01
O 04 Sprayer, fungicide and insecticide tank mix
+ 1.2160101 .15
T Spray pest control chemicals on growing crop.  Crop is not killed.
T In the MCREW management screen the user must select the kind of weeds killed in the growing crop as external residue.   080404 DTL
T Cloned from Defoliate (spray) crop.oprn, Changed the P31 to No crop kill and added G4 to add material to field MAS 9-28-06
+
#------------
D 20/07/01
O 04 Sprayer, insecticide post emergence
+ 1.2160101 0.15
T Spray pest control chemicals on growing crop.   Crop is not killed.  11/17/01 DTL
T
T Added to the DB.  This assumes no crop flattening.  4-5-12 MAS
+
#------------
D 20/08/01
O 04 Sprayer, insecticide post emergence
+ 1.2160101 0.15
T Spray pest control chemicals on growing crop.   Crop is not killed.  11/17/01 DTL
T
T Added to the DB.  This assumes no crop flattening.  4-5-12 MAS
+
#------------
D 10/09/01
O 04 Harvest, tobacco, burley
+ 3.2738733 .15
T Harvest of burley tobacco where entire plant is cut and removed leaving only short stubble.  021109 DTL
T Modified to remove the entire plant MAS 8-27-10
T Estimate that 10% of the stem remains.  Plant is cut and removed by hand.
T Removed 100% of the flower fraction because some of the plant mass may have gone to fruiting or grain. 12-19-11 MAS
T
T ARS record - filename is:  Harvest Tobacco - leaf (hand pick).oprn
T This record is based on the "Harvest Template (pick and remove).oprn" template.
T The plant material harvested was changed from "grain" to "leaves".
T This operation record is designed to represent a typical tobacco leaf
T harvesting operation that removes all the leaves without cutting the crop stalks
T and kills the crop.  No flattening of any standing stalks occurs.
T 200x	Created - Fred Fox
T Nov 01, 2005	Updated notes - Larry Wagner
T Detailed info regarding this operation record:
+
G 02 Biomass Manipulation
+ 1.0
P 31 Kill or Defoliate Growing Crop
+ 2
P 62 Remove (by age pool) Plant/Residue Material
+ 1 1 0 1 1 3 2 0 0.95 0.9 0.0 0.0
P 34 Change Standing Biomass Fall Rate
+ 0 1.0 1.0 1.0 1.0 1.0
+ 1.0 1.0 1.0 1.0 1.0
P 40 End crop Biomass Manipulation
#------------
D 15/10/01
O 03 Disk, tandem light finishing
+ 3.7415698 19.5 2.2351363 0.0 2.2351363 1.3410819 2.6821637
T 6/8/01 DTL RUSLE.  7in sp.  This is tool used to finish a seedbed.  MAS 10-26-06
+
G 01 Tillage
+ 101.600204 0.5 1.0 101.600204 76.20015 127.00026
P 01 Break Crust
P 02 Random Roughness
+ 1 15.240031
P 05 Ridges and Dikes
+ 1 12.700026 177.80035 0.0 0.0 0.0
P 11 Aggregate Crushing
+ 2.8 0.75
P 12 Soil Loosening
+ 0.75
P 13 Soil Layer Mixing
+ 0.35
P 31 Kill or Defoliate Growing Crop
+ 2
P 40 End crop Biomass Manipulation
P 24 Flatten Standing Biomass
+ 0 0.85 0.7 0.6 0.5 1.0
P 25 Bury Flat Biomass
+ 1 0.73 0.63 0.55 0.4 0.73
P 26 Resurface Buried Biomass
+ 0.02 0.04 0.02 0.05 0.02
P 34 Change Standing Biomass Fall Rate
+ 7 3.0 2.5 2.0 1.5 1.0
+ 0.5 0.6 0.7 0.8 1.0
#------------
D 01/11/01
O 03 Drill or air seeder single disk openers 7-10 in spac
+ 3.2738733 2.44 2.2351363 0.0 2.2351363 1.5645955 2.9056773
T Drill or Air seeder with single disk no-till openers  JD 750 or similar openers. (No-till air drill)
T Based on Drill, no-till single disk 7-10 spacing. 102403 DTL. RUSLE MAS 10-26-06
T G2 was added into file in front of the flattening (P24), burial (P25), and resurfacing (P26) factors because the area affected is less than 1.0 and
T the RUSLE values were normalized to 1.0.  This change will imulate the correct residue changes based on the method set forth in RUSLE.
T RUSLE's factors have been redused to based on the area affected.
T The stalk fall rate factor (P34) was moved ahead of the new (G2) factor to set the fall rate to the less than 1.0 area affected.  8/7/07 MAS
+
G 01 Tillage
+ 63.500134 0.4 0.15 63.50013 50.800102 101.600204
P 01 Break Crust
P 02 Random Roughness
+ 1 7.6200156
P 05 Ridges and Dikes
+ 1 25.400051 203.20041 0.0 0.0 0.0
P 11 Aggregate Crushing
+ 2.8 0.75
P 12 Soil Loosening
+ 0.4
P 13 Soil Layer Mixing
+ 0.20
P 34 Change Standing Biomass Fall Rate
+ 7 3.0 2.5 2.0 1.5 1.0
+ 0.5 0.6 0.7 0.8 1.0
G 02 Biomass Manipulation
+ 1.0
P 24 Flatten Standing Biomass
+ 0 0.6 0.4 0.35 0.15 1.0
P 25 Bury Flat Biomass
+ 1 0.05 0.04 0.03 0.02 0.03
P 26 Resurface Buried Biomass
+ 0.01 0.01 0.01 0.05 0.01
G 03 Crop Name
+ Wheat, winter cover
P 51 Seeding Configuration
+ 1 0.0 0
+ 220.0 8.0 0 2000 1.0 1.0 2
+ lbs/ac
+ 0 8930.0 5 1.0 0.6 0.8
+ 1.2 0.025 2.0 0.0 25.0 1 60 1800.0
+ -5.0 -15.0 0.005 0.05 0.035 30.0
+ 0.013 0.8013 0.4293 -0.086 -0.018 0.932 0.556 0.0736
+ 0.3293 -0.086 2.87 1.0 20.0 0.05 0 0.3
+ 28.571428 335.0 1.4 0.012 0.1 0.1 0.0 2
+ 0.0133 0.0133 0.0133 0.0133 0.04 0.0050 17.1 5.227942
+ -2.08165 0.548606 0 0.0 0.0 0.0 0.0 0.0
T Rusle Notes: Winter wheat cover.   Drilled in 7 inch rows.   Chemically killed  in late boot stage.  Not harvested for grain.
T Base location Columbia, MO. REV 61901 DTL
T
T Cloned 2-16-07 MAS
T
T Standing Fall rate reduced from 0.12 to 0.04 #/(# days) because
T WW-Chem fallow in SW KS showed too much standing residue was falling down.  Larry Wagner recommended we
T reduce fall rate. Dave L, Linda S., and I made runs to get the wt to match the standing stalk wt from Fred Fox stalk residue
T samples WERU Lab.  This rate left 24% of the starting count standing.  This is well within the range of values of two paper.
T Both paper showed about 46% left standing at the 440 day after harvest time.  David Nelson, ARS Akron, CO also confirmed
T that the orginal 8% standing was too low.  He thought that the 24% was much more resonable.  MAS 6-7-11
#------------
D 15/03/02
O 03 Plow, moldboard 6-7 inch depth
+ 17.491838 48.75 2.2351363 0.0 2.2351363 1.5645955 2.6821637
T Moldboard plow 6-7 inch operating depth.  020904 DTL
T MAS 11-29-07
+
G 01 Tillage
+ 152.4003 1.0 1.0 152.4003 101.600204 203.20041
P 01 Break Crust
P 02 Random Roughness
+ 1 48.260098
P 05 Ridges and Dikes
+ 1 25.400051 406.40082 0.0 0.0 0.0
P 11 Aggregate Crushing
+ 2.8 1.0
P 12 Soil Loosening
+ 1.0
P 13 Soil Layer Mixing
+ 0.7
P 14 Soil Layer Inversion
P 31 Kill or Defoliate Growing Crop
+ 2
P 40 End crop Biomass Manipulation
P 24 Flatten Standing Biomass
+ 0 0.98 0.98 0.95 0.75 1.0
P 25 Bury Flat Biomass
+ 3 0.99 0.98 0.98 0.85 0.97
P 26 Resurface Buried Biomass
+ 0.01 0.02 0.04 0.1 0.02
P 34 Change Standing Biomass Fall Rate
+ 7 3.0 2.5 2.0 1.5 1.0
+ 0.5 0.6 0.7 0.8 1.0
#------------
D 15/05/02
O 03 Disk, tandem secondary op
+ 4.4898834 32.5 2.2351363 0.0 2.2351363 1.3410819 2.6821637
T 9-in. Spacing, Front and Rear; Good for seedbed preparation/chemical incorporation in medium to heavy soils
T Works well in primary tillage in light to medium soils
T Provides good residue-handling capability.  MAS 10-26-06
+
G 01 Tillage
+ 127.00027 0.75 1.0 127.00026 76.20015 152.4003
P 01 Break Crust
P 02 Random Roughness
+ 1 15.240031
P 05 Ridges and Dikes
+ 1 50.800102 228.60046 0.0 0.0 0.0
P 11 Aggregate Crushing
+ 2.8 0.75
P 12 Soil Loosening
+ 0.85
P 13 Soil Layer Mixing
+ 0.4
P 31 Kill or Defoliate Growing Crop
+ 2
P 40 End crop Biomass Manipulation
P 24 Flatten Standing Biomass
+ 0 0.85 0.7 0.6 0.5 1.0
P 25 Bury Flat Biomass
+ 1 0.73 0.63 0.55 0.4 0.73
P 26 Resurface Buried Biomass
+ 0.02 0.04 0.02 0.05 0.02
P 34 Change Standing Biomass Fall Rate
+ 7 3.0 2.5 2.0 1.5 1.0
+ 0.5 0.6 0.7 0.8 1.0
#------------
D 25/05/02
O 04 Fert applic. surface broadcast
+ 1.4966278 0.0609375
T R2 Notes: Broadcast fertilizer spreader.  Wheel traffic only.  rev 082107 DTL
T
T Added to DB 4-12-12 MAS
+
G 01 Tillage
+ 0.0 0 0.05 0.0 0.0 0.0
P 01 Break Crust
P 02 Random Roughness
+ 1 8.8900175
P 11 Aggregate Crushing
+ 4.3 2.0
P 24 Flatten Standing Biomass
+ 0 0.25 0.2 0.15 0.1 1.0
P 26 Resurface Buried Biomass
+ 0.07 0.08 0.1 0.12 0.07
P 34 Change Standing Biomass Fall Rate
+ 0 1.0 1.0 1.0 1.0 1.0
+ 1.0 1.0 1.0 1.0 1.0
#------------
D 25/05/02
O 03 Disk, tandem light finishing
+ 3.7415698 19.5 2.2351363 0.0 2.2351363 1.3410819 2.6821637
T 6/8/01 DTL RUSLE.  7in sp.  This is tool used to finish a seedbed.  MAS 10-26-06
+
G 01 Tillage
+ 101.600204 0.5 1.0 101.600204 76.20015 127.00026
P 01 Break Crust
P 02 Random Roughness
+ 1 15.240031
P 05 Ridges and Dikes
+ 1 12.700026 177.80035 0.0 0.0 0.0
P 11 Aggregate Crushing
+ 2.8 0.75
P 12 Soil Loosening
+ 0.75
P 13 Soil Layer Mixing
+ 0.35
P 31 Kill or Defoliate Growing Crop
+ 2
P 40 End crop Biomass Manipulation
P 24 Flatten Standing Biomass
+ 0 0.85 0.7 0.6 0.5 1.0
P 25 Bury Flat Biomass
+ 1 0.73 0.63 0.55 0.4 0.73
P 26 Resurface Buried Biomass
+ 0.02 0.04 0.02 0.05 0.02
P 34 Change Standing Biomass Fall Rate
+ 7 3.0 2.5 2.0 1.5 1.0
+ 0.5 0.6 0.7 0.8 1.0
#------------
D 25/05/02
O 04 Sprayer, pre-emergence
+ 1.2160101 .15
T Spray pest control chemicals on growing crop.  Crop is not killed.
T In the MCREW management screen the user must select the kind of weeds killed in the growing crop as external residue.   080404 DTL
T Cloned from Defoliate (spray) crop.oprn, Changed the P31 to No crop kill and added G4 to add material to field MAS 9-28-06
+
G 03 Crop Name
+ weed residue; 0-3 mo
P 65 Add Crop Residue Amounts
+ 0.0 0.0 0.0 0.0 1
+ 0.0 0.0 0.0056042504 152.4003
+ 0.025 0.025 0.025 0.025 0.169 0.0050 17.1 5.227942
+ -1.20379 0.604887
T Enter crop notes here.
#------------
D 26/05/02
O 03 Planter, transplanter, vegetable
+ 7.4831395 3.12 0.89405453 0.0 0.89405453 0.44702727 1.3410819
T G2 was added into file in front of the flattening (P24), burial (P25), and resurfacing (P26) factors because the area affected is less than 1.0 and
T the RUSLE values were normalized to 1.0.  This change will imulate the correct residue changes based on the method set forth in RUSLE.
T RUSLE's factors have been redused to based on the area affected.
T The stalk fall rate factor (P34) was moved ahead of the new (G2) factor to set the fall rate to theless than 1.0 area affected.  8/7/07 MAS
T
T Changed the P5 to allow the preexisting ridges and furrows to set the ridge roughness.  MAS  12-30-2010
+
G 01 Tillage
+ 152.4003 0.4 0.2 152.4003 101.600204 203.20041
P 01 Break Crust
P 02 Random Roughness
+ 1 10.160021
P 05 Ridges and Dikes
+ 0 50.800102 762.0015 635.0013 0.0 0.0
P 11 Aggregate Crushing
+ 2.4 2.0
P 12 Soil Loosening
+ 0.6
P 13 Soil Layer Mixing
+ 0.3
P 34 Change Standing Biomass Fall Rate
+ 7 3.0 2.5 2.0 1.5 1.0
+ 0.5 0.6 0.7 0.8 1.0
G 02 Biomass Manipulation
+ 1.0
P 24 Flatten Standing Biomass
+ 0 0.3 0.25 0.2 0.1 1.0
P 25 Bury Flat Biomass
+ 1 .07 0.05 .04 .02 .03
P 26 Resurface Buried Biomass
+ 0.01 0.01 0.01 0.02 0.01
G 03 Crop Name
+ Tobacco, burley
P 51 Seeding Configuration
+ 1 0.0 2
+ 2.0 1.0 1 25 1.0 1.0 3
+ ton/ac
+ 11.0 8930.0 4 0.8 0.65 0.95
+ 2.5 0.025 2.0 8.0 25.0 0 100 1400.0
+ -5.0 -15.0 0.15 0.95 0.0 30.0
+ 0.0 0.8008 0.8341 -0.0737 0.0 1.0 1.1 0.01
+ 0.3726 -0.0744 2.0 1.0 10.0 0.03 1 1.1170388
+ 500.0 500.0 2.0 0.03 0.1 0.1 0.0 3
+ 0.02 0.02 0.02 0.02 0.2 0.0050 20.0 2.9797485
+ -1.20379 0.604887 .8308 0.025006166 0.0 0.0 0.0 0.0
T Cloned from WEPS tobacco, leaf, transplants 10-19-06 MAS
#------------
D 05/06/02
O 03 Cultivator, row 1 in ridge
+ 5.799433 14.63 2.2351363 0.0 2.2351363 0.89405453 2.4586499
T RUSLE:Row crop cultivator w/ sweeps leaving a 1" ridge 05-14-02 DTL
T G2 was added into file in front of the flattening (P24), burial (P25), and resurfacing (P26) factors because the area affected is less than 1.0 and
T the RUSLE values were normalized to 1.0.  This change will imulate the correct residue changes based on the method set forth in RUSLE.
T RUSLE's factors have been redused to based on the area affected.
T The stalk fall rate factor (P34) was moved ahead of the new (G2) factor to set the fall rate to the less than 1.0 area affected.  8/8/07 MAS
+
G 01 Tillage
+ 76.20015 0.5 .75 76.20015 50.800102 101.600204
P 01 Break Crust
P 02 Random Roughness
+ 1 7.6200156
P 05 Ridges and Dikes
+ 1 25.400051 762.0015 0.0 0.0 0.0
P 11 Aggregate Crushing
+ 3.0 1.0
P 12 Soil Loosening
+ 0.75
P 13 Soil Layer Mixing
+ 0.35
P 34 Change Standing Biomass Fall Rate
+ 4 3.0 2.5 2.0 1.5 1.0
+ 0.5 0.6 0.7 0.8 1.0
G 02 Biomass Manipulation
+ 1.0
P 24 Flatten Standing Biomass
+ 14 0.7 0.3 0.3 0.1 1.0
P 25 Bury Flat Biomass
+ 1 .57 0.5 0.44 0.32 0.64
P 26 Resurface Buried Biomass
+ 0.01 0.01 0.01 0.01 0.01
#------------
D 05/06/02
O 04 Sprayer, post emergence
+ 1.2160101 .15
T Spray pest control chemicals on growing crop.  Crop is not killed.
T In the MCREW management screen the user must select the kind of weeds killed in the growing crop as external residue.   080404 DTL
T Cloned from Defoliate (spray) crop.oprn, Changed the P31 to No crop kill and added G4 to add material to field MAS 9-28-06
T DO NOT LEAVE CROP COLUMN SET TO "no crop".  User must select the crop and then drill into the operation and specify the amount of weed
T mass that will be killed and turned into residue.
+
G 03 Crop Name
+ weed residue; 0-3 mo
P 65 Add Crop Residue Amounts
+ 0.0 0.0 0.0 0.028021252 1
+ 0.0 0.0 0.0056042504 152.4003
+ 0.025 0.025 0.025 0.025 0.169 0.0050 17.1 5.227942
+ -1.20379 0.604887
T Enter crop notes here.
#------------
D 20/06/02
O 03 Cultivator, row 3 in ridge
+ 5.799433 17.55 2.2351363 0.0 2.2351363 0.89405453 2.4586499
T Row crop cultivator w/ sweeps leaving a 3" ridge 05-14-02 DTL
T G2 was added into file in front of the flattening (P24), burial (P25), and resurfacing (P26) factors because the area affected is less than 1.0 and
T the RUSLE values were normalized to 1.0.  This change will imulate the correct residue changes based on the method set forth in RUSLE.
T RUSLE's factors have been redused to based on the area affected.
T The stalk fall rate factor (P34) was moved ahead of the new (G2) factor to set the fall rate to the  less than 1.0 area affected.  8/7/07 MAS
+
G 01 Tillage
+ 76.20015 0.5 .9 76.20015 50.800102 101.600204
P 01 Break Crust
P 02 Random Roughness
+ 1 15.240031
P 05 Ridges and Dikes
+ 1 76.20015 762.0015 0.0 0.0 0.0
P 11 Aggregate Crushing
+ 3.0 1.0
P 12 Soil Loosening
+ 0.75
P 13 Soil Layer Mixing
+ 0.35
P 34 Change Standing Biomass Fall Rate
+ 4 3.0 2.5 2.0 1.5 1.0
+ 0.5 0.6 0.7 0.8 1.0
G 02 Biomass Manipulation
+ 1.0
P 24 Flatten Standing Biomass
+ 14 0.7 0.3 0.3 0.1 1.0
P 25 Bury Flat Biomass
+ 1 0.68 0.6 0.52 0.39 0.77
P 26 Resurface Buried Biomass
+ 0.04 0.04 0.04 0.06 0.04
#------------
D 20/06/02
O 04 Sprayer, fungicide and insecticide tank mix
+ 1.2160101 .15
T Spray pest control chemicals on growing crop.  Crop is not killed.
T In the MCREW management screen the user must select the kind of weeds killed in the growing crop as external residue.   080404 DTL
T Cloned from Defoliate (spray) crop.oprn, Changed the P31 to No crop kill and added G4 to add material to field MAS 9-28-06
+
#------------
D 20/07/02
O 04 Sprayer, insecticide post emergence
+ 1.2160101 0.15
T Spray pest control chemicals on growing crop.   Crop is not killed.  11/17/01 DTL
T
T Added to the DB.  This assumes no crop flattening.  4-5-12 MAS
+
#------------
D 20/08/02
O 04 Sprayer, insecticide post emergence
+ 1.2160101 0.15
T Spray pest control chemicals on growing crop.   Crop is not killed.  11/17/01 DTL
T
T Added to the DB.  This assumes no crop flattening.  4-5-12 MAS
+
#------------
D 10/09/02
O 04 Harvest, tobacco, burley
+ 3.2738733 .15
T Harvest of burley tobacco where entire plant is cut and removed leaving only short stubble.  021109 DTL
T Modified to remove the entire plant MAS 8-27-10
T Estimate that 10% of the stem remains.  Plant is cut and removed by hand.
T Removed 100% of the flower fraction because some of the plant mass may have gone to fruiting or grain. 12-19-11 MAS
T
T ARS record - filename is:  Harvest Tobacco - leaf (hand pick).oprn
T This record is based on the "Harvest Template (pick and remove).oprn" template.
T The plant material harvested was changed from "grain" to "leaves".
T This operation record is designed to represent a typical tobacco leaf
T harvesting operation that removes all the leaves without cutting the crop stalks
T and kills the crop.  No flattening of any standing stalks occurs.
T 200x	Created - Fred Fox
T Nov 01, 2005	Updated notes - Larry Wagner
T Detailed info regarding this operation record:
+
G 02 Biomass Manipulation
+ 1.0
P 31 Kill or Defoliate Growing Crop
+ 2
P 62 Remove (by age pool) Plant/Residue Material
+ 1 1 0 1 1 3 2 0 0.95 0.9 0.0 0.0
P 34 Change Standing Biomass Fall Rate
+ 0 1.0 1.0 1.0 1.0 1.0
+ 1.0 1.0 1.0 1.0 1.0
P 40 End crop Biomass Manipulation
#------------
D 15/10/02
O 03 Disk, tandem light finishing
+ 3.7415698 19.5 2.2351363 0.0 2.2351363 1.3410819 2.6821637
T 6/8/01 DTL RUSLE.  7in sp.  This is tool used to finish a seedbed.  MAS 10-26-06
+
G 01 Tillage
+ 101.600204 0.5 1.0 101.600204 76.20015 127.00026
P 01 Break Crust
P 02 Random Roughness
+ 1 15.240031
P 05 Ridges and Dikes
+ 1 12.700026 177.80035 0.0 0.0 0.0
P 11 Aggregate Crushing
+ 2.8 0.75
P 12 Soil Loosening
+ 0.75
P 13 Soil Layer Mixing
+ 0.35
P 31 Kill or Defoliate Growing Crop
+ 2
P 40 End crop Biomass Manipulation
P 24 Flatten Standing Biomass
+ 0 0.85 0.7 0.6 0.5 1.0
P 25 Bury Flat Biomass
+ 1 0.73 0.63 0.55 0.4 0.73
P 26 Resurface Buried Biomass
+ 0.02 0.04 0.02 0.05 0.02
P 34 Change Standing Biomass Fall Rate
+ 7 3.0 2.5 2.0 1.5 1.0
+ 0.5 0.6 0.7 0.8 1.0
#------------
D 01/11/02
O 03 Drill or air seeder single disk openers 7-10 in spac
+ 3.2738733 2.44 2.2351363 0.0 2.2351363 1.5645955 2.9056773
T Drill or Air seeder with single disk no-till openers  JD 750 or similar openers. (No-till air drill)
T Based on Drill, no-till single disk 7-10 spacing. 102403 DTL. RUSLE MAS 10-26-06
T G2 was added into file in front of the flattening (P24), burial (P25), and resurfacing (P26) factors because the area affected is less than 1.0 and
T the RUSLE values were normalized to 1.0.  This change will imulate the correct residue changes based on the method set forth in RUSLE.
T RUSLE's factors have been redused to based on the area affected.
T The stalk fall rate factor (P34) was moved ahead of the new (G2) factor to set the fall rate to the less than 1.0 area affected.  8/7/07 MAS
+
G 01 Tillage
+ 63.500134 0.4 0.15 63.50013 50.800102 101.600204
P 01 Break Crust
P 02 Random Roughness
+ 1 7.6200156
P 05 Ridges and Dikes
+ 1 25.400051 203.20041 0.0 0.0 0.0
P 11 Aggregate Crushing
+ 2.8 0.75
P 12 Soil Loosening
+ 0.4
P 13 Soil Layer Mixing
+ 0.20
P 34 Change Standing Biomass Fall Rate
+ 7 3.0 2.5 2.0 1.5 1.0
+ 0.5 0.6 0.7 0.8 1.0
G 02 Biomass Manipulation
+ 1.0
P 24 Flatten Standing Biomass
+ 0 0.6 0.4 0.35 0.15 1.0
P 25 Bury Flat Biomass
+ 1 0.05 0.04 0.03 0.02 0.03
P 26 Resurface Buried Biomass
+ 0.01 0.01 0.01 0.05 0.01
G 03 Crop Name
+ Wheat, winter cover
P 51 Seeding Configuration
+ 1 0.0 0
+ 220.0 8.0 0 2000 1.0 1.0 2
+ lbs/ac
+ 0 8930.0 5 1.0 0.6 0.8
+ 1.2 0.025 2.0 0.0 25.0 1 60 1800.0
+ -5.0 -15.0 0.005 0.05 0.035 30.0
+ 0.013 0.8013 0.4293 -0.086 -0.018 0.932 0.556 0.0736
+ 0.3293 -0.086 2.87 1.0 20.0 0.05 0 0.3
+ 28.571428 335.0 1.4 0.012 0.1 0.1 0.0 2
+ 0.0133 0.0133 0.0133 0.0133 0.04 0.0050 17.1 5.227942
+ -2.08165 0.548606 0 0.0 0.0 0.0 0.0 0.0
T Rusle Notes: Winter wheat cover.   Drilled in 7 inch rows.   Chemically killed  in late boot stage.  Not harvested for grain.
T Base location Columbia, MO. REV 61901 DTL
T
T Cloned 2-16-07 MAS
T
T Standing Fall rate reduced from 0.12 to 0.04 #/(# days) because
T WW-Chem fallow in SW KS showed too much standing residue was falling down.  Larry Wagner recommended we
T reduce fall rate. Dave L, Linda S., and I made runs to get the wt to match the standing stalk wt from Fred Fox stalk residue
T samples WERU Lab.  This rate left 24% of the starting count standing.  This is well within the range of values of two paper.
T Both paper showed about 46% left standing at the 440 day after harvest time.  David Nelson, ARS Akron, CO also confirmed
T that the orginal 8% standing was too low.  He thought that the 24% was much more resonable.  MAS 6-7-11
#------------
D 15/03/03
O 03 Plow, moldboard 6-7 inch depth
+ 17.491838 48.75 2.2351363 0.0 2.2351363 1.5645955 2.6821637
T Moldboard plow 6-7 inch operating depth.  020904 DTL
T MAS 11-29-07
+
G 01 Tillage
+ 152.4003 1.0 1.0 152.4003 101.600204 203.20041
P 01 Break Crust
P 02 Random Roughness
+ 1 48.260098
P 05 Ridges and Dikes
+ 1 25.400051 406.40082 0.0 0.0 0.0
P 11 Aggregate Crushing
+ 2.8 1.0
P 12 Soil Loosening
+ 1.0
P 13 Soil Layer Mixing
+ 0.7
P 14 Soil Layer Inversion
P 31 Kill or Defoliate Growing Crop
+ 2
P 40 End crop Biomass Manipulation
P 24 Flatten Standing Biomass
+ 0 0.98 0.98 0.95 0.75 1.0
P 25 Bury Flat Biomass
+ 3 0.99 0.98 0.98 0.85 0.97
P 26 Resurface Buried Biomass
+ 0.01 0.02 0.04 0.1 0.02
P 34 Change Standing Biomass Fall Rate
+ 7 3.0 2.5 2.0 1.5 1.0
+ 0.5 0.6 0.7 0.8 1.0
#------------
D 15/05/03
O 03 Disk, tandem secondary op
+ 4.4898834 32.5 2.2351363 0.0 2.2351363 1.3410819 2.6821637
T 9-in. Spacing, Front and Rear; Good for seedbed preparation/chemical incorporation in medium to heavy soils
T Works well in primary tillage in light to medium soils
T Provides good residue-handling capability.  MAS 10-26-06
+
G 01 Tillage
+ 127.00027 0.75 1.0 127.00026 76.20015 152.4003
P 01 Break Crust
P 02 Random Roughness
+ 1 15.240031
P 05 Ridges and Dikes
+ 1 50.800102 228.60046 0.0 0.0 0.0
P 11 Aggregate Crushing
+ 2.8 0.75
P 12 Soil Loosening
+ 0.85
P 13 Soil Layer Mixing
+ 0.4
P 31 Kill or Defoliate Growing Crop
+ 2
P 40 End crop Biomass Manipulation
P 24 Flatten Standing Biomass
+ 0 0.85 0.7 0.6 0.5 1.0
P 25 Bury Flat Biomass
+ 1 0.73 0.63 0.55 0.4 0.73
P 26 Resurface Buried Biomass
+ 0.02 0.04 0.02 0.05 0.02
P 34 Change Standing Biomass Fall Rate
+ 7 3.0 2.5 2.0 1.5 1.0
+ 0.5 0.6 0.7 0.8 1.0
#------------
D 25/05/03
O 04 Fert applic. surface broadcast
+ 1.4966278 0.0609375
T R2 Notes: Broadcast fertilizer spreader.  Wheel traffic only.  rev 082107 DTL
T
T Added to DB 4-12-12 MAS
+
G 01 Tillage
+ 0.0 0 0.05 0.0 0.0 0.0
P 01 Break Crust
P 02 Random Roughness
+ 1 8.8900175
P 11 Aggregate Crushing
+ 4.3 2.0
P 24 Flatten Standing Biomass
+ 0 0.25 0.2 0.15 0.1 1.0
P 26 Resurface Buried Biomass
+ 0.07 0.08 0.1 0.12 0.07
P 34 Change Standing Biomass Fall Rate
+ 0 1.0 1.0 1.0 1.0 1.0
+ 1.0 1.0 1.0 1.0 1.0
#------------
D 25/05/03
O 03 Disk, tandem light finishing
+ 3.7415698 19.5 2.2351363 0.0 2.2351363 1.3410819 2.6821637
T 6/8/01 DTL RUSLE.  7in sp.  This is tool used to finish a seedbed.  MAS 10-26-06
+
G 01 Tillage
+ 101.600204 0.5 1.0 101.600204 76.20015 127.00026
P 01 Break Crust
P 02 Random Roughness
+ 1 15.240031
P 05 Ridges and Dikes
+ 1 12.700026 177.80035 0.0 0.0 0.0
P 11 Aggregate Crushing
+ 2.8 0.75
P 12 Soil Loosening
+ 0.75
P 13 Soil Layer Mixing
+ 0.35
P 31 Kill or Defoliate Growing Crop
+ 2
P 40 End crop Biomass Manipulation
P 24 Flatten Standing Biomass
+ 0 0.85 0.7 0.6 0.5 1.0
P 25 Bury Flat Biomass
+ 1 0.73 0.63 0.55 0.4 0.73
P 26 Resurface Buried Biomass
+ 0.02 0.04 0.02 0.05 0.02
P 34 Change Standing Biomass Fall Rate
+ 7 3.0 2.5 2.0 1.5 1.0
+ 0.5 0.6 0.7 0.8 1.0
#------------
D 25/05/03
O 04 Sprayer, pre-emergence
+ 1.2160101 .15
T Spray pest control chemicals on growing crop.  Crop is not killed.
T In the MCREW management screen the user must select the kind of weeds killed in the growing crop as external residue.   080404 DTL
T Cloned from Defoliate (spray) crop.oprn, Changed the P31 to No crop kill and added G4 to add material to field MAS 9-28-06
+
G 03 Crop Name
+ weed residue; 0-3 mo
P 65 Add Crop Residue Amounts
+ 0.0 0.0 0.0 0.0 1
+ 0.0 0.0 0.0056042504 152.4003
+ 0.025 0.025 0.025 0.025 0.169 0.0050 17.1 5.227942
+ -1.20379 0.604887
T Enter crop notes here.
#------------
D 26/05/03
O 03 Planter, transplanter, vegetable
+ 7.4831395 3.12 0.89405453 0.0 0.89405453 0.44702727 1.3410819
T G2 was added into file in front of the flattening (P24), burial (P25), and resurfacing (P26) factors because the area affected is less than 1.0 and
T the RUSLE values were normalized to 1.0.  This change will imulate the correct residue changes based on the method set forth in RUSLE.
T RUSLE's factors have been redused to based on the area affected.
T The stalk fall rate factor (P34) was moved ahead of the new (G2) factor to set the fall rate to theless than 1.0 area affected.  8/7/07 MAS
T
T Changed the P5 to allow the preexisting ridges and furrows to set the ridge roughness.  MAS  12-30-2010
+
G 01 Tillage
+ 152.4003 0.4 0.2 152.4003 101.600204 203.20041
P 01 Break Crust
P 02 Random Roughness
+ 1 10.160021
P 05 Ridges and Dikes
+ 0 50.800102 762.0015 635.0013 0.0 0.0
P 11 Aggregate Crushing
+ 2.4 2.0
P 12 Soil Loosening
+ 0.6
P 13 Soil Layer Mixing
+ 0.3
P 34 Change Standing Biomass Fall Rate
+ 7 3.0 2.5 2.0 1.5 1.0
+ 0.5 0.6 0.7 0.8 1.0
G 02 Biomass Manipulation
+ 1.0
P 24 Flatten Standing Biomass
+ 0 0.3 0.25 0.2 0.1 1.0
P 25 Bury Flat Biomass
+ 1 .07 0.05 .04 .02 .03
P 26 Resurface Buried Biomass
+ 0.01 0.01 0.01 0.02 0.01
G 03 Crop Name
+ Tobacco, burley
P 51 Seeding Configuration
+ 1 0.0 2
+ 2.0 1.0 1 25 1.0 1.0 3
+ ton/ac
+ 11.0 8930.0 4 0.8 0.65 0.95
+ 2.5 0.025 2.0 8.0 25.0 0 100 1400.0
+ -5.0 -15.0 0.15 0.95 0.0 30.0
+ 0.0 0.8008 0.8341 -0.0737 0.0 1.0 1.1 0.01
+ 0.3726 -0.0744 2.0 1.0 10.0 0.03 1 1.1170388
+ 500.0 500.0 2.0 0.03 0.1 0.1 0.0 3
+ 0.02 0.02 0.02 0.02 0.2 0.0050 20.0 2.9797485
+ -1.20379 0.604887 .8308 0.025006166 0.0 0.0 0.0 0.0
T Cloned from WEPS tobacco, leaf, transplants 10-19-06 MAS
#------------
D 05/06/03
O 03 Cultivator, row 1 in ridge
+ 5.799433 14.63 2.2351363 0.0 2.2351363 0.89405453 2.4586499
T RUSLE:Row crop cultivator w/ sweeps leaving a 1" ridge 05-14-02 DTL
T G2 was added into file in front of the flattening (P24), burial (P25), and resurfacing (P26) factors because the area affected is less than 1.0 and
T the RUSLE values were normalized to 1.0.  This change will imulate the correct residue changes based on the method set forth in RUSLE.
T RUSLE's factors have been redused to based on the area affected.
T The stalk fall rate factor (P34) was moved ahead of the new (G2) factor to set the fall rate to the less than 1.0 area affected.  8/8/07 MAS
+
G 01 Tillage
+ 76.20015 0.5 .75 76.20015 50.800102 101.600204
P 01 Break Crust
P 02 Random Roughness
+ 1 7.6200156
P 05 Ridges and Dikes
+ 1 25.400051 762.0015 0.0 0.0 0.0
P 11 Aggregate Crushing
+ 3.0 1.0
P 12 Soil Loosening
+ 0.75
P 13 Soil Layer Mixing
+ 0.35
P 34 Change Standing Biomass Fall Rate
+ 4 3.0 2.5 2.0 1.5 1.0
+ 0.5 0.6 0.7 0.8 1.0
G 02 Biomass Manipulation
+ 1.0
P 24 Flatten Standing Biomass
+ 14 0.7 0.3 0.3 0.1 1.0
P 25 Bury Flat Biomass
+ 1 .57 0.5 0.44 0.32 0.64
P 26 Resurface Buried Biomass
+ 0.01 0.01 0.01 0.01 0.01
#------------
D 05/06/03
O 04 Sprayer, post emergence
+ 1.2160101 .15
T Spray pest control chemicals on growing crop.  Crop is not killed.
T In the MCREW management screen the user must select the kind of weeds killed in the growing crop as external residue.   080404 DTL
T Cloned from Defoliate (spray) crop.oprn, Changed the P31 to No crop kill and added G4 to add material to field MAS 9-28-06
T DO NOT LEAVE CROP COLUMN SET TO "no crop".  User must select the crop and then drill into the operation and specify the amount of weed
T mass that will be killed and turned into residue.
+
G 03 Crop Name
+ weed residue; 0-3 mo
P 65 Add Crop Residue Amounts
+ 0.0 0.0 0.0 0.028021252 1
+ 0.0 0.0 0.0056042504 152.4003
+ 0.025 0.025 0.025 0.025 0.169 0.0050 17.1 5.227942
+ -1.20379 0.604887
T Enter crop notes here.
#------------
D 20/06/03
O 03 Cultivator, row 3 in ridge
+ 5.799433 17.55 2.2351363 0.0 2.2351363 0.89405453 2.4586499
T Row crop cultivator w/ sweeps leaving a 3" ridge 05-14-02 DTL
T G2 was added into file in front of the flattening (P24), burial (P25), and resurfacing (P26) factors because the area affected is less than 1.0 and
T the RUSLE values were normalized to 1.0.  This change will imulate the correct residue changes based on the method set forth in RUSLE.
T RUSLE's factors have been redused to based on the area affected.
T The stalk fall rate factor (P34) was moved ahead of the new (G2) factor to set the fall rate to the  less than 1.0 area affected.  8/7/07 MAS
+
G 01 Tillage
+ 76.20015 0.5 .9 76.20015 50.800102 101.600204
P 01 Break Crust
P 02 Random Roughness
+ 1 15.240031
P 05 Ridges and Dikes
+ 1 76.20015 762.0015 0.0 0.0 0.0
P 11 Aggregate Crushing
+ 3.0 1.0
P 12 Soil Loosening
+ 0.75
P 13 Soil Layer Mixing
+ 0.35
P 34 Change Standing Biomass Fall Rate
+ 4 3.0 2.5 2.0 1.5 1.0
+ 0.5 0.6 0.7 0.8 1.0
G 02 Biomass Manipulation
+ 1.0
P 24 Flatten Standing Biomass
+ 14 0.7 0.3 0.3 0.1 1.0
P 25 Bury Flat Biomass
+ 1 0.68 0.6 0.52 0.39 0.77
P 26 Resurface Buried Biomass
+ 0.04 0.04 0.04 0.06 0.04
#------------
D 20/06/03
O 04 Sprayer, fungicide and insecticide tank mix
+ 1.2160101 .15
T Spray pest control chemicals on growing crop.  Crop is not killed.
T In the MCREW management screen the user must select the kind of weeds killed in the growing crop as external residue.   080404 DTL
T Cloned from Defoliate (spray) crop.oprn, Changed the P31 to No crop kill and added G4 to add material to field MAS 9-28-06
+
#------------
D 20/07/03
O 04 Sprayer, insecticide post emergence
+ 1.2160101 0.15
T Spray pest control chemicals on growing crop.   Crop is not killed.  11/17/01 DTL
T
T Added to the DB.  This assumes no crop flattening.  4-5-12 MAS
+
#------------
D 20/08/03
O 04 Sprayer, insecticide post emergence
+ 1.2160101 0.15
T Spray pest control chemicals on growing crop.   Crop is not killed.  11/17/01 DTL
T
T Added to the DB.  This assumes no crop flattening.  4-5-12 MAS
+
#------------
D 10/09/03
O 04 Harvest, tobacco, burley
+ 3.2738733 .15
T Harvest of burley tobacco where entire plant is cut and removed leaving only short stubble.  021109 DTL
T Modified to remove the entire plant MAS 8-27-10
T Estimate that 10% of the stem remains.  Plant is cut and removed by hand.
T Removed 100% of the flower fraction because some of the plant mass may have gone to fruiting or grain. 12-19-11 MAS
T
T ARS record - filename is:  Harvest Tobacco - leaf (hand pick).oprn
T This record is based on the "Harvest Template (pick and remove).oprn" template.
T The plant material harvested was changed from "grain" to "leaves".
T This operation record is designed to represent a typical tobacco leaf
T harvesting operation that removes all the leaves without cutting the crop stalks
T and kills the crop.  No flattening of any standing stalks occurs.
T 200x	Created - Fred Fox
T Nov 01, 2005	Updated notes - Larry Wagner
T Detailed info regarding this operation record:
+
G 02 Biomass Manipulation
+ 1.0
P 31 Kill or Defoliate Growing Crop
+ 2
P 62 Remove (by age pool) Plant/Residue Material
+ 1 1 0 1 1 3 2 0 0.95 0.9 0.0 0.0
P 34 Change Standing Biomass Fall Rate
+ 0 1.0 1.0 1.0 1.0 1.0
+ 1.0 1.0 1.0 1.0 1.0
P 40 End crop Biomass Manipulation
#------------
D 15/10/03
O 03 Disk, tandem light finishing
+ 3.7415698 19.5 2.2351363 0.0 2.2351363 1.3410819 2.6821637
T 6/8/01 DTL RUSLE.  7in sp.  This is tool used to finish a seedbed.  MAS 10-26-06
+
G 01 Tillage
+ 101.600204 0.5 1.0 101.600204 76.20015 127.00026
P 01 Break Crust
P 02 Random Roughness
+ 1 15.240031
P 05 Ridges and Dikes
+ 1 12.700026 177.80035 0.0 0.0 0.0
P 11 Aggregate Crushing
+ 2.8 0.75
P 12 Soil Loosening
+ 0.75
P 13 Soil Layer Mixing
+ 0.35
P 31 Kill or Defoliate Growing Crop
+ 2
P 40 End crop Biomass Manipulation
P 24 Flatten Standing Biomass
+ 0 0.85 0.7 0.6 0.5 1.0
P 25 Bury Flat Biomass
+ 1 0.73 0.63 0.55 0.4 0.73
P 26 Resurface Buried Biomass
+ 0.02 0.04 0.02 0.05 0.02
P 34 Change Standing Biomass Fall Rate
+ 7 3.0 2.5 2.0 1.5 1.0
+ 0.5 0.6 0.7 0.8 1.0
#------------
D 01/11/03
O 03 Drill or air seeder single disk openers 7-10 in spac
+ 3.2738733 2.44 2.2351363 0.0 2.2351363 1.5645955 2.9056773
T Drill or Air seeder with single disk no-till openers  JD 750 or similar openers. (No-till air drill)
T Based on Drill, no-till single disk 7-10 spacing. 102403 DTL. RUSLE MAS 10-26-06
T G2 was added into file in front of the flattening (P24), burial (P25), and resurfacing (P26) factors because the area affected is less than 1.0 and
T the RUSLE values were normalized to 1.0.  This change will imulate the correct residue changes based on the method set forth in RUSLE.
T RUSLE's factors have been redused to based on the area affected.
T The stalk fall rate factor (P34) was moved ahead of the new (G2) factor to set the fall rate to the less than 1.0 area affected.  8/7/07 MAS
+
G 01 Tillage
+ 63.500134 0.4 0.15 63.50013 50.800102 101.600204
P 01 Break Crust
P 02 Random Roughness
+ 1 7.6200156
P 05 Ridges and Dikes
+ 1 25.400051 203.20041 0.0 0.0 0.0
P 11 Aggregate Crushing
+ 2.8 0.75
P 12 Soil Loosening
+ 0.4
P 13 Soil Layer Mixing
+ 0.20
P 34 Change Standing Biomass Fall Rate
+ 7 3.0 2.5 2.0 1.5 1.0
+ 0.5 0.6 0.7 0.8 1.0
G 02 Biomass Manipulation
+ 1.0
P 24 Flatten Standing Biomass
+ 0 0.6 0.4 0.35 0.15 1.0
P 25 Bury Flat Biomass
+ 1 0.05 0.04 0.03 0.02 0.03
P 26 Resurface Buried Biomass
+ 0.01 0.01 0.01 0.05 0.01
G 03 Crop Name
+ Wheat, winter cover
P 51 Seeding Configuration
+ 1 0.0 0
+ 220.0 8.0 0 2000 1.0 1.0 2
+ lbs/ac
+ 0 8930.0 5 1.0 0.6 0.8
+ 1.2 0.025 2.0 0.0 25.0 1 60 1800.0
+ -5.0 -15.0 0.005 0.05 0.035 30.0
+ 0.013 0.8013 0.4293 -0.086 -0.018 0.932 0.556 0.0736
+ 0.3293 -0.086 2.87 1.0 20.0 0.05 0 0.3
+ 28.571428 335.0 1.4 0.012 0.1 0.1 0.0 2
+ 0.0133 0.0133 0.0133 0.0133 0.04 0.0050 17.1 5.227942
+ -2.08165 0.548606 0 0.0 0.0 0.0 0.0 0.0
T Rusle Notes: Winter wheat cover.   Drilled in 7 inch rows.   Chemically killed  in late boot stage.  Not harvested for grain.
T Base location Columbia, MO. REV 61901 DTL
T
T Cloned 2-16-07 MAS
T
T Standing Fall rate reduced from 0.12 to 0.04 #/(# days) because
T WW-Chem fallow in SW KS showed too much standing residue was falling down.  Larry Wagner recommended we
T reduce fall rate. Dave L, Linda S., and I made runs to get the wt to match the standing stalk wt from Fred Fox stalk residue
T samples WERU Lab.  This rate left 24% of the starting count standing.  This is well within the range of values of two paper.
T Both paper showed about 46% left standing at the 440 day after harvest time.  David Nelson, ARS Akron, CO also confirmed
T that the orginal 8% standing was too low.  He thought that the 24% was much more resonable.  MAS 6-7-11
#------------
D 10/04/04
O 03 Chisel, st. pt
+ 9.353924 45.5 2.2351363 0.0 2.2351363 1.5645955 2.9056773
T Enter Operation notes here
+
G 01 Tillage
+ 177.80035 0.75 1.0 177.80035 101.600204 203.20041
P 01 Break Crust
P 02 Random Roughness
+ 1 38.100075
P 05 Ridges and Dikes
+ 1 76.20015 381.00076 101.600204 0.0 0.0
P 11 Aggregate Crushing
+ 2.4 -2.0
P 12 Soil Loosening
+ 0.85
P 13 Soil Layer Mixing
+ 0.37
P 31 Kill or Defoliate Growing Crop
+ 2
P 40 End crop Biomass Manipulation
P 24 Flatten Standing Biomass
+ 0 0.6 0.4 0.25 0.1 1.0
P 25 Bury Flat Biomass
+ 1 0.76 0.68 0.58 0.5 0.9
P 26 Resurface Buried Biomass
+ 0.05 0.06 0.07 0.2 0.05
P 34 Change Standing Biomass Fall Rate
+ 7 3.0 2.5 2.0 1.5 1.0
+ 0.5 0.6 0.7 0.8 1.0
#------------
D 15/04/04
O 03 Disk, tandem secondary op
+ 4.4898834 32.5 2.2351363 0.0 2.2351363 1.3410819 2.6821637
T 9-in. Spacing, Front and Rear; Good for seedbed preparation/chemical incorporation in medium to heavy soils
T Works well in primary tillage in light to medium soils
T Provides good residue-handling capability.  MAS 10-26-06
+
G 01 Tillage
+ 127.00027 0.75 1.0 127.00026 76.20015 152.4003
P 01 Break Crust
P 02 Random Roughness
+ 1 15.240031
P 05 Ridges and Dikes
+ 1 50.800102 228.60046 0.0 0.0 0.0
P 11 Aggregate Crushing
+ 2.8 0.75
P 12 Soil Loosening
+ 0.85
P 13 Soil Layer Mixing
+ 0.4
P 31 Kill or Defoliate Growing Crop
+ 2
P 40 End crop Biomass Manipulation
P 24 Flatten Standing Biomass
+ 0 0.85 0.7 0.6 0.5 1.0
P 25 Bury Flat Biomass
+ 1 0.73 0.63 0.55 0.4 0.73
P 26 Resurface Buried Biomass
+ 0.02 0.04 0.02 0.05 0.02
P 34 Change Standing Biomass Fall Rate
+ 7 3.0 2.5 2.0 1.5 1.0
+ 0.5 0.6 0.7 0.8 1.0
#------------
D 20/04/04
O 04 Fert applic. surface broadcast
+ 1.4966278 0.0609375
T R2 Notes: Broadcast fertilizer spreader.  Wheel traffic only.  rev 082107 DTL
T
T Added to DB 4-12-12 MAS
+
G 01 Tillage
+ 0.0 0 0.05 0.0 0.0 0.0
P 01 Break Crust
P 02 Random Roughness
+ 1 8.8900175
P 11 Aggregate Crushing
+ 4.3 2.0
P 24 Flatten Standing Biomass
+ 0 0.25 0.2 0.15 0.1 1.0
P 26 Resurface Buried Biomass
+ 0.07 0.08 0.1 0.12 0.07
P 34 Change Standing Biomass Fall Rate
+ 0 1.0 1.0 1.0 1.0 1.0
+ 1.0 1.0 1.0 1.0 1.0
#------------
D 20/04/04
O 03 Disk, tandem secondary op
+ 4.4898834 32.5 2.2351363 0.0 2.2351363 1.3410819 2.6821637
T 9-in. Spacing, Front and Rear; Good for seedbed preparation/chemical incorporation in medium to heavy soils
T Works well in primary tillage in light to medium soils
T Provides good residue-handling capability.  MAS 10-26-06
+
G 01 Tillage
+ 127.00027 0.75 1.0 127.00026 76.20015 152.4003
P 01 Break Crust
P 02 Random Roughness
+ 1 15.240031
P 05 Ridges and Dikes
+ 1 50.800102 228.60046 0.0 0.0 0.0
P 11 Aggregate Crushing
+ 2.8 0.75
P 12 Soil Loosening
+ 0.85
P 13 Soil Layer Mixing
+ 0.4
P 31 Kill or Defoliate Growing Crop
+ 2
P 40 End crop Biomass Manipulation
P 24 Flatten Standing Biomass
+ 0 0.85 0.7 0.6 0.5 1.0
P 25 Bury Flat Biomass
+ 1 0.73 0.63 0.55 0.4 0.73
P 26 Resurface Buried Biomass
+ 0.02 0.04 0.02 0.05 0.02
P 34 Change Standing Biomass Fall Rate
+ 7 3.0 2.5 2.0 1.5 1.0
+ 0.5 0.6 0.7 0.8 1.0
#------------
D 25/04/04
O 03 Drill or air seeder single disk openers 7-10 in spac
+ 3.2738733 2.44 2.2351363 0.0 2.2351363 1.5645955 2.9056773
T Drill or Air seeder with single disk no-till openers  JD 750 or similar openers. (No-till air drill)
T Based on Drill, no-till single disk 7-10 spacing. 102403 DTL. RUSLE MAS 10-26-06
T G2 was added into file in front of the flattening (P24), burial (P25), and resurfacing (P26) factors because the area affected is less than 1.0 and
T the RUSLE values were normalized to 1.0.  This change will imulate the correct residue changes based on the method set forth in RUSLE.
T RUSLE's factors have been redused to based on the area affected.
T The stalk fall rate factor (P34) was moved ahead of the new (G2) factor to set the fall rate to the less than 1.0 area affected.  8/7/07 MAS
+
G 01 Tillage
+ 63.500134 0.4 0.15 63.50013 50.800102 101.600204
P 01 Break Crust
P 02 Random Roughness
+ 1 7.6200156
P 05 Ridges and Dikes
+ 1 25.400051 203.20041 0.0 0.0 0.0
P 11 Aggregate Crushing
+ 2.8 0.75
P 12 Soil Loosening
+ 0.4
P 13 Soil Layer Mixing
+ 0.20
P 34 Change Standing Biomass Fall Rate
+ 7 3.0 2.5 2.0 1.5 1.0
+ 0.5 0.6 0.7 0.8 1.0
G 02 Biomass Manipulation
+ 1.0
P 24 Flatten Standing Biomass
+ 0 0.6 0.4 0.35 0.15 1.0
P 25 Bury Flat Biomass
+ 1 0.05 0.04 0.03 0.02 0.03
P 26 Resurface Buried Biomass
+ 0.01 0.01 0.01 0.05 0.01
G 03 Crop Name
+ Alfalfa, hay
P 51 Seeding Configuration
+ 1 0.0 0
+ 688.0 1 0 6.5 1.0 1 2
+ ton/ac
+ 15 4.465 3 1 0.69 0.9
+ 1 0.01 2 2.999999999999999 30 1 120 1800
+ -5 -9.444445 0.01 0.95 0 24
+ 0.023 0.55 0.63 -0.061 -0.024 0.9911 0.6435 0.0494
+ 0.5 -0.09 0.16108 0.5981 30 0.05 0 0.3
+ 17.009697 110 0.6 0.013 0.2 0.2 0.1 2
+ 0.0536 0.0536 0.0536 0.0536 0.2 0.0020 20 5.227942
+ -1.20379 0.604887 0 0 0 0.0 0.0 0.0
T Size ranges
T J.J. rquez-Ortiz, J.F.S. Lamb, L.D. Johnson, D.K. Barnes and R.E. Stucker, 1999, Heritability of crown traits in alfalfa, Crop Science, Vol 39, Issue 1 pgs. 38-43
T Crown Depth (distance from the soil level to the top of the tap root) - 0.5cm to 5cm
T Crown width (just below the soil surface) - 2cm to 12cm or greater
T Number of crown stems - 2 to 10 or more
T Crown stem width - 2mm to 6mm or greater
T Number of crown buds - none to 12 or more
T
T D.K. Barnes, R.B. Pearce, G.E. Carlson, R.H. Hart, and C.H. Hanson. 1969. SPecific Leaf Weight Differences in Alfalfa Associated with Variety and
T Plant Age. Crop Science, Vol 9, pgs. 421-423.
T Values of Specific leaf weight measured in the paper varied from 2.15 to 4.3, with early season growth mostly in the area of 2.15 to 2.72 mg/cm^2
T Conversion to m^2/kg is * 10^6 mg/kg * 10^-4 m^2/cm^2 = 100 / mg/cm^2
T
T 2.15 mg/cm^2 = 100 / 2.15 m^2/kg = 46.5 m^2/kg, 100 / 2.72 = 36.8, 100 / 4.3 = 23.3
T
T M. H. Hall, C. J. Nelson, J. H. Coutts and R. C. Stout. 2004. Effect of Seeding Rate on Alfalfa Stand Longevity. Agron. J. 96:717-722
T Stem densities for the MO94 study (data not presented) were not different among seeding rates at any sampling time. There were 623 stems m–2 13 MAP
T and only 350 stems m–2 by 25 MAP. Stem density remained nearly constant at that level through 49 MAP. During the same time period, plant density
T declined from an average of 100 down to 25 plants m–2. This means that there was a fourfold increase in stems per plant from 25 to 49 MAP during
T the same time period. Thereafter, stem density continued to decline to 290 and 260 stems m–2 at 63 and 73 MAP, respectively, while plant density fell
T below 15 plants m–2 during the same time period. Crowns develop stems in response to light (Cowett and Sprague, 1962) and apparently could not
T continue to maintain high stem density with the thin stand and older plants.
T
T data as shown above.
T MAP = months after planting
T SPM2 = stems per square meter
T PPM2 = plants per square meter
T SPP = stems per plant
T
T MAP	SPM2	PPM2	 SPP
T 13	623	100	62.3
T 25	350	36	9.7
T 49	350	25	14
T 63	290	16	18
T 73	260	13	20
T
T With the critical period of alfalfa being establishment, a stem count, equals plant count of 400 stems per square meter is used to try and get early cover.
T
T Fick, G.W., D.A. Holt, D.G. Lugg. 1988. Environmental Physiology and Crop Growth. in A.A. Hanson, D.K. Barnes, R.R. Hill , Jr., eds. 1988 Alfalfa and Alfalfa
T Improvement. Agronomy Monograph Number 29. American Society of Agronomy.
T page 181. Growth temperatures: GDD base from 0 to 5 C, varies depending on time of year. GDD totals 0 C base, 700 to bud, 880 to first flower,
T 1075 to full bloom, 1900 to ripe seed stages. Suggests a GDD max temperature around 30
T
T An issue in Yuma, AS.  The plant was growing too high, too soon, and allowing too much erosion in this time period.
T Changes were made: Leaf Fraction 0.41 to 0.63, Crop Ht coff a 0.3 to 0.5, Crop Ht coff b -0.075 to -0.09, Stem Silh area a 3.9 to 0.16108
T Stem silhouette area b 1.0 to 0.5981  Fred Fox, ARS 5-23-11
T
T The biomass adjustment factor has been set to 1.0 from the 0.6 that Fred had.  The biomass conversion eff factor was moved from 30 to 24 to match yield
T of the standard alfalfa run in Moses Lake, WA and now in Yuma, AZ.  The record runs a little under the 6 ton/ac yield in ML, and somewhat over the 10 t/ac for
T Yuma.  The seed weight was increased from 0.00007 to 0.0006 to increase the intial growth of the fall planting.There is about 1500 lbs of growth going into
T winter in WA and about 2400 lbs/ac at the first harvest in AZ.    Yuma will need to lower the Biomass Adjustment factor to 0.8 to get the 12 t/ac yield needed.
T MAS 5-26-11
#------------
D 25/06/04
O 04 Harvest, hay, legume
+ 17.959534 .15
T Harvest legume hay crops such as Alfalfa and Red clover and grass-legume mixed hay such as Alfalfa-Bromegrass.
T Use Harvest, grass hay" for pure grass hay. Rev 11/17/01 DTL"  MAS 11-29-06
T
T Reset the fuel use to 1.92 gal/ac MAS 10-21-11
+
G 02 Biomass Manipulation
+ 1.0
P 31 Kill or Defoliate Growing Crop
+ 0
P 42 Cut/Remove Biomass to Height (flags)
+ 1 0 0 0 0 101.600204 .9 .9 1
P 34 Change Standing Biomass Fall Rate
+ 0 1.1 1.08 1.06 1.04 1.0
+ 0.9 0.92 0.93 0.95 1.0
P 40 End crop Biomass Manipulation
P 24 Flatten Standing Biomass
+ 14 .6 .5 .4 .5 .5
#------------
D 04/08/04
O 04 Harvest, hay, legume
+ 17.959534 .15
T Harvest legume hay crops such as Alfalfa and Red clover and grass-legume mixed hay such as Alfalfa-Bromegrass.
T Use Harvest, grass hay" for pure grass hay. Rev 11/17/01 DTL"  MAS 11-29-06
T
T Reset the fuel use to 1.92 gal/ac MAS 10-21-11
+
G 02 Biomass Manipulation
+ 1.0
P 31 Kill or Defoliate Growing Crop
+ 0
P 42 Cut/Remove Biomass to Height (flags)
+ 1 0 0 0 0 101.600204 .9 .9 1
P 34 Change Standing Biomass Fall Rate
+ 0 1.1 1.08 1.06 1.04 1.0
+ 0.9 0.92 0.93 0.95 1.0
P 40 End crop Biomass Manipulation
P 24 Flatten Standing Biomass
+ 14 .6 .5 .4 .5 .5
#------------
D 13/09/04
O 04 Harvest, hay, legume
+ 17.959534 .15
T Harvest legume hay crops such as Alfalfa and Red clover and grass-legume mixed hay such as Alfalfa-Bromegrass.
T Use Harvest, grass hay" for pure grass hay. Rev 11/17/01 DTL"  MAS 11-29-06
T
T Reset the fuel use to 1.92 gal/ac MAS 10-21-11
+
G 02 Biomass Manipulation
+ 1.0
P 31 Kill or Defoliate Growing Crop
+ 0
P 42 Cut/Remove Biomass to Height (flags)
+ 1 0 0 0 0 101.600204 .9 .9 1
P 34 Change Standing Biomass Fall Rate
+ 0 1.1 1.08 1.06 1.04 1.0
+ 0.9 0.92 0.93 0.95 1.0
P 40 End crop Biomass Manipulation
P 24 Flatten Standing Biomass
+ 14 .6 .5 .4 .5 .5
#------------
D 15/11/04
O 04 Fert applic. surface broadcast
+ 1.4966278 0.0609375
T R2 Notes: Broadcast fertilizer spreader.  Wheel traffic only.  rev 082107 DTL
T
T Added to DB 4-12-12 MAS
+
G 01 Tillage
+ 0.0 0 0.05 0.0 0.0 0.0
P 01 Break Crust
P 02 Random Roughness
+ 1 8.8900175
P 11 Aggregate Crushing
+ 4.3 2.0
P 24 Flatten Standing Biomass
+ 0 0.25 0.2 0.15 0.1 1.0
P 26 Resurface Buried Biomass
+ 0.07 0.08 0.1 0.12 0.07
P 34 Change Standing Biomass Fall Rate
+ 0 1.0 1.0 1.0 1.0 1.0
+ 1.0 1.0 1.0 1.0 1.0
#------------
D 30/05/05
O 04 Harvest, hay, legume
+ 17.959534 .15
T Harvest legume hay crops such as Alfalfa and Red clover and grass-legume mixed hay such as Alfalfa-Bromegrass.
T Use Harvest, grass hay" for pure grass hay. Rev 11/17/01 DTL"  MAS 11-29-06
T
T Reset the fuel use to 1.92 gal/ac MAS 10-21-11
+
G 02 Biomass Manipulation
+ 1.0
P 31 Kill or Defoliate Growing Crop
+ 0
P 42 Cut/Remove Biomass to Height (flags)
+ 1 0 0 0 0 101.600204 .9 .9 1
P 34 Change Standing Biomass Fall Rate
+ 0 1.1 1.08 1.06 1.04 1.0
+ 0.9 0.92 0.93 0.95 1.0
P 40 End crop Biomass Manipulation
P 24 Flatten Standing Biomass
+ 14 .6 .5 .4 .5 .5
#------------
D 09/07/05
O 04 Harvest, hay, legume
+ 17.959534 .15
T Harvest legume hay crops such as Alfalfa and Red clover and grass-legume mixed hay such as Alfalfa-Bromegrass.
T Use Harvest, grass hay" for pure grass hay. Rev 11/17/01 DTL"  MAS 11-29-06
T
T Reset the fuel use to 1.92 gal/ac MAS 10-21-11
+
G 02 Biomass Manipulation
+ 1.0
P 31 Kill or Defoliate Growing Crop
+ 0
P 42 Cut/Remove Biomass to Height (flags)
+ 1 0 0 0 0 101.600204 .9 .9 1
P 34 Change Standing Biomass Fall Rate
+ 0 1.1 1.08 1.06 1.04 1.0
+ 0.9 0.92 0.93 0.95 1.0
P 40 End crop Biomass Manipulation
P 24 Flatten Standing Biomass
+ 14 .6 .5 .4 .5 .5
#------------
D 27/09/05
O 04 Harvest, hay, legume
+ 17.959534 .15
T Harvest legume hay crops such as Alfalfa and Red clover and grass-legume mixed hay such as Alfalfa-Bromegrass.
T Use Harvest, grass hay" for pure grass hay. Rev 11/17/01 DTL"  MAS 11-29-06
T
T Reset the fuel use to 1.92 gal/ac MAS 10-21-11
+
G 02 Biomass Manipulation
+ 1.0
P 31 Kill or Defoliate Growing Crop
+ 0
P 42 Cut/Remove Biomass to Height (flags)
+ 1 0 0 0 0 101.600204 .9 .9 1
P 34 Change Standing Biomass Fall Rate
+ 0 1.1 1.08 1.06 1.04 1.0
+ 0.9 0.92 0.93 0.95 1.0
P 40 End crop Biomass Manipulation
P 24 Flatten Standing Biomass
+ 14 .6 .5 .4 .5 .5
#------------
D 15/11/05
O 04 Fert applic. surface broadcast
+ 1.4966278 0.0609375
T R2 Notes: Broadcast fertilizer spreader.  Wheel traffic only.  rev 082107 DTL
T
T Added to DB 4-12-12 MAS
+
G 01 Tillage
+ 0.0 0 0.05 0.0 0.0 0.0
P 01 Break Crust
P 02 Random Roughness
+ 1 8.8900175
P 11 Aggregate Crushing
+ 4.3 2.0
P 24 Flatten Standing Biomass
+ 0 0.25 0.2 0.15 0.1 1.0
P 26 Resurface Buried Biomass
+ 0.07 0.08 0.1 0.12 0.07
P 34 Change Standing Biomass Fall Rate
+ 0 1.0 1.0 1.0 1.0 1.0
+ 1.0 1.0 1.0 1.0 1.0
#------------
D 30/05/06
O 04 Harvest, hay, legume
+ 17.959534 .15
T Harvest legume hay crops such as Alfalfa and Red clover and grass-legume mixed hay such as Alfalfa-Bromegrass.
T Use Harvest, grass hay" for pure grass hay. Rev 11/17/01 DTL"  MAS 11-29-06
T
T Reset the fuel use to 1.92 gal/ac MAS 10-21-11
+
G 02 Biomass Manipulation
+ 1.0
P 31 Kill or Defoliate Growing Crop
+ 0
P 42 Cut/Remove Biomass to Height (flags)
+ 1 0 0 0 0 101.600204 .9 .9 1
P 34 Change Standing Biomass Fall Rate
+ 0 1.1 1.08 1.06 1.04 1.0
+ 0.9 0.92 0.93 0.95 1.0
P 40 End crop Biomass Manipulation
P 24 Flatten Standing Biomass
+ 14 .6 .5 .4 .5 .5
#------------
D 09/07/06
O 04 Harvest, hay, legume
+ 17.959534 .15
T Harvest legume hay crops such as Alfalfa and Red clover and grass-legume mixed hay such as Alfalfa-Bromegrass.
T Use Harvest, grass hay" for pure grass hay. Rev 11/17/01 DTL"  MAS 11-29-06
T
T Reset the fuel use to 1.92 gal/ac MAS 10-21-11
+
G 02 Biomass Manipulation
+ 1.0
P 31 Kill or Defoliate Growing Crop
+ 0
P 42 Cut/Remove Biomass to Height (flags)
+ 1 0 0 0 0 101.600204 .9 .9 1
P 34 Change Standing Biomass Fall Rate
+ 0 1.1 1.08 1.06 1.04 1.0
+ 0.9 0.92 0.93 0.95 1.0
P 40 End crop Biomass Manipulation
P 24 Flatten Standing Biomass
+ 14 .6 .5 .4 .5 .5
#------------
D 27/09/06
O 04 Harvest, hay, legume
+ 17.959534 .15
T Harvest legume hay crops such as Alfalfa and Red clover and grass-legume mixed hay such as Alfalfa-Bromegrass.
T Use Harvest, grass hay" for pure grass hay. Rev 11/17/01 DTL"  MAS 11-29-06
T
T Reset the fuel use to 1.92 gal/ac MAS 10-21-11
+
G 02 Biomass Manipulation
+ 1.0
P 31 Kill or Defoliate Growing Crop
+ 0
P 42 Cut/Remove Biomass to Height (flags)
+ 1 0 0 0 0 101.600204 .9 .9 1
P 34 Change Standing Biomass Fall Rate
+ 0 1.1 1.08 1.06 1.04 1.0
+ 0.9 0.92 0.93 0.95 1.0
P 40 End crop Biomass Manipulation
P 24 Flatten Standing Biomass
+ 14 .6 .5 .4 .5 .5
#------------
D 15/11/06
O 04 Fert applic. surface broadcast
+ 1.4966278 0.0609375
T R2 Notes: Broadcast fertilizer spreader.  Wheel traffic only.  rev 082107 DTL
T
T Added to DB 4-12-12 MAS
+
G 01 Tillage
+ 0.0 0 0.05 0.0 0.0 0.0
P 01 Break Crust
P 02 Random Roughness
+ 1 8.8900175
P 11 Aggregate Crushing
+ 4.3 2.0
P 24 Flatten Standing Biomass
+ 0 0.25 0.2 0.15 0.1 1.0
P 26 Resurface Buried Biomass
+ 0.07 0.08 0.1 0.12 0.07
P 34 Change Standing Biomass Fall Rate
+ 0 1.0 1.0 1.0 1.0 1.0
+ 1.0 1.0 1.0 1.0 1.0
#------------
D 30/05/07
O 04 Harvest, hay, legume
+ 17.959534 .15
T Harvest legume hay crops such as Alfalfa and Red clover and grass-legume mixed hay such as Alfalfa-Bromegrass.
T Use Harvest, grass hay" for pure grass hay. Rev 11/17/01 DTL"  MAS 11-29-06
T
T Reset the fuel use to 1.92 gal/ac MAS 10-21-11
+
G 02 Biomass Manipulation
+ 1.0
P 31 Kill or Defoliate Growing Crop
+ 0
P 42 Cut/Remove Biomass to Height (flags)
+ 1 0 0 0 0 101.600204 .9 .9 1
P 34 Change Standing Biomass Fall Rate
+ 0 1.1 1.08 1.06 1.04 1.0
+ 0.9 0.92 0.93 0.95 1.0
P 40 End crop Biomass Manipulation
P 24 Flatten Standing Biomass
+ 14 .6 .5 .4 .5 .5
#------------
D 09/07/07
O 04 Harvest, hay, legume
+ 17.959534 .15
T Harvest legume hay crops such as Alfalfa and Red clover and grass-legume mixed hay such as Alfalfa-Bromegrass.
T Use Harvest, grass hay" for pure grass hay. Rev 11/17/01 DTL"  MAS 11-29-06
T
T Reset the fuel use to 1.92 gal/ac MAS 10-21-11
+
G 02 Biomass Manipulation
+ 1.0
P 31 Kill or Defoliate Growing Crop
+ 0
P 42 Cut/Remove Biomass to Height (flags)
+ 1 0 0 0 0 101.600204 .9 .9 1
P 34 Change Standing Biomass Fall Rate
+ 0 1.1 1.08 1.06 1.04 1.0
+ 0.9 0.92 0.93 0.95 1.0
P 40 End crop Biomass Manipulation
P 24 Flatten Standing Biomass
+ 14 .6 .5 .4 .5 .5
#------------
D 27/09/07
O 04 Harvest, hay, legume
+ 17.959534 .15
T Harvest legume hay crops such as Alfalfa and Red clover and grass-legume mixed hay such as Alfalfa-Bromegrass.
T Use Harvest, grass hay" for pure grass hay. Rev 11/17/01 DTL"  MAS 11-29-06
T
T Reset the fuel use to 1.92 gal/ac MAS 10-21-11
+
G 02 Biomass Manipulation
+ 1.0
P 31 Kill or Defoliate Growing Crop
+ 0
P 42 Cut/Remove Biomass to Height (flags)
+ 1 0 0 0 0 101.600204 .9 .9 1
P 34 Change Standing Biomass Fall Rate
+ 0 1.1 1.08 1.06 1.04 1.0
+ 0.9 0.92 0.93 0.95 1.0
P 40 End crop Biomass Manipulation
P 24 Flatten Standing Biomass
+ 14 .6 .5 .4 .5 .5
#------------
*END
*EOF
