Version: 1.5
*START 4
N Originating Program: RUSLE2
N Skel Format Version: 1.1
N This management file was originally converted from the NRCS standard XML format on - Thu Jul 05 09:35:44 PDT 2012
N This management file was updated to contain the most current crop and operation records for WEPS on - Tue Dec 17 21:13:39 CST 2013
#------------
D 01/03/01
O 03 Disk, tandem heavy primary op
+ 7.0154433 39 2.2351363 0.0 2.2351363 1.3410819 2.6821637
T 11-12in. Spacing, Front and Rear
T Recommended for primary tillage in medium to heavy soils
T Excellent residue-handling capability. MAS 10-26-06
+
G 01 Tillage
+ 152.4003 1.0 1.0 152.4003 101.600204 177.80035
P 01 Break Crust
P 02 Random Roughness
+ 1 38.100075
P 05 Ridges and Dikes
+ 1 101.600204 279.40057 0.0 0.0 0.0
P 11 Aggregate Crushing
+ 2.8 0.75
P 12 Soil Loosening
+ 0.9
P 13 Soil Layer Mixing
+ 0.4
P 31 Kill or Defoliate Growing Crop
+ 2
P 40 End crop Biomass Manipulation
P 24 Flatten Standing Biomass
+ 0 1.0 0.9 0.8 0.5 1.0
P 25 Bury Flat Biomass
+ 1 0.95 0.85 0.8 0.6 0.95
P 26 Resurface Buried Biomass
+ 0.05 0.06 0.07 0.08 0.05
P 34 Change Standing Biomass Fall Rate
+ 7 3.0 2.5 2.0 1.5 1.0
+ 0.5 0.6 0.7 0.8 1.0
#------------
D 01/03/01
O 03 Disk, tandem light finishing
+ 3.7415698 19.5 2.2351363 0.0 2.2351363 1.3410819 2.6821637
T 6/8/01 DTL RUSLE.  7in sp.  This is tool used to finish a seedbed.  MAS 10-26-06
+
G 01 Tillage
+ 101.600204 0.5 1.0 101.600204 76.20015 127.00026
P 01 Break Crust
P 02 Random Roughness
+ 1 15.240031
P 05 Ridges and Dikes
+ 1 12.700026 177.80035 0.0 0.0 0.0
P 11 Aggregate Crushing
+ 2.8 0.75
P 12 Soil Loosening
+ 0.75
P 13 Soil Layer Mixing
+ 0.35
P 31 Kill or Defoliate Growing Crop
+ 2
P 40 End crop Biomass Manipulation
P 24 Flatten Standing Biomass
+ 0 0.85 0.7 0.6 0.5 1.0
P 25 Bury Flat Biomass
+ 1 0.73 0.63 0.55 0.4 0.73
P 26 Resurface Buried Biomass
+ 0.02 0.04 0.02 0.05 0.02
P 34 Change Standing Biomass Fall Rate
+ 7 3.0 2.5 2.0 1.5 1.0
+ 0.5 0.6 0.7 0.8 1.0
#------------
D 02/03/01
O 03 Drill or air seeder single disk openers 7-10 in spac
+ 3.2738733 2.44 2.2351363 0.0 2.2351363 1.5645955 2.9056773
T Drill or Air seeder with single disk no-till openers  JD 750 or similar openers. (No-till air drill)
T Based on Drill, no-till single disk 7-10 spacing. 102403 DTL. RUSLE MAS 10-26-06
T G2 was added into file in front of the flattening (P24), burial (P25), and resurfacing (P26) factors because the area affected is less than 1.0 and
T the RUSLE values were normalized to 1.0.  This change will imulate the correct residue changes based on the method set forth in RUSLE.
T RUSLE's factors have been redused to based on the area affected.
T The stalk fall rate factor (P34) was moved ahead of the new (G2) factor to set the fall rate to the less than 1.0 area affected.  8/7/07 MAS
+
G 01 Tillage
+ 63.500134 0.4 0.15 63.50013 50.800102 101.600204
P 01 Break Crust
P 02 Random Roughness
+ 1 7.6200156
P 05 Ridges and Dikes
+ 1 25.400051 203.20041 0.0 0.0 0.0
P 11 Aggregate Crushing
+ 2.8 0.75
P 12 Soil Loosening
+ 0.4
P 13 Soil Layer Mixing
+ 0.20
P 34 Change Standing Biomass Fall Rate
+ 7 3.0 2.5 2.0 1.5 1.0
+ 0.5 0.6 0.7 0.8 1.0
G 02 Biomass Manipulation
+ 1.0
P 24 Flatten Standing Biomass
+ 0 0.6 0.4 0.35 0.15 1.0
P 25 Bury Flat Biomass
+ 1 0.05 0.04 0.03 0.02 0.03
P 26 Resurface Buried Biomass
+ 0.01 0.01 0.01 0.05 0.01
G 03 Crop Name
+ Tall Fescue
P 51 Seeding Configuration
+ 1 0.0 0
+ 400.0 1.0 0 3000 1 1.0 2
+ lbs/ac
+ 0 8930.0 6 1.0 0.69 0.9
+ 1.0 0.01 2.0 3.0 30.0 1 120 1800.0
+ -5.0 -9.444445 0.01 0.95 0.0 45
+ 0.023 0.8063 0.4146 -0.061 -0.024 0.9911 0.6435 0.0494
+ 0.3 -0.075 3.9 1.0 30 0.05 0 0.3
+ 2.0 110.0 0.6 0.013 0.2 0.2 0.1 2
+ 0.0536 0.0536 0.0536 0.0536 0.2 0.0020 20.0 5.227942
+ -1.20379 0.604887 0.0 0.0 0.0 0.0 0.0 0.0
T This record was cloned from the Dryland Alfalfa record that Fred Fox and I worked on mid 2008.  It was the only record we could
T find that would grow biomass and regrow correctly after cutting.  All of the ARS grass records were tested and none would grow correctly.
T
T This record will grow biomass in most cases.  The amount can be adjusted using the biomass adjustment factor in the mgt editor.
T This is considered a tempoary record to use until the WERU and NRCS staff has time to refine the data.
T Do not use the growth values for grazing management.
T MAS 8-7-08
T
T See Alfalfa, hay notes.  This record was cloned from the Alfalfa file, and some of the factors changed to represent dryland alfalfa
T Yield is from and OR state crop guide and the growth trials were from MT.  Yield is set at 1.5 t/ac.
T Calibration of yield must be done manually by adding up the cuttings each year and averaging the years.
T If too high or too low use the biomass adjument factor to reduce or increase the forage produced.
T Grass is not considered in this file.  MAS 8-7-08
T
T Changed the cover to mass value to match Fosters finest stem curve, Small Grain and Alfalfa.  Reference pg. 179 Ag Handbook 703.
T No crop has a larger number (finer stems) than .000586.  This matches RUSLE2.  MAS 12-21-10
#------------
D 05/11/01
O 04 Graze, continuous
+ 9.353924E-8 0.4875
T Continuous Grazing system. Long duration grazing periods 12-20-01 DTL.  30% removal of Crop (green) biomass each time used and
T and 50% removal of the flat residue each time used.  Mas 1-17-07
T
T Restructured processes.  Moved all grazing to O4 for energy and stir cal.
T
T Crop removal (green standing) is cal by using Rusle factors
T Port of Tt biomas affected (%)-(Port of Tt biomas affected (%))x(Portion of affected left on surface (%)
T Graze, continous Example: 0.3-(0.3 x 0.5) = 0.15
T
T Flattening Residue is cal by using Rusle Factors
T Port of Tt biomas affected (%) x Portion of affected left on surface (%)
T Graze, continous Example 0.3 x 0.5 = 0.15
T This value was used for the Mod residue (Wheat) values were reduced by 10% or increased by 10% of the value for each residue class.
T MAS 4-2-08  Changed stem removal from 0.3 to 0 to prevent the stand from thining.  MAS 1-6-11
T Changed reports to include only the current green crop biomass.  Multiple report values are confusing users.  MAS 6-21-11
+
G 02 Biomass Manipulation
+ 1
P 62 Remove (by age pool) Plant/Residue Material
+ 1 0 1 0 1 1 0 .30 .30 0.0 0.0 0.0
P 62 Remove (by age pool) Plant/Residue Material
+ 0 0 1 0 2 4 2 .05 .05 .05 0 0
P 62 Remove (by age pool) Plant/Residue Material
+ 0 0 1 0 1 4 2 .1 .1 .1 0 0
P 24 Flatten Standing Biomass
+ 1 0.20 0.15 0.10 0.01 0.01
#------------
D 20/04/02
O 04 Graze, continuous
+ 9.353924E-8 0.4875
T Continuous Grazing system. Long duration grazing periods 12-20-01 DTL.  30% removal of Crop (green) biomass each time used and
T and 50% removal of the flat residue each time used.  Mas 1-17-07
T
T Restructured processes.  Moved all grazing to O4 for energy and stir cal.
T
T Crop removal (green standing) is cal by using Rusle factors
T Port of Tt biomas affected (%)-(Port of Tt biomas affected (%))x(Portion of affected left on surface (%)
T Graze, continous Example: 0.3-(0.3 x 0.5) = 0.15
T
T Flattening Residue is cal by using Rusle Factors
T Port of Tt biomas affected (%) x Portion of affected left on surface (%)
T Graze, continous Example 0.3 x 0.5 = 0.15
T This value was used for the Mod residue (Wheat) values were reduced by 10% or increased by 10% of the value for each residue class.
T MAS 4-2-08  Changed stem removal from 0.3 to 0 to prevent the stand from thining.  MAS 1-6-11
T Changed reports to include only the current green crop biomass.  Multiple report values are confusing users.  MAS 6-21-11
+
G 02 Biomass Manipulation
+ 1
P 62 Remove (by age pool) Plant/Residue Material
+ 1 0 1 0 1 1 0 .30 .30 0.0 0.0 0.0
P 62 Remove (by age pool) Plant/Residue Material
+ 0 0 1 0 2 4 2 .05 .05 .05 0 0
P 62 Remove (by age pool) Plant/Residue Material
+ 0 0 1 0 1 4 2 .1 .1 .1 0 0
P 24 Flatten Standing Biomass
+ 1 0.20 0.15 0.10 0.01 0.01
#------------
D 05/11/02
O 04 Graze, continuous
+ 9.353924E-8 0.4875
T Continuous Grazing system. Long duration grazing periods 12-20-01 DTL.  30% removal of Crop (green) biomass each time used and
T and 50% removal of the flat residue each time used.  Mas 1-17-07
T
T Restructured processes.  Moved all grazing to O4 for energy and stir cal.
T
T Crop removal (green standing) is cal by using Rusle factors
T Port of Tt biomas affected (%)-(Port of Tt biomas affected (%))x(Portion of affected left on surface (%)
T Graze, continous Example: 0.3-(0.3 x 0.5) = 0.15
T
T Flattening Residue is cal by using Rusle Factors
T Port of Tt biomas affected (%) x Portion of affected left on surface (%)
T Graze, continous Example 0.3 x 0.5 = 0.15
T This value was used for the Mod residue (Wheat) values were reduced by 10% or increased by 10% of the value for each residue class.
T MAS 4-2-08  Changed stem removal from 0.3 to 0 to prevent the stand from thining.  MAS 1-6-11
T Changed reports to include only the current green crop biomass.  Multiple report values are confusing users.  MAS 6-21-11
+
G 02 Biomass Manipulation
+ 1
P 62 Remove (by age pool) Plant/Residue Material
+ 1 0 1 0 1 1 0 .30 .30 0.0 0.0 0.0
P 62 Remove (by age pool) Plant/Residue Material
+ 0 0 1 0 2 4 2 .05 .05 .05 0 0
P 62 Remove (by age pool) Plant/Residue Material
+ 0 0 1 0 1 4 2 .1 .1 .1 0 0
P 24 Flatten Standing Biomass
+ 1 0.20 0.15 0.10 0.01 0.01
#------------
D 20/04/03
O 04 Graze, continuous
+ 9.353924E-8 0.4875
T Continuous Grazing system. Long duration grazing periods 12-20-01 DTL.  30% removal of Crop (green) biomass each time used and
T and 50% removal of the flat residue each time used.  Mas 1-17-07
T
T Restructured processes.  Moved all grazing to O4 for energy and stir cal.
T
T Crop removal (green standing) is cal by using Rusle factors
T Port of Tt biomas affected (%)-(Port of Tt biomas affected (%))x(Portion of affected left on surface (%)
T Graze, continous Example: 0.3-(0.3 x 0.5) = 0.15
T
T Flattening Residue is cal by using Rusle Factors
T Port of Tt biomas affected (%) x Portion of affected left on surface (%)
T Graze, continous Example 0.3 x 0.5 = 0.15
T This value was used for the Mod residue (Wheat) values were reduced by 10% or increased by 10% of the value for each residue class.
T MAS 4-2-08  Changed stem removal from 0.3 to 0 to prevent the stand from thining.  MAS 1-6-11
T Changed reports to include only the current green crop biomass.  Multiple report values are confusing users.  MAS 6-21-11
+
G 02 Biomass Manipulation
+ 1
P 62 Remove (by age pool) Plant/Residue Material
+ 1 0 1 0 1 1 0 .30 .30 0.0 0.0 0.0
P 62 Remove (by age pool) Plant/Residue Material
+ 0 0 1 0 2 4 2 .05 .05 .05 0 0
P 62 Remove (by age pool) Plant/Residue Material
+ 0 0 1 0 1 4 2 .1 .1 .1 0 0
P 24 Flatten Standing Biomass
+ 1 0.20 0.15 0.10 0.01 0.01
#------------
D 05/11/03
O 04 Graze, continuous
+ 9.353924E-8 0.4875
T Continuous Grazing system. Long duration grazing periods 12-20-01 DTL.  30% removal of Crop (green) biomass each time used and
T and 50% removal of the flat residue each time used.  Mas 1-17-07
T
T Restructured processes.  Moved all grazing to O4 for energy and stir cal.
T
T Crop removal (green standing) is cal by using Rusle factors
T Port of Tt biomas affected (%)-(Port of Tt biomas affected (%))x(Portion of affected left on surface (%)
T Graze, continous Example: 0.3-(0.3 x 0.5) = 0.15
T
T Flattening Residue is cal by using Rusle Factors
T Port of Tt biomas affected (%) x Portion of affected left on surface (%)
T Graze, continous Example 0.3 x 0.5 = 0.15
T This value was used for the Mod residue (Wheat) values were reduced by 10% or increased by 10% of the value for each residue class.
T MAS 4-2-08  Changed stem removal from 0.3 to 0 to prevent the stand from thining.  MAS 1-6-11
T Changed reports to include only the current green crop biomass.  Multiple report values are confusing users.  MAS 6-21-11
+
G 02 Biomass Manipulation
+ 1
P 62 Remove (by age pool) Plant/Residue Material
+ 1 0 1 0 1 1 0 .30 .30 0.0 0.0 0.0
P 62 Remove (by age pool) Plant/Residue Material
+ 0 0 1 0 2 4 2 .05 .05 .05 0 0
P 62 Remove (by age pool) Plant/Residue Material
+ 0 0 1 0 1 4 2 .1 .1 .1 0 0
P 24 Flatten Standing Biomass
+ 1 0.20 0.15 0.10 0.01 0.01
#------------
D 20/04/04
O 04 Graze, continuous
+ 9.353924E-8 0.4875
T Continuous Grazing system. Long duration grazing periods 12-20-01 DTL.  30% removal of Crop (green) biomass each time used and
T and 50% removal of the flat residue each time used.  Mas 1-17-07
T
T Restructured processes.  Moved all grazing to O4 for energy and stir cal.
T
T Crop removal (green standing) is cal by using Rusle factors
T Port of Tt biomas affected (%)-(Port of Tt biomas affected (%))x(Portion of affected left on surface (%)
T Graze, continous Example: 0.3-(0.3 x 0.5) = 0.15
T
T Flattening Residue is cal by using Rusle Factors
T Port of Tt biomas affected (%) x Portion of affected left on surface (%)
T Graze, continous Example 0.3 x 0.5 = 0.15
T This value was used for the Mod residue (Wheat) values were reduced by 10% or increased by 10% of the value for each residue class.
T MAS 4-2-08  Changed stem removal from 0.3 to 0 to prevent the stand from thining.  MAS 1-6-11
T Changed reports to include only the current green crop biomass.  Multiple report values are confusing users.  MAS 6-21-11
+
G 02 Biomass Manipulation
+ 1
P 62 Remove (by age pool) Plant/Residue Material
+ 1 0 1 0 1 1 0 .30 .30 0.0 0.0 0.0
P 62 Remove (by age pool) Plant/Residue Material
+ 0 0 1 0 2 4 2 .05 .05 .05 0 0
P 62 Remove (by age pool) Plant/Residue Material
+ 0 0 1 0 1 4 2 .1 .1 .1 0 0
P 24 Flatten Standing Biomass
+ 1 0.20 0.15 0.10 0.01 0.01
#------------
D 05/11/04
O 04 Graze, continuous
+ 9.353924E-8 0.4875
T Continuous Grazing system. Long duration grazing periods 12-20-01 DTL.  30% removal of Crop (green) biomass each time used and
T and 50% removal of the flat residue each time used.  Mas 1-17-07
T
T Restructured processes.  Moved all grazing to O4 for energy and stir cal.
T
T Crop removal (green standing) is cal by using Rusle factors
T Port of Tt biomas affected (%)-(Port of Tt biomas affected (%))x(Portion of affected left on surface (%)
T Graze, continous Example: 0.3-(0.3 x 0.5) = 0.15
T
T Flattening Residue is cal by using Rusle Factors
T Port of Tt biomas affected (%) x Portion of affected left on surface (%)
T Graze, continous Example 0.3 x 0.5 = 0.15
T This value was used for the Mod residue (Wheat) values were reduced by 10% or increased by 10% of the value for each residue class.
T MAS 4-2-08  Changed stem removal from 0.3 to 0 to prevent the stand from thining.  MAS 1-6-11
T Changed reports to include only the current green crop biomass.  Multiple report values are confusing users.  MAS 6-21-11
+
G 02 Biomass Manipulation
+ 1
P 62 Remove (by age pool) Plant/Residue Material
+ 1 0 1 0 1 1 0 .30 .30 0.0 0.0 0.0
P 62 Remove (by age pool) Plant/Residue Material
+ 0 0 1 0 2 4 2 .05 .05 .05 0 0
P 62 Remove (by age pool) Plant/Residue Material
+ 0 0 1 0 1 4 2 .1 .1 .1 0 0
P 24 Flatten Standing Biomass
+ 1 0.20 0.15 0.10 0.01 0.01
#------------
*END
*EOF
