Version: 1.5
*START 2
N Originating Program: RUSLE2
N Skel Format Version: 1.1
N This management file was originally converted from the NRCS standard XML format on - Thu Jul 05 09:36:45 PDT 2012
N This management file was updated to contain the most current crop and operation records for WEPS on - Tue Dec 17 21:11:02 CST 2013
#------------
D 20/02/01
O 03 Disk, tandem secondary op
+ 4.4898834 32.5 2.2351363 0.0 2.2351363 1.3410819 2.6821637
T 9-in. Spacing, Front and Rear; Good for seedbed preparation/chemical incorporation in medium to heavy soils
T Works well in primary tillage in light to medium soils
T Provides good residue-handling capability.  MAS 10-26-06
+
G 01 Tillage
+ 127.00027 0.75 1.0 127.00026 76.20015 152.4003
P 01 Break Crust
P 02 Random Roughness
+ 1 15.240031
P 05 Ridges and Dikes
+ 1 50.800102 228.60046 0.0 0.0 0.0
P 11 Aggregate Crushing
+ 2.8 0.75
P 12 Soil Loosening
+ 0.85
P 13 Soil Layer Mixing
+ 0.4
P 31 Kill or Defoliate Growing Crop
+ 2
P 40 End crop Biomass Manipulation
P 24 Flatten Standing Biomass
+ 0 0.85 0.7 0.6 0.5 1.0
P 25 Bury Flat Biomass
+ 1 0.73 0.63 0.55 0.4 0.73
P 26 Resurface Buried Biomass
+ 0.02 0.04 0.02 0.05 0.02
P 34 Change Standing Biomass Fall Rate
+ 7 3.0 2.5 2.0 1.5 1.0
+ 0.5 0.6 0.7 0.8 1.0
#------------
D 01/03/01
O 04 Fert applic. surface broadcast
+ 1.4966278 0.0609375
T R2 Notes: Broadcast fertilizer spreader.  Wheel traffic only.  rev 082107 DTL
T
T Added to DB 4-12-12 MAS
+
G 01 Tillage
+ 0.0 0 0.05 0.0 0.0 0.0
P 01 Break Crust
P 02 Random Roughness
+ 1 8.8900175
P 11 Aggregate Crushing
+ 4.3 2.0
P 24 Flatten Standing Biomass
+ 0 0.25 0.2 0.15 0.1 1.0
P 26 Resurface Buried Biomass
+ 0.07 0.08 0.1 0.12 0.07
P 34 Change Standing Biomass Fall Rate
+ 0 1.0 1.0 1.0 1.0 1.0
+ 1.0 1.0 1.0 1.0 1.0
#------------
D 06/03/01
O 03 Disk, tandem light finishing
+ 3.7415698 19.5 2.2351363 0.0 2.2351363 1.3410819 2.6821637
T 6/8/01 DTL RUSLE.  7in sp.  This is tool used to finish a seedbed.  MAS 10-26-06
+
G 01 Tillage
+ 101.600204 0.5 1.0 101.600204 76.20015 127.00026
P 01 Break Crust
P 02 Random Roughness
+ 1 15.240031
P 05 Ridges and Dikes
+ 1 12.700026 177.80035 0.0 0.0 0.0
P 11 Aggregate Crushing
+ 2.8 0.75
P 12 Soil Loosening
+ 0.75
P 13 Soil Layer Mixing
+ 0.35
P 31 Kill or Defoliate Growing Crop
+ 2
P 40 End crop Biomass Manipulation
P 24 Flatten Standing Biomass
+ 0 0.85 0.7 0.6 0.5 1.0
P 25 Bury Flat Biomass
+ 1 0.73 0.63 0.55 0.4 0.73
P 26 Resurface Buried Biomass
+ 0.02 0.04 0.02 0.05 0.02
P 34 Change Standing Biomass Fall Rate
+ 7 3.0 2.5 2.0 1.5 1.0
+ 0.5 0.6 0.7 0.8 1.0
#------------
D 09/03/01
O 03 Planting, manual
+ 0.0 .78 0.44702727 0.0 0.44702727 0.44702727 0.44702727
T Manual planting with hoe or shovel.  11/16/05 DTL
T G2 was added into file in front of the flattening (P24), burial (P25), and resurfacing (P26) factors because the area affected is less than 1.0 and
T the RUSLE values were normalized to 1.0.  This change will imulate the correct residue changes based on the method set forth in RUSLE.
T RUSLE's factors have been redused to based on the area affected.
T The stalk fall rate factor (P34) was moved ahead of the new (G2) factor to set the fall rate to the less than 1.0 area affected.  8/7/07 MAS
+
G 01 Tillage
+ 50.800102 .5 .3 50.800102 25.400051 76.20015
P 01 Break Crust
P 02 Random Roughness
+ 1 22.860044
P 05 Ridges and Dikes
+ 1 25.400051 762.0015 609.6012 0.0 0.0
P 11 Aggregate Crushing
+ 2.8 2
P 12 Soil Loosening
+ .3
P 13 Soil Layer Mixing
+ .3
P 34 Change Standing Biomass Fall Rate
+ 7 3.0 2.5 2.0 1.5 1.0
+ 0.5 0.6 0.7 0.8 1.0
G 02 Biomass Manipulation
+ 1.0
P 25 Bury Flat Biomass
+ 1 0.15 0.12 0.09 0.078 0.01
P 26 Resurface Buried Biomass
+ .007 .008 .01 .12 0.01
G 03 Crop Name
+ Onion, bulb dry
P 51 Seeding Configuration
+ 1 0.0 2
+ 33.0 1.0 1 300.0 1.0 1.0 5
+ cwt/ac
+ 91.0 89.3 7 1.0 0.65 0.9
+ 1.2 0.025 0.7 7.0 29.0 1 120 1200.0
+ -5.0 -15.0 0.01 0.95 0.0 30.0
+ 0.0095 0.8707 0.5278 -0.0407 -6.0E-4 1.0048 0.613 0.0512
+ 0.5078 -0.0407 0.9 1.0 9.5 0.05 1 0.27499595
+ 350.0 350.0 3.0 0.03 0.0 0.0 0.9 1
+ 0.02 0.02 0.02 0.02 0.2 0.0050 20.0 5.227942
+ -1.20379 0.604887 0.0358 0.03127172 0.0 0.0 0.0 0.0
T Cloned from ARS dry bulb transplant record.  Change yield and harvest index to RUSLE Vidalia.
T MAS 10-25-07
#------------
D 03/04/01
O 03 Weed control, manual hoe
+ 9.353924E-8 3.315 0.44702727 0.0 0.44702727 0.44702727 0.44702727
T Added to WEPS 4-12-12 MAS
T
T R2 Note: gaw 01-22-02\nManually control weeds in small fields using hoe or similar tool that disturbs soil surface.
T Weeds added to surface.\nThis operation does not kill existing crop.
T User selects type of residue material added and dry weight. rev043008DTL
T
T
T Derived from
T Cultivator - row crop (30 inch row spacing, 1 inch ridge height)
T reduced speed, reduced depth, reduced area affected, removed ridge
+ 
G 01 Tillage
+ 76.20015 0.9 0.85 76.20015 25.400051 101.600204
P 01 Break Crust
P 02 Random Roughness
+ 1 12.700026
P 11 Aggregate Crushing
+ 3.0 1.0
P 12 Soil Loosening
+ 0.75
P 13 Soil Layer Mixing
+ 0.35
P 25 Bury Flat Biomass
+ 1 0.425 0.34 0.255 0.221 0.323
P 26 Resurface Buried Biomass
+ 0.04 0.04 0.04 0.06 0.04
P 34 Change Standing Biomass Fall Rate
+ 4 3.0 2.5 2.0 1.5 1.0
+ 0.5 0.6 0.7 0.8 1.0
G 03 Crop Name
+ weed residue; 0-3 mo
P 65 Add Crop Residue Amounts
+ 0.0 0.0 0.0 0.028021252 1
+ 0.0 0.0 0.0056042504 152.4003
+ 0.025 0.025 0.025 0.025 0.169 0.0050 17.1 5.227942
+ -1.20379 0.604887
T Enter crop notes here.
#------------
D 17/04/01
O 03 Weed control, manual hoe
+ 9.353924E-8 3.315 0.44702727 0.0 0.44702727 0.44702727 0.44702727
T Added to WEPS 4-12-12 MAS
T
T R2 Note: gaw 01-22-02\nManually control weeds in small fields using hoe or similar tool that disturbs soil surface.
T Weeds added to surface.\nThis operation does not kill existing crop.
T User selects type of residue material added and dry weight. rev043008DTL
T
T
T Derived from
T Cultivator - row crop (30 inch row spacing, 1 inch ridge height)
T reduced speed, reduced depth, reduced area affected, removed ridge
+ 
G 01 Tillage
+ 76.20015 0.9 0.85 76.20015 25.400051 101.600204
P 01 Break Crust
P 02 Random Roughness
+ 1 12.700026
P 11 Aggregate Crushing
+ 3.0 1.0
P 12 Soil Loosening
+ 0.75
P 13 Soil Layer Mixing
+ 0.35
P 25 Bury Flat Biomass
+ 1 0.425 0.34 0.255 0.221 0.323
P 26 Resurface Buried Biomass
+ 0.04 0.04 0.04 0.06 0.04
P 34 Change Standing Biomass Fall Rate
+ 4 3.0 2.5 2.0 1.5 1.0
+ 0.5 0.6 0.7 0.8 1.0
G 03 Crop Name
+ weed residue; 0-3 mo
P 65 Add Crop Residue Amounts
+ 0.0 0.0 0.0 0.028021252 1
+ 0.0 0.0 0.0056042504 152.4003
+ 0.025 0.025 0.025 0.025 0.169 0.0050 17.1 5.227942
+ -1.20379 0.604887
T Enter crop notes here.
#------------
D 01/05/01
O 03 Weed control, manual hoe
+ 9.353924E-8 3.315 0.44702727 0.0 0.44702727 0.44702727 0.44702727
T Added to WEPS 4-12-12 MAS
T
T R2 Note: gaw 01-22-02\nManually control weeds in small fields using hoe or similar tool that disturbs soil surface.
T Weeds added to surface.\nThis operation does not kill existing crop.
T User selects type of residue material added and dry weight. rev043008DTL
T
T
T Derived from
T Cultivator - row crop (30 inch row spacing, 1 inch ridge height)
T reduced speed, reduced depth, reduced area affected, removed ridge
+ 
G 01 Tillage
+ 76.20015 0.9 0.85 76.20015 25.400051 101.600204
P 01 Break Crust
P 02 Random Roughness
+ 1 12.700026
P 11 Aggregate Crushing
+ 3.0 1.0
P 12 Soil Loosening
+ 0.75
P 13 Soil Layer Mixing
+ 0.35
P 25 Bury Flat Biomass
+ 1 0.425 0.34 0.255 0.221 0.323
P 26 Resurface Buried Biomass
+ 0.04 0.04 0.04 0.06 0.04
P 34 Change Standing Biomass Fall Rate
+ 4 3.0 2.5 2.0 1.5 1.0
+ 0.5 0.6 0.7 0.8 1.0
G 03 Crop Name
+ weed residue; 0-3 mo
P 65 Add Crop Residue Amounts
+ 0.0 0.0 0.0 0.028021252 1
+ 0.0 0.0 0.0056042504 152.4003
+ 0.025 0.025 0.025 0.025 0.169 0.0050 17.1 5.227942
+ -1.20379 0.604887
T Enter crop notes here.
#------------
D 15/05/01
O 03 Weed control, manual hoe
+ 9.353924E-8 3.315 0.44702727 0.0 0.44702727 0.44702727 0.44702727
T Added to WEPS 4-12-12 MAS
T
T R2 Note: gaw 01-22-02\nManually control weeds in small fields using hoe or similar tool that disturbs soil surface.
T Weeds added to surface.\nThis operation does not kill existing crop.
T User selects type of residue material added and dry weight. rev043008DTL
T
T
T Derived from
T Cultivator - row crop (30 inch row spacing, 1 inch ridge height)
T reduced speed, reduced depth, reduced area affected, removed ridge
+ 
G 01 Tillage
+ 76.20015 0.9 0.85 76.20015 25.400051 101.600204
P 01 Break Crust
P 02 Random Roughness
+ 1 12.700026
P 11 Aggregate Crushing
+ 3.0 1.0
P 12 Soil Loosening
+ 0.75
P 13 Soil Layer Mixing
+ 0.35
P 25 Bury Flat Biomass
+ 1 0.425 0.34 0.255 0.221 0.323
P 26 Resurface Buried Biomass
+ 0.04 0.04 0.04 0.06 0.04
P 34 Change Standing Biomass Fall Rate
+ 4 3.0 2.5 2.0 1.5 1.0
+ 0.5 0.6 0.7 0.8 1.0
G 03 Crop Name
+ weed residue; 0-3 mo
P 65 Add Crop Residue Amounts
+ 0.0 0.0 0.0 0.028021252 1
+ 0.0 0.0 0.0056042504 152.4003
+ 0.025 0.025 0.025 0.025 0.169 0.0050 17.1 5.227942
+ -1.20379 0.604887
T Enter crop notes here.
#------------
D 26/06/01
O 04 Harvest, hand pull
+ 3.2738733 2.275
T Hand harvest bulb crops like onions or garklic  leaving 4" diaimeter holes that are 3 to 5" deep.   rev042808 DTL
T
T Created 2-24-09  MAS
T Corrected the STIR and the fuel use data.  12-19-11 MAS
+
G 01 Tillage
+ 127.00025 0.4 0.35 127.00025 25.4000508001016 254.0005
P 01 Break Crust
P 02 Random Roughness
+ 1 30.480062
P 11 Aggregate Crushing
+ 1.4 -1.2
P 12 Soil Loosening
+ 0.3
P 13 Soil Layer Mixing
+ 0.05
G 02 Biomass Manipulation
+ 1.0
P 31 Kill or Defoliate Growing Crop
+ 2
P 62 Remove (by age pool) Plant/Residue Material
+ 1 1 0 1 1 3 2 0.0 0.99 0.99 1.0 0.0
P 34 Change Standing Biomass Fall Rate
+ 3 1.0 1.0 1.0 1.0 1.0
+ 1.0 1.0 1.0 1.0 1.0
P 40 End crop Biomass Manipulation
#------------
D 06/07/01
O 03 Disk, tandem secondary op
+ 4.4898834 32.5 2.2351363 0.0 2.2351363 1.3410819 2.6821637
T 9-in. Spacing, Front and Rear; Good for seedbed preparation/chemical incorporation in medium to heavy soils
T Works well in primary tillage in light to medium soils
T Provides good residue-handling capability.  MAS 10-26-06
+
G 01 Tillage
+ 127.00027 0.75 1.0 127.00026 76.20015 152.4003
P 01 Break Crust
P 02 Random Roughness
+ 1 15.240031
P 05 Ridges and Dikes
+ 1 50.800102 228.60046 0.0 0.0 0.0
P 11 Aggregate Crushing
+ 2.8 0.75
P 12 Soil Loosening
+ 0.85
P 13 Soil Layer Mixing
+ 0.4
P 31 Kill or Defoliate Growing Crop
+ 2
P 40 End crop Biomass Manipulation
P 24 Flatten Standing Biomass
+ 0 0.85 0.7 0.6 0.5 1.0
P 25 Bury Flat Biomass
+ 1 0.73 0.63 0.55 0.4 0.73
P 26 Resurface Buried Biomass
+ 0.02 0.04 0.02 0.05 0.02
P 34 Change Standing Biomass Fall Rate
+ 7 3.0 2.5 2.0 1.5 1.0
+ 0.5 0.6 0.7 0.8 1.0
#------------
D 06/07/01
O 04 Fert applic. surface broadcast
+ 1.4966278 0.0609375
T R2 Notes: Broadcast fertilizer spreader.  Wheel traffic only.  rev 082107 DTL
T
T Added to DB 4-12-12 MAS
+
G 01 Tillage
+ 0.0 0 0.05 0.0 0.0 0.0
P 01 Break Crust
P 02 Random Roughness
+ 1 8.8900175
P 11 Aggregate Crushing
+ 4.3 2.0
P 24 Flatten Standing Biomass
+ 0 0.25 0.2 0.15 0.1 1.0
P 26 Resurface Buried Biomass
+ 0.07 0.08 0.1 0.12 0.07
P 34 Change Standing Biomass Fall Rate
+ 0 1.0 1.0 1.0 1.0 1.0
+ 1.0 1.0 1.0 1.0 1.0
#------------
D 10/07/01
O 03 Planting, manual
+ 0.0 .78 0.44702727 0.0 0.44702727 0.44702727 0.44702727
T Manual planting with hoe or shovel.  11/16/05 DTL
T G2 was added into file in front of the flattening (P24), burial (P25), and resurfacing (P26) factors because the area affected is less than 1.0 and
T the RUSLE values were normalized to 1.0.  This change will imulate the correct residue changes based on the method set forth in RUSLE.
T RUSLE's factors have been redused to based on the area affected.
T The stalk fall rate factor (P34) was moved ahead of the new (G2) factor to set the fall rate to the less than 1.0 area affected.  8/7/07 MAS
+
G 01 Tillage
+ 50.800102 .5 .3 50.800102 25.400051 76.20015
P 01 Break Crust
P 02 Random Roughness
+ 1 22.860044
P 05 Ridges and Dikes
+ 1 25.400051 762.0015 609.6012 0.0 0.0
P 11 Aggregate Crushing
+ 2.8 2
P 12 Soil Loosening
+ .3
P 13 Soil Layer Mixing
+ .3
P 34 Change Standing Biomass Fall Rate
+ 7 3.0 2.5 2.0 1.5 1.0
+ 0.5 0.6 0.7 0.8 1.0
G 02 Biomass Manipulation
+ 1.0
P 25 Bury Flat Biomass
+ 1 0.15 0.12 0.09 0.078 0.01
P 26 Resurface Buried Biomass
+ .007 .008 .01 .12 0.01
G 03 Crop Name
+ Tomato, fresh mkt
P 51 Seeding Configuration
+ 1 0.0 2
+ 2.0 1.0 1 300 1.0 1.0 0
+ cwt/ac
+ 94.0 89.3 4 1.0 0.65 0.95
+ 0.8 0.025 1.5 10.0 27.0 0 70 750.0
+ -1.0 -4.0 0.15 0.95 0.0 30.0
+ -0.0198 0.6575 0.4807 -0.1453 -0.336 1.3726 0.5408 0.1081
+ 0.4807 -0.1453 3.08 1.0 31.1 0.01 1 1.1170388
+ 1700.0 1700.0 3.0 0.03 0.0 0.0 0.0 1
+ 0.02 0.02 0.02 0.02 0.2 0.0050 20.0 2.7
+ -1.20379 0.604887 0.0767 0.012329351 0.0 0.0 0.0 0.0
T This records comes from ARS tomato transplant record and has the yield,
T Residue yield ration and the yield intercept changed to RUSLE values MAS 3-6-07
T Made changes as Fred instructed, mass of planting MAS 3/15/07
#------------
D 31/07/01
O 03 Weed control, manual hoe
+ 9.353924E-8 3.315 0.44702727 0.0 0.44702727 0.44702727 0.44702727
T Added to WEPS 4-12-12 MAS
T
T R2 Note: gaw 01-22-02\nManually control weeds in small fields using hoe or similar tool that disturbs soil surface.
T Weeds added to surface.\nThis operation does not kill existing crop.
T User selects type of residue material added and dry weight. rev043008DTL
T
T
T Derived from
T Cultivator - row crop (30 inch row spacing, 1 inch ridge height)
T reduced speed, reduced depth, reduced area affected, removed ridge
+ 
G 01 Tillage
+ 76.20015 0.9 0.85 76.20015 25.400051 101.600204
P 01 Break Crust
P 02 Random Roughness
+ 1 12.700026
P 11 Aggregate Crushing
+ 3.0 1.0
P 12 Soil Loosening
+ 0.75
P 13 Soil Layer Mixing
+ 0.35
P 25 Bury Flat Biomass
+ 1 0.425 0.34 0.255 0.221 0.323
P 26 Resurface Buried Biomass
+ 0.04 0.04 0.04 0.06 0.04
P 34 Change Standing Biomass Fall Rate
+ 4 3.0 2.5 2.0 1.5 1.0
+ 0.5 0.6 0.7 0.8 1.0
G 03 Crop Name
+ weed residue; 0-3 mo
P 65 Add Crop Residue Amounts
+ 0.0 0.0 0.0 0.028021252 1
+ 0.0 0.0 0.0056042504 152.4003
+ 0.025 0.025 0.025 0.025 0.169 0.0050 17.1 5.227942
+ -1.20379 0.604887
T Enter crop notes here.
#------------
D 14/08/01
O 03 Weed control, manual hoe
+ 9.353924E-8 3.315 0.44702727 0.0 0.44702727 0.44702727 0.44702727
T Added to WEPS 4-12-12 MAS
T
T R2 Note: gaw 01-22-02\nManually control weeds in small fields using hoe or similar tool that disturbs soil surface.
T Weeds added to surface.\nThis operation does not kill existing crop.
T User selects type of residue material added and dry weight. rev043008DTL
T
T
T Derived from
T Cultivator - row crop (30 inch row spacing, 1 inch ridge height)
T reduced speed, reduced depth, reduced area affected, removed ridge
+ 
G 01 Tillage
+ 76.20015 0.9 0.85 76.20015 25.400051 101.600204
P 01 Break Crust
P 02 Random Roughness
+ 1 12.700026
P 11 Aggregate Crushing
+ 3.0 1.0
P 12 Soil Loosening
+ 0.75
P 13 Soil Layer Mixing
+ 0.35
P 25 Bury Flat Biomass
+ 1 0.425 0.34 0.255 0.221 0.323
P 26 Resurface Buried Biomass
+ 0.04 0.04 0.04 0.06 0.04
P 34 Change Standing Biomass Fall Rate
+ 4 3.0 2.5 2.0 1.5 1.0
+ 0.5 0.6 0.7 0.8 1.0
G 03 Crop Name
+ weed residue; 0-3 mo
P 65 Add Crop Residue Amounts
+ 0.0 0.0 0.0 0.028021252 1
+ 0.0 0.0 0.0056042504 152.4003
+ 0.025 0.025 0.025 0.025 0.169 0.0050 17.1 5.227942
+ -1.20379 0.604887
T Enter crop notes here.
#------------
D 28/08/01
O 03 Weed control, manual hoe
+ 9.353924E-8 3.315 0.44702727 0.0 0.44702727 0.44702727 0.44702727
T Added to WEPS 4-12-12 MAS
T
T R2 Note: gaw 01-22-02\nManually control weeds in small fields using hoe or similar tool that disturbs soil surface.
T Weeds added to surface.\nThis operation does not kill existing crop.
T User selects type of residue material added and dry weight. rev043008DTL
T
T
T Derived from
T Cultivator - row crop (30 inch row spacing, 1 inch ridge height)
T reduced speed, reduced depth, reduced area affected, removed ridge
+ 
G 01 Tillage
+ 76.20015 0.9 0.85 76.20015 25.400051 101.600204
P 01 Break Crust
P 02 Random Roughness
+ 1 12.700026
P 11 Aggregate Crushing
+ 3.0 1.0
P 12 Soil Loosening
+ 0.75
P 13 Soil Layer Mixing
+ 0.35
P 25 Bury Flat Biomass
+ 1 0.425 0.34 0.255 0.221 0.323
P 26 Resurface Buried Biomass
+ 0.04 0.04 0.04 0.06 0.04
P 34 Change Standing Biomass Fall Rate
+ 4 3.0 2.5 2.0 1.5 1.0
+ 0.5 0.6 0.7 0.8 1.0
G 03 Crop Name
+ weed residue; 0-3 mo
P 65 Add Crop Residue Amounts
+ 0.0 0.0 0.0 0.028021252 1
+ 0.0 0.0 0.0056042504 152.4003
+ 0.025 0.025 0.025 0.025 0.169 0.0050 17.1 5.227942
+ -1.20379 0.604887
T Enter crop notes here.
#------------
D 22/09/01
O 04 Harvest, hand pick vegetables
+ 3.2738733 0.15
T Hand pick tomato, artichoke, peppers, strawberries or similar crops
T with multiple harvests from the same plants.  12-13-2011 DTL
T This is a partial harvest only 50% of the yield is taken with this harvest.
T This operation MUST be followed by a final harvest operation.
T Crops that use multiple harvests must be manually calibrated.
T Added 12-27-11 MAS
+
G 02 Biomass Manipulation
+ 1.0
P 31 Kill or Defoliate Growing Crop
+ 0
P 62 Remove (by age pool) Plant/Residue Material
+ 1 0 0 0 3 3 2 0.5 0.0 0.0 0.0 0.0
P 40 End crop Biomass Manipulation
#------------
D 29/09/01
O 04 Harvest, hand pick vegetables
+ 3.2738733 0.15
T Hand pick tomato, artichoke, peppers, strawberries or similar crops
T with multiple harvests from the same plants.  12-13-2011 DTL
T This is a partial harvest only 50% of the yield is taken with this harvest.
T This operation MUST be followed by a final harvest operation.
T Crops that use multiple harvests must be manually calibrated.
T Added 12-27-11 MAS
+
G 02 Biomass Manipulation
+ 1.0
P 31 Kill or Defoliate Growing Crop
+ 0
P 62 Remove (by age pool) Plant/Residue Material
+ 1 0 0 0 3 3 2 0.5 0.0 0.0 0.0 0.0
P 40 End crop Biomass Manipulation
#------------
D 06/10/01
O 04 Harvest, hand pick vegetables
+ 3.2738733 0.15
T Hand pick tomato, artichoke, peppers, strawberries or similar crops
T with multiple harvests from the same plants.  12-13-2011 DTL
T This is a partial harvest only 50% of the yield is taken with this harvest.
T This operation MUST be followed by a final harvest operation.
T Crops that use multiple harvests must be manually calibrated.
T Added 12-27-11 MAS
+
G 02 Biomass Manipulation
+ 1.0
P 31 Kill or Defoliate Growing Crop
+ 0
P 62 Remove (by age pool) Plant/Residue Material
+ 1 0 0 0 3 3 2 0.5 0.0 0.0 0.0 0.0
P 40 End crop Biomass Manipulation
#------------
D 13/10/01
O 04 Harvest, hand pick vegetables
+ 3.2738733 0.15
T Hand pick tomato, artichoke, peppers, strawberries or similar crops
T with multiple harvests from the same plants.  12-13-2011 DTL
T This is a partial harvest only 50% of the yield is taken with this harvest.
T This operation MUST be followed by a final harvest operation.
T Crops that use multiple harvests must be manually calibrated.
T Added 12-27-11 MAS
+
G 02 Biomass Manipulation
+ 1.0
P 31 Kill or Defoliate Growing Crop
+ 0
P 62 Remove (by age pool) Plant/Residue Material
+ 1 0 0 0 3 3 2 0.5 0.0 0.0 0.0 0.0
P 40 End crop Biomass Manipulation
#------------
D 20/10/01
O 04 Harvest, hand pick vegetables
+ 3.2738733 0.15
T Hand pick tomato, artichoke, peppers, strawberries or similar crops
T with multiple harvests from the same plants.  12-13-2011 DTL
T This is a partial harvest only 50% of the yield is taken with this harvest.
T This operation MUST be followed by a final harvest operation.
T Crops that use multiple harvests must be manually calibrated.
T Added 12-27-11 MAS
+
G 02 Biomass Manipulation
+ 1.0
P 31 Kill or Defoliate Growing Crop
+ 0
P 62 Remove (by age pool) Plant/Residue Material
+ 1 0 0 0 3 3 2 0.5 0.0 0.0 0.0 0.0
P 40 End crop Biomass Manipulation
#------------
D 27/10/01
O 04 Harvest, hand pick vegetables
+ 3.2738733 0.15
T Hand pick tomato, artichoke, peppers, strawberries or similar crops
T with multiple harvests from the same plants.  12-13-2011 DTL
T This is a partial harvest only 50% of the yield is taken with this harvest.
T This operation MUST be followed by a final harvest operation.
T Crops that use multiple harvests must be manually calibrated.
T Added 12-27-11 MAS
+
G 02 Biomass Manipulation
+ 1.0
P 31 Kill or Defoliate Growing Crop
+ 0
P 62 Remove (by age pool) Plant/Residue Material
+ 1 0 0 0 3 3 2 0.5 0.0 0.0 0.0 0.0
P 40 End crop Biomass Manipulation
#------------
D 03/11/01
O 04 Harvest, hand pick vegetables
+ 3.2738733 0.15
T Hand pick tomato, artichoke, peppers, strawberries or similar crops
T with multiple harvests from the same plants.  12-13-2011 DTL
T This is a partial harvest only 50% of the yield is taken with this harvest.
T This operation MUST be followed by a final harvest operation.
T Crops that use multiple harvests must be manually calibrated.
T Added 12-27-11 MAS
+
G 02 Biomass Manipulation
+ 1.0
P 31 Kill or Defoliate Growing Crop
+ 0
P 62 Remove (by age pool) Plant/Residue Material
+ 1 0 0 0 3 3 2 0.5 0.0 0.0 0.0 0.0
P 40 End crop Biomass Manipulation
#------------
D 10/11/01
O 04 Harvest, hand pick vegetables
+ 3.2738733 0.15
T Hand pick tomato, artichoke, peppers, strawberries or similar crops
T with multiple harvests from the same plants.  12-13-2011 DTL
T This is a partial harvest only 50% of the yield is taken with this harvest.
T This operation MUST be followed by a final harvest operation.
T Crops that use multiple harvests must be manually calibrated.
T Added 12-27-11 MAS
+
G 02 Biomass Manipulation
+ 1.0
P 31 Kill or Defoliate Growing Crop
+ 0
P 62 Remove (by age pool) Plant/Residue Material
+ 1 0 0 0 3 3 2 0.5 0.0 0.0 0.0 0.0
P 40 End crop Biomass Manipulation
#------------
D 06/02/02
O 03 Disk, tandem secondary op
+ 4.4898834 32.5 2.2351363 0.0 2.2351363 1.3410819 2.6821637
T 9-in. Spacing, Front and Rear; Good for seedbed preparation/chemical incorporation in medium to heavy soils
T Works well in primary tillage in light to medium soils
T Provides good residue-handling capability.  MAS 10-26-06
+
G 01 Tillage
+ 127.00027 0.75 1.0 127.00026 76.20015 152.4003
P 01 Break Crust
P 02 Random Roughness
+ 1 15.240031
P 05 Ridges and Dikes
+ 1 50.800102 228.60046 0.0 0.0 0.0
P 11 Aggregate Crushing
+ 2.8 0.75
P 12 Soil Loosening
+ 0.85
P 13 Soil Layer Mixing
+ 0.4
P 31 Kill or Defoliate Growing Crop
+ 2
P 40 End crop Biomass Manipulation
P 24 Flatten Standing Biomass
+ 0 0.85 0.7 0.6 0.5 1.0
P 25 Bury Flat Biomass
+ 1 0.73 0.63 0.55 0.4 0.73
P 26 Resurface Buried Biomass
+ 0.02 0.04 0.02 0.05 0.02
P 34 Change Standing Biomass Fall Rate
+ 7 3.0 2.5 2.0 1.5 1.0
+ 0.5 0.6 0.7 0.8 1.0
#------------
D 22/02/02
O 04 Fert applic. surface broadcast
+ 1.4966278 0.0609375
T R2 Notes: Broadcast fertilizer spreader.  Wheel traffic only.  rev 082107 DTL
T
T Added to DB 4-12-12 MAS
+
G 01 Tillage
+ 0.0 0 0.05 0.0 0.0 0.0
P 01 Break Crust
P 02 Random Roughness
+ 1 8.8900175
P 11 Aggregate Crushing
+ 4.3 2.0
P 24 Flatten Standing Biomass
+ 0 0.25 0.2 0.15 0.1 1.0
P 26 Resurface Buried Biomass
+ 0.07 0.08 0.1 0.12 0.07
P 34 Change Standing Biomass Fall Rate
+ 0 1.0 1.0 1.0 1.0 1.0
+ 1.0 1.0 1.0 1.0 1.0
#------------
D 27/02/02
O 03 Planting, manual
+ 0.0 .78 0.44702727 0.0 0.44702727 0.44702727 0.44702727
T Manual planting with hoe or shovel.  11/16/05 DTL
T G2 was added into file in front of the flattening (P24), burial (P25), and resurfacing (P26) factors because the area affected is less than 1.0 and
T the RUSLE values were normalized to 1.0.  This change will imulate the correct residue changes based on the method set forth in RUSLE.
T RUSLE's factors have been redused to based on the area affected.
T The stalk fall rate factor (P34) was moved ahead of the new (G2) factor to set the fall rate to the less than 1.0 area affected.  8/7/07 MAS
+
G 01 Tillage
+ 50.800102 .5 .3 50.800102 25.400051 76.20015
P 01 Break Crust
P 02 Random Roughness
+ 1 22.860044
P 05 Ridges and Dikes
+ 1 25.400051 762.0015 609.6012 0.0 0.0
P 11 Aggregate Crushing
+ 2.8 2
P 12 Soil Loosening
+ .3
P 13 Soil Layer Mixing
+ .3
P 34 Change Standing Biomass Fall Rate
+ 7 3.0 2.5 2.0 1.5 1.0
+ 0.5 0.6 0.7 0.8 1.0
G 02 Biomass Manipulation
+ 1.0
P 25 Bury Flat Biomass
+ 1 0.15 0.12 0.09 0.078 0.01
P 26 Resurface Buried Biomass
+ .007 .008 .01 .12 0.01
G 03 Crop Name
+ Cabbage
P 51 Seeding Configuration
+ 1 0.0 2
+ 2.9999999999999996 1 1 39000 1 1 2
+ lbs/ac
+ 93 8930 4 1 0.65 0.95
+ 0.45720553 0.01 0.7 4.000000000000002 24 0 55 1300.0
+ -5 -15 0.01 0.95 0 19
+ 0.194 0.6956 0.3922 -0.1253 0 1 1.1 0.01
+ 0.4995 -0.0944 0.1 1 20 0.05 1 0.9120584
+ 2000 2000 2 0.03 0 0 0 1
+ 0.02 0.02 0.02 0.02 0.2 0.0050 20 2.7
+ -1.20379 0.604887 0 0.0 0 0.0 0.0 0.0
T Harvest index from RUSLE "Cabage", Yield from Producing Veg Crops, Ware & McCollum Not the same as RUSLE.  MAS 5/10/06
T
T
T Adjusted cover factor to ARS (larger size residue) based on size of the root balls  MAS 12-30-10
#------------
D 13/03/02
O 03 Weed control, manual hoe
+ 9.353924E-8 3.315 0.44702727 0.0 0.44702727 0.44702727 0.44702727
T Added to WEPS 4-12-12 MAS
T
T R2 Note: gaw 01-22-02\nManually control weeds in small fields using hoe or similar tool that disturbs soil surface.
T Weeds added to surface.\nThis operation does not kill existing crop.
T User selects type of residue material added and dry weight. rev043008DTL
T
T
T Derived from
T Cultivator - row crop (30 inch row spacing, 1 inch ridge height)
T reduced speed, reduced depth, reduced area affected, removed ridge
+ 
G 01 Tillage
+ 76.20015 0.9 0.85 76.20015 25.400051 101.600204
P 01 Break Crust
P 02 Random Roughness
+ 1 12.700026
P 11 Aggregate Crushing
+ 3.0 1.0
P 12 Soil Loosening
+ 0.75
P 13 Soil Layer Mixing
+ 0.35
P 25 Bury Flat Biomass
+ 1 0.425 0.34 0.255 0.221 0.323
P 26 Resurface Buried Biomass
+ 0.04 0.04 0.04 0.06 0.04
P 34 Change Standing Biomass Fall Rate
+ 4 3.0 2.5 2.0 1.5 1.0
+ 0.5 0.6 0.7 0.8 1.0
G 03 Crop Name
+ weed residue; 0-3 mo
P 65 Add Crop Residue Amounts
+ 0.0 0.0 0.0 0.028021252 1
+ 0.0 0.0 0.0056042504 152.4003
+ 0.025 0.025 0.025 0.025 0.169 0.0050 17.1 5.227942
+ -1.20379 0.604887
T Enter crop notes here.
#------------
D 27/03/02
O 03 Weed control, manual hoe
+ 9.353924E-8 3.315 0.44702727 0.0 0.44702727 0.44702727 0.44702727
T Added to WEPS 4-12-12 MAS
T
T R2 Note: gaw 01-22-02\nManually control weeds in small fields using hoe or similar tool that disturbs soil surface.
T Weeds added to surface.\nThis operation does not kill existing crop.
T User selects type of residue material added and dry weight. rev043008DTL
T
T
T Derived from
T Cultivator - row crop (30 inch row spacing, 1 inch ridge height)
T reduced speed, reduced depth, reduced area affected, removed ridge
+ 
G 01 Tillage
+ 76.20015 0.9 0.85 76.20015 25.400051 101.600204
P 01 Break Crust
P 02 Random Roughness
+ 1 12.700026
P 11 Aggregate Crushing
+ 3.0 1.0
P 12 Soil Loosening
+ 0.75
P 13 Soil Layer Mixing
+ 0.35
P 25 Bury Flat Biomass
+ 1 0.425 0.34 0.255 0.221 0.323
P 26 Resurface Buried Biomass
+ 0.04 0.04 0.04 0.06 0.04
P 34 Change Standing Biomass Fall Rate
+ 4 3.0 2.5 2.0 1.5 1.0
+ 0.5 0.6 0.7 0.8 1.0
G 03 Crop Name
+ weed residue; 0-3 mo
P 65 Add Crop Residue Amounts
+ 0.0 0.0 0.0 0.028021252 1
+ 0.0 0.0 0.0056042504 152.4003
+ 0.025 0.025 0.025 0.025 0.169 0.0050 17.1 5.227942
+ -1.20379 0.604887
T Enter crop notes here.
#------------
D 10/04/02
O 03 Weed control, manual hoe
+ 9.353924E-8 3.315 0.44702727 0.0 0.44702727 0.44702727 0.44702727
T Added to WEPS 4-12-12 MAS
T
T R2 Note: gaw 01-22-02\nManually control weeds in small fields using hoe or similar tool that disturbs soil surface.
T Weeds added to surface.\nThis operation does not kill existing crop.
T User selects type of residue material added and dry weight. rev043008DTL
T
T
T Derived from
T Cultivator - row crop (30 inch row spacing, 1 inch ridge height)
T reduced speed, reduced depth, reduced area affected, removed ridge
+ 
G 01 Tillage
+ 76.20015 0.9 0.85 76.20015 25.400051 101.600204
P 01 Break Crust
P 02 Random Roughness
+ 1 12.700026
P 11 Aggregate Crushing
+ 3.0 1.0
P 12 Soil Loosening
+ 0.75
P 13 Soil Layer Mixing
+ 0.35
P 25 Bury Flat Biomass
+ 1 0.425 0.34 0.255 0.221 0.323
P 26 Resurface Buried Biomass
+ 0.04 0.04 0.04 0.06 0.04
P 34 Change Standing Biomass Fall Rate
+ 4 3.0 2.5 2.0 1.5 1.0
+ 0.5 0.6 0.7 0.8 1.0
G 03 Crop Name
+ weed residue; 0-3 mo
P 65 Add Crop Residue Amounts
+ 0.0 0.0 0.0 0.028021252 1
+ 0.0 0.0 0.0056042504 152.4003
+ 0.025 0.025 0.025 0.025 0.169 0.0050 17.1 5.227942
+ -1.20379 0.604887
T Enter crop notes here.
#------------
D 06/05/02
O 04 Harvest, hand pick vegetables
+ 3.2738733 0.15
T Hand pick tomato, artichoke, peppers, strawberries or similar crops
T with multiple harvests from the same plants.  12-13-2011 DTL
T This is a partial harvest only 50% of the yield is taken with this harvest.
T This operation MUST be followed by a final harvest operation.
T Crops that use multiple harvests must be manually calibrated.
T Added 12-27-11 MAS
+
G 02 Biomass Manipulation
+ 1.0
P 31 Kill or Defoliate Growing Crop
+ 0
P 62 Remove (by age pool) Plant/Residue Material
+ 1 0 0 0 3 3 2 0.5 0.0 0.0 0.0 0.0
P 40 End crop Biomass Manipulation
#------------
D 13/05/02
O 04 Harvest, hand pick vegetables
+ 3.2738733 0.15
T Hand pick tomato, artichoke, peppers, strawberries or similar crops
T with multiple harvests from the same plants.  12-13-2011 DTL
T This is a partial harvest only 50% of the yield is taken with this harvest.
T This operation MUST be followed by a final harvest operation.
T Crops that use multiple harvests must be manually calibrated.
T Added 12-27-11 MAS
+
G 02 Biomass Manipulation
+ 1.0
P 31 Kill or Defoliate Growing Crop
+ 0
P 62 Remove (by age pool) Plant/Residue Material
+ 1 0 0 0 3 3 2 0.5 0.0 0.0 0.0 0.0
P 40 End crop Biomass Manipulation
#------------
D 20/05/02
O 04 Harvest, hand pick vegetables
+ 3.2738733 0.15
T Hand pick tomato, artichoke, peppers, strawberries or similar crops
T with multiple harvests from the same plants.  12-13-2011 DTL
T This is a partial harvest only 50% of the yield is taken with this harvest.
T This operation MUST be followed by a final harvest operation.
T Crops that use multiple harvests must be manually calibrated.
T Added 12-27-11 MAS
+
G 02 Biomass Manipulation
+ 1.0
P 31 Kill or Defoliate Growing Crop
+ 0
P 62 Remove (by age pool) Plant/Residue Material
+ 1 0 0 0 3 3 2 0.5 0.0 0.0 0.0 0.0
P 40 End crop Biomass Manipulation
#------------
D 21/05/02
O 03 Disk, tandem secondary op
+ 4.4898834 32.5 2.2351363 0.0 2.2351363 1.3410819 2.6821637
T 9-in. Spacing, Front and Rear; Good for seedbed preparation/chemical incorporation in medium to heavy soils
T Works well in primary tillage in light to medium soils
T Provides good residue-handling capability.  MAS 10-26-06
+
G 01 Tillage
+ 127.00027 0.75 1.0 127.00026 76.20015 152.4003
P 01 Break Crust
P 02 Random Roughness
+ 1 15.240031
P 05 Ridges and Dikes
+ 1 50.800102 228.60046 0.0 0.0 0.0
P 11 Aggregate Crushing
+ 2.8 0.75
P 12 Soil Loosening
+ 0.85
P 13 Soil Layer Mixing
+ 0.4
P 31 Kill or Defoliate Growing Crop
+ 2
P 40 End crop Biomass Manipulation
P 24 Flatten Standing Biomass
+ 0 0.85 0.7 0.6 0.5 1.0
P 25 Bury Flat Biomass
+ 1 0.73 0.63 0.55 0.4 0.73
P 26 Resurface Buried Biomass
+ 0.02 0.04 0.02 0.05 0.02
P 34 Change Standing Biomass Fall Rate
+ 7 3.0 2.5 2.0 1.5 1.0
+ 0.5 0.6 0.7 0.8 1.0
#------------
D 24/05/02
O 03 Planter, small veg seed
+ 3.3674128 .59 0.89405453 0.0 0.89405453 0.44702727 1.3410819
T Small seed planter like used in planting small seeded vegetables in 25 to 30" rows.
T Shallow depth and minimal disturbance in fine seedbed.  Like Planet Junior.  12-10-01 DTL
T G2 was added into file in front of the flattening (P24), burial (P25), and resurfacing (P26) factors because the area affected is less than 1.0 and
T the RUSLE values were normalized to 1.0.  This change will imulate the correct residue changes based on the method set forth in RUSLE.
T RUSLE's factors have been redused to based on the area affected.
T The stalk fall rate factor (P34) was moved ahead of the new (G2) factor to set the fall rate to theless than 1.0 area affected.  8/7/07 MAS
T
T Changed the P5 to allow the preexisting ridges and furrows to set the ridge roughness.  MAS  12-30-2010
+
G 01 Tillage
+ 25.400051 0.5 .15 25.400051 12.700026 50.800102
P 01 Break Crust
P 02 Random Roughness
+ 1 7.6200156
P 05 Ridges and Dikes
+ 0 25.400051 762.0015 711.2014 0.0 0.0
P 11 Aggregate Crushing
+ 2.8 0.75
P 12 Soil Loosening
+ 0.6
P 13 Soil Layer Mixing
+ 0.35
P 34 Change Standing Biomass Fall Rate
+ 7 3.0 2.5 2.0 1.5 1.0
+ 0.5 0.6 0.7 0.8 1.0
G 02 Biomass Manipulation
+ 1.0
P 24 Flatten Standing Biomass
+ 0 .3 .25 .2 0.1 1.0
P 25 Bury Flat Biomass
+ 1 .0525 .0375 .03 .015 .03
P 26 Resurface Buried Biomass
+ 0.01 .01 .01 0.05 .01
G 03 Crop Name
+ Cucumber
P 51 Seeding Configuration
+ 1 0.0 2
+ 24.711494 1.0 1 29000 1.0 1.0 0
+ lb/ac
+ 96.1 8930 4 0.8 0.65 0.9
+ 0.4 0.025 1.1 10.0 32.0 0 70 900.0
+ -5.0 -15.0 0.15 0.95 0.0 30.0
+ -0.0062 0.9478 0.3633 -0.0721 -0.0083 1.005 0.7292 0.0562
+ 0.3633 -0.0721 2.0 1.0 20.0 0.05 0 6.0957026
+ 25.641026 25.641026 1.3 0.011 0.0 0.0 0.0 1
+ 0.02 0.02 0.02 0.02 0.2 0.0050 20.0 5.227942
+ -1.20379 0.604887 0.0688 0.024658702 0.0 0.0 0.0 0.0
T RUSLE2 notes.  4/17/03 gaw.   Yield for machine harvest. High production, related to one or more of the following - irrigation,
T high fertility, favorable climate, productive soils and varieties.  Type locations: CA, FL, TX.
T
T I made changes to the harvest index to match the Cucumber, HIGH PRO record in RUSLE2.  MAS 11-24-08
T Corrected the plant pop and yield.  MAS 5-11-09
#------------
D 14/06/02
O 03 Weed control, manual hoe
+ 9.353924E-8 3.315 0.44702727 0.0 0.44702727 0.44702727 0.44702727
T Added to WEPS 4-12-12 MAS
T
T R2 Note: gaw 01-22-02\nManually control weeds in small fields using hoe or similar tool that disturbs soil surface.
T Weeds added to surface.\nThis operation does not kill existing crop.
T User selects type of residue material added and dry weight. rev043008DTL
T
T
T Derived from
T Cultivator - row crop (30 inch row spacing, 1 inch ridge height)
T reduced speed, reduced depth, reduced area affected, removed ridge
+ 
G 01 Tillage
+ 76.20015 0.9 0.85 76.20015 25.400051 101.600204
P 01 Break Crust
P 02 Random Roughness
+ 1 12.700026
P 11 Aggregate Crushing
+ 3.0 1.0
P 12 Soil Loosening
+ 0.75
P 13 Soil Layer Mixing
+ 0.35
P 25 Bury Flat Biomass
+ 1 0.425 0.34 0.255 0.221 0.323
P 26 Resurface Buried Biomass
+ 0.04 0.04 0.04 0.06 0.04
P 34 Change Standing Biomass Fall Rate
+ 4 3.0 2.5 2.0 1.5 1.0
+ 0.5 0.6 0.7 0.8 1.0
G 03 Crop Name
+ weed residue; 0-3 mo
P 65 Add Crop Residue Amounts
+ 0.0 0.0 0.0 0.028021252 1
+ 0.0 0.0 0.0056042504 152.4003
+ 0.025 0.025 0.025 0.025 0.169 0.0050 17.1 5.227942
+ -1.20379 0.604887
T Enter crop notes here.
#------------
D 28/06/02
O 03 Weed control, manual hoe
+ 9.353924E-8 3.315 0.44702727 0.0 0.44702727 0.44702727 0.44702727
T Added to WEPS 4-12-12 MAS
T
T R2 Note: gaw 01-22-02\nManually control weeds in small fields using hoe or similar tool that disturbs soil surface.
T Weeds added to surface.\nThis operation does not kill existing crop.
T User selects type of residue material added and dry weight. rev043008DTL
T
T
T Derived from
T Cultivator - row crop (30 inch row spacing, 1 inch ridge height)
T reduced speed, reduced depth, reduced area affected, removed ridge
+ 
G 01 Tillage
+ 76.20015 0.9 0.85 76.20015 25.400051 101.600204
P 01 Break Crust
P 02 Random Roughness
+ 1 12.700026
P 11 Aggregate Crushing
+ 3.0 1.0
P 12 Soil Loosening
+ 0.75
P 13 Soil Layer Mixing
+ 0.35
P 25 Bury Flat Biomass
+ 1 0.425 0.34 0.255 0.221 0.323
P 26 Resurface Buried Biomass
+ 0.04 0.04 0.04 0.06 0.04
P 34 Change Standing Biomass Fall Rate
+ 4 3.0 2.5 2.0 1.5 1.0
+ 0.5 0.6 0.7 0.8 1.0
G 03 Crop Name
+ weed residue; 0-3 mo
P 65 Add Crop Residue Amounts
+ 0.0 0.0 0.0 0.028021252 1
+ 0.0 0.0 0.0056042504 152.4003
+ 0.025 0.025 0.025 0.025 0.169 0.0050 17.1 5.227942
+ -1.20379 0.604887
T Enter crop notes here.
#------------
D 18/07/02
O 04 Harvest, hand pick vegetables
+ 3.2738733 0.15
T Hand pick tomato, artichoke, peppers, strawberries or similar crops
T with multiple harvests from the same plants.  12-13-2011 DTL
T This is a partial harvest only 50% of the yield is taken with this harvest.
T This operation MUST be followed by a final harvest operation.
T Crops that use multiple harvests must be manually calibrated.
T Added 12-27-11 MAS
+
G 02 Biomass Manipulation
+ 1.0
P 31 Kill or Defoliate Growing Crop
+ 0
P 62 Remove (by age pool) Plant/Residue Material
+ 1 0 0 0 3 3 2 0.5 0.0 0.0 0.0 0.0
P 40 End crop Biomass Manipulation
#------------
D 25/07/02
O 04 Harvest, hand pick vegetables
+ 3.2738733 0.15
T Hand pick tomato, artichoke, peppers, strawberries or similar crops
T with multiple harvests from the same plants.  12-13-2011 DTL
T This is a partial harvest only 50% of the yield is taken with this harvest.
T This operation MUST be followed by a final harvest operation.
T Crops that use multiple harvests must be manually calibrated.
T Added 12-27-11 MAS
+
G 02 Biomass Manipulation
+ 1.0
P 31 Kill or Defoliate Growing Crop
+ 0
P 62 Remove (by age pool) Plant/Residue Material
+ 1 0 0 0 3 3 2 0.5 0.0 0.0 0.0 0.0
P 40 End crop Biomass Manipulation
#------------
D 01/08/02
O 04 Harvest, hand pick vegetables
+ 3.2738733 0.15
T Hand pick tomato, artichoke, peppers, strawberries or similar crops
T with multiple harvests from the same plants.  12-13-2011 DTL
T This is a partial harvest only 50% of the yield is taken with this harvest.
T This operation MUST be followed by a final harvest operation.
T Crops that use multiple harvests must be manually calibrated.
T Added 12-27-11 MAS
+
G 02 Biomass Manipulation
+ 1.0
P 31 Kill or Defoliate Growing Crop
+ 0
P 62 Remove (by age pool) Plant/Residue Material
+ 1 0 0 0 3 3 2 0.5 0.0 0.0 0.0 0.0
P 40 End crop Biomass Manipulation
#------------
D 08/08/02
O 04 Harvest, hand pick vegetables
+ 3.2738733 0.15
T Hand pick tomato, artichoke, peppers, strawberries or similar crops
T with multiple harvests from the same plants.  12-13-2011 DTL
T This is a partial harvest only 50% of the yield is taken with this harvest.
T This operation MUST be followed by a final harvest operation.
T Crops that use multiple harvests must be manually calibrated.
T Added 12-27-11 MAS
+
G 02 Biomass Manipulation
+ 1.0
P 31 Kill or Defoliate Growing Crop
+ 0
P 62 Remove (by age pool) Plant/Residue Material
+ 1 0 0 0 3 3 2 0.5 0.0 0.0 0.0 0.0
P 40 End crop Biomass Manipulation
#------------
D 15/08/02
O 04 Harvest, hand pick vegetables
+ 3.2738733 0.15
T Hand pick tomato, artichoke, peppers, strawberries or similar crops
T with multiple harvests from the same plants.  12-13-2011 DTL
T This is a partial harvest only 50% of the yield is taken with this harvest.
T This operation MUST be followed by a final harvest operation.
T Crops that use multiple harvests must be manually calibrated.
T Added 12-27-11 MAS
+
G 02 Biomass Manipulation
+ 1.0
P 31 Kill or Defoliate Growing Crop
+ 0
P 62 Remove (by age pool) Plant/Residue Material
+ 1 0 0 0 3 3 2 0.5 0.0 0.0 0.0 0.0
P 40 End crop Biomass Manipulation
#------------
D 22/08/02
O 04 Harvest, hand pick vegetables
+ 3.2738733 0.15
T Hand pick tomato, artichoke, peppers, strawberries or similar crops
T with multiple harvests from the same plants.  12-13-2011 DTL
T This is a partial harvest only 50% of the yield is taken with this harvest.
T This operation MUST be followed by a final harvest operation.
T Crops that use multiple harvests must be manually calibrated.
T Added 12-27-11 MAS
+
G 02 Biomass Manipulation
+ 1.0
P 31 Kill or Defoliate Growing Crop
+ 0
P 62 Remove (by age pool) Plant/Residue Material
+ 1 0 0 0 3 3 2 0.5 0.0 0.0 0.0 0.0
P 40 End crop Biomass Manipulation
#------------
D 23/08/02
O 03 Disk, tandem secondary op
+ 4.4898834 32.5 2.2351363 0.0 2.2351363 1.3410819 2.6821637
T 9-in. Spacing, Front and Rear; Good for seedbed preparation/chemical incorporation in medium to heavy soils
T Works well in primary tillage in light to medium soils
T Provides good residue-handling capability.  MAS 10-26-06
+
G 01 Tillage
+ 127.00027 0.75 1.0 127.00026 76.20015 152.4003
P 01 Break Crust
P 02 Random Roughness
+ 1 15.240031
P 05 Ridges and Dikes
+ 1 50.800102 228.60046 0.0 0.0 0.0
P 11 Aggregate Crushing
+ 2.8 0.75
P 12 Soil Loosening
+ 0.85
P 13 Soil Layer Mixing
+ 0.4
P 31 Kill or Defoliate Growing Crop
+ 2
P 40 End crop Biomass Manipulation
P 24 Flatten Standing Biomass
+ 0 0.85 0.7 0.6 0.5 1.0
P 25 Bury Flat Biomass
+ 1 0.73 0.63 0.55 0.4 0.73
P 26 Resurface Buried Biomass
+ 0.02 0.04 0.02 0.05 0.02
P 34 Change Standing Biomass Fall Rate
+ 7 3.0 2.5 2.0 1.5 1.0
+ 0.5 0.6 0.7 0.8 1.0
#------------
D 23/08/02
O 04 Fert applic. surface broadcast
+ 1.4966278 0.0609375
T R2 Notes: Broadcast fertilizer spreader.  Wheel traffic only.  rev 082107 DTL
T
T Added to DB 4-12-12 MAS
+
G 01 Tillage
+ 0.0 0 0.05 0.0 0.0 0.0
P 01 Break Crust
P 02 Random Roughness
+ 1 8.8900175
P 11 Aggregate Crushing
+ 4.3 2.0
P 24 Flatten Standing Biomass
+ 0 0.25 0.2 0.15 0.1 1.0
P 26 Resurface Buried Biomass
+ 0.07 0.08 0.1 0.12 0.07
P 34 Change Standing Biomass Fall Rate
+ 0 1.0 1.0 1.0 1.0 1.0
+ 1.0 1.0 1.0 1.0 1.0
#------------
D 28/08/02
O 03 Planter, small veg seed
+ 3.3674128 .59 0.89405453 0.0 0.89405453 0.44702727 1.3410819
T Small seed planter like used in planting small seeded vegetables in 25 to 30" rows.
T Shallow depth and minimal disturbance in fine seedbed.  Like Planet Junior.  12-10-01 DTL
T G2 was added into file in front of the flattening (P24), burial (P25), and resurfacing (P26) factors because the area affected is less than 1.0 and
T the RUSLE values were normalized to 1.0.  This change will imulate the correct residue changes based on the method set forth in RUSLE.
T RUSLE's factors have been redused to based on the area affected.
T The stalk fall rate factor (P34) was moved ahead of the new (G2) factor to set the fall rate to theless than 1.0 area affected.  8/7/07 MAS
T
T Changed the P5 to allow the preexisting ridges and furrows to set the ridge roughness.  MAS  12-30-2010
+
G 01 Tillage
+ 25.400051 0.5 .15 25.400051 12.700026 50.800102
P 01 Break Crust
P 02 Random Roughness
+ 1 7.6200156
P 05 Ridges and Dikes
+ 0 25.400051 762.0015 711.2014 0.0 0.0
P 11 Aggregate Crushing
+ 2.8 0.75
P 12 Soil Loosening
+ 0.6
P 13 Soil Layer Mixing
+ 0.35
P 34 Change Standing Biomass Fall Rate
+ 7 3.0 2.5 2.0 1.5 1.0
+ 0.5 0.6 0.7 0.8 1.0
G 02 Biomass Manipulation
+ 1.0
P 24 Flatten Standing Biomass
+ 0 .3 .25 .2 0.1 1.0
P 25 Bury Flat Biomass
+ 1 .0525 .0375 .03 .015 .03
P 26 Resurface Buried Biomass
+ 0.01 .01 .01 0.05 .01
G 03 Crop Name
+ Lettuce, leaf
P 51 Seeding Configuration
+ 1 0.0 2
+ 9 1 1 35300 1 1 3
+ lbs/ac
+ 90 8930 4 1 0.65 0.95
+ 0.3048037 0.025 0.8 0 18.199999999999996 0 75 1100
+ -5 -15 0.01 0.95 0 19
+ 0.3128 0.576 0.6898 -0.1533 0 1 1.1 0.01
+ 0.4995 -0.0944 0.1 1 30 0.05 1 0.2562663
+ 500 500 1.5 0.01 0 0 0 1
+ 0.02 0.02 0.02 0.02 0.2 0.0050 20 5.227942
+ -1.20379 0.604887 0 0 0 0.0 0.0 0.0
T Enter crop notes here.
T Calibrated from run [new run_2.wjr] on:
T Tue Feb 13 08:17:13 CST 2007
T 35300 lbs/ac	1.0 -->  2.560
T Calibrated from run [new run_7.wjr] on:
T Tue Feb 13 08:48:39 CST 2007
T 35300 lbs/ac	2.56 -->  3.712
T Calibrated from run [new run_9.wjr] on:
T Tue Feb 13 09:00:50 CST 2007
T 35300 lbs/ac	3.712 -->  4.826
#------------
D 12/09/02
O 03 Weed control, manual hoe
+ 9.353924E-8 3.315 0.44702727 0.0 0.44702727 0.44702727 0.44702727
T Added to WEPS 4-12-12 MAS
T
T R2 Note: gaw 01-22-02\nManually control weeds in small fields using hoe or similar tool that disturbs soil surface.
T Weeds added to surface.\nThis operation does not kill existing crop.
T User selects type of residue material added and dry weight. rev043008DTL
T
T
T Derived from
T Cultivator - row crop (30 inch row spacing, 1 inch ridge height)
T reduced speed, reduced depth, reduced area affected, removed ridge
+ 
G 01 Tillage
+ 76.20015 0.9 0.85 76.20015 25.400051 101.600204
P 01 Break Crust
P 02 Random Roughness
+ 1 12.700026
P 11 Aggregate Crushing
+ 3.0 1.0
P 12 Soil Loosening
+ 0.75
P 13 Soil Layer Mixing
+ 0.35
P 25 Bury Flat Biomass
+ 1 0.425 0.34 0.255 0.221 0.323
P 26 Resurface Buried Biomass
+ 0.04 0.04 0.04 0.06 0.04
P 34 Change Standing Biomass Fall Rate
+ 4 3.0 2.5 2.0 1.5 1.0
+ 0.5 0.6 0.7 0.8 1.0
G 03 Crop Name
+ weed residue; 0-3 mo
P 65 Add Crop Residue Amounts
+ 0.0 0.0 0.0 0.028021252 1
+ 0.0 0.0 0.0056042504 152.4003
+ 0.025 0.025 0.025 0.025 0.169 0.0050 17.1 5.227942
+ -1.20379 0.604887
T Enter crop notes here.
#------------
D 26/09/02
O 03 Weed control, manual hoe
+ 9.353924E-8 3.315 0.44702727 0.0 0.44702727 0.44702727 0.44702727
T Added to WEPS 4-12-12 MAS
T
T R2 Note: gaw 01-22-02\nManually control weeds in small fields using hoe or similar tool that disturbs soil surface.
T Weeds added to surface.\nThis operation does not kill existing crop.
T User selects type of residue material added and dry weight. rev043008DTL
T
T
T Derived from
T Cultivator - row crop (30 inch row spacing, 1 inch ridge height)
T reduced speed, reduced depth, reduced area affected, removed ridge
+ 
G 01 Tillage
+ 76.20015 0.9 0.85 76.20015 25.400051 101.600204
P 01 Break Crust
P 02 Random Roughness
+ 1 12.700026
P 11 Aggregate Crushing
+ 3.0 1.0
P 12 Soil Loosening
+ 0.75
P 13 Soil Layer Mixing
+ 0.35
P 25 Bury Flat Biomass
+ 1 0.425 0.34 0.255 0.221 0.323
P 26 Resurface Buried Biomass
+ 0.04 0.04 0.04 0.06 0.04
P 34 Change Standing Biomass Fall Rate
+ 4 3.0 2.5 2.0 1.5 1.0
+ 0.5 0.6 0.7 0.8 1.0
G 03 Crop Name
+ weed residue; 0-3 mo
P 65 Add Crop Residue Amounts
+ 0.0 0.0 0.0 0.028021252 1
+ 0.0 0.0 0.0056042504 152.4003
+ 0.025 0.025 0.025 0.025 0.169 0.0050 17.1 5.227942
+ -1.20379 0.604887
T Enter crop notes here.
#------------
D 10/10/02
O 03 Weed control, manual hoe
+ 9.353924E-8 3.315 0.44702727 0.0 0.44702727 0.44702727 0.44702727
T Added to WEPS 4-12-12 MAS
T
T R2 Note: gaw 01-22-02\nManually control weeds in small fields using hoe or similar tool that disturbs soil surface.
T Weeds added to surface.\nThis operation does not kill existing crop.
T User selects type of residue material added and dry weight. rev043008DTL
T
T
T Derived from
T Cultivator - row crop (30 inch row spacing, 1 inch ridge height)
T reduced speed, reduced depth, reduced area affected, removed ridge
+ 
G 01 Tillage
+ 76.20015 0.9 0.85 76.20015 25.400051 101.600204
P 01 Break Crust
P 02 Random Roughness
+ 1 12.700026
P 11 Aggregate Crushing
+ 3.0 1.0
P 12 Soil Loosening
+ 0.75
P 13 Soil Layer Mixing
+ 0.35
P 25 Bury Flat Biomass
+ 1 0.425 0.34 0.255 0.221 0.323
P 26 Resurface Buried Biomass
+ 0.04 0.04 0.04 0.06 0.04
P 34 Change Standing Biomass Fall Rate
+ 4 3.0 2.5 2.0 1.5 1.0
+ 0.5 0.6 0.7 0.8 1.0
G 03 Crop Name
+ weed residue; 0-3 mo
P 65 Add Crop Residue Amounts
+ 0.0 0.0 0.0 0.028021252 1
+ 0.0 0.0 0.0056042504 152.4003
+ 0.025 0.025 0.025 0.025 0.169 0.0050 17.1 5.227942
+ -1.20379 0.604887
T Enter crop notes here.
#------------
D 27/10/02
O 04 Harvest, hand pick vegetables
+ 3.2738733 0.15
T Hand pick tomato, artichoke, peppers, strawberries or similar crops
T with multiple harvests from the same plants.  12-13-2011 DTL
T This is a partial harvest only 50% of the yield is taken with this harvest.
T This operation MUST be followed by a final harvest operation.
T Crops that use multiple harvests must be manually calibrated.
T Added 12-27-11 MAS
+
G 02 Biomass Manipulation
+ 1.0
P 31 Kill or Defoliate Growing Crop
+ 0
P 62 Remove (by age pool) Plant/Residue Material
+ 1 0 0 0 3 3 2 0.5 0.0 0.0 0.0 0.0
P 40 End crop Biomass Manipulation
#------------
D 03/11/02
O 04 Harvest, hand pick vegetables
+ 3.2738733 0.15
T Hand pick tomato, artichoke, peppers, strawberries or similar crops
T with multiple harvests from the same plants.  12-13-2011 DTL
T This is a partial harvest only 50% of the yield is taken with this harvest.
T This operation MUST be followed by a final harvest operation.
T Crops that use multiple harvests must be manually calibrated.
T Added 12-27-11 MAS
+
G 02 Biomass Manipulation
+ 1.0
P 31 Kill or Defoliate Growing Crop
+ 0
P 62 Remove (by age pool) Plant/Residue Material
+ 1 0 0 0 3 3 2 0.5 0.0 0.0 0.0 0.0
P 40 End crop Biomass Manipulation
#------------
D 10/11/02
O 04 Harvest, hand pick vegetables
+ 3.2738733 0.15
T Hand pick tomato, artichoke, peppers, strawberries or similar crops
T with multiple harvests from the same plants.  12-13-2011 DTL
T This is a partial harvest only 50% of the yield is taken with this harvest.
T This operation MUST be followed by a final harvest operation.
T Crops that use multiple harvests must be manually calibrated.
T Added 12-27-11 MAS
+
G 02 Biomass Manipulation
+ 1.0
P 31 Kill or Defoliate Growing Crop
+ 0
P 62 Remove (by age pool) Plant/Residue Material
+ 1 0 0 0 3 3 2 0.5 0.0 0.0 0.0 0.0
P 40 End crop Biomass Manipulation
#------------
D 17/11/02
O 04 Harvest, hand pick vegetables
+ 3.2738733 0.15
T Hand pick tomato, artichoke, peppers, strawberries or similar crops
T with multiple harvests from the same plants.  12-13-2011 DTL
T This is a partial harvest only 50% of the yield is taken with this harvest.
T This operation MUST be followed by a final harvest operation.
T Crops that use multiple harvests must be manually calibrated.
T Added 12-27-11 MAS
+
G 02 Biomass Manipulation
+ 1.0
P 31 Kill or Defoliate Growing Crop
+ 0
P 62 Remove (by age pool) Plant/Residue Material
+ 1 0 0 0 3 3 2 0.5 0.0 0.0 0.0 0.0
P 40 End crop Biomass Manipulation
#------------
D 24/11/02
O 04 Harvest, hand pick vegetables
+ 3.2738733 0.15
T Hand pick tomato, artichoke, peppers, strawberries or similar crops
T with multiple harvests from the same plants.  12-13-2011 DTL
T This is a partial harvest only 50% of the yield is taken with this harvest.
T This operation MUST be followed by a final harvest operation.
T Crops that use multiple harvests must be manually calibrated.
T Added 12-27-11 MAS
+
G 02 Biomass Manipulation
+ 1.0
P 31 Kill or Defoliate Growing Crop
+ 0
P 62 Remove (by age pool) Plant/Residue Material
+ 1 0 0 0 3 3 2 0.5 0.0 0.0 0.0 0.0
P 40 End crop Biomass Manipulation
#------------
*END
*EOF
