Version: 1.5
*START 1
N Originating Program: RUSLE2
N Skel Format Version: 1.1
N This management file was originally converted from the NRCS standard XML format on - Tue Oct 16 13:25:47 PDT 2012
N This management file was updated to contain the most current crop and operation records for WEPS on - Tue Dec 17 20:07:37 CST 2013
#------------
D 25/04/01
O 03 Plow, moldboard
+ 17.491838 65 2.2351363 0.0 2.2351363 1.5645955 2.6821637
T Moldboard plow 8 inch operating depth.  060701 DTL  Modified flattening and burial per McCool and Foster 05/21/02 DTL RUSLE MAS 10-26-06
+
G 01 Tillage
+ 203.20041 1.0 1.0 203.20041 152.4003 254.0005
P 01 Break Crust
P 02 Random Roughness
+ 1 48.260098
P 05 Ridges and Dikes
+ 1 25.400051 406.40082 0.0 0.0 0.0
P 11 Aggregate Crushing
+ 2.8 1.0
P 12 Soil Loosening
+ 1.0
P 13 Soil Layer Mixing
+ 0.7
P 14 Soil Layer Inversion
P 31 Kill or Defoliate Growing Crop
+ 2
P 40 End crop Biomass Manipulation
P 24 Flatten Standing Biomass
+ 0 1 1 1 0.75 1.0
P 25 Bury Flat Biomass
+ 3 0.99 0.99 0.99 0.85 0.97
P 26 Resurface Buried Biomass
+ 0.01 0.02 0.04 0.1 0.02
P 34 Change Standing Biomass Fall Rate
+ 7 3.0 2.5 2.0 1.5 1.0
+ 0.5 0.6 0.7 0.8 1.0
#------------
D 05/05/01
O 03 Disk, tandem secondary op
+ 4.4898834 32.5 2.2351363 0.0 2.2351363 1.3410819 2.6821637
T 9-in. Spacing, Front and Rear; Good for seedbed preparation/chemical incorporation in medium to heavy soils
T Works well in primary tillage in light to medium soils
T Provides good residue-handling capability.  MAS 10-26-06
+
G 01 Tillage
+ 127.00027 0.75 1.0 127.00026 76.20015 152.4003
P 01 Break Crust
P 02 Random Roughness
+ 1 15.240031
P 05 Ridges and Dikes
+ 1 50.800102 228.60046 0.0 0.0 0.0
P 11 Aggregate Crushing
+ 2.8 0.75
P 12 Soil Loosening
+ 0.85
P 13 Soil Layer Mixing
+ 0.4
P 31 Kill or Defoliate Growing Crop
+ 2
P 40 End crop Biomass Manipulation
P 24 Flatten Standing Biomass
+ 0 0.85 0.7 0.6 0.5 1.0
P 25 Bury Flat Biomass
+ 1 0.73 0.63 0.55 0.4 0.73
P 26 Resurface Buried Biomass
+ 0.02 0.04 0.02 0.05 0.02
P 34 Change Standing Biomass Fall Rate
+ 7 3.0 2.5 2.0 1.5 1.0
+ 0.5 0.6 0.7 0.8 1.0
#------------
D 10/05/01
O 03 Disk, tandem light finishing
+ 3.7415698 19.5 2.2351363 0.0 2.2351363 1.3410819 2.6821637
T 6/8/01 DTL RUSLE.  7in sp.  This is tool used to finish a seedbed.  MAS 10-26-06
+
G 01 Tillage
+ 101.600204 0.5 1.0 101.600204 76.20015 127.00026
P 01 Break Crust
P 02 Random Roughness
+ 1 15.240031
P 05 Ridges and Dikes
+ 1 12.700026 177.80035 0.0 0.0 0.0
P 11 Aggregate Crushing
+ 2.8 0.75
P 12 Soil Loosening
+ 0.75
P 13 Soil Layer Mixing
+ 0.35
P 31 Kill or Defoliate Growing Crop
+ 2
P 40 End crop Biomass Manipulation
P 24 Flatten Standing Biomass
+ 0 0.85 0.7 0.6 0.5 1.0
P 25 Bury Flat Biomass
+ 1 0.73 0.63 0.55 0.4 0.73
P 26 Resurface Buried Biomass
+ 0.02 0.04 0.02 0.05 0.02
P 34 Change Standing Biomass Fall Rate
+ 7 3.0 2.5 2.0 1.5 1.0
+ 0.5 0.6 0.7 0.8 1.0
#------------
D 15/05/01
O 04 Fert applic. surface broadcast
+ 1.4966278 0.0609375
T R2 Notes: Broadcast fertilizer spreader.  Wheel traffic only.  rev 082107 DTL
T
T Added to DB 4-12-12 MAS
+
G 01 Tillage
+ 0.0 0 0.05 0.0 0.0 0.0
P 01 Break Crust
P 02 Random Roughness
+ 1 8.8900175
P 11 Aggregate Crushing
+ 4.3 2.0
P 24 Flatten Standing Biomass
+ 0 0.25 0.2 0.15 0.1 1.0
P 26 Resurface Buried Biomass
+ 0.07 0.08 0.1 0.12 0.07
P 34 Change Standing Biomass Fall Rate
+ 0 1.0 1.0 1.0 1.0 1.0
+ 1.0 1.0 1.0 1.0 1.0
#------------
D 16/05/01
O 03 Bedder, hipper, disk hiller
+ 4.2092657 26 2.0116227 0.0 2.0116227 1.5645955 2.2351363
T This is an 8 in high tool to reform beds from RUSLE 6-7-01 DTL
T
T Corrected the tillage depths and other residue values 11-1-11
+
G 01 Tillage
+ 101.600204 0.9 1.0 101.600204 50.800102 127.00025
P 01 Break Crust
P 02 Random Roughness
+ 1 15.240031
P 11 Aggregate Crushing
+ 3.0 2.0
P 12 Soil Loosening
+ 0.75
P 13 Soil Layer Mixing
+ 0.75
P 05 Ridges and Dikes
+ 1 203.20041 760.0 381.00076 0.0 0.0
P 31 Kill or Defoliate Growing Crop
+ 2
P 40 End crop Biomass Manipulation
P 24 Flatten Standing Biomass
+ 0 1 0.90 0.9 0.5 1.00
P 25 Bury Flat Biomass
+ 1 0.95 0.92 0.85 0.5 0.6
P 26 Resurface Buried Biomass
+ 0.02 0.02 0.02 0.05 0.03
P 34 Change Standing Biomass Fall Rate
+ 7 3.0 2.5 2.0 1.5 1.0
+ 0.5 0.6 0.7 0.8 1.0
#------------
D 25/05/01
O 03 Planter, transplanter, vegetable on 8 inch high beds
+ 7.4831395 3.12 0.89405453 0.0 0.89405453 0.44702727 1.3410819
T Vegetable transplanter on 8 inch beds or ridges.11/15/02  DTL
T G2 was added into file in front of the flattening (P24), burial (P25), and resurfacing (P26) factors because the area affected is less than 1.0 and
T the RUSLE values were normalized to 1.0.  This change will imulate the correct residue changes based on the method set forth in RUSLE.
T RUSLE's factors have been redused to based on the area affected.
T The stalk fall rate factor (P34) was moved ahead of the new (G2) factor to set the fall rate to the less than 1.0 area affected.  8/7/07 MAS
+
G 01 Tillage
+ 101.600204 0.5 .2 101.600204 76.20015 127.00026
P 01 Break Crust
P 02 Random Roughness
+ 1 10.160021
P 05 Ridges and Dikes
+ 1 203.20041 762.0015 355.6007 0.0 0.0
P 11 Aggregate Crushing
+ 2.4 2
P 12 Soil Loosening
+ 0.6
P 13 Soil Layer Mixing
+ 0.3
P 34 Change Standing Biomass Fall Rate
+ 7 3.0 2.5 2.0 1.5 1.0
+ 0.5 0.6 0.7 0.8 1.0
G 02 Biomass Manipulation
+ 1.0
P 24 Flatten Standing Biomass
+ 0 .3 .25 .2 0.1 1.0
P 25 Bury Flat Biomass
+ 1 .07 .05 .04 .02 .04
P 26 Resurface Buried Biomass
+ .01 .01 .01 .02 0.01
G 03 Crop Name
+ Potato, sweet
P 51 Seeding Configuration
+ 1 0.0 2
+ 7.0 4.0 1 22000 1.0 1.0 5
+ cwt/ac
+ 72.8 89.3 7 1.0 0.65 0.8
+ 0.8 0.05 1.2192148 14.0 29.0 0 125 1300.0
+ -5.0 -15.0 0.15 0.95 0.0 15.0
+ 0.0 0.8563 0.4163 -0.061 -0.0030 0.9911 0.4425 0.0494
+ 0.4163 -0.061 2.6 1.0 30.0 0.05 0 0.9143554
+ 12000.0 2700.0 3.0 0.03 0.0 0.0 0.9 1
+ 0.02 0.02 0.02 0.02 0.2 0.0050 20.0 5.227942
+ -1.20379 0.604887 .1071 0.016016947 0.0 0.0 0.0 0.0
T Enter crop notes here.
#------------
D 15/06/01
O 03 Cultivator, row 3 in ridge
+ 5.799433 17.55 2.2351363 0.0 2.2351363 0.89405453 2.4586499
T Row crop cultivator w/ sweeps leaving a 3" ridge 05-14-02 DTL
T G2 was added into file in front of the flattening (P24), burial (P25), and resurfacing (P26) factors because the area affected is less than 1.0 and
T the RUSLE values were normalized to 1.0.  This change will imulate the correct residue changes based on the method set forth in RUSLE.
T RUSLE's factors have been redused to based on the area affected.
T The stalk fall rate factor (P34) was moved ahead of the new (G2) factor to set the fall rate to the  less than 1.0 area affected.  8/7/07 MAS
+
G 01 Tillage
+ 76.20015 0.5 .9 76.20015 50.800102 101.600204
P 01 Break Crust
P 02 Random Roughness
+ 1 15.240031
P 05 Ridges and Dikes
+ 1 76.20015 762.0015 0.0 0.0 0.0
P 11 Aggregate Crushing
+ 3.0 1.0
P 12 Soil Loosening
+ 0.75
P 13 Soil Layer Mixing
+ 0.35
P 34 Change Standing Biomass Fall Rate
+ 4 3.0 2.5 2.0 1.5 1.0
+ 0.5 0.6 0.7 0.8 1.0
G 02 Biomass Manipulation
+ 1.0
P 24 Flatten Standing Biomass
+ 14 0.7 0.3 0.3 0.1 1.0
P 25 Bury Flat Biomass
+ 1 0.68 0.6 0.52 0.39 0.77
P 26 Resurface Buried Biomass
+ 0.04 0.04 0.04 0.06 0.04
#------------
D 25/06/01
O 03 Cultivator, row 3 in ridge
+ 5.799433 17.55 2.2351363 0.0 2.2351363 0.89405453 2.4586499
T Row crop cultivator w/ sweeps leaving a 3" ridge 05-14-02 DTL
T G2 was added into file in front of the flattening (P24), burial (P25), and resurfacing (P26) factors because the area affected is less than 1.0 and
T the RUSLE values were normalized to 1.0.  This change will imulate the correct residue changes based on the method set forth in RUSLE.
T RUSLE's factors have been redused to based on the area affected.
T The stalk fall rate factor (P34) was moved ahead of the new (G2) factor to set the fall rate to the  less than 1.0 area affected.  8/7/07 MAS
+
G 01 Tillage
+ 76.20015 0.5 .9 76.20015 50.800102 101.600204
P 01 Break Crust
P 02 Random Roughness
+ 1 15.240031
P 05 Ridges and Dikes
+ 1 76.20015 762.0015 0.0 0.0 0.0
P 11 Aggregate Crushing
+ 3.0 1.0
P 12 Soil Loosening
+ 0.75
P 13 Soil Layer Mixing
+ 0.35
P 34 Change Standing Biomass Fall Rate
+ 4 3.0 2.5 2.0 1.5 1.0
+ 0.5 0.6 0.7 0.8 1.0
G 02 Biomass Manipulation
+ 1.0
P 24 Flatten Standing Biomass
+ 14 0.7 0.3 0.3 0.1 1.0
P 25 Bury Flat Biomass
+ 1 0.68 0.6 0.52 0.39 0.77
P 26 Resurface Buried Biomass
+ 0.04 0.04 0.04 0.06 0.04
#------------
D 05/07/01
O 03 Cultivator, row between beds
+ 5.799433 10.56 2.2351363 0.0 2.2351363 0.89405453 2.4586499
T Cultivator w/ opposing gangs of disk hillers.  Used to cultivate between Sugarcane beds. 020106 DTL
T G2 was added into file in front of the flattening (P24), burial (P25), and resurfacing (P26) factors because the area affected is less than 1.0 and
T the RUSLE values were normalized to 1.0.  This change will imulate the correct residue changes based on the method set forth in RUSLE.
T RUSLE's factors have been redused to based on the area affected.
T The stalk fall rate factor (P34) was moved ahead of the new (G2) factor to set the fall rate to the  less than 1.0 area affected.  8/7/07 MAS
T Cloned from row cultivator.  11-22-07 MAS
T
T Changed the P5 Ridge and Dikes to reflect the height of the previous tillage.  The operation now will show the ridge height of the planter or
T the previous tillage.  MAS 6-3-11
+
G 01 Tillage
+ 63.500126 0.5 .65 63.500126 50.800102 101.600204
P 01 Break Crust
P 02 Random Roughness
+ 1 15.240031
P 05 Ridges and Dikes
+ 0 76.20015 762.0015 355.6007 0.0 0.0
P 11 Aggregate Crushing
+ 3.0 1.0
P 12 Soil Loosening
+ 0.75
P 13 Soil Layer Mixing
+ 0.35
P 34 Change Standing Biomass Fall Rate
+ 4 3.0 2.5 2.0 1.5 1.0
+ 0.5 0.6 0.7 0.8 1.0
G 02 Biomass Manipulation
+ 1.0
P 24 Flatten Standing Biomass
+ 14 0.7 0.3 0.3 0.1 1.0
P 25 Bury Flat Biomass
+ 1 0.49 0.44 0.38 0.28 0.55
P 26 Resurface Buried Biomass
+ 0.7 0.3 0.3 0.1 1
#------------
D 25/07/01
O 04 Sprayer, fungicide and insecticide tank mix
+ 1.2160101 .15
T Spray pest control chemicals on growing crop.  Crop is not killed.
T In the MCREW management screen the user must select the kind of weeds killed in the growing crop as external residue.   080404 DTL
T Cloned from Defoliate (spray) crop.oprn, Changed the P31 to No crop kill and added G4 to add material to field MAS 9-28-06
+
#------------
D 15/08/01
O 04 Sprayer, fungicide and insecticide tank mix
+ 1.2160101 .15
T Spray pest control chemicals on growing crop.  Crop is not killed.
T In the MCREW management screen the user must select the kind of weeds killed in the growing crop as external residue.   080404 DTL
T Cloned from Defoliate (spray) crop.oprn, Changed the P31 to No crop kill and added G4 to add material to field MAS 9-28-06
+
#------------
D 13/09/01
O 03 Harvest, dig root crops res. on surf
+ 17.491838 13.752375 1.3410819 0.0 1.5645955 1.3410819 2.9056773
T Harvest, root crops like potatoes, sugar beets, carrots, and onions.
T Surface is rough with 4 ridges and much of the residue is buried.
T Rev 11-18-04 DTL RUSLE MAS 10-26-06
T
T P24 was changed to show that all residue types are flattened.
T This havest now flattens all residue types 100%.  MAS 1-18-11
T Corrected P25 decimal value "bury flat residue"  07 to 0.07:  jkp 130910
+
G 01 Tillage
+ 177.80035 1.0 1.0 177.80035 152.4003 203.20041
P 01 Break Crust
P 02 Random Roughness
+ 1 16.510033
P 05 Ridges and Dikes
+ 1 101.600204 3657.6072 3048.006 0.0 0.0
P 11 Aggregate Crushing
+ 1.4 -1.2
P 12 Soil Loosening
+ 0.7
P 13 Soil Layer Mixing
+ 0.9
P 31 Kill or Defoliate Growing Crop
+ 2
G 02 Biomass Manipulation
+ 1.0
P 62 Remove (by age pool) Plant/Residue Material
+ 1 1 0 1 1 3 2 0.0 0.0 0.0 1.0 0.0
P 40 End crop Biomass Manipulation
P 24 Flatten Standing Biomass
+ 0 1.0 1.0 1.0 1.0 1.0
P 25 Bury Flat Biomass
+ 2 0.07 .08 .1 .12 .07
P 26 Resurface Buried Biomass
+ 0.01 0.01 0.03 0.01 0.01
#------------
*END
*EOF
