Version: 1.5
*START 1
N Originating Program: RUSLE2
N Skel Format Version: 1.1
N This management file was originally converted from the NRCS standard XML format on - Tue Oct 16 13:25:16 PDT 2012
N This management file was updated to contain the most current crop and operation records for WEPS on - Tue Dec 17 20:09:39 CST 2013
#------------
D 10/06/01
O 03 Disk, tandem heavy primary op
+ 7.0154433 39 2.2351363 0.0 2.2351363 1.3410819 2.6821637
T 11-12in. Spacing, Front and Rear
T Recommended for primary tillage in medium to heavy soils
T Excellent residue-handling capability. MAS 10-26-06
+
G 01 Tillage
+ 152.4003 1.0 1.0 152.4003 101.600204 177.80035
P 01 Break Crust
P 02 Random Roughness
+ 1 38.100075
P 05 Ridges and Dikes
+ 1 101.600204 279.40057 0.0 0.0 0.0
P 11 Aggregate Crushing
+ 2.8 0.75
P 12 Soil Loosening
+ 0.9
P 13 Soil Layer Mixing
+ 0.4
P 31 Kill or Defoliate Growing Crop
+ 2
P 40 End crop Biomass Manipulation
P 24 Flatten Standing Biomass
+ 0 1.0 0.9 0.8 0.5 1.0
P 25 Bury Flat Biomass
+ 1 0.95 0.85 0.8 0.6 0.95
P 26 Resurface Buried Biomass
+ 0.05 0.06 0.07 0.08 0.05
P 34 Change Standing Biomass Fall Rate
+ 7 3.0 2.5 2.0 1.5 1.0
+ 0.5 0.6 0.7 0.8 1.0
#------------
D 11/06/01
O 04 Fert applic. surface broadcast
+ 1.4966278 0.0609375
T R2 Notes: Broadcast fertilizer spreader.  Wheel traffic only.  rev 082107 DTL
T
T Added to DB 4-12-12 MAS
+
G 01 Tillage
+ 0.0 0 0.05 0.0 0.0 0.0
P 01 Break Crust
P 02 Random Roughness
+ 1 8.8900175
P 11 Aggregate Crushing
+ 4.3 2.0
P 24 Flatten Standing Biomass
+ 0 0.25 0.2 0.15 0.1 1.0
P 26 Resurface Buried Biomass
+ 0.07 0.08 0.1 0.12 0.07
P 34 Change Standing Biomass Fall Rate
+ 0 1.0 1.0 1.0 1.0 1.0
+ 1.0 1.0 1.0 1.0 1.0
#------------
D 12/06/01
O 03 Disk, tandem light finishing
+ 3.7415698 19.5 2.2351363 0.0 2.2351363 1.3410819 2.6821637
T 6/8/01 DTL RUSLE.  7in sp.  This is tool used to finish a seedbed.  MAS 10-26-06
+
G 01 Tillage
+ 101.600204 0.5 1.0 101.600204 76.20015 127.00026
P 01 Break Crust
P 02 Random Roughness
+ 1 15.240031
P 05 Ridges and Dikes
+ 1 12.700026 177.80035 0.0 0.0 0.0
P 11 Aggregate Crushing
+ 2.8 0.75
P 12 Soil Loosening
+ 0.75
P 13 Soil Layer Mixing
+ 0.35
P 31 Kill or Defoliate Growing Crop
+ 2
P 40 End crop Biomass Manipulation
P 24 Flatten Standing Biomass
+ 0 0.85 0.7 0.6 0.5 1.0
P 25 Bury Flat Biomass
+ 1 0.73 0.63 0.55 0.4 0.73
P 26 Resurface Buried Biomass
+ 0.02 0.04 0.02 0.05 0.02
P 34 Change Standing Biomass Fall Rate
+ 7 3.0 2.5 2.0 1.5 1.0
+ 0.5 0.6 0.7 0.8 1.0
#------------
D 20/06/01
O 03 Drill or air seeder single disk openers 7-10 in spac
+ 3.2738733 2.44 2.2351363 0.0 2.2351363 1.5645955 2.9056773
T Drill or Air seeder with single disk no-till openers  JD 750 or similar openers. (No-till air drill)
T Based on Drill, no-till single disk 7-10 spacing. 102403 DTL. RUSLE MAS 10-26-06
T G2 was added into file in front of the flattening (P24), burial (P25), and resurfacing (P26) factors because the area affected is less than 1.0 and
T the RUSLE values were normalized to 1.0.  This change will imulate the correct residue changes based on the method set forth in RUSLE.
T RUSLE's factors have been redused to based on the area affected.
T The stalk fall rate factor (P34) was moved ahead of the new (G2) factor to set the fall rate to the less than 1.0 area affected.  8/7/07 MAS
+
G 01 Tillage
+ 63.500134 0.4 0.15 63.50013 50.800102 101.600204
P 01 Break Crust
P 02 Random Roughness
+ 1 7.6200156
P 05 Ridges and Dikes
+ 1 25.400051 203.20041 0.0 0.0 0.0
P 11 Aggregate Crushing
+ 2.8 0.75
P 12 Soil Loosening
+ 0.4
P 13 Soil Layer Mixing
+ 0.20
P 34 Change Standing Biomass Fall Rate
+ 7 3.0 2.5 2.0 1.5 1.0
+ 0.5 0.6 0.7 0.8 1.0
G 02 Biomass Manipulation
+ 1.0
P 24 Flatten Standing Biomass
+ 0 0.6 0.4 0.35 0.15 1.0
P 25 Bury Flat Biomass
+ 1 0.05 0.04 0.03 0.02 0.03
P 26 Resurface Buried Biomass
+ 0.01 0.01 0.01 0.05 0.01
G 03 Crop Name
+ Sorghum, forage
P 51 Seeding Configuration
+ 1 0.0 0
+ 62.0 5.0 0 10 1.0 1.0 2
+ ton/ac
+ 0 4.465 4 1.0 0.46 0.8
+ 1.9812241 0.025 2.0 10.0 27.5 1 110 1500.0
+ -5.0 -15.0 0.01 0.95 0.0 40
+ -0.0302 0.9263 0.3728 -0.065 -0.018 1.015 0.7224 0.039
+ 0.3728 -0.065 0.03985145 0.42 19.2 0.05 0 0.7
+ 8.333333 13.0 3.0 0.03 0.1 0.1 0.0 3
+ 0.01 0.01 0.01 0.01 0.153 0.01 20.0 3.0
+ -1.20379 0.604887 0.0 0.0 0.0 0.0 0.0 0.0
T This file is most like  forage sorghum silage 20 ton  30" row spacing.  Base location Columbia, MO REV 61801 DTL
T
T The residue ratio is set to Sorghum, silage from RUSLE.  If you need a hay file use Sorghum, hay.
T MAS 4-27-08
T
T Changed the flag to not selectect for calabration from calabration  MAS 9-2-09
T Changed the flag from day maturity to heat units.  MAS 9-2-09
#------------
D 25/07/01
O 04 Harvest, hay, grass
+ 17.959534 .15
T Harvest legume hay crops such as Alfalfa and Red clover and grass-legume mixed hay such as Alfalfa-Bromegrass.
T Use Harvest, grass hay" for pure grass hay. Rev 11/17/01 DTL"  MAS 11-29-06
T
T Reset the fuel use to 1.92 gal/ac MAS 10-21-11
+
G 02 Biomass Manipulation
+ 1.0
P 31 Kill or Defoliate Growing Crop
+ 0
P 42 Cut/Remove Biomass to Height (flags)
+ 1 0 0 0 0 101.600204 .85 .85 1
P 34 Change Standing Biomass Fall Rate
+ 0 1.1 1.08 1.06 1.04 1.0
+ 0.9 0.92 0.93 0.95 1.0
P 40 End crop Biomass Manipulation
P 24 Flatten Standing Biomass
+ 14 .6 .5 .4 .5 .5
#------------
D 18/08/01
O 04 Harvest, hay, grass
+ 17.959534 .15
T Harvest legume hay crops such as Alfalfa and Red clover and grass-legume mixed hay such as Alfalfa-Bromegrass.
T Use Harvest, grass hay" for pure grass hay. Rev 11/17/01 DTL"  MAS 11-29-06
T
T Reset the fuel use to 1.92 gal/ac MAS 10-21-11
+
G 02 Biomass Manipulation
+ 1.0
P 31 Kill or Defoliate Growing Crop
+ 0
P 42 Cut/Remove Biomass to Height (flags)
+ 1 0 0 0 0 101.600204 .85 .85 1
P 34 Change Standing Biomass Fall Rate
+ 0 1.1 1.08 1.06 1.04 1.0
+ 0.9 0.92 0.93 0.95 1.0
P 40 End crop Biomass Manipulation
P 24 Flatten Standing Biomass
+ 14 .6 .5 .4 .5 .5
#------------
D 13/09/01
O 04 Harvest, hay, no regrowth
+ 17.959534 .15
T Hay harvest with no regrowth. Use to harvest crops like oat hay or other annuals which are killed by hay harvest.  10/27/01 DTL
T All crops killed.  MAS 5/9/07
T
T Reset the fuel use to 1.92 gal/ac MAS 10-21-11
T
T Removed the warnings and changed it so it can not be used to calibrate.  4-3-12 MAS
+
G 02 Biomass Manipulation
+ 1.0
P 31 Kill or Defoliate Growing Crop
+ 2
P 42 Cut/Remove Biomass to Height (flags)
+ 1 0 0 0 0 50.800102 .9 .9 1
P 40 End crop Biomass Manipulation
P 24 Flatten Standing Biomass
+ 0 0.25 0.25 0.25 0.25 0.25
#------------
*END
*EOF
