Version: 1.5
*START 1
N Originating Program: RUSLE2
N Skel Format Version: 1.1
N This management file was originally converted from the NRCS standard XML format on - Tue Oct 16 13:26:13 PDT 2012
N This management file was updated to contain the most current crop and operation records for WEPS on - Tue Dec 17 19:56:40 CST 2013
#------------
D 19/02/01
O 03 Manure spreader, slurry
+ 11.505327 .29 1.7881091 0.0 1.7881091 1.3410819 3.5762181
T Created from RUSLE file MAS 9/19/06.
T This assumes a defult residue type of  manure slurry using a solid spread with a liquid end gate spreader.
T User needs to change to the correct manure type, make a calulation on the dry matter applied, and change the value in MCREW.
T This opn is built for an application of 10 ton/ac 10% dry matter surface applied manure.
T 10 tons x 2000 lbs/ac = 20,000 lbs/ac x 0.1 = 2,000 lbs/ac applied.
T MAS 12-5-07
+
G 01 Tillage
+ 0.0 0 1 0.0 0.0 0.0
P 24 Flatten Standing Biomass
+ 14 .1 .1 .1 .1 1.0
G 03 Crop Name
+ manure, slurry
P 66 Add Manure Residue Amount
+ 0.0 0.0 0.0 0.0 1
+ 0.0 0.0 0.0 0.0
+ 0.22417001 0.0
+ .06 .06 .06 .06 0.169 0.0050 1 0.6500045
+ -2.08165 0.548606
T Enter crop notes here.
#------------
*END
*EOF
