Version: 1.5
*START 3
N Originating Program: RUSLE2
N Skel Format Version: 1.1
N This management file was originally converted from the NRCS standard XML format on - Tue Oct 16 13:27:08 PDT 2012
N This management file was updated to contain the most current crop and operation records for WEPS on - Tue Dec 17 19:54:02 CST 2013
#------------
D 20/03/01
O 04 Fert applic. surface broadcast
+ 1.4966278 0.0609375
T R2 Notes: Broadcast fertilizer spreader.  Wheel traffic only.  rev 082107 DTL
T
T Added to DB 4-12-12 MAS
+
G 01 Tillage
+ 0.0 0 0.05 0.0 0.0 0.0
P 01 Break Crust
P 02 Random Roughness
+ 1 8.8900175
P 11 Aggregate Crushing
+ 4.3 2.0
P 24 Flatten Standing Biomass
+ 0 0.25 0.2 0.15 0.1 1.0
P 26 Resurface Buried Biomass
+ 0.07 0.08 0.1 0.12 0.07
P 34 Change Standing Biomass Fall Rate
+ 0 1.0 1.0 1.0 1.0 1.0
+ 1.0 1.0 1.0 1.0 1.0
#------------
D 07/06/01
O 04 Harvest, killing crop 20pct standing stubble
+ 14.311503 .15
T ARS record - filename is:  Harvest Wheat - grain (combine cutterbar header).oprn
T This operation record is designed to represent actual field harvesting operation
T of removing the grain from small grain crops with a cutterbar head on a combine.
T This harvesting operation record removes all the reproductive component of a crop above the
T cutting height.  Typically this is specified as the "yield" component in the crop record.
T The non-harvested crop plant material above the specified cut height becomes flat residue.
T The remaining above ground crop material below the specified cut height becomes standing residue.
T Nov 02, 2005	Created - Larry Wagner
T Detailed info regarding this operation record:
T This harvest record specifies the actual cut height dependent upon the height
T of the crop.  The cut height is specified as a fraction of the crop height.
T Added 0.2 for the flatting of the combine and tire trafic for haulling grain.
T MAS 1-18-07
T The harvesting operation could also have an effect on the "standing stalk"
T fall rate and fall threshold values.  The default "biomass pool" flag parameter
T is set to "No adjustments applied" so that no "stalk residue decay rate change" will occur.
T However, this flag value can be changed along with the default parameter values
T to change the "stalk residue decay processes".
+
G 02 Biomass Manipulation
+ 1.0
P 31 Kill or Defoliate Growing Crop
+ 2
P 43 Cut/Remove Biomass by Fraction (flags)
+ 1 1 0 1 0.65 1 0 0
P 34 Change Standing Biomass Fall Rate
+ 0 1.0 1.0 1.0 1.0 1.0
+ 1.0 1.0 1.0 1.0 1.0
P 40 End crop Biomass Manipulation
P 24 Flatten Standing Biomass
+ 0 0.2 0.2 0.2 0.2 1
#------------
D 10/06/01
O 04 Sprayer, kill crop
+ 1.2160101 0.15
T All crop types are killed, green grow turned to residue, standing.  MAS 12-27-11
T
T Added Flattening to the operation to match R2 (P-24).  This will tend to increase erosion on systems that using
T cover crops by causing less standing residue from the crop or cover crop killed.  MAS 4-3-12
T
T After a conference call, Linda Scheffe, Dave Lightle, Mike Sporcic, and Fred Fox, we decided to change the flattening
T from 0.7-0.5 to 0.05 for all residue type due to wheel traffic only.  Plant canopy change over time is not considered.
T Normal plant senescence built into the model will handle plant changes.  MAS 4-5-12
+ 
G 02 Biomass Manipulation
+ 1.0
P 24 Flatten Standing Biomass
+ 0 0.05 0.05 0.05 0.05 0.05
P 31 Kill or Defoliate Growing Crop
+ 2
P 40 End crop Biomass Manipulation
#------------
D 11/06/01
O 04 Fert applic. surface broadcast
+ 1.4966278 0.0609375
T R2 Notes: Broadcast fertilizer spreader.  Wheel traffic only.  rev 082107 DTL
T
T Added to DB 4-12-12 MAS
+
G 01 Tillage
+ 0.0 0 0.05 0.0 0.0 0.0
P 01 Break Crust
P 02 Random Roughness
+ 1 8.8900175
P 11 Aggregate Crushing
+ 4.3 2.0
P 24 Flatten Standing Biomass
+ 0 0.25 0.2 0.15 0.1 1.0
P 26 Resurface Buried Biomass
+ 0.07 0.08 0.1 0.12 0.07
P 34 Change Standing Biomass Fall Rate
+ 0 1.0 1.0 1.0 1.0 1.0
+ 1.0 1.0 1.0 1.0 1.0
#------------
D 20/06/01
O 03 Drill or air seeder single disk openers 7-10 in spac
+ 3.2738733 2.44 2.2351363 0.0 2.2351363 1.5645955 2.9056773
T Drill or Air seeder with single disk no-till openers  JD 750 or similar openers. (No-till air drill)
T Based on Drill, no-till single disk 7-10 spacing. 102403 DTL. RUSLE MAS 10-26-06
T G2 was added into file in front of the flattening (P24), burial (P25), and resurfacing (P26) factors because the area affected is less than 1.0 and
T the RUSLE values were normalized to 1.0.  This change will imulate the correct residue changes based on the method set forth in RUSLE.
T RUSLE's factors have been redused to based on the area affected.
T The stalk fall rate factor (P34) was moved ahead of the new (G2) factor to set the fall rate to the less than 1.0 area affected.  8/7/07 MAS
+
G 01 Tillage
+ 63.500134 0.4 0.15 63.50013 50.800102 101.600204
P 01 Break Crust
P 02 Random Roughness
+ 1 7.6200156
P 05 Ridges and Dikes
+ 1 25.400051 203.20041 0.0 0.0 0.0
P 11 Aggregate Crushing
+ 2.8 0.75
P 12 Soil Loosening
+ 0.4
P 13 Soil Layer Mixing
+ 0.20
P 34 Change Standing Biomass Fall Rate
+ 7 3.0 2.5 2.0 1.5 1.0
+ 0.5 0.6 0.7 0.8 1.0
G 02 Biomass Manipulation
+ 1.0
P 24 Flatten Standing Biomass
+ 0 0.6 0.4 0.35 0.15 1.0
P 25 Bury Flat Biomass
+ 1 0.05 0.04 0.03 0.02 0.03
P 26 Resurface Buried Biomass
+ 0.01 0.01 0.01 0.05 0.01
G 03 Crop Name
+ Soybean, groups V, VI, VII, and VIII
P 51 Seeding Configuration
+ 1 0.0 0
+ 27.0 1.0 1 30 1.0 1.0 0
+ bu/ac
+ 13 148.7 1 0.8 0.65 0.8
+ 1.5 0.05 1.5240185 10.0 25.0 0 120 1800.0
+ -5.0 -15.0 0.01 0.95 0.0 25.0
+ 0.023 0.8063 0.4146 -0.061 -0.024 0.9911 0.6435 0.0494
+ 0.4146 -0.061 2.83 1.0 26.0 0.05 0 0.5
+ 111.111115 111.111115 1.5 0.015 0.0 0.0 0.0 1
+ 0.03 0.03 0.03 0.03 0.2 0.01 20.0 5.227942
+ -1.20379 0.604887 1.8 0.026900401 0.0 0.0 0.0 0.0
T RUSLE Notes: Soybeans in maturity groups V, VI, VII, and VIII.  7 inch row spacing Southern growing conditions  REV1071104 DTL
T This was cloned from the WEPS MG V file. MAS 10-19-06
T Days to mature set to losest maturity group days from planting minus 10 days.
T group V is 130 days - 10 = 120 days MAS 3-21-07
T
T WEPS yields are adjusted to the middle of the yield for the group
T and different than the RUSLE records (RUSLE gives the bottom of the group).
T MAS 7/31/07
#------------
D 10/07/01
O 04 Sprayer, post emergence
+ 1.2160101 .15
T Spray pest control chemicals on growing crop.  Crop is not killed.
T In the MCREW management screen the user must select the kind of weeds killed in the growing crop as external residue.   080404 DTL
T Cloned from Defoliate (spray) crop.oprn, Changed the P31 to No crop kill and added G4 to add material to field MAS 9-28-06
T DO NOT LEAVE CROP COLUMN SET TO "no crop".  User must select the crop and then drill into the operation and specify the amount of weed
T mass that will be killed and turned into residue.
+
G 03 Crop Name
+ weed residue; 0-3 mo
P 65 Add Crop Residue Amounts
+ 0.0 0.0 0.0 0.028021252 1
+ 0.0 0.0 0.0056042504 152.4003
+ 0.025 0.025 0.025 0.025 0.169 0.0050 17.1 5.227942
+ -1.20379 0.604887
T Enter crop notes here.
#------------
D 01/09/01
O 04 Sprayer, fungicide and insecticide tank mix
+ 1.2160101 .15
T Spray pest control chemicals on growing crop.  Crop is not killed.
T In the MCREW management screen the user must select the kind of weeds killed in the growing crop as external residue.   080404 DTL
T Cloned from Defoliate (spray) crop.oprn, Changed the P31 to No crop kill and added G4 to add material to field MAS 9-28-06
+
#------------
D 27/11/01
O 04 Harvest, killing crop 20pct standing stubble
+ 14.311503 .15
T ARS record - filename is:  Harvest Wheat - grain (combine cutterbar header).oprn
T This operation record is designed to represent actual field harvesting operation
T of removing the grain from small grain crops with a cutterbar head on a combine.
T This harvesting operation record removes all the reproductive component of a crop above the
T cutting height.  Typically this is specified as the "yield" component in the crop record.
T The non-harvested crop plant material above the specified cut height becomes flat residue.
T The remaining above ground crop material below the specified cut height becomes standing residue.
T Nov 02, 2005	Created - Larry Wagner
T Detailed info regarding this operation record:
T This harvest record specifies the actual cut height dependent upon the height
T of the crop.  The cut height is specified as a fraction of the crop height.
T Added 0.2 for the flatting of the combine and tire trafic for haulling grain.
T MAS 1-18-07
T The harvesting operation could also have an effect on the "standing stalk"
T fall rate and fall threshold values.  The default "biomass pool" flag parameter
T is set to "No adjustments applied" so that no "stalk residue decay rate change" will occur.
T However, this flag value can be changed along with the default parameter values
T to change the "stalk residue decay processes".
+
G 02 Biomass Manipulation
+ 1.0
P 31 Kill or Defoliate Growing Crop
+ 2
P 43 Cut/Remove Biomass by Fraction (flags)
+ 1 1 0 1 0.65 1 0 0
P 34 Change Standing Biomass Fall Rate
+ 0 1.0 1.0 1.0 1.0 1.0
+ 1.0 1.0 1.0 1.0 1.0
P 40 End crop Biomass Manipulation
P 24 Flatten Standing Biomass
+ 0 0.2 0.2 0.2 0.2 1
#------------
D 01/12/01
O 03 Plow, moldboard
+ 17.491838 65 2.2351363 0.0 2.2351363 1.5645955 2.6821637
T Moldboard plow 8 inch operating depth.  060701 DTL  Modified flattening and burial per McCool and Foster 05/21/02 DTL RUSLE MAS 10-26-06
+
G 01 Tillage
+ 203.20041 1.0 1.0 203.20041 152.4003 254.0005
P 01 Break Crust
P 02 Random Roughness
+ 1 48.260098
P 05 Ridges and Dikes
+ 1 25.400051 406.40082 0.0 0.0 0.0
P 11 Aggregate Crushing
+ 2.8 1.0
P 12 Soil Loosening
+ 1.0
P 13 Soil Layer Mixing
+ 0.7
P 14 Soil Layer Inversion
P 31 Kill or Defoliate Growing Crop
+ 2
P 40 End crop Biomass Manipulation
P 24 Flatten Standing Biomass
+ 0 1 1 1 0.75 1.0
P 25 Bury Flat Biomass
+ 3 0.99 0.99 0.99 0.85 0.97
P 26 Resurface Buried Biomass
+ 0.01 0.02 0.04 0.1 0.02
P 34 Change Standing Biomass Fall Rate
+ 7 3.0 2.5 2.0 1.5 1.0
+ 0.5 0.6 0.7 0.8 1.0
#------------
D 10/03/02
O 03 Disk, tandem heavy primary op
+ 7.0154433 39 2.2351363 0.0 2.2351363 1.3410819 2.6821637
T 11-12in. Spacing, Front and Rear
T Recommended for primary tillage in medium to heavy soils
T Excellent residue-handling capability. MAS 10-26-06
+
G 01 Tillage
+ 152.4003 1.0 1.0 152.4003 101.600204 177.80035
P 01 Break Crust
P 02 Random Roughness
+ 1 38.100075
P 05 Ridges and Dikes
+ 1 101.600204 279.40057 0.0 0.0 0.0
P 11 Aggregate Crushing
+ 2.8 0.75
P 12 Soil Loosening
+ 0.9
P 13 Soil Layer Mixing
+ 0.4
P 31 Kill or Defoliate Growing Crop
+ 2
P 40 End crop Biomass Manipulation
P 24 Flatten Standing Biomass
+ 0 1.0 0.9 0.8 0.5 1.0
P 25 Bury Flat Biomass
+ 1 0.95 0.85 0.8 0.6 0.95
P 26 Resurface Buried Biomass
+ 0.05 0.06 0.07 0.08 0.05
P 34 Change Standing Biomass Fall Rate
+ 7 3.0 2.5 2.0 1.5 1.0
+ 0.5 0.6 0.7 0.8 1.0
#------------
D 01/04/02
O 03 Disk, tandem secondary op
+ 4.4898834 32.5 2.2351363 0.0 2.2351363 1.3410819 2.6821637
T 9-in. Spacing, Front and Rear; Good for seedbed preparation/chemical incorporation in medium to heavy soils
T Works well in primary tillage in light to medium soils
T Provides good residue-handling capability.  MAS 10-26-06
+
G 01 Tillage
+ 127.00027 0.75 1.0 127.00026 76.20015 152.4003
P 01 Break Crust
P 02 Random Roughness
+ 1 15.240031
P 05 Ridges and Dikes
+ 1 50.800102 228.60046 0.0 0.0 0.0
P 11 Aggregate Crushing
+ 2.8 0.75
P 12 Soil Loosening
+ 0.85
P 13 Soil Layer Mixing
+ 0.4
P 31 Kill or Defoliate Growing Crop
+ 2
P 40 End crop Biomass Manipulation
P 24 Flatten Standing Biomass
+ 0 0.85 0.7 0.6 0.5 1.0
P 25 Bury Flat Biomass
+ 1 0.73 0.63 0.55 0.4 0.73
P 26 Resurface Buried Biomass
+ 0.02 0.04 0.02 0.05 0.02
P 34 Change Standing Biomass Fall Rate
+ 7 3.0 2.5 2.0 1.5 1.0
+ 0.5 0.6 0.7 0.8 1.0
#------------
D 10/04/02
O 03 Bedder, hipper, disk hiller
+ 4.2092657 26 2.0116227 0.0 2.0116227 1.5645955 2.2351363
T This is an 8 in high tool to reform beds from RUSLE 6-7-01 DTL
T
T Corrected the tillage depths and other residue values 11-1-11
+
G 01 Tillage
+ 101.600204 0.9 1.0 101.600204 50.800102 127.00025
P 01 Break Crust
P 02 Random Roughness
+ 1 15.240031
P 11 Aggregate Crushing
+ 3.0 2.0
P 12 Soil Loosening
+ 0.75
P 13 Soil Layer Mixing
+ 0.75
P 05 Ridges and Dikes
+ 1 203.20041 760.0 381.00076 0.0 0.0
P 31 Kill or Defoliate Growing Crop
+ 2
P 40 End crop Biomass Manipulation
P 24 Flatten Standing Biomass
+ 0 1 0.90 0.9 0.5 1.00
P 25 Bury Flat Biomass
+ 1 0.95 0.92 0.85 0.5 0.6
P 26 Resurface Buried Biomass
+ 0.02 0.02 0.02 0.05 0.03
P 34 Change Standing Biomass Fall Rate
+ 7 3.0 2.5 2.0 1.5 1.0
+ 0.5 0.6 0.7 0.8 1.0
#------------
D 20/04/02
O 03 Bed shaper
+ 3.554491 19.5 2.2351363 0.0 2.2351363 1.5645955 2.9056773
T RUSLE Notes: Bed shaping operation on existing beds.  May include drip tape installation. 10/28/01 DTL
T Cloned 2-15-07 MAS
T G2 was added into file in front of the flattening (P24), burial (P25), and resurfacing (P26) factors because the area affected is less than 1.0 and
T the RUSLE values were normalized to 1.0.  This change will imulate the correct residue changes based on the method set forth in RUSLE.
T RUSLE's factors have been redused to based on the area affected.
T The stalk fall rate factor (P34) was moved ahead of the new (G2) factor to set the fall rate to the  less than 1.0 area affected.  8/8/07 MAS
+
G 01 Tillage
+ 101.600204 .6 .75 101.600204 76.20015 152.4003
P 01 Break Crust
P 02 Random Roughness
+ 1 15.240031
P 11 Aggregate Crushing
+ 3.0 -0.22
P 12 Soil Loosening
+ 0.75
P 13 Soil Layer Mixing
+ 0.05
P 05 Ridges and Dikes
+ 1 203.20041 760.0 381.00076 0.0 0.0
P 34 Change Standing Biomass Fall Rate
+ 7 3.0 2.5 2.0 1.5 1.0
+ 0.5 0.6 0.7 0.8 1.0
G 02 Biomass Manipulation
+ 1.0
P 24 Flatten Standing Biomass
+ 0 0.5 0.45 0.4 0.3 1.00
P 25 Bury Flat Biomass
+ 1 0.38 0.3 0.23 0.2 0.28
P 26 Resurface Buried Biomass
+ 0.02 0.02 0.02 0.02 0.02
#------------
D 01/05/02
O 03 Planter, transplanter, vegetable on 8 inch high beds
+ 7.4831395 3.12 0.89405453 0.0 0.89405453 0.44702727 1.3410819
T Vegetable transplanter on 8 inch beds or ridges.11/15/02  DTL
T G2 was added into file in front of the flattening (P24), burial (P25), and resurfacing (P26) factors because the area affected is less than 1.0 and
T the RUSLE values were normalized to 1.0.  This change will imulate the correct residue changes based on the method set forth in RUSLE.
T RUSLE's factors have been redused to based on the area affected.
T The stalk fall rate factor (P34) was moved ahead of the new (G2) factor to set the fall rate to the less than 1.0 area affected.  8/7/07 MAS
+
G 01 Tillage
+ 101.600204 0.5 .2 101.600204 76.20015 127.00026
P 01 Break Crust
P 02 Random Roughness
+ 1 10.160021
P 05 Ridges and Dikes
+ 1 203.20041 762.0015 355.6007 0.0 0.0
P 11 Aggregate Crushing
+ 2.4 2
P 12 Soil Loosening
+ 0.6
P 13 Soil Layer Mixing
+ 0.3
P 34 Change Standing Biomass Fall Rate
+ 7 3.0 2.5 2.0 1.5 1.0
+ 0.5 0.6 0.7 0.8 1.0
G 02 Biomass Manipulation
+ 1.0
P 24 Flatten Standing Biomass
+ 0 .3 .25 .2 0.1 1.0
P 25 Bury Flat Biomass
+ 1 .07 .05 .04 .02 .04
P 26 Resurface Buried Biomass
+ .01 .01 .01 .02 0.01
G 03 Crop Name
+ Tobacco, flue cured
P 51 Seeding Configuration
+ 1 0.0 2
+ 2.0 1.0 1 25 1.0 1.0 3
+ ton/ac
+ 11.0 8930.0 4 0.8 0.65 0.95
+ 2.5 0.025 2.0 8.0 25.0 0 100 1400.0
+ -5.0 -15.0 0.15 0.95 0.0 30.0
+ 0.0 0.8008 0.8341 -0.0737 0.0 1.0 1.1 0.01
+ 0.3726 -0.0744 2.0 1.0 10.0 0.03 1 1.1170388
+ 500.0 500.0 2.0 0.03 0.1 0.1 0.0 3
+ 0.02 0.02 0.02 0.02 0.2 0.0050 20.0 2.9797485
+ -1.20379 0.604887 .8308 0.025006166 0.0 0.0 0.0 0.0
T Enter crop notes here.
#------------
D 10/05/02
O 03 Cultivator, row 3 in ridge
+ 5.799433 17.55 2.2351363 0.0 2.2351363 0.89405453 2.4586499
T Row crop cultivator w/ sweeps leaving a 3" ridge 05-14-02 DTL
T G2 was added into file in front of the flattening (P24), burial (P25), and resurfacing (P26) factors because the area affected is less than 1.0 and
T the RUSLE values were normalized to 1.0.  This change will imulate the correct residue changes based on the method set forth in RUSLE.
T RUSLE's factors have been redused to based on the area affected.
T The stalk fall rate factor (P34) was moved ahead of the new (G2) factor to set the fall rate to the  less than 1.0 area affected.  8/7/07 MAS
+
G 01 Tillage
+ 76.20015 0.5 .9 76.20015 50.800102 101.600204
P 01 Break Crust
P 02 Random Roughness
+ 1 15.240031
P 05 Ridges and Dikes
+ 1 76.20015 762.0015 0.0 0.0 0.0
P 11 Aggregate Crushing
+ 3.0 1.0
P 12 Soil Loosening
+ 0.75
P 13 Soil Layer Mixing
+ 0.35
P 34 Change Standing Biomass Fall Rate
+ 4 3.0 2.5 2.0 1.5 1.0
+ 0.5 0.6 0.7 0.8 1.0
G 02 Biomass Manipulation
+ 1.0
P 24 Flatten Standing Biomass
+ 14 0.7 0.3 0.3 0.1 1.0
P 25 Bury Flat Biomass
+ 1 0.68 0.6 0.52 0.39 0.77
P 26 Resurface Buried Biomass
+ 0.04 0.04 0.04 0.06 0.04
#------------
D 20/05/02
O 03 Cultivator, row 3 in ridge
+ 5.799433 17.55 2.2351363 0.0 2.2351363 0.89405453 2.4586499
T Row crop cultivator w/ sweeps leaving a 3" ridge 05-14-02 DTL
T G2 was added into file in front of the flattening (P24), burial (P25), and resurfacing (P26) factors because the area affected is less than 1.0 and
T the RUSLE values were normalized to 1.0.  This change will imulate the correct residue changes based on the method set forth in RUSLE.
T RUSLE's factors have been redused to based on the area affected.
T The stalk fall rate factor (P34) was moved ahead of the new (G2) factor to set the fall rate to the  less than 1.0 area affected.  8/7/07 MAS
+
G 01 Tillage
+ 76.20015 0.5 .9 76.20015 50.800102 101.600204
P 01 Break Crust
P 02 Random Roughness
+ 1 15.240031
P 05 Ridges and Dikes
+ 1 76.20015 762.0015 0.0 0.0 0.0
P 11 Aggregate Crushing
+ 3.0 1.0
P 12 Soil Loosening
+ 0.75
P 13 Soil Layer Mixing
+ 0.35
P 34 Change Standing Biomass Fall Rate
+ 4 3.0 2.5 2.0 1.5 1.0
+ 0.5 0.6 0.7 0.8 1.0
G 02 Biomass Manipulation
+ 1.0
P 24 Flatten Standing Biomass
+ 14 0.7 0.3 0.3 0.1 1.0
P 25 Bury Flat Biomass
+ 1 0.68 0.6 0.52 0.39 0.77
P 26 Resurface Buried Biomass
+ 0.04 0.04 0.04 0.06 0.04
#------------
D 25/05/02
O 04 Sprayer, insecticide post emergence
+ 1.2160101 0.15
T Spray pest control chemicals on growing crop.   Crop is not killed.  11/17/01 DTL
T
T Added to the DB.  This assumes no crop flattening.  4-5-12 MAS
+
#------------
D 01/06/02
O 03 Cultivator, row 3 in ridge
+ 5.799433 17.55 2.2351363 0.0 2.2351363 0.89405453 2.4586499
T Row crop cultivator w/ sweeps leaving a 3" ridge 05-14-02 DTL
T G2 was added into file in front of the flattening (P24), burial (P25), and resurfacing (P26) factors because the area affected is less than 1.0 and
T the RUSLE values were normalized to 1.0.  This change will imulate the correct residue changes based on the method set forth in RUSLE.
T RUSLE's factors have been redused to based on the area affected.
T The stalk fall rate factor (P34) was moved ahead of the new (G2) factor to set the fall rate to the  less than 1.0 area affected.  8/7/07 MAS
+
G 01 Tillage
+ 76.20015 0.5 .9 76.20015 50.800102 101.600204
P 01 Break Crust
P 02 Random Roughness
+ 1 15.240031
P 05 Ridges and Dikes
+ 1 76.20015 762.0015 0.0 0.0 0.0
P 11 Aggregate Crushing
+ 3.0 1.0
P 12 Soil Loosening
+ 0.75
P 13 Soil Layer Mixing
+ 0.35
P 34 Change Standing Biomass Fall Rate
+ 4 3.0 2.5 2.0 1.5 1.0
+ 0.5 0.6 0.7 0.8 1.0
G 02 Biomass Manipulation
+ 1.0
P 24 Flatten Standing Biomass
+ 14 0.7 0.3 0.3 0.1 1.0
P 25 Bury Flat Biomass
+ 1 0.68 0.6 0.52 0.39 0.77
P 26 Resurface Buried Biomass
+ 0.04 0.04 0.04 0.06 0.04
#------------
D 05/06/02
O 04 Sprayer, insecticide post emergence
+ 1.2160101 0.15
T Spray pest control chemicals on growing crop.   Crop is not killed.  11/17/01 DTL
T
T Added to the DB.  This assumes no crop flattening.  4-5-12 MAS
+
#------------
D 10/06/02
O 03 Cultivator, row between beds
+ 5.799433 10.56 2.2351363 0.0 2.2351363 0.89405453 2.4586499
T Cultivator w/ opposing gangs of disk hillers.  Used to cultivate between Sugarcane beds. 020106 DTL
T G2 was added into file in front of the flattening (P24), burial (P25), and resurfacing (P26) factors because the area affected is less than 1.0 and
T the RUSLE values were normalized to 1.0.  This change will imulate the correct residue changes based on the method set forth in RUSLE.
T RUSLE's factors have been redused to based on the area affected.
T The stalk fall rate factor (P34) was moved ahead of the new (G2) factor to set the fall rate to the  less than 1.0 area affected.  8/7/07 MAS
T Cloned from row cultivator.  11-22-07 MAS
T
T Changed the P5 Ridge and Dikes to reflect the height of the previous tillage.  The operation now will show the ridge height of the planter or
T the previous tillage.  MAS 6-3-11
+
G 01 Tillage
+ 63.500126 0.5 .65 63.500126 50.800102 101.600204
P 01 Break Crust
P 02 Random Roughness
+ 1 15.240031
P 05 Ridges and Dikes
+ 0 76.20015 762.0015 355.6007 0.0 0.0
P 11 Aggregate Crushing
+ 3.0 1.0
P 12 Soil Loosening
+ 0.75
P 13 Soil Layer Mixing
+ 0.35
P 34 Change Standing Biomass Fall Rate
+ 4 3.0 2.5 2.0 1.5 1.0
+ 0.5 0.6 0.7 0.8 1.0
G 02 Biomass Manipulation
+ 1.0
P 24 Flatten Standing Biomass
+ 14 0.7 0.3 0.3 0.1 1.0
P 25 Bury Flat Biomass
+ 1 0.49 0.44 0.38 0.28 0.55
P 26 Resurface Buried Biomass
+ 0.7 0.3 0.3 0.1 1
#------------
D 20/06/02
O 04 Sprayer, fungicide and insecticide tank mix
+ 1.2160101 .15
T Spray pest control chemicals on growing crop.  Crop is not killed.
T In the MCREW management screen the user must select the kind of weeds killed in the growing crop as external residue.   080404 DTL
T Cloned from Defoliate (spray) crop.oprn, Changed the P31 to No crop kill and added G4 to add material to field MAS 9-28-06
+
#------------
D 01/07/02
O 04 Sprayer, growth regulator
+ 1.2160101 0.15
T R2 Notes: Spray growth regulators on growing crop.   Crop is not killed.  11/17/01 DTL.
T Revised Sprayer, insecticide for application of plant growth regulators for cotton
T (for example, Pix and Mepichlor). rev 082211 LOS.
T
T Added to the DB.  This assumes no crop flattening.  4-12-12 MAS
+
#------------
D 10/07/02
O 04 Sprayer, growth regulator
+ 1.2160101 0.15
T R2 Notes: Spray growth regulators on growing crop.   Crop is not killed.  11/17/01 DTL.
T Revised Sprayer, insecticide for application of plant growth regulators for cotton
T (for example, Pix and Mepichlor). rev 082211 LOS.
T
T Added to the DB.  This assumes no crop flattening.  4-12-12 MAS
+
#------------
D 20/07/02
O 04 Sprayer, growth regulator
+ 1.2160101 0.15
T R2 Notes: Spray growth regulators on growing crop.   Crop is not killed.  11/17/01 DTL.
T Revised Sprayer, insecticide for application of plant growth regulators for cotton
T (for example, Pix and Mepichlor). rev 082211 LOS.
T
T Added to the DB.  This assumes no crop flattening.  4-12-12 MAS
+
#------------
D 01/08/02
O 04 Harvest, hand pick
+ 3.2738733 0.15
T Hand pick lettuce or similar crops or to represent one final picking of fruit or berry crops.
T Do not use for multiple pickings of fruit or berry crops unless a regrowth vegetation file representing
T regrowth between pickings is available in the database to be called in.
T This is not the case for strawberries.  12132011 DTL
T Added 3/29/07 MAS
T Reworked the values MAS 2-24-09
T Added the change to flat on the crop type.  8-27-10
T This operation takes all of the yield, and can be used to calibrate the yield. 12-27-11 MAS
T Adjusted the Energy use to 0.000000010 gal/ac  2-23-12
T
T Changed the fuel use from 0.000000010 to 0.36 g/ac 4-17-12 MAS
+
G 02 Biomass Manipulation
+ 1.0
P 31 Kill or Defoliate Growing Crop
+ 0
P 62 Remove (by age pool) Plant/Residue Material
+ 1 1 0 1 3 3 2 1.0 0.0 0.0 0.0 0.0
P 40 End crop Biomass Manipulation
#------------
D 25/08/02
O 04 Harvest, hand pick
+ 3.2738733 0.15
T Hand pick lettuce or similar crops or to represent one final picking of fruit or berry crops.
T Do not use for multiple pickings of fruit or berry crops unless a regrowth vegetation file representing
T regrowth between pickings is available in the database to be called in.
T This is not the case for strawberries.  12132011 DTL
T Added 3/29/07 MAS
T Reworked the values MAS 2-24-09
T Added the change to flat on the crop type.  8-27-10
T This operation takes all of the yield, and can be used to calibrate the yield. 12-27-11 MAS
T Adjusted the Energy use to 0.000000010 gal/ac  2-23-12
T
T Changed the fuel use from 0.000000010 to 0.36 g/ac 4-17-12 MAS
+
G 02 Biomass Manipulation
+ 1.0
P 31 Kill or Defoliate Growing Crop
+ 0
P 62 Remove (by age pool) Plant/Residue Material
+ 1 1 0 1 3 3 2 1.0 0.0 0.0 0.0 0.0
P 40 End crop Biomass Manipulation
#------------
D 12/09/02
O 04 Harvest, tobacco, flue cured
+ 3.2738733 0.15
T Harvest of flue cured tobacco where lower mature leaves are systematically picked and removed leaving only the central stalk.
T Use this operation on the date that represents the end of the harvest period.  11/27/01 DTL
T LEAVES ARE PICKED BY HAND.  100% of the remaining leaves are havested.
T Removed 100% of the flower fraction because some of the plant mass may have gone to fruiting or grain.
T Cannot be calibrated because this is a partial harvest.  Change the bio adjustment factor manually.
T Crop not killed.  12-19-11 MAS
+
G 02 Biomass Manipulation
+ 0.8
P 31 Kill or Defoliate Growing Crop
+ 0
P 62 Remove (by age pool) Plant/Residue Material
+ 1 0 0 0 1 3 2 0 0.95 0.0 0.0 0.0
P 34 Change Standing Biomass Fall Rate
+ 0 1.0 1.0 1.0 1.0 1.0
+ 1.0 1.0 1.0 1.0 1.0
P 40 End crop Biomass Manipulation
#------------
D 15/09/02
O 04 Sprayer, kill crop
+ 1.2160101 0.15
T All crop types are killed, green grow turned to residue, standing.  MAS 12-27-11
T
T Added Flattening to the operation to match R2 (P-24).  This will tend to increase erosion on systems that using
T cover crops by causing less standing residue from the crop or cover crop killed.  MAS 4-3-12
T
T After a conference call, Linda Scheffe, Dave Lightle, Mike Sporcic, and Fred Fox, we decided to change the flattening
T from 0.7-0.5 to 0.05 for all residue type due to wheel traffic only.  Plant canopy change over time is not considered.
T Normal plant senescence built into the model will handle plant changes.  MAS 4-5-12
+ 
G 02 Biomass Manipulation
+ 1.0
P 24 Flatten Standing Biomass
+ 0 0.05 0.05 0.05 0.05 0.05
P 31 Kill or Defoliate Growing Crop
+ 2
P 40 End crop Biomass Manipulation
#------------
D 17/09/02
O 03 Disk, tandem light finishing
+ 3.7415698 19.5 2.2351363 0.0 2.2351363 1.3410819 2.6821637
T 6/8/01 DTL RUSLE.  7in sp.  This is tool used to finish a seedbed.  MAS 10-26-06
+
G 01 Tillage
+ 101.600204 0.5 1.0 101.600204 76.20015 127.00026
P 01 Break Crust
P 02 Random Roughness
+ 1 15.240031
P 05 Ridges and Dikes
+ 1 12.700026 177.80035 0.0 0.0 0.0
P 11 Aggregate Crushing
+ 2.8 0.75
P 12 Soil Loosening
+ 0.75
P 13 Soil Layer Mixing
+ 0.35
P 31 Kill or Defoliate Growing Crop
+ 2
P 40 End crop Biomass Manipulation
P 24 Flatten Standing Biomass
+ 0 0.85 0.7 0.6 0.5 1.0
P 25 Bury Flat Biomass
+ 1 0.73 0.63 0.55 0.4 0.73
P 26 Resurface Buried Biomass
+ 0.02 0.04 0.02 0.05 0.02
P 34 Change Standing Biomass Fall Rate
+ 7 3.0 2.5 2.0 1.5 1.0
+ 0.5 0.6 0.7 0.8 1.0
#------------
D 25/09/02
O 03 Drill or air seeder single disk openers 7-10 in spac
+ 3.2738733 2.44 2.2351363 0.0 2.2351363 1.5645955 2.9056773
T Drill or Air seeder with single disk no-till openers  JD 750 or similar openers. (No-till air drill)
T Based on Drill, no-till single disk 7-10 spacing. 102403 DTL. RUSLE MAS 10-26-06
T G2 was added into file in front of the flattening (P24), burial (P25), and resurfacing (P26) factors because the area affected is less than 1.0 and
T the RUSLE values were normalized to 1.0.  This change will imulate the correct residue changes based on the method set forth in RUSLE.
T RUSLE's factors have been redused to based on the area affected.
T The stalk fall rate factor (P34) was moved ahead of the new (G2) factor to set the fall rate to the less than 1.0 area affected.  8/7/07 MAS
+
G 01 Tillage
+ 63.500134 0.4 0.15 63.50013 50.800102 101.600204
P 01 Break Crust
P 02 Random Roughness
+ 1 7.6200156
P 05 Ridges and Dikes
+ 1 25.400051 203.20041 0.0 0.0 0.0
P 11 Aggregate Crushing
+ 2.8 0.75
P 12 Soil Loosening
+ 0.4
P 13 Soil Layer Mixing
+ 0.20
P 34 Change Standing Biomass Fall Rate
+ 7 3.0 2.5 2.0 1.5 1.0
+ 0.5 0.6 0.7 0.8 1.0
G 02 Biomass Manipulation
+ 1.0
P 24 Flatten Standing Biomass
+ 0 0.6 0.4 0.35 0.15 1.0
P 25 Bury Flat Biomass
+ 1 0.05 0.04 0.03 0.02 0.03
P 26 Resurface Buried Biomass
+ 0.01 0.01 0.01 0.05 0.01
G 03 Crop Name
+ Rye, winter cover
P 51 Seeding Configuration
+ 1 0.0 0
+ 220.0 8.0 0 2240 1.0 1.0 2
+ lbs/ac
+ 0 8930 5 1.0 0.6 0.8
+ 1.2 0.025 1.2192148 0.0 25.0 1 60 1472.2223
+ -5.0 -15.0 0.005 0.05 0.035 30.0
+ 0.013 0.8013 0.4293 -0.086 -0.018 0.932 0.556 0.0736
+ 0.3293 -0.086 2.87 1.0 20.0 0.05 0 0.3
+ 28.571428 335.0 1.4 0.012 0.1 0.1 0.0 2
+ 0.0133 0.0133 0.0133 0.0133 0.12 0.0050 17.1 5.227942
+ -2.08165 0.548606 0 0.0 0.0 0.0 0.0 0.0
T RUSLE Notes: Rye, as winter cover. Killed in vegetative stage the following spring.
T Decomposition  0.017 like grass forages. Rev 021705 DTL
T
T Cloned 2-16-07 MAS
T Lowered the heat units from 3600 to 2650 to match the core crop runs for OK  MAS 10-29-08
#------------
D 10/03/03
O 03 Plow, moldboard
+ 17.491838 65 2.2351363 0.0 2.2351363 1.5645955 2.6821637
T Moldboard plow 8 inch operating depth.  060701 DTL  Modified flattening and burial per McCool and Foster 05/21/02 DTL RUSLE MAS 10-26-06
+
G 01 Tillage
+ 203.20041 1.0 1.0 203.20041 152.4003 254.0005
P 01 Break Crust
P 02 Random Roughness
+ 1 48.260098
P 05 Ridges and Dikes
+ 1 25.400051 406.40082 0.0 0.0 0.0
P 11 Aggregate Crushing
+ 2.8 1.0
P 12 Soil Loosening
+ 1.0
P 13 Soil Layer Mixing
+ 0.7
P 14 Soil Layer Inversion
P 31 Kill or Defoliate Growing Crop
+ 2
P 40 End crop Biomass Manipulation
P 24 Flatten Standing Biomass
+ 0 1 1 1 0.75 1.0
P 25 Bury Flat Biomass
+ 3 0.99 0.99 0.99 0.85 0.97
P 26 Resurface Buried Biomass
+ 0.01 0.02 0.04 0.1 0.02
P 34 Change Standing Biomass Fall Rate
+ 7 3.0 2.5 2.0 1.5 1.0
+ 0.5 0.6 0.7 0.8 1.0
#------------
D 20/03/03
O 03 Disk, tandem secondary op
+ 4.4898834 32.5 2.2351363 0.0 2.2351363 1.3410819 2.6821637
T 9-in. Spacing, Front and Rear; Good for seedbed preparation/chemical incorporation in medium to heavy soils
T Works well in primary tillage in light to medium soils
T Provides good residue-handling capability.  MAS 10-26-06
+
G 01 Tillage
+ 127.00027 0.75 1.0 127.00026 76.20015 152.4003
P 01 Break Crust
P 02 Random Roughness
+ 1 15.240031
P 05 Ridges and Dikes
+ 1 50.800102 228.60046 0.0 0.0 0.0
P 11 Aggregate Crushing
+ 2.8 0.75
P 12 Soil Loosening
+ 0.85
P 13 Soil Layer Mixing
+ 0.4
P 31 Kill or Defoliate Growing Crop
+ 2
P 40 End crop Biomass Manipulation
P 24 Flatten Standing Biomass
+ 0 0.85 0.7 0.6 0.5 1.0
P 25 Bury Flat Biomass
+ 1 0.73 0.63 0.55 0.4 0.73
P 26 Resurface Buried Biomass
+ 0.02 0.04 0.02 0.05 0.02
P 34 Change Standing Biomass Fall Rate
+ 7 3.0 2.5 2.0 1.5 1.0
+ 0.5 0.6 0.7 0.8 1.0
#------------
D 01/04/03
O 03 Disk, tandem light finishing
+ 3.7415698 19.5 2.2351363 0.0 2.2351363 1.3410819 2.6821637
T 6/8/01 DTL RUSLE.  7in sp.  This is tool used to finish a seedbed.  MAS 10-26-06
+
G 01 Tillage
+ 101.600204 0.5 1.0 101.600204 76.20015 127.00026
P 01 Break Crust
P 02 Random Roughness
+ 1 15.240031
P 05 Ridges and Dikes
+ 1 12.700026 177.80035 0.0 0.0 0.0
P 11 Aggregate Crushing
+ 2.8 0.75
P 12 Soil Loosening
+ 0.75
P 13 Soil Layer Mixing
+ 0.35
P 31 Kill or Defoliate Growing Crop
+ 2
P 40 End crop Biomass Manipulation
P 24 Flatten Standing Biomass
+ 0 0.85 0.7 0.6 0.5 1.0
P 25 Bury Flat Biomass
+ 1 0.73 0.63 0.55 0.4 0.73
P 26 Resurface Buried Biomass
+ 0.02 0.04 0.02 0.05 0.02
P 34 Change Standing Biomass Fall Rate
+ 7 3.0 2.5 2.0 1.5 1.0
+ 0.5 0.6 0.7 0.8 1.0
#------------
D 10/04/03
O 03 Bedder, hipper, disk hiller
+ 4.2092657 26 2.0116227 0.0 2.0116227 1.5645955 2.2351363
T This is an 8 in high tool to reform beds from RUSLE 6-7-01 DTL
T
T Corrected the tillage depths and other residue values 11-1-11
+
G 01 Tillage
+ 101.600204 0.9 1.0 101.600204 50.800102 127.00025
P 01 Break Crust
P 02 Random Roughness
+ 1 15.240031
P 11 Aggregate Crushing
+ 3.0 2.0
P 12 Soil Loosening
+ 0.75
P 13 Soil Layer Mixing
+ 0.75
P 05 Ridges and Dikes
+ 1 203.20041 760.0 381.00076 0.0 0.0
P 31 Kill or Defoliate Growing Crop
+ 2
P 40 End crop Biomass Manipulation
P 24 Flatten Standing Biomass
+ 0 1 0.90 0.9 0.5 1.00
P 25 Bury Flat Biomass
+ 1 0.95 0.92 0.85 0.5 0.6
P 26 Resurface Buried Biomass
+ 0.02 0.02 0.02 0.05 0.03
P 34 Change Standing Biomass Fall Rate
+ 7 3.0 2.5 2.0 1.5 1.0
+ 0.5 0.6 0.7 0.8 1.0
#------------
D 20/04/03
O 03 Bed shaper
+ 3.554491 19.5 2.2351363 0.0 2.2351363 1.5645955 2.9056773
T RUSLE Notes: Bed shaping operation on existing beds.  May include drip tape installation. 10/28/01 DTL
T Cloned 2-15-07 MAS
T G2 was added into file in front of the flattening (P24), burial (P25), and resurfacing (P26) factors because the area affected is less than 1.0 and
T the RUSLE values were normalized to 1.0.  This change will imulate the correct residue changes based on the method set forth in RUSLE.
T RUSLE's factors have been redused to based on the area affected.
T The stalk fall rate factor (P34) was moved ahead of the new (G2) factor to set the fall rate to the  less than 1.0 area affected.  8/8/07 MAS
+
G 01 Tillage
+ 101.600204 .6 .75 101.600204 76.20015 152.4003
P 01 Break Crust
P 02 Random Roughness
+ 1 15.240031
P 11 Aggregate Crushing
+ 3.0 -0.22
P 12 Soil Loosening
+ 0.75
P 13 Soil Layer Mixing
+ 0.05
P 05 Ridges and Dikes
+ 1 203.20041 760.0 381.00076 0.0 0.0
P 34 Change Standing Biomass Fall Rate
+ 7 3.0 2.5 2.0 1.5 1.0
+ 0.5 0.6 0.7 0.8 1.0
G 02 Biomass Manipulation
+ 1.0
P 24 Flatten Standing Biomass
+ 0 0.5 0.45 0.4 0.3 1.00
P 25 Bury Flat Biomass
+ 1 0.38 0.3 0.23 0.2 0.28
P 26 Resurface Buried Biomass
+ 0.02 0.02 0.02 0.02 0.02
#------------
D 01/05/03
O 03 Planter, transplanter, vegetable on 8 inch high beds
+ 7.4831395 3.12 0.89405453 0.0 0.89405453 0.44702727 1.3410819
T Vegetable transplanter on 8 inch beds or ridges.11/15/02  DTL
T G2 was added into file in front of the flattening (P24), burial (P25), and resurfacing (P26) factors because the area affected is less than 1.0 and
T the RUSLE values were normalized to 1.0.  This change will imulate the correct residue changes based on the method set forth in RUSLE.
T RUSLE's factors have been redused to based on the area affected.
T The stalk fall rate factor (P34) was moved ahead of the new (G2) factor to set the fall rate to the less than 1.0 area affected.  8/7/07 MAS
+
G 01 Tillage
+ 101.600204 0.5 .2 101.600204 76.20015 127.00026
P 01 Break Crust
P 02 Random Roughness
+ 1 10.160021
P 05 Ridges and Dikes
+ 1 203.20041 762.0015 355.6007 0.0 0.0
P 11 Aggregate Crushing
+ 2.4 2
P 12 Soil Loosening
+ 0.6
P 13 Soil Layer Mixing
+ 0.3
P 34 Change Standing Biomass Fall Rate
+ 7 3.0 2.5 2.0 1.5 1.0
+ 0.5 0.6 0.7 0.8 1.0
G 02 Biomass Manipulation
+ 1.0
P 24 Flatten Standing Biomass
+ 0 .3 .25 .2 0.1 1.0
P 25 Bury Flat Biomass
+ 1 .07 .05 .04 .02 .04
P 26 Resurface Buried Biomass
+ .01 .01 .01 .02 0.01
G 03 Crop Name
+ Tobacco, flue cured
P 51 Seeding Configuration
+ 1 0.0 2
+ 2.0 1.0 1 25 1.0 1.0 3
+ ton/ac
+ 11.0 8930.0 4 0.8 0.65 0.95
+ 2.5 0.025 2.0 8.0 25.0 0 100 1400.0
+ -5.0 -15.0 0.15 0.95 0.0 30.0
+ 0.0 0.8008 0.8341 -0.0737 0.0 1.0 1.1 0.01
+ 0.3726 -0.0744 2.0 1.0 10.0 0.03 1 1.1170388
+ 500.0 500.0 2.0 0.03 0.1 0.1 0.0 3
+ 0.02 0.02 0.02 0.02 0.2 0.0050 20.0 2.9797485
+ -1.20379 0.604887 .8308 0.025006166 0.0 0.0 0.0 0.0
T Enter crop notes here.
#------------
D 10/05/03
O 03 Cultivator, row 3 in ridge
+ 5.799433 17.55 2.2351363 0.0 2.2351363 0.89405453 2.4586499
T Row crop cultivator w/ sweeps leaving a 3" ridge 05-14-02 DTL
T G2 was added into file in front of the flattening (P24), burial (P25), and resurfacing (P26) factors because the area affected is less than 1.0 and
T the RUSLE values were normalized to 1.0.  This change will imulate the correct residue changes based on the method set forth in RUSLE.
T RUSLE's factors have been redused to based on the area affected.
T The stalk fall rate factor (P34) was moved ahead of the new (G2) factor to set the fall rate to the  less than 1.0 area affected.  8/7/07 MAS
+
G 01 Tillage
+ 76.20015 0.5 .9 76.20015 50.800102 101.600204
P 01 Break Crust
P 02 Random Roughness
+ 1 15.240031
P 05 Ridges and Dikes
+ 1 76.20015 762.0015 0.0 0.0 0.0
P 11 Aggregate Crushing
+ 3.0 1.0
P 12 Soil Loosening
+ 0.75
P 13 Soil Layer Mixing
+ 0.35
P 34 Change Standing Biomass Fall Rate
+ 4 3.0 2.5 2.0 1.5 1.0
+ 0.5 0.6 0.7 0.8 1.0
G 02 Biomass Manipulation
+ 1.0
P 24 Flatten Standing Biomass
+ 14 0.7 0.3 0.3 0.1 1.0
P 25 Bury Flat Biomass
+ 1 0.68 0.6 0.52 0.39 0.77
P 26 Resurface Buried Biomass
+ 0.04 0.04 0.04 0.06 0.04
#------------
D 20/05/03
O 03 Cultivator, row 3 in ridge
+ 5.799433 17.55 2.2351363 0.0 2.2351363 0.89405453 2.4586499
T Row crop cultivator w/ sweeps leaving a 3" ridge 05-14-02 DTL
T G2 was added into file in front of the flattening (P24), burial (P25), and resurfacing (P26) factors because the area affected is less than 1.0 and
T the RUSLE values were normalized to 1.0.  This change will imulate the correct residue changes based on the method set forth in RUSLE.
T RUSLE's factors have been redused to based on the area affected.
T The stalk fall rate factor (P34) was moved ahead of the new (G2) factor to set the fall rate to the  less than 1.0 area affected.  8/7/07 MAS
+
G 01 Tillage
+ 76.20015 0.5 .9 76.20015 50.800102 101.600204
P 01 Break Crust
P 02 Random Roughness
+ 1 15.240031
P 05 Ridges and Dikes
+ 1 76.20015 762.0015 0.0 0.0 0.0
P 11 Aggregate Crushing
+ 3.0 1.0
P 12 Soil Loosening
+ 0.75
P 13 Soil Layer Mixing
+ 0.35
P 34 Change Standing Biomass Fall Rate
+ 4 3.0 2.5 2.0 1.5 1.0
+ 0.5 0.6 0.7 0.8 1.0
G 02 Biomass Manipulation
+ 1.0
P 24 Flatten Standing Biomass
+ 14 0.7 0.3 0.3 0.1 1.0
P 25 Bury Flat Biomass
+ 1 0.68 0.6 0.52 0.39 0.77
P 26 Resurface Buried Biomass
+ 0.04 0.04 0.04 0.06 0.04
#------------
D 25/05/03
O 04 Sprayer, insecticide post emergence
+ 1.2160101 0.15
T Spray pest control chemicals on growing crop.   Crop is not killed.  11/17/01 DTL
T
T Added to the DB.  This assumes no crop flattening.  4-5-12 MAS
+
#------------
D 01/06/03
O 03 Cultivator, row 3 in ridge
+ 5.799433 17.55 2.2351363 0.0 2.2351363 0.89405453 2.4586499
T Row crop cultivator w/ sweeps leaving a 3" ridge 05-14-02 DTL
T G2 was added into file in front of the flattening (P24), burial (P25), and resurfacing (P26) factors because the area affected is less than 1.0 and
T the RUSLE values were normalized to 1.0.  This change will imulate the correct residue changes based on the method set forth in RUSLE.
T RUSLE's factors have been redused to based on the area affected.
T The stalk fall rate factor (P34) was moved ahead of the new (G2) factor to set the fall rate to the  less than 1.0 area affected.  8/7/07 MAS
+
G 01 Tillage
+ 76.20015 0.5 .9 76.20015 50.800102 101.600204
P 01 Break Crust
P 02 Random Roughness
+ 1 15.240031
P 05 Ridges and Dikes
+ 1 76.20015 762.0015 0.0 0.0 0.0
P 11 Aggregate Crushing
+ 3.0 1.0
P 12 Soil Loosening
+ 0.75
P 13 Soil Layer Mixing
+ 0.35
P 34 Change Standing Biomass Fall Rate
+ 4 3.0 2.5 2.0 1.5 1.0
+ 0.5 0.6 0.7 0.8 1.0
G 02 Biomass Manipulation
+ 1.0
P 24 Flatten Standing Biomass
+ 14 0.7 0.3 0.3 0.1 1.0
P 25 Bury Flat Biomass
+ 1 0.68 0.6 0.52 0.39 0.77
P 26 Resurface Buried Biomass
+ 0.04 0.04 0.04 0.06 0.04
#------------
D 05/06/03
O 04 Sprayer, insecticide post emergence
+ 1.2160101 0.15
T Spray pest control chemicals on growing crop.   Crop is not killed.  11/17/01 DTL
T
T Added to the DB.  This assumes no crop flattening.  4-5-12 MAS
+
#------------
D 10/06/03
O 03 Cultivator, row between beds
+ 5.799433 10.56 2.2351363 0.0 2.2351363 0.89405453 2.4586499
T Cultivator w/ opposing gangs of disk hillers.  Used to cultivate between Sugarcane beds. 020106 DTL
T G2 was added into file in front of the flattening (P24), burial (P25), and resurfacing (P26) factors because the area affected is less than 1.0 and
T the RUSLE values were normalized to 1.0.  This change will imulate the correct residue changes based on the method set forth in RUSLE.
T RUSLE's factors have been redused to based on the area affected.
T The stalk fall rate factor (P34) was moved ahead of the new (G2) factor to set the fall rate to the  less than 1.0 area affected.  8/7/07 MAS
T Cloned from row cultivator.  11-22-07 MAS
T
T Changed the P5 Ridge and Dikes to reflect the height of the previous tillage.  The operation now will show the ridge height of the planter or
T the previous tillage.  MAS 6-3-11
+
G 01 Tillage
+ 63.500126 0.5 .65 63.500126 50.800102 101.600204
P 01 Break Crust
P 02 Random Roughness
+ 1 15.240031
P 05 Ridges and Dikes
+ 0 76.20015 762.0015 355.6007 0.0 0.0
P 11 Aggregate Crushing
+ 3.0 1.0
P 12 Soil Loosening
+ 0.75
P 13 Soil Layer Mixing
+ 0.35
P 34 Change Standing Biomass Fall Rate
+ 4 3.0 2.5 2.0 1.5 1.0
+ 0.5 0.6 0.7 0.8 1.0
G 02 Biomass Manipulation
+ 1.0
P 24 Flatten Standing Biomass
+ 14 0.7 0.3 0.3 0.1 1.0
P 25 Bury Flat Biomass
+ 1 0.49 0.44 0.38 0.28 0.55
P 26 Resurface Buried Biomass
+ 0.7 0.3 0.3 0.1 1
#------------
D 20/06/03
O 04 Sprayer, fungicide and insecticide tank mix
+ 1.2160101 .15
T Spray pest control chemicals on growing crop.  Crop is not killed.
T In the MCREW management screen the user must select the kind of weeds killed in the growing crop as external residue.   080404 DTL
T Cloned from Defoliate (spray) crop.oprn, Changed the P31 to No crop kill and added G4 to add material to field MAS 9-28-06
+
#------------
D 01/07/03
O 04 Sprayer, growth regulator
+ 1.2160101 0.15
T R2 Notes: Spray growth regulators on growing crop.   Crop is not killed.  11/17/01 DTL.
T Revised Sprayer, insecticide for application of plant growth regulators for cotton
T (for example, Pix and Mepichlor). rev 082211 LOS.
T
T Added to the DB.  This assumes no crop flattening.  4-12-12 MAS
+
#------------
D 10/07/03
O 04 Sprayer, growth regulator
+ 1.2160101 0.15
T R2 Notes: Spray growth regulators on growing crop.   Crop is not killed.  11/17/01 DTL.
T Revised Sprayer, insecticide for application of plant growth regulators for cotton
T (for example, Pix and Mepichlor). rev 082211 LOS.
T
T Added to the DB.  This assumes no crop flattening.  4-12-12 MAS
+
#------------
D 20/07/03
O 04 Sprayer, growth regulator
+ 1.2160101 0.15
T R2 Notes: Spray growth regulators on growing crop.   Crop is not killed.  11/17/01 DTL.
T Revised Sprayer, insecticide for application of plant growth regulators for cotton
T (for example, Pix and Mepichlor). rev 082211 LOS.
T
T Added to the DB.  This assumes no crop flattening.  4-12-12 MAS
+
#------------
D 01/08/03
O 04 Harvest, hand pick
+ 3.2738733 0.15
T Hand pick lettuce or similar crops or to represent one final picking of fruit or berry crops.
T Do not use for multiple pickings of fruit or berry crops unless a regrowth vegetation file representing
T regrowth between pickings is available in the database to be called in.
T This is not the case for strawberries.  12132011 DTL
T Added 3/29/07 MAS
T Reworked the values MAS 2-24-09
T Added the change to flat on the crop type.  8-27-10
T This operation takes all of the yield, and can be used to calibrate the yield. 12-27-11 MAS
T Adjusted the Energy use to 0.000000010 gal/ac  2-23-12
T
T Changed the fuel use from 0.000000010 to 0.36 g/ac 4-17-12 MAS
+
G 02 Biomass Manipulation
+ 1.0
P 31 Kill or Defoliate Growing Crop
+ 0
P 62 Remove (by age pool) Plant/Residue Material
+ 1 1 0 1 3 3 2 1.0 0.0 0.0 0.0 0.0
P 40 End crop Biomass Manipulation
#------------
D 25/08/03
O 04 Harvest, hand pick
+ 3.2738733 0.15
T Hand pick lettuce or similar crops or to represent one final picking of fruit or berry crops.
T Do not use for multiple pickings of fruit or berry crops unless a regrowth vegetation file representing
T regrowth between pickings is available in the database to be called in.
T This is not the case for strawberries.  12132011 DTL
T Added 3/29/07 MAS
T Reworked the values MAS 2-24-09
T Added the change to flat on the crop type.  8-27-10
T This operation takes all of the yield, and can be used to calibrate the yield. 12-27-11 MAS
T Adjusted the Energy use to 0.000000010 gal/ac  2-23-12
T
T Changed the fuel use from 0.000000010 to 0.36 g/ac 4-17-12 MAS
+
G 02 Biomass Manipulation
+ 1.0
P 31 Kill or Defoliate Growing Crop
+ 0
P 62 Remove (by age pool) Plant/Residue Material
+ 1 1 0 1 3 3 2 1.0 0.0 0.0 0.0 0.0
P 40 End crop Biomass Manipulation
#------------
D 12/09/03
O 04 Harvest, tobacco, flue cured
+ 3.2738733 0.15
T Harvest of flue cured tobacco where lower mature leaves are systematically picked and removed leaving only the central stalk.
T Use this operation on the date that represents the end of the harvest period.  11/27/01 DTL
T LEAVES ARE PICKED BY HAND.  100% of the remaining leaves are havested.
T Removed 100% of the flower fraction because some of the plant mass may have gone to fruiting or grain.
T Cannot be calibrated because this is a partial harvest.  Change the bio adjustment factor manually.
T Crop not killed.  12-19-11 MAS
+
G 02 Biomass Manipulation
+ 0.8
P 31 Kill or Defoliate Growing Crop
+ 0
P 62 Remove (by age pool) Plant/Residue Material
+ 1 0 0 0 1 3 2 0 0.95 0.0 0.0 0.0
P 34 Change Standing Biomass Fall Rate
+ 0 1.0 1.0 1.0 1.0 1.0
+ 1.0 1.0 1.0 1.0 1.0
P 40 End crop Biomass Manipulation
#------------
D 15/09/03
O 04 Sprayer, kill crop
+ 1.2160101 0.15
T All crop types are killed, green grow turned to residue, standing.  MAS 12-27-11
T
T Added Flattening to the operation to match R2 (P-24).  This will tend to increase erosion on systems that using
T cover crops by causing less standing residue from the crop or cover crop killed.  MAS 4-3-12
T
T After a conference call, Linda Scheffe, Dave Lightle, Mike Sporcic, and Fred Fox, we decided to change the flattening
T from 0.7-0.5 to 0.05 for all residue type due to wheel traffic only.  Plant canopy change over time is not considered.
T Normal plant senescence built into the model will handle plant changes.  MAS 4-5-12
+ 
G 02 Biomass Manipulation
+ 1.0
P 24 Flatten Standing Biomass
+ 0 0.05 0.05 0.05 0.05 0.05
P 31 Kill or Defoliate Growing Crop
+ 2
P 40 End crop Biomass Manipulation
#------------
D 16/09/03
O 04 Fert applic. surface broadcast
+ 1.4966278 0.0609375
T R2 Notes: Broadcast fertilizer spreader.  Wheel traffic only.  rev 082107 DTL
T
T Added to DB 4-12-12 MAS
+
G 01 Tillage
+ 0.0 0 0.05 0.0 0.0 0.0
P 01 Break Crust
P 02 Random Roughness
+ 1 8.8900175
P 11 Aggregate Crushing
+ 4.3 2.0
P 24 Flatten Standing Biomass
+ 0 0.25 0.2 0.15 0.1 1.0
P 26 Resurface Buried Biomass
+ 0.07 0.08 0.1 0.12 0.07
P 34 Change Standing Biomass Fall Rate
+ 0 1.0 1.0 1.0 1.0 1.0
+ 1.0 1.0 1.0 1.0 1.0
#------------
D 17/09/03
O 03 Disk, tandem light finishing
+ 3.7415698 19.5 2.2351363 0.0 2.2351363 1.3410819 2.6821637
T 6/8/01 DTL RUSLE.  7in sp.  This is tool used to finish a seedbed.  MAS 10-26-06
+
G 01 Tillage
+ 101.600204 0.5 1.0 101.600204 76.20015 127.00026
P 01 Break Crust
P 02 Random Roughness
+ 1 15.240031
P 05 Ridges and Dikes
+ 1 12.700026 177.80035 0.0 0.0 0.0
P 11 Aggregate Crushing
+ 2.8 0.75
P 12 Soil Loosening
+ 0.75
P 13 Soil Layer Mixing
+ 0.35
P 31 Kill or Defoliate Growing Crop
+ 2
P 40 End crop Biomass Manipulation
P 24 Flatten Standing Biomass
+ 0 0.85 0.7 0.6 0.5 1.0
P 25 Bury Flat Biomass
+ 1 0.73 0.63 0.55 0.4 0.73
P 26 Resurface Buried Biomass
+ 0.02 0.04 0.02 0.05 0.02
P 34 Change Standing Biomass Fall Rate
+ 7 3.0 2.5 2.0 1.5 1.0
+ 0.5 0.6 0.7 0.8 1.0
#------------
D 25/09/03
O 03 Drill or air seeder single disk openers 7-10 in spac
+ 3.2738733 2.44 2.2351363 0.0 2.2351363 1.5645955 2.9056773
T Drill or Air seeder with single disk no-till openers  JD 750 or similar openers. (No-till air drill)
T Based on Drill, no-till single disk 7-10 spacing. 102403 DTL. RUSLE MAS 10-26-06
T G2 was added into file in front of the flattening (P24), burial (P25), and resurfacing (P26) factors because the area affected is less than 1.0 and
T the RUSLE values were normalized to 1.0.  This change will imulate the correct residue changes based on the method set forth in RUSLE.
T RUSLE's factors have been redused to based on the area affected.
T The stalk fall rate factor (P34) was moved ahead of the new (G2) factor to set the fall rate to the less than 1.0 area affected.  8/7/07 MAS
+
G 01 Tillage
+ 63.500134 0.4 0.15 63.50013 50.800102 101.600204
P 01 Break Crust
P 02 Random Roughness
+ 1 7.6200156
P 05 Ridges and Dikes
+ 1 25.400051 203.20041 0.0 0.0 0.0
P 11 Aggregate Crushing
+ 2.8 0.75
P 12 Soil Loosening
+ 0.4
P 13 Soil Layer Mixing
+ 0.20
P 34 Change Standing Biomass Fall Rate
+ 7 3.0 2.5 2.0 1.5 1.0
+ 0.5 0.6 0.7 0.8 1.0
G 02 Biomass Manipulation
+ 1.0
P 24 Flatten Standing Biomass
+ 0 0.6 0.4 0.35 0.15 1.0
P 25 Bury Flat Biomass
+ 1 0.05 0.04 0.03 0.02 0.03
P 26 Resurface Buried Biomass
+ 0.01 0.01 0.01 0.05 0.01
G 03 Crop Name
+ Wheat, winter, mid-south
P 51 Seeding Configuration
+ 1 0.0 0
+ 220.0 8.0 1 40.0 1.0 1.0 0
+ bu/ac
+ 10.9 148.7 5 0.8 0.6 0.8
+ 1.2 0.025 2.0 0.0 25.0 1 270 1666.6667
+ -5.0 -15.0 0.005 0.05 0.035 30.0
+ 0.013 0.8013 0.4293 -0.086 -0.018 0.932 0.556 0.0736
+ 0.3293 -0.086 2.87 1.0 20.0 0.05 0 0.3
+ 28.571428 335.0 1.4 0.012 0.1 0.1 0.0 2
+ 0.0133 0.0133 0.0133 0.0133 0.04 0.0050 17.1 5.227942
+ -2.08165 0.548606 1.2778 0.08331279 0.0 0.0 0.0 0.0
T For use in CMZ 1,2,3
T
T Standing Fall rate reduced from 0.12 to 0.04 #/(# days) because
T WW-Chem fallow in SW KS showed too much standing residue was falling down.  Larry Wagner recommended we
T reduce fall rate. Dave L, Linda S., and I made runs to get the wt to match the standing stalk wt from Fred Fox stalk residue
T samples WERU Lab.  This rate left 24% of the starting count standing.  This is well within the range of values of two paper.
T Both paper showed about 46% left standing at the 440 day after harvest time.  David Nelson, ARS Akron, CO also confirmed
T that the orginal 8% standing was too low.  He thought that the 24% was much more resonable.  MAS 6-7-11
#------------
*END
*EOF
