Version: 1.5
*START 1
N Originating Program: RUSLE2
N Skel Format Version: 1.1
N This management file was originally converted from the NRCS standard XML format on - Tue Oct 16 13:24:27 PDT 2012
N This management file was updated to contain the most current crop and operation records for WEPS on - Tue Dec 17 20:12:48 CST 2013
#------------
D 10/03/01
O 03 Disk, tandem heavy primary op
+ 7.0154433 39 2.2351363 0.0 2.2351363 1.3410819 2.6821637
T 11-12in. Spacing, Front and Rear
T Recommended for primary tillage in medium to heavy soils
T Excellent residue-handling capability. MAS 10-26-06
+
G 01 Tillage
+ 152.4003 1.0 1.0 152.4003 101.600204 177.80035
P 01 Break Crust
P 02 Random Roughness
+ 1 38.100075
P 05 Ridges and Dikes
+ 1 101.600204 279.40057 0.0 0.0 0.0
P 11 Aggregate Crushing
+ 2.8 0.75
P 12 Soil Loosening
+ 0.9
P 13 Soil Layer Mixing
+ 0.4
P 31 Kill or Defoliate Growing Crop
+ 2
P 40 End crop Biomass Manipulation
P 24 Flatten Standing Biomass
+ 0 1.0 0.9 0.8 0.5 1.0
P 25 Bury Flat Biomass
+ 1 0.95 0.85 0.8 0.6 0.95
P 26 Resurface Buried Biomass
+ 0.05 0.06 0.07 0.08 0.05
P 34 Change Standing Biomass Fall Rate
+ 7 3.0 2.5 2.0 1.5 1.0
+ 0.5 0.6 0.7 0.8 1.0
#------------
D 11/03/01
O 04 Fert applic. surface broadcast
+ 1.4966278 0.0609375
T R2 Notes: Broadcast fertilizer spreader.  Wheel traffic only.  rev 082107 DTL
T
T Added to DB 4-12-12 MAS
+
G 01 Tillage
+ 0.0 0 0.05 0.0 0.0 0.0
P 01 Break Crust
P 02 Random Roughness
+ 1 8.8900175
P 11 Aggregate Crushing
+ 4.3 2.0
P 24 Flatten Standing Biomass
+ 0 0.25 0.2 0.15 0.1 1.0
P 26 Resurface Buried Biomass
+ 0.07 0.08 0.1 0.12 0.07
P 34 Change Standing Biomass Fall Rate
+ 0 1.0 1.0 1.0 1.0 1.0
+ 1.0 1.0 1.0 1.0 1.0
#------------
D 12/03/01
O 03 Disk, tandem light finishing
+ 3.7415698 19.5 2.2351363 0.0 2.2351363 1.3410819 2.6821637
T 6/8/01 DTL RUSLE.  7in sp.  This is tool used to finish a seedbed.  MAS 10-26-06
+
G 01 Tillage
+ 101.600204 0.5 1.0 101.600204 76.20015 127.00026
P 01 Break Crust
P 02 Random Roughness
+ 1 15.240031
P 05 Ridges and Dikes
+ 1 12.700026 177.80035 0.0 0.0 0.0
P 11 Aggregate Crushing
+ 2.8 0.75
P 12 Soil Loosening
+ 0.75
P 13 Soil Layer Mixing
+ 0.35
P 31 Kill or Defoliate Growing Crop
+ 2
P 40 End crop Biomass Manipulation
P 24 Flatten Standing Biomass
+ 0 0.85 0.7 0.6 0.5 1.0
P 25 Bury Flat Biomass
+ 1 0.73 0.63 0.55 0.4 0.73
P 26 Resurface Buried Biomass
+ 0.02 0.04 0.02 0.05 0.02
P 34 Change Standing Biomass Fall Rate
+ 7 3.0 2.5 2.0 1.5 1.0
+ 0.5 0.6 0.7 0.8 1.0
#------------
D 20/03/01
O 03 Planter, transplanter, vegetable
+ 7.4831395 3.12 0.89405453 0.0 0.89405453 0.44702727 1.3410819
T G2 was added into file in front of the flattening (P24), burial (P25), and resurfacing (P26) factors because the area affected is less than 1.0 and
T the RUSLE values were normalized to 1.0.  This change will imulate the correct residue changes based on the method set forth in RUSLE.
T RUSLE's factors have been redused to based on the area affected.
T The stalk fall rate factor (P34) was moved ahead of the new (G2) factor to set the fall rate to theless than 1.0 area affected.  8/7/07 MAS
T
T Changed the P5 to allow the preexisting ridges and furrows to set the ridge roughness.  MAS  12-30-2010
+
G 01 Tillage
+ 152.4003 0.4 0.2 152.4003 101.600204 203.20041
P 01 Break Crust
P 02 Random Roughness
+ 1 10.160021
P 05 Ridges and Dikes
+ 0 50.800102 762.0015 635.0013 0.0 0.0
P 11 Aggregate Crushing
+ 2.4 2.0
P 12 Soil Loosening
+ 0.6
P 13 Soil Layer Mixing
+ 0.3
P 34 Change Standing Biomass Fall Rate
+ 7 3.0 2.5 2.0 1.5 1.0
+ 0.5 0.6 0.7 0.8 1.0
G 02 Biomass Manipulation
+ 1.0
P 24 Flatten Standing Biomass
+ 0 0.3 0.25 0.2 0.1 1.0
P 25 Bury Flat Biomass
+ 1 .07 0.05 .04 .02 .03
P 26 Resurface Buried Biomass
+ 0.01 0.01 0.01 0.02 0.01
G 03 Crop Name
+ Cabbage
P 51 Seeding Configuration
+ 1 0.0 2
+ 2.9999999999999996 1 1 39000 1 1 2
+ lbs/ac
+ 93 8930 4 1 0.65 0.95
+ 0.45720553 0.01 0.7 4.000000000000002 24 0 55 1300.0
+ -5 -15 0.01 0.95 0 19
+ 0.194 0.6956 0.3922 -0.1253 0 1 1.1 0.01
+ 0.4995 -0.0944 0.1 1 20 0.05 1 0.9120584
+ 2000 2000 2 0.03 0 0 0 1
+ 0.02 0.02 0.02 0.02 0.2 0.0050 20 2.7
+ -1.20379 0.604887 0 0.0 0 0.0 0.0 0.0
T Harvest index from RUSLE "Cabage", Yield from Producing Veg Crops, Ware & McCollum Not the same as RUSLE.  MAS 5/10/06
T
T
T Adjusted cover factor to ARS (larger size residue) based on size of the root balls  MAS 12-30-10
#------------
D 15/04/01
O 03 Cultivator, row 3 in ridge
+ 5.799433 17.55 2.2351363 0.0 2.2351363 0.89405453 2.4586499
T Row crop cultivator w/ sweeps leaving a 3" ridge 05-14-02 DTL
T G2 was added into file in front of the flattening (P24), burial (P25), and resurfacing (P26) factors because the area affected is less than 1.0 and
T the RUSLE values were normalized to 1.0.  This change will imulate the correct residue changes based on the method set forth in RUSLE.
T RUSLE's factors have been redused to based on the area affected.
T The stalk fall rate factor (P34) was moved ahead of the new (G2) factor to set the fall rate to the  less than 1.0 area affected.  8/7/07 MAS
+
G 01 Tillage
+ 76.20015 0.5 .9 76.20015 50.800102 101.600204
P 01 Break Crust
P 02 Random Roughness
+ 1 15.240031
P 05 Ridges and Dikes
+ 1 76.20015 762.0015 0.0 0.0 0.0
P 11 Aggregate Crushing
+ 3.0 1.0
P 12 Soil Loosening
+ 0.75
P 13 Soil Layer Mixing
+ 0.35
P 34 Change Standing Biomass Fall Rate
+ 4 3.0 2.5 2.0 1.5 1.0
+ 0.5 0.6 0.7 0.8 1.0
G 02 Biomass Manipulation
+ 1.0
P 24 Flatten Standing Biomass
+ 14 0.7 0.3 0.3 0.1 1.0
P 25 Bury Flat Biomass
+ 1 0.68 0.6 0.52 0.39 0.77
P 26 Resurface Buried Biomass
+ 0.04 0.04 0.04 0.06 0.04
#------------
D 01/05/01
O 04 Sprayer, insecticide post emergence
+ 1.2160101 0.15
T Spray pest control chemicals on growing crop.   Crop is not killed.  11/17/01 DTL
T
T Added to the DB.  This assumes no crop flattening.  4-5-12 MAS
+
#------------
D 10/05/01
O 04 Sprayer, insecticide post emergence
+ 1.2160101 0.15
T Spray pest control chemicals on growing crop.   Crop is not killed.  11/17/01 DTL
T
T Added to the DB.  This assumes no crop flattening.  4-5-12 MAS
+
#------------
D 20/05/01
O 04 Sprayer, insecticide post emergence
+ 1.2160101 0.15
T Spray pest control chemicals on growing crop.   Crop is not killed.  11/17/01 DTL
T
T Added to the DB.  This assumes no crop flattening.  4-5-12 MAS
+
#------------
D 20/06/01
O 04 Harvest, cabbage and head lettuce
+ 12.627798 .15
T ARS record - filename is:  Harvest Wheat - grain (combine cutterbar header).oprn
T This operation record is designed to represent actual field harvesting operation
T of removing the grain from small grain crops with a cutterbar head on a combine.
T This harvesting operation record removes all the reproductive component of a crop above the
T cutting height.  Typically this is specified as the "yield" component in the crop record.
T The non-harvested crop plant material above the specified cut height becomes flat residue.
T The remaining above ground crop material below the specified cut height becomes standing residue.
T Nov 02, 2005	Created - Larry Wagner
T Detailed info regarding this operation record:
T This harvest record specifies the actual cut height dependent upon the height
T of the crop.  The cut height is specified as a fraction of the crop height.
T Some standing crop stalks could be flattened during the harvesting process,
T e.g. by the harvester's tire tracks.  Therefore, a flattening process is also a part of this
T operation record.  The default values are set to zero, assuming no flattening of standing
T stalks are occuring.  However, these can be set as necessary for the specific harvesting
T device used in the operation.
T The harvesting operation could also have an effect on the "standing stalk"
T fall rate and fall threshold values.  The default "biomass pool" flag parameter
T is set to "No adjustments applied" so that no "stalk residue decay rate change" will occur.
T However, this flag value can be changed along with the default parameter values
T to change the "stalk residue decay processes".
+
G 02 Biomass Manipulation
+ 1.0
P 31 Kill or Defoliate Growing Crop
+ 0
P 43 Cut/Remove Biomass by Fraction (flags)
+ 1 1 0 1 0.75 1 0.95 0
P 34 Change Standing Biomass Fall Rate
+ 0 1.0 1.0 1.0 1.0 1.0
+ 1.0 1.0 1.0 1.0 1.0
P 40 End crop Biomass Manipulation
P 24 Flatten Standing Biomass
+ 0 0.2 0.2 0.2 0 0.0
#------------
*END
*EOF
