Version: 1.5
*START 1
N Originating Program: RUSLE2
N Skel Format Version: 1.1
N This management file was originally converted from the NRCS standard XML format on - Tue Oct 16 13:26:14 PDT 2012
N This management file was updated to contain the most current crop and operation records for WEPS on - Tue Dec 17 19:56:22 CST 2013
#------------
D 19/04/01
O 03 Manure injector, liquid high disturb.30 inch
+ 14.592121 7.8 2.6821637 0.0 2.6821637 1.5645955 2.9056773
T WEPS uses manure applied on a dry weight bases.  You must add the lbs/ac dry matter applied.  The operation is defaulted to 0.  If it is appled to surface all would be on the surface.
T In this case 5% would be on the surface.
T If you apply 1000 gal/ac to a field and the it is a 5% solid slury, you would apply 417 lbs/ac liquid manure to the field.
T 1000 lbs/ac x 8.34 lbs/gal x 0.05 dry matter = 417 lbs/ac solids.   About 95% of material applied is incorporated into the soil.
T 02/10/03  DTL MAS 10-26-06
T G2 was added into file in front of the flattening (P24), burial (P25), and resurfacing (P26) factors because the area affected is less than 1.0 and
T the RUSLE values were normalized to 1.0.  This change will imulate the correct residue changes based on the method set forth in RUSLE.
T RUSLE's factors have been redused to based on the area affected.
T The stalk fall rate factor (P34) was moved ahead of the new (G2) factor to set the fall rate to the less than 1.0 area affected.  8/7/07 MAS
+
G 01 Tillage
+ 152.4003 0.8 0.5 152.4003 101.600204 254.0005
P 01 Break Crust
P 02 Random Roughness
+ 1 25.400051
P 05 Ridges and Dikes
+ 1 101.600204 762.0015 76.20015 0.0 0.0
P 11 Aggregate Crushing
+ 2.4 2.0
P 12 Soil Loosening
+ 0.8
P 13 Soil Layer Mixing
+ 0.35
P 34 Change Standing Biomass Fall Rate
+ 7 3.0 2.5 2.0 1.5 1.0
+ 0.5 0.6 0.7 0.8 1.0
G 02 Biomass Manipulation
+ 1.0
P 24 Flatten Standing Biomass
+ 14 0.6 0.5 0.5 0.4 1.0
P 25 Bury Flat Biomass
+ 4 .38 .335 .29 .215 .425
P 26 Resurface Buried Biomass
+ 0.05 0.05 0.05 0.1 .05
G 03 Crop Name
+ manure, liquid
P 66 Add Manure Residue Amount
+ 0.0 0.0 0.0 0.0 1
+ 0.0 0.0 0.0 0.0
+ 0.046739448 0.95
+ .06 .06 .06 .06 0.169 0.0050 1 0.6500045
+ -2.08165 0.548606
T Enter crop notes here.
#------------
*END
*EOF
