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GENERAL OVERVIEW

Snowpack


Precipitation


Temperature


STREAMFLOW

Streamflow forecasts of snowmelt runoff are as follows:                               
	FORECAST POINT(
	Percent of Ave. Flow
	Period

	Yukon River at Eagle

	92
	April - July

	Porcupine Ricer near International Boundary …..
	92
	April - July

	Yukon River near Stevens Village

	91
	April - July

	Tanana River at Fairbanks

	86
	April - July

	Tanana River at Nenana

	81
	April - July

	Little Chena River near Fairbanks

	62
	April - July

	Chena River near Two Rivers

	64
	April - July

	Salcha near Salchaket

	72
	April - July

	Sagvanirktok River near Pump Station 3

	79
	April - July

	Kuparuk River near Deadhorse

	73
	April - July

	Kuskokwim River at Crooked Creek

	73
	April - June

	Gulkana River at Sourdough

	66
	April - July

	Little Susitna River near Palmer

	66
	April - July

	Talkeetna River near Talkeetna

	78
	April - July

	Ship Creek near Anchorage

	93
	April - July

	Kenai River at Cooper Landing

	107
	April - July

	Gold Creek near Juneau

	100
	April - July

	SNOWMELT RUNOFF INDEX (SRI)
For streams that no longer have stream gauging stations.

	FORECAST POINT
	INDEX
	
	  Index
-2  to  -3

-1  to  -2

-1  to +1

+1 to +2

+2 to +3


	Key:

much below average snowmelt runoff

below average snowmelt runoff

average snowmelt runoff

above average snowmelt runoff

much above average snowmelt runoff

	Koyukuk River at Hughes

	-3.0
	
	
	

	MF Koyukuk R near Wiseman ……………………
	-2.7
	
	
	

	Slate Creek at Coldfoot…………………………….
	-2.7
	
	
	

	Beaver Creek above Victoria Creek

	-3.1
	
	
	

	Birch Creek below South Fork

	-2.5
	
	
	

	Caribou Creek at Chatanika

	-2.0
	
	
	

	Susitna River near Gold Creek

	-2.4
	
	
	

	Chulitna River near Talkeetna

	-3.0
	
	
	

	Deshka River at mouth near Willow

	-2.2
	
	
	

	Montana Creek at Parks Highway

	-1.8
	
	
	

	Willow Creek near Willow

	-2.4
	
	
	

	Skwentna River at Skwentna

	-1.6
	
	
	

	Chuitna River near Tyonek

	-2.0
	
	
	

	Campbell Creek near Spenard

	-1.5
	
	
	

	Indian Creek at Indian

	-1.2
	
	
	

	Bird Creek at Bird Creek

	-1.2
	
	
	

	Glacier Creek nr Girdwood ………………………..
	+2.8
	
	
	

	Six Mile Creek near Hope

	+2.2
	
	
	

	Resurrection Creek near Hope

	+0.4
	
	
	

	Grouse Ck at Grouse Lake Outlet nr Seward …..
	+0.2
	
	
	

	Anchor River near Anchor Point

	0.0
	
	
	

	Deep Creek  near Ninilchik

	+0.4
	
	
	

	Ninilchik River near Ninilchik

	+0.3
	
	
	

	Fritz Creek near Homer

	+0.6
	
	
	

	Skagway River at Skagway

	+1.8
	
	
	

	Municipal Watershed C nr Petersburg …………..
	-1.0
	
	
	


HOW FORECASTS ARE MADE

Most of the annual streamflow in the western United States originates as snowfall that has accumulated in the mountains during the winter and early spring.  As the snowpack accumulates, hydrologists estimate the runoff that will occur when it melts.  Measurements of the water content in the snow at selected manual snow courses and automated SNOTEL sites are used in the runoff estimates.  In addition, precipitation, antecedent streamflow, and indices of the El Niño / Southern Oscillation are used in computerized statistical and simulation models to prepare runoff forecasts.  These forecasts are coordinated between hydrologists in the Natural Resources Conservation Service and the National Weather Service.  Unless otherwise specified, all forecasts are for flows that would occur naturally without any upstream influences.

Forecasts of any kind, of course, are not perfect.  Streamflow forecast uncertainty arises from three primary sources: uncertain knowledge of future weather conditions, uncertainty in the forecasting procedure, and errors in the data.  The forecast, therefore, must be interpreted not as a single value but rather as a range of values with specific probabilities of occurrence.  The middle of the range is expressed by the 50% exceedance probability forecast, for which there is a 50% chance that the actual flow will be above and a 50% chance that the actual flow will be below this value.  To describe the expected range around this 50% value, four other forecasts are provided, two smaller flows (90% and 70% exceedance probability) and two larger flows (30%, and 10% exceedance probability).  For example, there is a 90% chance that the actual flow will be more than the 90% exceedance probability forecast.  The others can be interpreted similarly.

The wider the spread among these values, the more uncertainty there is in the forecast.  As the season progresses, forecasts become more accurate, primarily because a greater portion of the future weather conditions become known.  This accuracy is reflected by a narrowing of the range around the 50% exceedance probability forecast.  Users should take this uncertainty into consideration when making operational decisions by selecting forecasts corresponding to the level of risk they are willing to assume about the amount of water to be expected.  If users anticipate receiving a lesser supply of water, or if they wish to increase their chances of having an adequate supply of water for their operations, they may want to base their decisions on the 90% or 70% exceedance probability forecasts, or something in between.  On the other hand, if users are concerned about receiving too much water, such as the threat of flooding, they may want to base their decisions on the 30% or 10% exceedance probability forecasts, or something in between.  Regardless of the forecast value users choose for operations, they should be prepared to deal with either more or less water.  Users should remember that even if the 90% exceedance probability forecast is used, there is still a 10% chance of receiving less than this amount.  By using the exceedance probability information, users can determine the chances of receiving more or less water for their specific streamflow need.

UPPER YUKON BASIN(
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Current Basin Conditions


Upper Yukon Basin

	
	THIS YEAR
	LAST YEAR
	1971-2000 AVERAGE

	Snow Course
	Elev.
	Date
	Snow

Depth
	Water

Content
	Snow

Depth
	Water

Content
	Snow Depth
	Water

Content

	
	(feet)
	
	(inches)


	Arrowhead Lake
	3675
	3/30/10
	28
	6.3
	---
	---
	35
	7.9

	Atlin         
	2395
	3/28/10
	19
	4.6
	28
	6.1
	21
	4.9

	Beaver Creek 
	2150
	3/26/10
	18
	3.2
	27
	6.1
	17
	3.3

	Burns Lake  
	3650
	3/31/10
	30
	6.4
	48
	12.0
	37
	8.4

	Burwash Airstrip 
	2660
	3/26/10
	11
	1.8
	13
	2.3
	9
	1.7

	Calumet     
	4300
	3/29/10
	30
	6.1
	41
	9.5
	36
	7.6

	Casino Creek  
	3490
	3/29/10
	26
	5.0
	32
	7.4
	26
	4.9

	Chair Mountain 
	3500
	3/26/10
	20
	3.4
	33
	7.3
	19
	3.7

	Duke River   
	4300
	3/31/10
	22
	4.3*
	24
	5.2
	23
	4.1

	Edwards Lake   
	2720
	3/30/10
	24
	4.8
	35
	7.5
	30
	6.7

	Finlayson Airstrip
	3240
	3/31/10
	18
	4.4*
	30
	6.5
	23
	4.8

	Fuller Lake  
	3690
	3/30/10
	32
	7.8
	39
	8.7
	34
	7.9

	Grizzly Creek  
	3200
	3/31/10
	31
	6.8
	30
	7.0
	32
	6.9

	Hoole River 
	3400
	3/31/10
	26
	5.5
	37
	8.8
	24
	5.2

	Jordan Lake    
	3050
	3/31/10
	26
	5.5
	36
	8.1
	24
	5.2

	King Solomon Dome
	3540
	3/31/10
	28
	5.6
	35
	7.4
	29
	6.0

	Log Cabin (B.C.) 
	2900
	3/30/10
	56
	16.8
	61
	21.1
	49
	14.6

	Mayo Airport 
	1770
	3/29/10
	16
	2.1
	23
	5.0
	17
	3.7

	MacIntosh    
	3805
	3/29/10
	25
	5.2
	27
	5.2
	21
	3.8

	Meadow Creek  
	4050
	4/01/10
	54
	13.5*
	57
	15.4
	42
	10.4

	Midnight Dome 
	2805
	3/30/10
	28
	6.3
	32
	6.8
	28
	5.8

	Montana Mountain
	3350
	3/30/10
	26
	5.7
	34
	6.9
	25
	5.5

	Morley Lake  
	2700
	3/30/10
	19
	4.5*
	35
	7.5
	25
	5.9

	Mount Nansen  
	3350
	3/29/10
	22
	4.2
	24
	4.3
	17
	3.0

	Mt.Berdoe
	3400
	3/29/10
	27
	4.8
	30
	5.2
	22
	4.2

	Mt. McIntyre B 
	3600
	3/26/10
	33
	7.5
	37
	8.9
	28
	5.9

	Pelly Farm 
	1550
	3/28/10
	12
	2.1*
	21
	3.9
	15
	3.0

	Plata Airstrip 
	2720
	3/30/10
	27
	5.3*
	34
	7.6
	33
	7.5

	Rackla Lake   
	3410
	3/30/10
	33
	6.7
	37
	7.5
	37
	8.2

	Rose Creek
	3550
	No Report
	
	
	30
	5.7
	15
	3.9

	Russell Lake  
	3480
	3/30/10
	32
	6.4
	46
	10.4
	37
	8.9

	Satasha Lake  
	3805
	3/29/10
	22
	4.2
	28
	5.8
	21
	4.3

	Tagish       
	3540
	3/28/10
	29
	7.0
	35
	8.0
	26
	5.5

	Twin Creeks   
	2950
	3/30/10
	25
	4.9*
	39
	8.9
	32
	7.3

	White River
	2700
	No Report
	
	
	---
	---
	16
	3.0

	Whitehorse Airport
	2300
	4/01/10
	16
	3.2*
	30
	8.7
	19
	3.9

	Williams Creek 
	3000
	3/29/10
	23
	4.8
	28
	6.0
	18
	3.5

	Withers Lake   
	3200
	3/30/10
	33
	7.5
	40
	10.0
	39
	9.4

	Estimate*
	
	
	
	
	
	
	
	


STREAMFLOW FORECASTS

	   Forecast Point
	Forecast 

 Period
	30- Yr Average  (1000AF)
	50 

Percentile
	% of 

Average
	Max

(1000AF)
	Min

(1000AF)

	Yukon River At Eagle
	Apr-Jul
	34200
	31300
	92
	36400
	26200


WATERSHED SNOWPACK ANALYSIS

	Region / River Basin
	No. of Courses Averaged
	Percent of Last Year
	Percent of Average

	Above Whitehorse/ Tetlin
	10
	74
	112

	Dawson
	3
	88
	100

	Stewart/ Pelly
	14
	66
	80

	White River
	9
	75
	111


 CENTRAL YUKON BASIN(
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Current Basin Conditions

Central Yukon Basin

SNOWPACK DATA

	
	THIS YEAR
	LAST YEAR
	1971-2000 AVERAGE

	Snow Course
	Elev.
	Date
	Snow

Depth
	Water

Content
	Snow

Depth
	Water

Content
	Snow Depth
	Water

Content

	
	(feet)
	
	(inches)

	Borealis
	1330
	No Survey
	
	
	25
	5.4
	28
	5.2

	Boundary
	3300
	4/03/10
	21
	4.1
	29
	7.5
	25
	5.3

	Cathedral Creek
	1800
	3/29/10
	21
	3.5
	26
	4.9
	--
	--

	Chicken Airstrip
	1650
	4/03/10
	10
	2.1
	20
	4.7
	16
	3.2

	Circle Hot Springs
	860
	4/02/10
	19
	3.3
	28
	4.7
	26
	4.5

	Coal Creek
	1000
	3/29/10
	16
	2.7
	24
	4.5
	---
	---

	Copper Creek
	2000
	3/29/10
	15
	2.7
	16
	3.5
	---
	---

	Cresent Creek
	2600
	3/29/10
	20
	3.4
	21
	3.9
	---
	---

	Eagle Plains
	2330
	3/31/10
	32
	5.9
	31
	6.4
	32
	7.0

	Eagle River
	1120
	3/31/10
	26
	4.7
	28
	5.0
	27
	5.5

	Fort Yukon
	430
	3/29/10
	16
	2.8
	20
	4.1
	20
	3.8

	Fossil       
	1400
	No Survey
	
	
	23
	5.0
	---
	---

	Graphite Lake
	600
	No Report
	
	
	---
	---
	---
	--

	Hess Creek   
	1000
	3/29/10
	21
	4.0
	31
	5.9
	26
	5.4

	Lost Chicken Hill
	2100
	4/03/10
	12
	2.2
	24
	4.6
	---
	---

	Lower Beaver Creek
	400
	No Report
	
	
	---
	---
	---
	--

	Mission Creek   
	900
	3/23/10
	14
	2.5
	13
	3.0
	18
	4.1

	Mt. Fairplay
	3100
	4/03/10
	15
	3.4
	20
	5.0
	20
	4.3

	Old Crow
	980
	3/30/10
	24
	4.6
	33
	6.7
	25
	4.6

	Riff's Ridge
	2130
	4/01/10
	29
	5.5*
	30
	6.1
	29
	5.7

	Seven Mile
	600
	3/29/10
	20
	3.5
	32
	6.6
	26
	5.2

	Stack Pup Creek
	1620
	4/02/10
	20
	2.9
	26
	4.3
	25
	4.4

	Step Mountain
	2850
	3/29/10
	14
	2.6
	30
	5.6
	---
	---

	Thirty Mile    
	1350
	3/29/10
	18
	3.0
	29
	5.6
	37
	8.1

	Three Fingers
	3350
	3/29/10
	19
	3.1
	29
	5.6
	---
	---

	Upper Nome Creek
	2650
	3/31/10
	14
	2.9*
	27
	6.0
	---
	---

	Vunzik Lake
	500
	No Report
	
	
	---
	---
	---
	---

	Windy Gap    
	1900
	4/01/10
	18
	4.2
	26
	5.7
	31
	5.7

	Wolf         
	1200
	4/01/10
	13
	2.4
	21
	4.5
	27
	4.8


estimate *
STREAMFLOW FORECASTS

	Forecast Point
	Forecast 

 Period
	30- Yr Average  (1000AF)
	50 

Percentile
	% of 

Average
	Max

(1000AF)
	Min

(1000AF)

	Porcupine River near International Boundary
	Apr-Jul
	5640
	5170
	92
	7520
	3550

	Yukon River  near Stevens Village
	Apr-Jul
	48200
	43900
	91
	49900
	37900


PRECIPITATION DATA





INCHES ACCUMULATED SINCE OCTOBER 1st

	Precipitation

 Gauge
	
	
	
	
	1971-2000
	% of

	
	Elevation (feet)
	Date
	This Year
	Last Year
	Ave
	Average

	Atigun Pass**
	4800
	3/31/10
	4.8
	6.9
	8.1
	59

	Chandalar Shelf**  
	3300
	4/01/10
	3.1
	6.0
	5.3
	58

	Eagle Summit
	3650
	3/31/10
	3.5
	5.5
	5.9
	66

	Fort Yukon      
	430
	3/31/10
	1.7
	4.0
	4.2
	50

	Mission Creek    
	900
	No Report
	
	4.7
	5.2
	

	Upper Nome Creek
	2650
	3/31/10
	3.1
	6.7
	6.8
	46


**Wyoming shielded gauge

WATERSHED SNOWPACK ANALYSIS
	Region / River Basin
	No. of Courses Averaged
	Percent of Last Year
	Percent of Average

	Forty Mile
	5
	58
	70

	Porcupine (Y.T.)
	4
	86
	91

	White Mountains
	4
	66
	63

	Yukon Flats
	4
	64
	73


TANANA BASIN(
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Current Basin Conditions

Tanana Basin

SNOWPACK DATA 

	
	THIS YEAR
	LAST YEAR
	1971-2000 AVERAGE

	Snow Course
	Elev.
	Date
	Snow

Depth
	Water

Content
	Snow

Depth
	Water

Content
	Snow Depth
	Water

Content

	
	(feet)
	
	(inches)


	Bonanza Creek 
	1150
	3/31/10
	14
	2.2
	28
	5.7
	23
	5.0

	Caribou Creek      
	1250
	3/31/10
	12
	2.4
	25
	5.3
	23
	5.0

	Caribou Mine
	1150
	3/30/10
	14
	2.4
	56
	6.0
	27
	5.6

	Caribou Snow Pillow 
	900
	3/31/10
	16
	2.4
	26
	5.1
	23
	4.8

	Chisana
	3320
	3/31/10
	18
	3.4
	27
	5.6
	22
	3.7

	Cleary Summit      
	2230
	4/02/10
	20
	4.4
	31
	6.0
	31
	6.7

	Colorado Creek     
	700
	4/02/10
	11
	2.3
	23
	4.1
	23
	4.7

	Edgar Creek
	2400
	No Report
	
	
	30
	5.7
	28
	7.0

	Fairbanks FO
	450
	4/02/10
	10
	1.8
	26
	4.6
	23
	4.5

	Faith Creek                
	1900
	4/02/10
	15
	2.4
	26
	5.0
	28
	4.9

	Fielding Lake       
	3000
	3/31/10
	25
	6.0
	46
	13.2
	46
	12.0

	Fort Greely
	1500
	4/01/10
	14
	2.8
	15
	3.2
	17
	3.6

	French Creek 
	1800
	4/01/10
	13
	2.4
	29
	6.3
	27
	6.4

	Gerstle River  
	1200
	4/01/10
	15
	2.2
	21
	4.0
	18
	3.4

	Gold King
	1700
	No Report
	
	
	18
	3.6
	21
	4.3

	Granite Creek      
	1240
	4/01/10
	13
	3.9
	22
	4.3
	18
	3.8

	Jatahmund Lake  
	2180
	3/31/10
	16
	2.9
	24
	5.1
	18
	3.2

	Kantishna 
	1550
	3/29/10
	15
	2.2
	31
	5.8
	30
	5.7

	Lake Minchumina 
	730
	3/29/10
	13
	1.7
	27
	5.0
	21
	4.4

	Little Chena Bottom
	1460
	3/30/10
	9
	1.2
	18
	3.3
	21
	4.3

	Little Chena Ridge
	2000
	3/30/10
	8
	1.8
	18
	3.4
	28
	5.9

	Lost Creek
	3030
	No Report
	
	
	20
	4.9
	21
	4.2

	Mentasta Pass     
	2430
	3/31/10
	22
	4.5
	31
	6.7
	28
	6.7

	Monument Creek
	1850
	3/30/10
	15
	2.2
	26
	6.2
	25
	5.2

	Mt. Ryan
	2800
	3/30/10
	19
	3.2
	33
	6.2
	31
	6.8

	Munson Ridge
	3100
	3/30/10
	25
	5.2
	40
	9.0
	38
	9.1

	Paradise Hill 
	2200
	3/31/10
	13
	2.8
	24
	4.8
	18
	3.6

	Ptarmigan Airstrip
	2400
	No Report
	
	
	20
	4.0
	18
	3.7

	Ptarmigan Creek
	2230
	4/02/10
	20
	3.2
	25
	4.7
	19
	3.8

	Rock Creek Bottom
	2250
	3/31/10
	15
	2.0
	17
	3.5
	22
	4.3

	Rock Creek Ridge 
	2600
	3/31/10
	15
	2.0
	20
	3.9
	26
	5.3

	Shaw Creek Flats
	980
	4/01/10
	14
	2.2
	18
	4.0
	16
	3.4

	Stampede
	1800
	No Survey
	
	
	---
	---
	---
	---

	Teuchet Creek
	1640
	3/31/10
	16
	3.0
	26
	6.0
	23
	4.4

	Tok Junction       
	1650
	3/31/10
	19
	3.1
	21
	3.8
	19
	3.6

	Upper Chena
	3000
	3/30/10
	20
	3.9
	35
	7.4
	33
	7.8

	Upper Chena Pillow
	2850
	3/30/10
	19
	3.2
	36
	7.8
	32
	7.5

	Upper Wood River
	2990
	No Report
	
	
	25
	4.7
	28
	5.7


Estimate *

STREAMFLOW FORECASTS

	Forecast Point
	Forecast 

 Period
	30- Yr Average  (1000AF)
	        50

Percentile
	% of 

Average
	Max

(1000AF)
	Min

(1000AF)

	Tanana River at Fairbanks
	Apr-Jul
	7100
	6110
	86
	7070
	5150

	Little Chena R.  near Fairbanks
	Apr-Jul
	    78.0
	48
	62
	76
	20

	Chena River near Two Rivers
	Apr-Jul
	270
	173
	64
	290
	58

	Salcha River near Salchaket
	Apr-Jul
	625
	450
	72
	655
	285

	Tanana River at Nenana
	Apr-Jul
	9000
	7290
	81
	8480
	6100


WATERSHED SNOWPACK ANALYSIS

	Region / River Basin
	No. of Courses Averaged
	Percent of Last Year
	Percent of Average

	Chatanika
	4
	54
	54

	Chena Basin
	11
	51
	47

	Lower Tanana Valley
	7
	41
	38

	Mid Tanana Valley (Delta Junction)
	7
	56
	61

	Upper Tanana Valley (Tok)
	6
	62
	83


WESTERN INTERIOR BASINS(
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Current Basin Conditions
Koyukuk


Kuskokwim


Lower Yukon


Western Interior Basins 

SNOWPACK DATA

	
	THIS YEAR
	LAST YEAR
	1971-2000 AVERAGE

	Snow Course
	Elev.
	Date
	Snow

Depth
	Water

Content
	Snow

Depth
	Water

Content
	Snow Depth
	Water

Content

	
	(feet)
	
	(inches)


Koyukuk

	Bettles Field 
	640
	4/01/10
	20
	3.2
	37
	8.4
	32
	6.9

	Bonanza Forks 
	1200
	3/29/10
	14
	1.8
	33
	6.9
	27
	5.6

	Cloverleaf
	170
	3/30/10
	19
	3.6
	36
	8.6
	---
	---

	Coldfoot    
	1040
	3/31/10
	15
	3.2
	37
	9.0
	31
	6.9

	Colville Bend
	170
	3/30/10
	15
	2.7
	33
	8.3
	---
	---

	Disaster Creek 
	1550
	3/29/10
	15
	2.3
	27
	5.5
	23
	4.4

	Huggins Creek
	290
	3/31/10
	15
	2.3
	48
	10.8
	---
	---

	JR Slough
	160
	No Survey
	
	
	34
	8.6
	---
	---

	Kaldoyeit 
	750
	3/31/10
	11
	2.2
	31
	6.6
	---
	---

	Kanuti-Chelatna 
	670
	No Report
	
	
	39
	8.8
	---
	---

	Kanuti-Kilolitna 
	550
	3/31/10
	8
	1.5
	27
	6.2
	--
	---

	Lake Todatonen
	550
	3/31/10
	16
	2.2
	44
	9.6
	28
	5.5

	Minnkokut        
	580
	3/31/10
	21
	3.5
	46
	10.6
	---
	--

	Nolitna
	560
	No Report
	
	
	39
	8.2
	---
	---

	Table Mountain  
	2200
	3/29/10
	13
	1.6
	29
	6.3
	24
	4.9

	Taiholman
	540
	3/31/10
	3
	0.5
	4
	1.0
	---
	---

	Treat Island
	190
	3/31/10
	8
	1.5
	21
	5.0
	---
	---


Kuskokwim 

	Aniak Farm
	80
	3/31/10
	8
	1.5*
	---
	---
	---
	---

	Hoholitna River
	773
	No Report
	
	
	---
	---
	---
	---

	Holitna River
	257
	4/01/10
	31
	5.5
	54
	13.8
	---
	---

	Holokuk River
	367
	4/01/10
	6
	1.7
	19
	4.8
	---
	---

	Johnny Slu
	180
	4/01/10
	19
	3.5
	18
	12.3
	---
	---

	Kogruk River
	193
	4/01/10
	42
	7.2
	62
	16.1
	---
	---

	Lake Minchumina  
	730
	3/29/10
	13
	1.7
	27
	5.0
	21
	4.4

	Lower Aniak
	164
	No Report
	
	
	32
	8.1
	---
	---

	McGrath     
	340
	3/30/10
	19
	3.5
	39
	9.9
	30
	6.5

	Middle Kuskokwim
	297
	4/01/10
	10
	2.0
	42
	10.7
	---
	---

	N. Fork Kuskokwim
	512
	No Report
	
	
	44
	11.2
	---
	---

	Nixon Fork Kuskowim
	508
	No Report
	
	
	---
	---
	
	

	Purkeypile Mine 
	2025
	3/29/10
	18
	3.1
	23
	5.2
	21
	4.1

	Telaquana Lake 
	1550
	4/03/10
	10
	2.2
	23
	6.5
	20
	4.5


Lower Yukon

	Deer Creek
	195
	3/30/10
	15
	2.7
	36
	7.5
	---
	---

	Grouch Creek
	220
	3/30/10
	33
	6.8
	59
	14.0
	---
	---

	Holikachuk   
	100
	3/30/10
	39
	7.8
	54
	13.0
	---
	---

	Horsefly Creek 
	180
	3/30/10
	37
	7.2
	45
	11.0
	---
	---

	Innoko Inn
	200
	3/30/10
	20
	3.8
	---
	---
	---
	---

	Little Mud River
	855
	3/30/10
	15
	2.6
	27
	6.0
	---
	---

	Lower Nowitna River
	205
	3/30/10
	17
	3.1
	25
	5.5
	---
	---

	Menotl Creek 
	380
	No Report
	
	
	48
	13.5
	---
	---

	Middle Innoko 
	150
	3/30/10
	34
	7.0
	50
	12.8
	---
	---

	Nine Mile Island
	140
	3/30/10
	15
	2.7
	41
	9.6
	---
	---

	Pike Trap Lake
	130
	3/30/10
	5
	1.0
	20
	4.4
	---
	---

	Squirrel Creek
	150
	3/30/10
	19
	3.4
	35
	8.6
	---
	---

	Tozikaket
	600
	3/31/10
	11
	1.4
	30
	6.5
	24
	5.0

	Upper Innoko
	180
	3/30/10
	26
	5.2
	50
	12.0
	---
	---

	Wapoo Hills  
	220
	3/30/10
	38
	7.5
	57
	13.5
	---
	---

	Yankee Slough 
	100
	3/30/10
	41
	8.2
	45
	11.0
	---
	---

	Yetna River
	120
	3/30/10
	34
	7.0e
	---
	---
	---
	---


STREAMFLOW FORECASTS

	Forecast Point
	Forecast 

 Period
	30- Yr Average  (1000AF)
	50 

Percentile
	% of 

Average
	Max

(1000AF)
	Min

(1000AF)

	Kuskokwim River at Crooked Creek
	Apr-Jun
	10500
	76650
	73
	10200
	5080


WATERSHED SNOWPACK ANALYSIS

	Region / River Basin
	No. of Courses Averaged
	Percent of Last Year
	Percent of Average

	Koyukuk
	6
	31
	41

	Upper Kuskokwim
	4
	39
	50

	Lower Yukon
	11
	52
	65


ARCTIC AND KOTZEBUE SOUND(
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Current Basin Conditions
Arctic


Kotzebue


Arctic and Kotzebue Sound

PRECIPITATION DATA


INCHES ACCUMULATED SINCE OCTOBER 1ST

	Precipitation

Gauge
	
	
	
	
	1971-2000
	% of

	
	Elevation (feet)
	Date
	This Year
	Last Year
	Ave
	Average


Arctic

	Atigun Camp   
	3400
	4/01/10
	2.4
	3.2
	5.0
	48

	Atigun Pass 
	4800
	3/31/10
	4.8
	6.9
	8.1
	59

	Barrow 
	25
	No Report
	
	3.1
	3.0
	---

	Imnaviat Creek
	3050
	3/31/10
	2.8
	4.8
	3.9
	72

	Prudhoe Bay 
	30
	No Report
	
	3.0
	3.8
	---

	Sagwon
	1000
	No Report
	
	3.5
	3.3
	---


Kotzebue Sound

	Kivalina
	50
	3/31/10
	1.6
	4.4
	---
	---

	Red Dog**  

	950
	3/31/10
	2.3
	4.3
	6.3
	36


** Wyoming Shielded Gauge

STREAMFLOW FORECASTS

	Forecast Point
	Forecast 

 Period
	30- Yr Average  (1000AF)
	      50 Percentile
	% of 

Average
	Max

(1000AF)
	Min

(1000AF)

	Sagvanirktok River near Pump Station 3
	May- Jul
	685
	540
	79
	795
	365

	Kuparuk River near Deadhorse
	April - Jul
	795
	580
	73
	825
	405


WATERSHED SNOWPACK ANALYSIS

	Region / River Basin
	No. of Courses Averaged
	Percent of Last Year
	Percent of Average

	Arctic Coast
	No Report
	
	

	Dalton Highway
	3
	67
	59


NORTON SOUND/SOUTHWEST DELTA/BRISTOL BAY(
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Current Basin Conditions

Norton Sound


Southwest Delta


Bristol Bay

NORTON SOUND/SOUTHWEST DELTA/BRISTOL BAY(
SNOWPACK DATA
	
	THIS YEAR
	LAST YEAR
	1971-2000 AVERAGE

	Snow Course
	Elev.
	Date
	Snow

Depth
	Water

Content
	Snow

Depth
	Water

Content
	Snow Depth
	Water

Content

	
	(feet)
	
	(inches)


Bristol Bay 

	Brooks Camp 
	150
	3/31/10
	8
	1.5
	---
	---
	---
	---

	Fishtrap Lake
	1800
	No Report
	
	
	37
	8.9
	40
	10.5

	Port Alsworth
	270
	No Report
	
	
	28
	6.8
	12
	4.1

	Three Forks
	900
	3/31/10
	6
	1.5
	---
	---
	---
	---

	Upper Twin Lakes
	2000
	No Report
	
	
	24
	5.8
	27
	7.2


Norton Sound 

	Johnson’s Camp
	25
	3/31/10
	5
	1.2*
	26
	5.5
	---
	---

	Pargon Creek
	100
	3/31/10
	8
	2.3*
	33
	7.4
	---
	---

	Rocky Point 
	500
	3/31/10
	14
	2.6*
	37
	8.2
	---
	---


estimate*
PRECIPITATION DATA



INCHES ACCUMULATED SINCE OCTOBER 1ST

	Precipitation

 Gauge
	
	
	
	
	1971-2000
	% of

	
	Elevation (feet)
	Date
	This Year
	Last Year
	Ave
	Average

	Pargon Creek
	100
	3/31/10
	2.4
	4.3
	4.7
	51

	Rocky Point
	500
	3/31/10
	3.7
	8.3
	5.3
	70
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COPPER BASIN(
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Current Basin Conditions


Copper Basin

SNOWPACK DATA

	
	THIS YEAR
	LAST YEAR
	1971-2000 AVERAGE

	Snow Course
	Elev.
	Date
	Snow

Depth
	Water

Content
	Snow

Depth
	Water

Content
	Snow Depth
	Water

Content

	
	(feet)
	
	(inches)


	Chistochina 
	1950
	3/31/10
	17
	3.1
	25
	4.6
	22
	4.1

	Chokosna
	1550
	No Report
	
	
	17
	4.9
	22
	3.9

	Dadina Lake   
	2160
	3/31/10
	25
	5.3
	31
	6.5
	27
	5.9

	Haggard Creek
	2540
	3/31/10
	22
	4.1
	35
	7.1
	29
	6.3

	Horsepasture Pass 
	4300
	3/31/10
	24
	5.8
	24
	5.1
	29
	6.4

	Kenny Lake School 
	1300
	3/31/10
	16
	3.2
	15
	3.4
	17
	3.7

	Lake Louise   
	2400
	3/31/10
	17
	3.3
	28
	5.4
	23
	4.6

	Little Nelchina 
	2650
	3/31/10
	22
	4.8
	29
	5.0
	25
	5.3

	Long Glacier
	4820
	4/01/10
	26
	6.5
	48
	14.5
	---
	---

	Lost Creek
	3030
	No  Report
	
	
	20
	4.9
	21
	4.2

	May Creek
	1610
	3/31/10
	27
	3.5
	28
	5.8
	23
	5.0

	May Creek
	1610
	4/1/10
	21
	4.8
	28
	8.0
	23
	5.0

	Mentasta Pass  
	2430
	3/31/10
	22
	4.5
	31
	6.7
	28
	6.7

	Monsoon Lake  
	3100
	3/31/10
	16
	2.6
	33
	6.7
	28
	6.4

	Mt. Eyak
	1405
	3/31/10
	85
	34.4
	74
	23.4
	75
	24.2

	Notch
	2645
	No Survey
	
	
	12
	3.5
	---
	---

	Paxson    
	2650
	3/31/10
	20
	3.8
	39
	8.3
	32
	7.8

	Sanford River 
	2280
	3/31/10
	24
	5.6
	34
	7.5
	28
	6.2

	St. Anne Lake 
	1990
	3/31/10
	22
	4.5
	22
	4.2
	25
	5.5

	Tazlina   
	1225
	3/31/10
	17
	3.8
	13
	2.9
	19
	4.2

	Tebay Lake
	1930
	4/02/10
	30
	8.4
	54
	16.5
	---
	---

	Tolsona Creek
	2000
	3/31/10
	19
	3.3
	22
	4.4
	22
	4.1

	Tsaina River
	1650
	3/30/10
	64
	17.9
	42
	12.4
	57
	17.6

	Twin Lakes 
	2400
	3/31/10
	23
	5.2
	19
	4.1
	28
	6.4

	Upper Tsaina River
	1750
	3/30/10
	76
	22.2
	50
	15.6
	70
	21.7

	Worthington Glacier
	2100
	3/30/10
	85
	28.4
	65
	22.1
	72
	24.9


estimate*
PRECIPITATION DATA



INCHES ACCUMULATED SINCE OCTOBER 1ST

	Precipitation

 Gauge
	
	
	
	
	1971-2000
	% of

	
	Elevation (feet)
	Date
	This Year
	Last Year
	Ave
	Average

	May Creek
	1610
	3/31/10
	5.8
	7.8
	5.7
	102

	Strawberry Reef
	50
	3/31/10
	39.2
	38.2
	46.7
	84

	Upper Tsaina River
	1750
	3/31/10
	20.8
	24.5
	26.7
	78


STREAMFLOW FORECASTS

	Forecast Point
	Forecast 

 Period
	30- Yr Average  (1000AF)
	       50 

Percentile
	% of 

Average
	Max

(1000AF)
	Min

(1000AF)

	Gulkana River at Sourdough
	Apr-Jul
	475
	315
	66
	465
	164


WATERSHED SNOWPACK ANALYSIS

	Region / River Basin
	No. of Courses Averaged
	Percent of Last Year
	Percent of Average

	Alaska Range
	4
	49
	52

	Basin Floor
	6
	76
	79

	Chugach Range
	6
	131
	101

	Talkeetna Mountains
	3
	109
	91

	Wrangell Mountains
	4
	60
	84


MATANUSKA - SUSITNA BASINS(
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Current Basin Conditions

Matanuska - Susitna Basins

SNOWPACK DATA

	
	THIS YEAR
	LAST YEAR
	1971-2000 AVERAGE

	Snow Course
	Elev.
	Date
	Snow

Depth
	Water

Content
	Snow

Depth
	Water

Content
	Snow Depth
	Water

Content

	
	(feet)
	
	(inches)


	Alexander Lake 
	160
	3/31/10
	34
	10.0
	53
	14..3
	44
	12.0

	Archangel Road 
	2200
	3/31/10
	33
	9.1
	55
	16.6
	50.0
	16.3

	Bentalit Lodge
	150
	3/31/10
	29
	5.8
	34
	8.2
	---
	---

	Blueberry Hill 
	1200
	4/02/10
	32
	9.6
	56
	16.8
	58
	16.0

	Chelatna Lake  
	1450
	3/29/10
	30
	8.6
	---
	---
	44
	11.6

	Clearwater Lake 
	2650
	3/31/10
	16
	2.8
	30
	5.2
	27
	5.7

	Curtis Lake
	2850
	3/31/10
	13
	2.1
	25
	4.9
	---
	---

	Denali View  
	700
	4/02/10
	28
	8.1
	49
	14.6
	50
	13.4

	Dunkle Hills
	2700
	3/29/10
	29
	8.3
	---
	---
	---
	---

	Dutch Hills 
	3100
	3/29/10
	45
	14.0
	102
	28.5
	80
	27.5

	E. Fork Chulitna
	1800
	4/02/10
	30
	8.4
	54
	13.8
	54
	14.0

	Eldridge Glacier
	3400
	No Survey
	
	
	---
	---
	---
	---

	Fishhook Basin  
	3300
	3/31/10
	36
	10.3
	68
	21.8
	64
	20.5

	Fog Lakes      
	2120
	3/31/10
	16
	2.9
	31
	5.4
	28
	6.2

	Halfway Slough
	350
	4/02/10
	16
	4.6
	32
	8.7
	---
	---

	Independence Mine 
	3550
	3/31/10
	40
	11.7
	74
	24.5
	70
	24.2

	Independence Mine 
	3550
	3/31/10
	30
	8.1
	63
	18.6
	56
	20.0

	Lake Louise       
	2400
	3/31/10
	17
	3.3
	28
	5.4
	23
	4.6

	Little Susitna 
	1700
	3/31/10
	29
	8.2
	44
	12.6
	43
	13.3

	Monahan Flat
	2710
	3/31/10
	22
	3.7
	40
	7.5
	35
	8.1

	Moose Creek Ranch
	450
	3/31/10
	11
	3.1
	14
	3.2
	---
	---

	Nugget Bench 
	2010
	3/29/10
	39
	10.4
	66
	16.7
	55
	15.5

	Ramsdyke Creek
	2220
	3/29/10
	44
	13.0
	89
	23.5
	69
	22.0

	Sheep Mountain  
	2900
	3/31/10
	25
	6.3
	21
	4.5
	26
	6.0

	Skwentna       
	160
	No Survey
	
	
	47
	11.8
	42
	11.6

	Square Lake   
	2950
	3/31/10
	16
	3.0
	24
	4.2
	22
	4.2

	Susitna Valley High
	375
	4/02/10
	24
	6.2
	35
	8.4
	39
	10.2

	Talkeetna    
	350
	4/02/10
	18
	5.7
	38
	10.2
	34
	8.7

	Tokositna Valley 
	850
	3/31/10
	39
	11.0
	58
	13.8
	62
	18.7

	Tyone River 
	2500
	No Survey
	
	
	---
	---
	24
	5.2

	Upper Oshetna
	3150
	3/31/10
	19
	4.0
	---
	---
	---
	---

	Upper Sanona
	3100
	3/31/10
	25
	5.2
	31
	6.4
	---
	---

	Ward Lake
	2700
	No Survey
	
	
	---
	---
	25
	5.3

	Willow Airstrip 
	200
	4/02/10
	17
	5.0
	31
	7.5
	31
	8.1


STREAMFLOW FORECASTS

	Forecast Point
	Forecast 

 Period
	30- Yr Average  (1000AF)
	50 

Percentile
	% of 

Average
	Max

(1000AF)
	Min

(1000AF)

	Little Susitna River near Palmer
	Apr-Jul
	    86
	57
	66
	78
	36

	Talkeetna River near Talkeetna
	Apr-Jul
	1630
	1270
	78
	1530
	1010


PRECIPITATION DATA



INCHES ACCUMULATED SINCE OCTOBER 1ST

	Precipitation

Gauge
	
	
	
	
	1971-2000
	% of

	
	Elevation (ft.)
	Date
	This Year
	Last Year
	Ave
	Average

	Independence Mine
	3550
	3/31/10
	11.0
	18.0
	25.9
	42

	Monahan Flat
	2710
	3/31/10
	4.5
	6.8
	8.3
	54

	Susitna Valley High
	375
	3/31/10
	8.3
	13.0
	11.7
	71

	Tokositna Valley
	850
	3/31/10
	12.0
	22.4
	20.1
	60


WATERSHED SNOWPACK ANALYSIS

	Region / River Basin
	No. of Courses Averaged
	Percent of Last Year
	Percent of Average

	Lower Susitna
	5
	66
	69

	Matanuska/Little Susitna
	7
	60
	59

	Peters Hills
	6
	61
	59

	Upper Susitna
	9
	65
	67


NORTHERN COOK INLET*
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Current Basin Conditions

( For more information contact the Natural Resources Conservation Service in Anchorage.

Northern Cook Inlet

SNOW PACK DATA


	
	This Year
	Last Year
	1971-2000 Average

	Snow Course
	Elev.
	Date
	Snow

Depth
	Water

Content
	Snow

Depth
	Water

Content
	Snow Depth
	Water

Content

	
	(feet)
	
	Inches


	Anchorage Hillside 
	2080
	3/31/10
	38
	10.4
	43
	9.0
	38
	10.4

	Arctic Ski Bowl
	3000
	4/02/10
	29
	8.2
	27
	7.0
	43
	14.0

	Arctic Valley #1
	500
	4/02/10
	18
	4.7
	12
	2.3
	14
	3.6

	Arctic Valley #2
	1000
	4/02/10
	23
	5.0
	16
	3.5
	20
	5.1

	Arctic Valley #3
	1450
	4/02/10
	27
	7.6
	28
	7.1
	28
	7.3

	Arctic Valley #4
	2030
	4/02/10
	25
	6.8
	32
	7.1
	29
	7.7

	Chuitna Plateau
	1540
	3/31/10
	49
	16.5
	89
	29.8
	86
	26.9

	Congahbuna Lake
	500
	3/31/10
	24
	7.5
	44
	12.1
	38
	10.8

	Granite Point
	250
	3/31/10
	10
	3.0
	---
	---
	15
	5.6

	Indian Pass   
	2350
	3/31/10
	58
	19.6
	76
	22.7
	71
	23.7

	Kincaid Park  
	250
	4/01/10
	16
	4.7
	20
	5.0
	16
	4.2

	Lone Ridge
	1675
	3/31/10
	79
	27.6
	98
	5.0
	86
	33.1

	Moraine
	2100
	3/31/10
	40
	11.0
	27
	8.0
	29
	8.0

	Mt. Alyeska  
	1540
	3/31/10
	111
	35.5
	106
	32.3
	107
	36.9

	Point Mackenzie  
	200
	3/31/10
	13
	3.9
	22
	5.6
	18
	4.4

	Portage Valley 
	50
	4/01/10
	58
	21.6
	72
	21.3
	39
	15.0

	South Campbell Creek
	1200
	4/02/10
	29
	7.5
	57
	23
	28
	7.4


STREAMFLOW FORECASTS

	Forecast Point
	Forecast 

 Period
	30- Yr Average  (1000AF)
	50 

Percentile
	% of 

Average
	Max

(1000AF)
	Min

(1000AF)

	Ship Creek near Anchorage
	Apr-Jul
	58.0
	54
	93
	66
	42


PRECIPITATION DATA



INCHES ACCUMULATED SINCE OCTOBER 1ST

	Precipitation

Gauge
	
	
	
	
	1971-2000
	% of

	
	Elevation (feet)
	Date
	This Year
	Last Year
	Ave
	Average

	Anchorage Hillside
	2080
	3/31/10
	13.9
	15.5
	       13.1
	106

	Indian Pass  
	2350
	3/31/10
	23.3
	26.6
	23.9
	98

	Moraine
	2100
	3/31/10
	12.0
	10.4
	  9.7
	124

	Mt. Alyeska    
	1540
	3/31/10
	44.5
	35.9
	43.6
	103

	Point Mackenzie 
	200
	3/31/10
	6.0
	9.7
	  8.1
	75


WATERSHED SNOWPACK ANALYSIS

	Region / River Basin
	No. of Courses Averaged
	Percent of Last Year
	Percent of Average

	Beluga
	4
	69
	73

	Campbell Creek
	3
	108
	105

	Ship Creek
	8
	108
	92

	Turnagain Arm
	3
	125
	116


KENAI PENINSULA(
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Current Basin Conditions
Kenai Peninsula

SNOWPACK DATA

	
	THIS YEAR
	LAST YEAR
	1971-2000 AVERAGE

	Snow Course
	Elev.
	Date
	Snow

Depth
	Water

Content
	Snow

Depth
	Water

Content
	Snow Depth
	Water

Content

	
	(feet)
	
	(inches)


	Anchor River Divide
	1600
	3/31/10
	48
	14.0
	32
	7.8
	43
	12.6

	Bertha Creek
	950
	3/26/10
	72
	22.9
	47
	15.3
	57
	17.6

	Bridge Creek 
	1300
	3/30/10
	44
	13.3
	23
	5.4
	44
	12.9

	Cooper Lake   
	1200
	3/31/10
	54
	17.8
	31
	9.8
	50
	15.6

	Demonstration Forest 
	780
	3/30/10
	35
	10.2
	20
	5.2
	32
	9.5

	Eagle Lake
	1400
	4/01/10
	46
	13.0
	35
	9.0
	42
	12.7

	Grandview     
	1100
	3/31/10
	132
	41.6
	105
	28.9
	83
	28.0

	Grouse Creek Divide
	700
	3/31/10
	62
	20.8
	44
	10.8
	58
	19.5

	Jean Lake   
	620
	3/31/10
	17
	4.0
	14
	1.9
	15
	4.0

	Kachemak Creek
	1660
	3/31/10
	75
	25.6
	38
	12.9
	---
	---

	Kenai Moose Pens    
	300
	3/28/10
	16
	3.8
	19
	5.0
	15
	4.1

	Kenai Summit
	1390
	3/26/10
	57
	18.5
	49
	11.4
	46
	14.3

	McNeil Canyon 
	1320
	3/31/10
	45
	15.4*
	30
	7.5
	38
	10.7

	Moose Pass  
	700
	3/26/10
	28
	9.1
	26
	5.5
	21
	7.1

	Nuka Glacier 
	1250
	3/31/10
	109
	40.7
	60
	21.1
	95
	39.5

	Pass Creek
	1200
	3/27/10
	35
	9.4
	33
	8.5
	32
	8.6

	Port Graham  
	300
	4/02/10
	37
	13.2
	31
	9.4
	20
	5.9

	Resurrection Pass
	2250
	3/27/10
	38
	10.8
	38
	9.0
	38
	10.9

	Snug Harbor Road 
	500
	3/31/10
	21
	7.1
	16
	4.0
	18
	5.1

	Summit Creek 
	1400
	3/26/10
	46
	13.5
	39
	9.1
	44
	12.1

	Turnagain Pass
	1880
	3/31/10
	149
	44.6
	107
	27.6
	106
	36.0


estimate*
STREAMFLOW FORECASTS

	Forecast Point
	Forecast 

 Period
	30- Yr Average  (1000AF)
	50 

Percentile
	% of 

Average
	Max

(1000AF)
	Min

(1000AF)

	Kenai River at Cooper Landing
	Apr-Jul
	925
	990
	107
	1110
	865


PRECIPITATION DATA 

            INCHES ACCUMULATED SINCE OCTOBER 1ST

	Precipitation

Gauge
	
	
	
	
	1971-2000
	% of

	
	Elevation (feet)
	Date
	This Year
	Last Year
	Ave
	Average

	Anchor River Divide
	1600
	3/31/10
	16.3
	13.6
	18.5
	88

	Cooper Lake
	1200
	3/31/10
	25.2
	23.6
	23.3
	109

	Grandview 
	1100
	3/31/10
	48.5
	33.3
	36.8
	132

	Grouse Creek Divide 
	 700
	3/31/10
	41.7
	30.2
	35.3
	118

	Kachemak Creek
	1660
	3/31/10
	44.4
	25.4
	39.4
	112

	Kenai Moose Pens 
	 300
	3/31/10
	5.7
	8.8
	  8.2
	70

	McNeil Canyon   
	1320
	3/31/10
	16.6
	12.2
	15.7
	106

	Middle Fork Bradley**
	2300
	3/31/10
	32.3
	25.7
	34.6
	93

	Nuka Glacier**    
	1250
	3/31/10
	46.6
	26.7
	54.7
	85

	Port Graham
	300
	3/31/10
	45.6
	33.0
	40.1
	114

	Summit Creek      
	1400
	3/31/10
	17.2
	15.4
	16.2
	106

	Turnagain Pass    
	1880
	3/31/10
	47.1
	29.6
	39.8
	119


**Wyoming shielded gauge


WATERSHED SNOWPACK ANALYSIS

	Region / River Basin
	No. of Courses Averaged
	Percent of Last Year
	Percent of Average

	Bradley Lake/Southern Kenai Peninsula
	2
	170
	109

	Ninilchik Dome
	5
	189
	113

	Northern Kenai Mountains
	13
	153
	121

	Northern Kenai Flats
	1
	58
	71


WESTERN GULF(
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Current Basin Conditions


Western Gulf

SNOWPACK DATA

	
	THIS YEAR
	LAST YEAR
	1971-2000 AVERAGE

	Snow Course
	Elev.
	Date
	Snow

Depth
	Water

Content
	Snow

Depth
	Water

Content
	Snow Depth
	Water

Content

	
	(feet)
	
	(inches)


	Exit Glacier 
	400
	3/31/10
	56
	20.2
	47
	12.5
	57
	15.9

	Grouse Creek Divide
	700
	3/31/10
	65
	20.8
	44
	10.8
	58
	19.5

	Lowe River  
	600
	3/30/10
	58
	18.0
	43
	12.1
	54
	17.1

	Mt. Eyak
	1405
	3/31/10
	85
	34.4
	75
	23.3
	75
	24.2

	Nuka Glacier  
	1250
	3/31/10
	109
	40.7
	60
	21.1
	95
	39.5

	Sugarloaf Mountain 
	550
	3/31/10
	84
	27.5*
	78
	27.8
	87
	28.0

	Tsaina River   
	1650
	3/30/10
	64
	17.9
	42
	12.4
	57
	17.6

	Upper Tsaina River
	1750
	3/31/10
	75
	22.2 
	50
	15.6
	70
	21.7

	Valdez      
	50
	3/30/10
	53
	16.4
	52
	15.5
	54
	17.8

	Worthington Glacier
	2100
	3/30/10
	85
	28.4
	65
	22.1
	72
	24.9


estimate*
PRECIPITATION DATA




INCHES ACCUMULATED SINCE OCTOBER 1ST

	Precipitation

Gauge
	
	
	
	
	1971-2000
	% of

	
	Elevation (feet)
	Date
	This Year
	Last Year
	Ave
	Average

	Esther Island
	50
	3/31/10
	79.9
	72.7
	81.7
	98

	Grouse Creek Divide 
	700
	3/31/10
	41.7
	30.2
	35.5
	118

	Mt. Eyak
	1405
	3/31/10
	60.8
	56.0
	67.5
	90

	Nuka Glacier**  
	1250
	3/31/10
	46.6
	26.7
	54.7
	85

	Port San Juan
	50
	3/31/10
	84.7
	56.0
	75.5
	113

	Seal Island
	30
	No Report
	
	34.4
	40.4
	---

	Strawberry Reef
	50
	3/31/10
	39.2
	38.2
	46.7
	84

	Sugarloaf Mountain
	550
	3/31/10
	37.9
	39.2
	40.5
	94

	Tatitlek
	50
	No Report
	
	41.3
	38.4
	---

	Upper Tsaina River
	1750
	3/31/10
	20.8
	24.5
	26.8
	78


**Wyoming shielded gauge

*Copper Valley Electric Association

WATERSHED SNOWPACK ANALYSIS

	Region / River Basin
	No. of Courses Averaged
	Percent of Last Year
	Percent of Average


	Lowe River (Valdez)
	4
	115
	101

	Eyak Lake
	1
	148
	142


SOUTHEAST(
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Snowcover:


SOUTHEAST

SNOWPACK DATA

	
	THIS YEAR
	LAST YEAR
	1971-2000 AVERAGE

	SNOW COURSE
	ELEV.
	DATE
	SNOW

DEPTH
	WATER

CONTENT
	SNOW DEPTH
	WATER

CONTENT
	SNOW DEPTH
	WATER

CONTENT

	Cropley Lake
	1650
	3/30/10
	87
	30.9
	125
	42.0
	81
	30.3

	Eagle Crest  
	1200
	3/30/10
	49
	19.4
	110
	30.1
	54
	18.5

	Fish Creek  
	500
	3/30/10
	0
	0.0
	43
	14.6
	19
	6.2

	Institute Creek
	1350
	4/02/10
	28
	10.9
	New
	
	
	

	Lake Grace Pass
	1900
	No Report
	
	
	152
	57.5
	118
	45.5

	Long Lake
	850
	4/02/10
	99
	39.8
	137
	49.9
	110
	44.1

	Lost Lake
	425
	No Report
	
	
	67
	25.5
	39
	15.0

	Mint Creek Ridge
	1900
	No Report
	
	
	137
	44.5
	117
	43.6

	Moore Creek Bridge 
	2250
	3/31/10
	71
	22.6
	71
	25.8
	73
	20.0

	Petersburg Reservoir
	550
	3/30/10
	0
	0.0
	69
	21.5
	15
	6.2

	Petersburg Ridge
	1650
	3/30/10
	71
	28.5
	127
	40.8
	71
	26.4

	Rainbow Falls
	500
	4/02/10
	0
	0.0
	New
	
	
	

	Speel River
	280
	3/28/10
	64
	23.2
	132
	48.0
	78
	31.1

	Upper Swan Lake
	1700
	No Report
	
	
	87
	30.7
	60
	23.1

	West Creek
	470
	No Report
	
	
	38
	12.8
	---
	---

	Upper Silvas
	2300
	No Report
	
	
	---
	---
	---
	---


STREAMFLOW FORECASTS

	   FORECAST POINT
	FORECAST 

 PERIOD
	30- YR AVERAGE  (1000AF)
	50 

PERCENTILE
	% OF 

AVERAGE
	MAX

(kaf)
	MIN

(kaf)

	Gold Creek near Juneau
	Apr- Jul
	33
	33
	100
	41
	25


PRECIPITATION DATA
INCHES ACCUMULATED SINCE OCTOBER 1ST

	Precipitation

Gauge
	
	
	
	
	71-2000
	% of

	
	Elev.
	Date
	This Year
	Last Year
	Ave
	Average

	Long Lake
	850
	4/02/10
	84.5
	97.6
	  96.4
	88

	Moore Creek Bridge
	2250
	3/30/10
	30.9
	23.5
	  26.8
	109

	Snettisham   
	25
	3/31/10
	85.6
	130.1
	106.8
	80

	Swan Lake  
	50
	No Report
	
	101.7
	  88.2
	---


WATERSHED SNOWPACK ANALYSIS

	REGION / RIVER BASIN
	# COURSES AVERAGED
	PERCENT OF LAST YEAR
	PERCENT OF AVERAGE

	Douglas Island
	3
	58
	91

	Long Lake
	2
	64
	84

	Petersburg
	2
	46
	87

	Swan Lake
	No Report
	
	


For further information contact:

NRCS Alaska web site:  www.ak.nrcs.usda.gov/snow/

Alaska Meteor Burst Communication System (AMBCS) web site:  www.ambcs.org
NRCS Anchorage Support Staff

510 L Street, Suite 270

Anchorage, Alaska  99501-1949

Telephone (907) 271-2424, Extension 113; 

Facsimile (907) 271-3951; or e-mail:  Richard.McClure@ak.usda.gov

Copper Center Field Office

Catherine Hadley, District Conservationist

Telephone:  (907) 822-4484  

Facsimile:  (907) 822-4489

e-mail:  Catherine.Hadley@ak.usda.gov

Delta Junction Field Office

Catherine Hadley, District Conservationist

Telephone (907) 895-4241 x 103

Facsimile:  (907) 895-5003

e-mail:  Catherine.Hadley@ak.usda.gov

Fairbanks Field Office

Joanne Kuykendall, District Conservationist

Telephone (907) 479-3159 x 110

Facsimile:  (907) 479-6998

e-mail:  Joanne.Kuykendall@ak.usda.gov

Homer Field Office

Mark Kinney, District Conservationist

Telephone (907) 235-8177 x 103

Facsimile:  (907) 235-2364

e-mail:  Mark.Kinney@ak.usda.gov

Mat-Su Field Office

District Conservationist, Keith Griswold
Telephone (907) 373-6492 x 101

Facsimile:  (907) 373-7192

e-mail:  Keith.Griswold@ak.usda.gov
The large central basin is comparable to last month and varies from below normal in the eastern part to much below normal in the western part of the basin.  The Mission Creek snow course was measured at 61 percent of normal.


The Coal Creek snow course in the Yukon Charlie National Park has 16 inches of snow depth with 2.7 inches of water content.  


The Forty Mile basin received little snow and is 70 percent of average, exemplified by the Boundary snow course which is 77 percent of average.  


In Canada, the Porcupine River basin is 91 percent of normal with the Old Crow snow course at 117 percent.  Eagle Plains and Eagle River are in the 85 percent of average range.


The Upper Nome Creek SNOTEL site has 14 inches of snow and an estimated 2.9 inches of water content, near 55 percent of average. 


The four White Mountains snow courses are 63 percent of average.








The regions north and west of the Alaska Range generally received less than average precipitation for the month of March.  Indicative, Chandalar Camp, which located just south of Atigun Pass, received 0.6 inches of precipitation in March, 0.7 inches is normal.  The site’s precipitation gauge has received 3.1 inches since October 1st, 58 percent of normal.  However, the Granite Creek SNOTEL site, southeast of Delta Junction, received 0.3 inches which is right at normal for the month.  It has received 3.6 inches of precipitation since October 1st, 116 percent of normal.


In South Central, the Moraine SNOTEL site received an above normal amount for the month, it received 2.7 inches of precipitation with average being 1.2 inches.  The total for the year since October 1st is 12.0, 124 percent of normal.  The Independence Mine SNOTEL site 30 miles to the north across the Matanuska Valley received .9 inches for the month and 11.0 inches of precipitation since October 1st, 61 percent of average.  The Grandview SNOTEL sites received 13.0 inches for the month, normal is 5.4 inches.  Southeast Alaska received more than normal precipitation as indicated at the Snettisham Hydro-electric power plant receiving 18.0 inches, normal is 11.6 inches.








The temperatures were below normal on the west, southwest coast and south to Homer.  Nome was 7 deg F below normal, Bethel was 10 deg F below, Dillingham was 5 deg F below and Homer was 2 deg F below normal.   Anchorage was right at normal for the month with a low of negative 3 deg F the 10th of the month and a high of 43 deg F each day for the last 3 days of the month.  Fairbanks was 1 deg F above normal for the month with a low of negative 25 deg F on the 13th and a high of 48 deg F on the 28th.  Juneau was 3 deg F above normal for the month with a low of 25 deg F on the 8th and a high of 47 deg F on the 29th.








The snowpack across the state is similar to last month with the regions north of the Alaska Range just below average near the Canadian border to minimum of records along the Dalton Highway south of the Brooks Range in the upper Koyukuk basin.


The large Central Yukon and Tanana basins vary from near normal in the eastern part to much below normal in the western part of the basin.  The Chena basin is 47 percent of average.  One snow course, Little Chena Bottom has a record low of 9 inches of depth with 1.2 inches of water content.  The previous low was 1.6 inches in 1981.  


Four snow courses in the upper Koyukuk basin have record low snow water contents.  Starting in the north is Table Mountain with 1.6 inches of snow water content, previous record low was 2.3 inches set in 2007.  To the south and west of Bettles, Lake Todatonten has 2.2 inches of snow water content, the previous low was 3.1 in 2007.  On the Dalton Highway, the Bonanza Forks and Thirty Mile snow courses have had wild fires disturbing or removing the vegetation at the snow courses in 2004 and 2005 respectively.  Both of the water contents are lower than the previous record low set for both courses in 2007.


South of the Alaska Range, the Northern Kenai Mountains had a significant increase in snowpack and water content, the 13 snow courses are 121 percent of average, up from 98 percent last month.  They range from 99 percent of normal at Resurrection Pass to 149 percent of normal at Grandview.  Grandview SNOTEL site has 132 inches (11 feet) of snow depth with 41.6 inches of water content.


Southeast Alaska received significant snow above 800 feet of elevation in March.  The Long Lake SNOTEL site, 60 miles southeast of Juneau in the Snettisham Hydro-electric project watershed, is reporting 99 inches of snow and 39.8 inches of water content which is 90 percent of average, up from 78 percent last month. 




















The Tanana basin remains very similar to last month being near normal in the southeast to much, much below normal in the western portion of the basin.


In the upper Tanana basin, the Chisana SNOTEL site is reporting 92 percent of average water content and the Tok snow course measured 86 percent of average water content.  Beaver Creek snow course in the Yukon Territories is 97 percent of average.


For the Delta Junction area and south, the Fielding Lake snow course is 50 percent of average and Granite Creek is 101 percent of average.


For the lower Tanana valley, French Creek is 38 percent of average and Bonanza Creek is 44 percent of average.  The combined 7 snow courses in the lower basin are 38 percent of average.


The Chena basin is 47 percent of average.  One snow course, Little Chena Bottom has a record low of 9 inches of depth with 1.2 inches of water content.  The previous low was 1.6 inches in 1981.  The Chatanika basin is 54 percent of average.





























The snow water contents in the south and east side of the basin are near or above average with Worthington Glacier near Thompson Pass at 114 percent of normal. The Upper Tsaina River SNOTEL site has 76 inches of snow depth with 22.2 inches of water content, 102 percent of normal.   The Kenny Lake snow course is now below average with 16 inches of snow depth and 3.2 inches of water content, 86 percent of average.


The Basin Floor average of 6 snow courses is 79 percent ranging from 93 percent of average at Tazlina to 65 percent of average at Haggard Creek.  The Chugach Range is 101 percent of average, up 12 percent from last month.  The Alaska Range dropped 4 percent from last month and is 52 percent of normal with the snow course Fielding Lake at 50 percent of normal.  To the west, the Talkeetna Mountains are 91 percent of normal water content.  The four Wrangell Mountain snow courses are 89 percent of average with the Dadina Lake and Sanford River both being 90 percent of average.


The expected volume flow for the Gulkana River at Sourdough for the April through July time period is 315,000 acre-feet, 66 percent of average.











The Northern Cook Inlet region varies from 54 percent of average at Granite Point, near Tyonek, to 138 percent of average at Moraine.  The Moraine SNOTEL site, in the Eklutna watershed, has 40 inches of snow depth with 11.0 inches of water content.  The Granite Point snow course has 10 inches of snow depth with 3.0 inches of water content.


For the SNOTEL sites in the Anchorage area; Indian Pass is 83 percent of average with 58 inches of snow and 19.6 inches of water content, Anchorage Hillside is 100 percent of average reporting 38 inches of snow with 10.4 inches of water content and Mt. Alyeska has 111 inches of snow and 35.5 inches of water content, which is 97 percent of average, up 18 percent from last month.


For the west side of Cook Inlet, the Beluga aerial markers are 73 percent of average with 49 inches of snow at Chuitna Plateau and 79 inches of snow at Lone Ridge.  The Congahbuna Lake snow course has 24 inches of snow depth with 7.5 inches of water content, 69 percent of average.


The Portage snow course received significant snow in March with 58 inches and 21.6 inches of snow water content being measured, 144 percent of normal.  Last month there was 27 inches with 10.0 inches of water content.


The expected volume flow from snowmelt runoff for the Ship Creek near Anchorage for the April through July time frame is 54,000 acre-ft, 93 percent of average.








The Brooks Camp aerial marker has 8 inches of snow depth, up 2 inches from last month. The Three Forks aerial marker has 6 inches of snow depth, down an inch from last month.






































Four snow courses in the upper Koyukuk basin have record low snow water contents.  Starting in the north is Table Mountain with 1.6 inches of snow water content, previous record low was 2.3 inches set in 2007.  To the south and west of Bettles, Lake Todatonten has 2.2 inches of water content, the previous low was 3.1 in 2007.  On the Dalton Highway, the Bonanza Forks and Thirty Mile snow courses have had wild fires disturbing or removing the vegetation at the snow courses in 2004 and 2005 respectively.  Both of the water contents are lower than the previous record low set for both courses in 2007.


Near Galena, the Colville Bend snow course has 15 inches of snow depth, last year there was 33 inches.  This is a similar ratio for the snow courses in the lower Koyukuk and Yukon area near Galena.








The Lake Minchumina snow course has 1.7 inches of snow water content, the 2nd lowest year, the low is 1.5 inches measured in 2004.  The McGrath snow course has 19 inches of snow with 3.5 inches of water content, 54 percent of normal.  The Telaquana Lake snow course has 10 inches of snow depth with 2.2 inches of snow water content, 49 percent of average. 











The Tozikaket snow course is a record low 28 percent of average with 1.4 inches of snow water content, the previous record of 2.2 inches was measured in 2007.


The snow courses in the Innoko Wildlife Refuge are around 65 percent of normal, varying from 39 inches of snow depth at Holikachuk to 20 inches at the Innoko Inn.  











The Atigun Pass SNOTEL site has received 5.3 inches of precipitation since October 1st or 65 percent of average.  It has 25 inches of snow on the ground.  The Imnaviat Creek SNOTEL site has received 2.8 inches of precipitation, 72 percent of normal.  











The Red Dog mine precipitation gauge received 2.3 inches of precipitation since October 1st, 36 percent of normal.  




















The Kenai Peninsula received significant snow in March.  The Northern Kenai Mountains had a significant increase in snowpack with all snow courses going up in water content and the 13 snow courses are 121 percent of average, up from 98 percent last month.  They range from 99 percent of normal at Resurrection Pass to 149 percent of normal at Grandview.  Grandview SNOTEL site has 132 inches (11 feet) of snow depth with 41.6 inches of water content.


 Northeast of Homer, the Anchor River Divide SNOTEL site reported 40 inches of snow depth with 14.0 inches of water content, and is 111 percent of average.


Across Kachemak Bay from Homer, Port Graham SNOTEL site has 37 inches of snow with 13.2 inches of snow water content, and is 129 percent of average.


In the Bradley Lake Hydro-electric power watershed, the Nuka Glacier SNOTEL site has 109 inches of snow depth with 40.7 inches of water content, up approximately 19 inches of water content from last month, and currently is 103 percent of average. The Kachemak Creek SNOTEL site has 75 inches of snow with 25.6 inches of water content.  The Middle Fork Bradley SNOTEL site has received 32.3 inches of precipitation since October 1st, 93 percent of average.


The expected volume flow from snowmelt runoff for the Kenai River at Cooper Landing for the April through July time frame is 990,000 acre-ft, 107 percent of average, up 11 percent from last month.

















The Susitna Basin snow courses range from below average to well below average.  The 11 snow courses in the Upper Susitna Basin are below average at 65 percent. Snow water contents range from 48 percent of average at the Fog Lakes snow course to 82 percent of average at the Upper Oshetna River snow course.


For the Lower Susitna snow courses, the west side of the basin is below average as indicated by Alexander Lake which measured 10.0 inches of snow water content, 83 percent of average. The east side of the basin along the Parks Highway is well below average with the SNOTEL site at Susitna Valley High reporting 6.2 inches of water content, only 54 percent of average.


The Peter Hills snow courses are 59 percent of average with Nugget Bench at 67 percent of average and the Dutch Hills aerial marker showing 45 inches of snow with an estimated 14.0 inches of water content, 51 percent of average.  This is a record low water content with the previous low being 14.1 inches measured in 1996.


The Hatcher Pass snow courses vary from 48 percent of average at the Independence Mine snow course to 62 percent of average at the Little Susitna snow course.


The Sheep Mountain snow course water content is 6.3 inches, 105 percent of average.


The Snowmelt Runoff Index for the Deshka River at mouth near Willow is -2.2, much below average snowmelt runoff.























The snow course water contents vary from 143 percent of average in the Yukon basin above White River to 57 percent of average in the Stewart/Pelly basin.   The snow course in the White River basin, Mount Nansen, has the same water content as last year.  The low snow course is Mayo Airport located in the Stewart/Pelly basin. The Stewart/Pelly basin is up 1 percent from last month to 79 percent of average.  


The Dawson region is up from 74 percent last month to 100 percent of normal and the White River basin is 110 percent of normal.  


The Whitehorse/Teslin basin is 112 percent of average, the Log Cabin snow course went up 3.7 inches of water content or 13 percent, to 115 percent or normal.


The expected volume flow from snowmelt runoff for the Yukon River at Eagle for the April through July time frame is 31,300,000 acre-ft, 92 percent of average.
































In March, Southeast Alaska received significant snow above 800 feet of elevation.  The Eagle Crest snow course has 49 inches of snow with 19.4 inches of water content, up 7.3 inches of water content from last month.


The Long Lake SNOTEL site, 60 miles southeast of Juneau in the Snettisham Hydro-electric project watershed, is reporting 99 inches of snow and 39.8 inches of water content, which is 90 percent of average. 


The Petersburg Reservoir snow course has no snow while the Petersburg Ridge snow course has 71 inches with 28.5 inches of water content, 108 percent of average water content.


The Moore Creek Bridge snow course, north of Skagway, has 71 inches of snow depth with 22.6 inches of water content, 113 percent of average.  The precipitation received at Moore Creek since October 1st is 29.1 inches, 109 percent of average.


























































































































Two new snow survey sites have been measured this year on the Kwethluk River, Upper and Lower Kwethluk east of Bethel.  Both snow courses had 4 inches of snow on them the 16th of March.  Neither site has seen more than 4 inches this winter having been measured 4 times to date. 

















The Rocky Point SNOTEL site has 14 inches of snow on the ground and an estimated 2.6 inches of water content. The Johnson Camp SNOTEL site, in the “blow hole” at Solomon, 30 miles east of Nome, has 5 inches of snow on the ground as of March 31st, last year there was 26 inches of snow depth.





























The SNOTEL site at Mt. Eyak is above average, reporting 85 inches of snow depth and 34.4 inches of snow water content, up 9.0 inches of water content from last month.


Sugarloaf Mountain SNOTEL site is at 550 feet of elevation, perched above the Solomon Gulch Hydroelectric and the town of Valdez, and reported 84 inches of snow depth and an estimated 27.5 inches of water content, 95 percent of average.  The precipitation gauge has caught 37.9 inches since October 1st, which is 94 percent of average.


The Esther Island precipitation gauge has caught 79.9 inches of precipitation since October 1st 98 percent of average with 15.0 inches being caught in the month of March.


The Strawberry Reef SNOTEL site, located east of Cordova, is 84 percent of average and has caught 37.9 inches of water since October 1st.
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( See regional summaries for the forecast period and the actual forecasted flow volumes.





( For further information contact the Natural Resources Conservation Service in Anchorage.


( For further information contact the Natural Resources Conservation Service in Fairbanks.


( For further information contact the Natural Resources Conservation Service in Fairbanks or Delta Junction.


( For further information contact the Natural Resources Conservation Service in Anchorage.


( For further information contact the Natural Resources Conservation Service in Anchorage.


( For further information contact the Natural Resources Conservation Service in Anchorage.


( For further information contact the Natural Resources Conservation Service in Anchorage.


( For more information contact the Natural Resources Conservation Service in Copper River, Delta Junction or Anchorage. 





( For more information contact the Natural Resources Conservation Service in Wasilla.





( For more information contact the Natural Resources Conservation Service in Homer.


( For more information contact the Natural Resources Conservation Service in Copper Center.


( For further information contact the Natural Resources Conservation Service in Anchorage.
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