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GENERAL OVERVIEW

Snowpack

Precipitation


Temperature



STREAMFLOW
Streamflow forecasts of snowmelt runoff are as follows:                            

	FORECAST POINT(
	Percent of Ave. Flow
	Period

	Yukon River at Eagle

	89
	April - July

	Porcupine River nr Int’l Boundary…………………
	83
	

	Yukon River near Stevens Village

	88
	April - July

	Tanana River at Fairbanks

	88
	April - July

	Tanana River at Nenana

	82
	April - July

	Little Chena River near Fairbanks

	68
	April - July

	Chena River near Two Rivers

	66
	April - July

	Salcha near Salchaket

	74
	April - July

	Sagvanirktok River near Pump Station 3

	83
	April - July

	Kuparuk River near Deadhorse

	76
	April - July

	Kuskokwim River at Crooked Creek

	76
	April - June

	Gulkana River at Sourdough

	69
	April - July

	Little Susitna River near Palmer

	64
	April - July

	Talkeetna River near Talkeetna

	77
	April - July

	Ship Creek near Anchorage

	83
	April - July

	Kenai River at Cooper Landing

	96
	April - July

	Gold Creek near Juneau

	91
	April - July

	SNOWMELT RUNOFF INDEX (SRI)
For streams that no longer have stream gauging stations.

	FORECAST POINT
	INDEX
	
	  Index
-2  to  -3

-1  to  -2

-1  to +1

+1 to +2

+2 to +3


	Key:

much below average snowmelt runoff

below average snowmelt runoff

average snowmelt runoff

above average snowmelt runoff

much above average snowmelt runoff

	Koyukuk River at Hughes

	-3.0
	
	
	

	MF Koyukuk R near Wiseman …………………………
	-2.8
	
	
	

	Slate Creek at Coldfoot…………………………………
	-2.7
	
	
	

	Beaver Creek above Victoria Creek

	-3.0
	
	
	

	Birch Creek below South Fork

	-2.5
	
	
	

	Caribou Creek at Chatanika

	-1.8
	
	
	

	Susitna River near Gold Creek

	-2.2
	
	
	

	Chulitna River near Talkeetna

	-3.0
	
	
	

	Deshka River at mouth near Willow

	-2.4
	
	
	

	Montana Creek at Parks Highway

	-2.0
	
	
	

	Willow Creek near Willow

	-2.3
	
	
	

	Skwentna River at Skwentna

	-1.4
	
	
	

	Chuitna River near Tyonek

	-1.5
	
	
	

	Campbell Creek near Spenard

	-1.6
	
	
	

	Indian Creek at Indian

	-2.2
	
	
	

	Bird Creek at Bird Creek

	-2.2
	
	
	

	Glacier Creek nr Girdwood …………………………….
	+0.3
	
	
	

	Six Mile Creek near Hope

	+0.7
	
	
	

	Resurrection Creek near Hope

	+0.3
	
	
	

	Grouse Ck at Grouse Lake Outlet nr Seward ………..
	-1.0
	
	
	

	Anchor River near Anchor Point

	+0.2
	
	
	

	Deep Creek  near Ninilchik

	-0.7
	
	
	

	Ninilchik River near Ninilchik

	-0.9
	
	
	

	Fritz Creek near Homer…………………………………
	+0.8
	
	
	

	Skagway River at Skagway

	+0.8
	
	
	

	Municipal Watershed C nr Petersburg ………………..
	-1.2
	
	
	


HOW FORECASTS ARE MADE

Most of the annual streamflow in the western United States originates as snowfall that has accumulated in the mountains during the winter and early spring.  As the snowpack accumulates, hydrologists estimate the runoff that will occur when it melts.  Measurements of snow water equivalent at selected manual snow courses and automated SNOTEL sites, along with precipitation, antecedent streamflow, and indices of the El Niño / Southern Oscillation are used in computerized statistical and simulation models to prepare runoff forecasts.  These forecasts are coordinated between hydrologists in the Natural Resources Conservation Service and the National Weather Service.  Unless otherwise specified, all forecasts are for flows that would occur naturally without any upstream influences.

Forecasts of any kind, of course, are not perfect.  Streamflow forecast uncertainty arises from three primary sources:  (1) uncertain knowledge of future weather conditions, (2) uncertainty in the forecasting procedure, and (3) errors in the data.  The forecast, therefore, must be interpreted not as a single value but rather as a range of values with specific probabilities of occurrence.  The middle of the range is expressed by the 50% exceedance probability forecast, for which there is a 50% chance that the actual flow will be above, and a 50% chance that the actual flow will be below, this value.  To describe the expected range around this 50% value, four other forecasts are provided, two smaller values (90% and 70% exceedance probability) and two larger values (30%, and 10% exceedance probability).  For example, there is a 90% chance that the actual flow will be more than the 90% exceedance probability forecast.  The others can be interpreted similarly.

The wider the spread among these values, the more uncertain the forecast.  As the season progresses, forecasts become more accurate, primarily because a greater portion of the future weather conditions become known; this is reflected by a narrowing of the range around the 50% exceedance probability forecast.  Users should take this uncertainty into consideration when making operational decisions by selecting forecasts corresponding to the level of risk they are willing to assume about the amount of water to be expected.  If users anticipate receiving a lesser supply of water, or if they wish to increase their chances of having an adequate supply of water for their operations, they may want to base their decisions on the 90% or 70% exceedance probability forecasts, or something in between.  On the other hand, if users are concerned about receiving too much water (for example, threat of flooding), they may want to base their decisions on the 30% or 10% exceedance probability forecasts, or something in between.  Regardless of the forecast value users choose for operations, they should be prepared to deal with either more or less water.  (Users should remember that even if the 90% exceedance probability forecast is used, there is still a 10% chance of receiving less than this amount.)  By using the exceedance probability information, users can easily determine the chances of receiving more or less water.

UPPER YUKON BASIN(
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Snow Course:

Upper Yukon Basin

	
	THIS YEAR
	LAST YEAR
	   1971-2000 AVERAGE

	SNOW COURSE
	ELEV.
	DATE
	SNOW

DEPTH
	WATER

CONTENT
	SNOW DEPTH
	WATER

CONTENT
	SNOW DEPTH
	WATER

CONTENT

	Arrowhead Lake  
	3680
	2/25/10
	26
	4.8
	---
	---
	32
	6.6

	Atlin         
	2400
	No Survey
	
	
	24
	5.6
	21
	4.4

	Beaver Creek 
	2150
	2/23/10
	15
	2.1
	26
	3.9
	17
	2.9

	Burns Lake  
	3650
	2/26/10
	33
	5.5
	44
	9.4
	33
	7.4

	Burwash Airstrip 
	2660
	2/23/10
	10
	1.7
	10
	1.2
	10
	1.6

	Calumet     
	4300
	2/24/10
	27
	4.3
	34
	6.3
	33
	6.7

	Casino Creek  
	3500
	2/23/10
	21
	3.0
	29
	4.9
	24
	4.0

	Chair Mountain 
	3500
	No Survey
	
	
	---
	---
	19
	3.3

	Duke River   
	4800
	3/02/10
	19
	3.8
	21
	4.6
	21
	3.7

	Edwards Lake   
	2720
	2/25/10
	23
	4.5
	31
	6.1
	29
	5.9

	Finlayson Airstrip
	3240
	2/26/10
	18
	4.2
	30
	5.7
	26
	4.5

	Fuller Lake  
	3700
	2/26/10
	33
	6.8
	34
	6.7
	29
	6.0

	Grizzly Creek  
	4000
	2/25/10
	26
	4.3
	28
	5.1
	22
	4.1

	Hoole River 
	3560
	2/26/10
	23
	4.6
	41
	7.9
	23
	4.6

	Jordan Lake    
	3050
	2/26/10
	24
	4.9
	35
	7.7
	24
	4.7

	King Solomon Dome
	3550
	2/24/10
	24
	4.2
	28
	5.2
	29
	5.9

	Log Cabin (B.C.) 
	2880
	2/25/10
	43
	13.1
	59
	17.9
	47
	12.8

	Mayo Airport 
	1620
	2/24/10
	17
	2.0
	20
	4.1
	18
	3.1

	MacIntosh    
	3800
	2/23/10
	22
	3.9
	24
	3.4
	19
	3.6

	Meadow Creek  
	4050
	2/24/10
	42
	10.8
	53
	12.2
	38
	9.0

	Midnight Dome 
	2800
	2/24/10
	24
	4.3
	26
	5.0
	27
	5.3

	Montana Mountain
	3340
	2/25/10
	23
	5.6
	31
	6.4
	24
	5.1

	Morley Lake  
	2700
	3/02/10
	19
	4.1
	---
	---
	24
	5.3

	Mount Nansen  
	3250
	2/23/10
	20
	3.0
	20
	2.7
	16
	2.6

	Mt. Berdoe  
	3390
	2/23/10
	26
	5.0
	30
	3.6
	21
	3.7

	Mt. McIntyre B 
	3700
	3/01/10
	28
	6.6
	35
	7.6
	26
	5.2

	Pelly Farm 
	1550
	2/23/10
	11
	1.9
	---
	---
	17
	3.0

	Plata Airstrip 
	2500
	2/25/10
	28
	5.1
	29
	6.1
	30
	6.4

	Rackla Lake   
	3410
	2/25/10
	30
	5.5
	33
	6.7
	33
	7.0

	Russell Lake  
	3480
	2/25/10
	31
	6.7
	39
	8.1
	36
	7.0

	Satasha Lake  
	3620
	2/23/10
	20
	3.2
	26
	3.6
	21
	3.8

	Tagish       
	3540
	2/24/10
	27
	5.0
	31
	7.2
	24
	4.8

	Twin Creeks   
	2950
	2/26/10
	26
	4.7
	39
	8.5
	31
	6.6

	White River  
	2500
	No Survey
	
	
	---
	---
	15
	2.4

	Whitehorse Airport
	2300
	3/02/10
	16
	3.2
	30
	6.6
	18
	3.5

	Williams Creek 
	2800
	2/23/10
	21
	3.8
	26
	5.3
	18
	3.0

	Withers Lake   
	3200
	2/23/10
	30                                                                                                                           
	6.2
	35
	8.4
	36
	8.2


STREAMFLOW FORECASTS

	   FORECAST POINT
	FORECAST 

 PERIOD
	30- YR AVERAGE  (1000AF)
	50 

PERCENTILE
	% OF 

AVERAGE
	MAX

(kaf)
	MIN

(kaf)

	Yukon River At Eagle
	Apr- Jul
	34200
	30600
	89
	104
	75


WATERSHED SNOWPACK ANALYSIS

	REGION / RIVER BASIN
	# COURSES AVERAGED
	PERCENT OF LAST YEAR
	PERCENT OF AVERAGE

	Above Whitehorse/ Tetlin
	9
	72
	107

	Dawson
	3
	84
	74

	Stewart/ Pelly
	14
	71
	79

	White River
	8
	92
	101


   CENTRAL YUKON BASIN(
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Snowcover:


Central Yukon Basin

SNOWPACK DATA

	
	THIS YEAR
	LAST YEAR
	1971-2000 AVERAGE

	SNOW COURSE
	ELEV.
	  DATE
	SNOW

DEPTH
	WATER

CONTENT
	SNOW DEPTH
	WATER

CONTENT
	SNOW DEPTH
	WATER

CONTENT


	Borealis
	1330
	2/26/10
	15
	2.6
	23
	4.0
	27
	4.4

	Boundary
	3500
	3/02/10
	21
	4.0
	22
	5.1
	24
	4.6

	Cathedral Creek
	1800
	2/28/10
	16
	2.5
	21
	3.8
	---
	---

	Chicken Airstrip
	1650
	3/01/10
	12
	2.1
	18
	3.1
	16
	2.7

	Circle Hot Springs
	860
	2/26/10
	20
	2.7
	25
	4.4
	22
	3.7

	Coal Creel
	1000
	2/28/10
	16
	2.4
	21
	3.7
	---
	---

	Copper Creek
	2000
	2/28/10
	17
	2.5
	17
	2.9
	---
	---

	Cresent  Creek
	2600
	2/28/10
	16
	2.3
	16
	2.7
	---
	---

	Eagle Plains
	2570
	2/25/10
	27
	4.6
	30
	5.7
	29
	5.9

	Eagle River
	1200
	2/25/10
	22
	3.2
	26
	4.0
	26
	4.5

	Fort Yukon
	430
	2/27/10
	16
	2.5
	18
	3.7
	19
	3.2

	Fossil       
	1400
	2/26/10
	13
	2.0
	20
	3.3
	28
	4.5

	Graphite Lake
	600
	No Survey
	
	
	---
	---
	17
	2.8

	Hess Creek   
	1000
	2/22/10
	18
	3.2
	---
	---
	25
	4.8

	Lost Chicken Hill
	2100
	3/02/10
	14
	2.3
	18
	3.4
	18
	3.1

	Lower Beaver Creek
	400
	3/03/10
	21
	3.0
	---
	---
	---
	---

	Mission Creek   
	900
	No Report
	
	
	13
	2.3
	18
	3.6

	Mt. Fairplay
	3100
	3/02/10
	17
	4.2
	19
	3.5
	20
	3.8

	Old Crow
	840
	3/01/10
	25
	4.5
	33
	6.0
	24
	3.9

	Riff's Ridge
	2130
	2/25/10
	29
	4.6
	29
	5.2
	27
	5.1

	Seven Mile
	600
	2/25/10
	18
	2.6
	---
	---
	26
	4.6

	Stack Pup Creek
	1620
	2/26/10
	19
	2.6
	26
	4.2
	24
	3.7

	Step Mountain
	2850
	2/28/10
	16
	2.4
	28
	4.7
	---
	---

	Thirty Mile    
	1350
	2/25/10
	18
	2.8
	---
	---
	35
	7.2

	Three Fingers
	3350
	2/25/10
	20
	2.7
	30
	5.0
	---
	---

	Vunzik Lake
	500
	3/03/10
	17
	2.6
	---
	---
	---
	---

	Upper Nome Creek
	2650
	2/28/10
	15
	2.6*
	24
	4.5
	---
	---

	Windy Gap    
	1900
	3/02/10
	16
	3.5
	24
	4.6
	29
	4.8

	Wolf         
	1200
	3/02/10
	12
	2.1
	18
	3.2
	26
	4.1


STREAMFLOW FORECASTS

	   FORECAST POINT
	FORECAST 

 PERIOD
	30- YR AVERAGE  (1000AF)
	50 

PERCENTILE
	% OF 

AVERAGE
	MAX

(kaf)
	MIN

(kaf)

	Porcupine River near Intl Boundary
	Apr-Jul
	5640
	4690
	83
	133
	60

	Yukon River near
Stevens Village
	Apr- Jul
	48200
	42400
	88
	103
	73


PRECIPITATION DATA





INCHES ACCUMULATED SINCE OCTOBER 1st

	Precipitation

 Gauge
	
	
	
	
	71-2000
	% of

	
	Elevation
	Date
	This Year
	Last Year
	Ave
	Average

	Atigun Pass**
	4800
	2/28/10
	3.7
	6.4
	7.1
	52

	Chandalar Shelf**  
	3300
	2/28/10
	2.5
	5.7
	4.6
	54

	Eagle Summit**
	3650
	2/28/10
	3.3
	4.5
	5.3
	62

	Fort Yukon      
	430
	2/28/10
	2.0
	3.6
	3.8
	53

	Mission Creek    
	900
	No Report
	
	4.4
	4.6
	---

	Upper Nome Creek
	2650
	2/28/10
	2.5
	4.8
	6.1
	41


**Wyoming Shielded Gauge

WATERSHED SNOWPACK ANALYSIS
	REGION / RIVER BASIN
	# COURSES AVERAGED
	PERCENT OF LAST YEAR
	PERCENT OF AVERAGE

	Forty Mile
	5
	83
	88

	Porcupine (Y.T.)
	4
	81
	87

	White Mountains
	6
	66
	59

	Yukon Flats
	6
	63
	65


TANANA  BASIN(
[image: image5.png]Water Equivalent, in.

Tanana Snowpack* (inches)

——Current  —+—Average

—&— Maximum  —e—Minimum

I A

7.0

6.0

5.0

4.0 /-

3.0

20

1.0

0.0

Feb Mar Apr May





[image: image6.png]Percent of Average

-2

Fairbanks Temperture

aMonthly

Oct Dec Feb Apr





Snowcover:


Tanana Basin

SNOWPACK DATA 

	
	THIS YEAR
	LAST YEAR
	1971-2000 AVERAGE

	SNOW COURSE
	ELEV.
	DATE
	SNOW

DEPTH
	WATER

CONTENT
	SNOW DEPTH
	WATER

CONTENT
	SNOW DEPTH
	WATER

CONTENT


	Bonanza Creek 
	1150
	3/01/10
	13
	1.7
	28
	4.6
	23
	4.7

	Caribou Creek      
	1250
	3/02/10
	13
	2.2
	22
	4.6
	24
	4.6

	Caribou Snow Pillow 
	900
	3/02/10
	14
	2.2
	25
	4.2
	24
	4.5

	Chisana
	3320
	2/28/10
	17
	3.1
	26
	4.9
	22
	3.4

	Cleary Summit      
	2230
	2/26/10
	20
	4.2
	27
	4.4
	29
	6.0

	Colorado Creek     
	700
	2/26/10
	18
	2.3
	21
	2.7
	23
	4.4

	Edgar Creek
	2400
	No Report
	
	
	---
	---
	27
	6.1

	Fairbanks FO
	450
	2/26/10
	12
	2.0
	25
	3.6
	23
	4.1

	Faith Creek                
	1900
	2/26/10
	14
	2.2
	22
	3.6
	27
	4.4

	Fielding Lake       
	3000
	2/27/10
	30
	5.8
	41
	9.6
	41
	10.2

	Fort Greely
	1500
	2/26/10
	18
	2.0
	15
	3.1
	18
	3.2

	French Creek 
	1800
	2/26/10
	14
	2.2*
	30
	5.4
	26
	5.9

	Gerstle River  
	1200
	2/26/10
	18
	1.6
	20
	2.8
	19
	3.0

	Gold King
	1700
	No Report
	
	
	---
	---
	21
	3.9

	Granite Creek      
	1240
	2/28/10
	14
	3.1
	22
	3.9
	19
	3.5

	Jatahmund Lake  
	2180
	3/01/10
	14
	2.2
	24
	4.1
	18
	2.9

	Kantishna 
	1550
	2/28/10
	14
	2.1*
	25
	4.4
	28
	5.3

	Lake Minchumina 
	730
	No Survey
	
	
	23
	3.5
	21
	4.0

	Little Chena Ridge
	2000
	2/28/10
	15*
	2.1
	23
	3.8
	27
	5.4

	Lost Creek
	3030
	No  Report
	
	
	17
	2.9
	26
	4.8

	Mentasta Pass     
	2430
	2/27/10
	23
	4.3
	26
	4.2
	26
	5.8

	Monument Creek
	1850
	2/28/10
	12*
	1.4
	23
	3.8
	24
	4.7

	Mt. Ryan
	2800
	2/28/10
	18*
	2.3
	26
	4.7
	30
	6.2

	Munson Ridge
	3100
	2/28/10
	25*
	4.4
	35
	6.8
	36
	8.3

	Paradise Hill 
	2200
	3/01/10
	14
	2.2
	21
	3.4
	18
	3.0

	Ptarmigan Airstrip
	2400
	No Report
	
	
	---
	---
	17
	3.1

	Ptarmigan Creek
	2230
	2/26/10
	18
	2.7
	24
	4.2
	17
	3.1

	Rock Creek Bottom
	2250
	3/01/10
	15
	1.8
	16
	3.2
	22
	4.2

	Rock Creek Ridge 
	2600
	3/01/10
	15
	1.8
	18
	3.8
	26
	4.9

	Shaw Creek Flats
	980
	2/26/10
	16
	1.7
	14
	2.3
	17
	3.1

	Stampede
	1800
	No Survey
	
	
	---
	---
	---
	---

	Teuchet Creek
	1640
	2/28/10
	10
	2.6
	22
	3.2
	23
	3.8

	Tok Junction       
	1650
	2/27/10
	20
	2.9
	18
	3.2
	19
	3.2

	Upper Chena Pillow
	2850
	2/28/10
	22
	3.1*
	37
	6.4
	30
	6.6

	Upper Wood River
	2990
	No Report
	
	
	---
	---
	27
	5.2


*Estimate
STREAMFLOW FORECASTS

	   FORECAST POINT
	FORECAST 

 PERIOD
	30- YR AVERAGE  (1000AF)
	50 

PERCENTILE
	% OF 

AVERAGE
	MAX

(kaf)
	MIN

(kaf)

	Tanana River at Fairbanks
	Apr- Jul
	7100
	6230
	88
	108
	79

	Little Chena River near Fairbanks
	Apr-Jul

	78

	
	
	
	

	Chena River near
Two Rivers
	Apr-Jul

	270
  
	179
	66
	128
	42

	Salcha River near Salchaket
	Apr- Jul
	  625
	460
	74
	112
	50

	Tanana River at Nenana
	Apr- Jul
	9000
	7420
	82
	101
	74


WATERSHED SNOWPACK ANALYSIS

	REGION / RIVER BASIN
	# COURSES AVERAGED
	PERCENT OF LAST YEAR
	PERCENT OF AVERAGE

	Chatanika
	4
	64
	55

	Chena Basin
	9
	55
	47

	Lower Tanana Valley
	5
	47
	37

	Mid Tanana Valley (Delta Junction)
	5
	68
	64

	Upper Tanana Valley (Tok)
	4
	77
	82


WESTERN INTERIOR BASINS(
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SNOWCOVER:

Koyukuk

Kuskokwim

Lower Yukon

Western Interior Basins
SNOWPACK DATA

	
	THIS YEAR
	LAST YEAR
	1971-2000 AVERAGE

	SNOW COURSE
	  ELEV.
	DATE
	SNOW

DEPTH
	WATER

CONTENT
	SNOW DEPTH
	WATER

CONTENT
	SNOW DEPTH
	WATER

CONTENT


Koyukuk

	Bettles Field 
	640
	3/01/10
	19
	2.5
	40
	7.8
	30
	6.1

	Bonanza Forks 
	1200
	2/25/10
	13
	2.0
	---
	---
	26
	5.1

	Cloverleaf
	170
	3/01/10
	21
	3.5
	45
	8.0
	---
	---

	Coldfoot    
	1040
	2/25/10
	16
	2.5
	45
	8.3
	30
	6.0

	Colville Bend
	170
	3/01/10
	15
	2.5
	45
	8.0
	---
	---

	Disaster Creek 
	1550
	2/26/10
	15
	1.8
	---
	---
	22
	3.6

	Huggins Creek
	290
	3/01/10
	10
	1.7
	57
	10.0
	---
	---

	JR Slough
	160
	3/01/10
	22
	3.5
	33
	5.7
	---
	---

	Kaldoyeit 
	750
	3/02/10
	12
	2.1
	27
	5.0
	---
	---

	Kanuti-Chalatna
	670
	3/02/10
	22
	3.0
	45
	7.8
	---
	---

	Kanuti-Kilolitna 
	550
	3/02/10
	6
	1.2
	31
	5.4
	---
	---

	Lake Todatonten
	550
	3/02/10
	15
	1.9
	49
	8.5
	27
	5.1

	Minnkokut        
	580
	3/03/10
	20
	2.8
	49
	8.5
	---
	---

	Nolitna
	560
	3/03/10
	15
	2.0
	40
	7.0
	---
	---

	Table Mountain  
	2200
	2/26/10
	11
	1.4
	---
	---
	23
	4.1

	Taiholman
	540
	3/02/10
	1
	0.2
	15
	2.5
	4
	1.3

	Treat Island
	190
	3/01/10
	6
	1.7
	---
	---
	---
	---


Kuskokwim 

	Holitna River
	257
	3/01/10
	24
	4.0
	---
	---
	---
	---

	Holokuk River
	367
	3/01/10
	7
	1.7
	---
	---
	---
	---

	Johnny Slu
	180
	No Report
	
	
	---
	---
	---
	---

	Kogruk
	493
	3/01/10
	33
	5.2
	---
	---
	---
	---

	Lake Minchumina  
	730
	No Survey
	
	
	23
	3.5
	21
	4.0

	Lower Aniak
	164
	No Report
	
	
	---
	---
	---
	---

	McGrath     
	340
	2/28/10
	10
	2.2*
	35
	7.9
	30
	5.7

	Middle Kuskokwim
	297
	No Report
	
	
	---
	---
	---
	---

	N. Fork Kuskokwim
	512
	3/03/10
	20
	4.0
	---
	---
	---
	---

	Purkeypile Mine 
	2025
	No Survey
	
	
	---
	---
	21
	4.2

	Telaquana Lake 
	1550
	3/04/10
	10
	1.6
	---
	---
	20
	4.0

	Upper Aniak
	781
	No Report
	
	
	---
	---
	
	

	Upper Twin Lakes 
	2000
	No Survey
	
	
	---
	---
	27
	7.0


Lower Yukon
	Deer Creek
	190
	3/01/10
	15
	2.6
	36
	6.2
	---
	---

	Grouch Creek
	220
	3/02/10
	31
	6.0
	57
	10.0
	40
	8.5

	Holikachuk   
	100
	3/02/10
	30
	6.1
	63
	11.0
	36
	7.8

	Horsefly Creek 
	180
	3/02/10
	34
	6.3
	43
	7.7
	28
	5.7

	Innoko Inn  
	200
	No Survey
	
	
	---
	---
	---
	---

	Little Mud River
	855
	3/01/10
	16
	2.5
	32
	5.5
	---
	---

	Lower Nowitna River
	205
	3/01/10
	18
	3.0
	36
	6.2
	---
	---

	Menotl Creek 
	380
	No Survey
	
	
	63
	11.0
	37
	8.2

	Middle Innoko 
	150
	3/02/10
	32
	5.9
	48
	8.5
	36
	7.4

	Nine Mile Island
	140
	3/01/10
	15
	2.3
	50
	8.8
	---
	---

	Pike Trap Lake
	130
	3/01/10
	7
	1.6
	24
	4.2
	---
	---

	Squirrel Creek
	150
	3/01/10
	21
	3.4
	45
	8.0
	---
	---

	Tozikaket
	600
	3/03/10
	10
	2.0
	---
	---
	23
	4.4

	Upper Innoko
	180
	3/02/10
	24
	4.5
	48
	8.5
	35
	7.8

	Wapoo Hills  
	220
	3/02/10
	33
	6.3
	63
	11.0
	32
	7.0

	Yankee Slough 
	100
	3/02/10
	39
	6.9
	48
	8.5
	41
	9.4

	Yetna River  
	120
	No Survey
	
	
	---
	---
	28
	5.9


STREAMFLOW FORECASTS

	   FORECAST POINT
	FORECAST 

 PERIOD
	30- YR AVERAGE  (1000AF)
	50 

PERCENTILE
	% OF 

AVERAGE
	MAX

(kaf)
	MIN

(kaf)

	Kuskokwim River at Crooked Creek
	Apr-Jul

	10500

	7980
	76
	120
	57


WATERSHED SNOWPACK ANALYSIS

	REGION / RIVER BASIN
	# COURSES AVERAGED
	PERCENT OF LAST YEAR
	PERCENT OF AVERAGE

	Koyukuk
	6
	28
	38

	Upper Kuskokwim
	2
	16
	40

	Lower Yukon
	9
	59
	85


ARCTIC AND KOTZEBUE SOUND(
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Snowcover:

Arctic


Kotzebue


Arctic and Kotzebue Sound

PRECIPITATION DATA


INCHES ACCUMULATED SINCE OCTOBER 1ST

	Precipitation

Gauge
	
	
	
	
	71-2000
	% of

	
	Elev.
	Date
	This Year
	Last Year
	Ave
	Average


Arctic

	Atigun Camp   
	3400
	2/28/10
	2.0
	3.0
	3.5
	57

	Atigun Pass 
	4800
	2/28/10
	3.7
	6.4
	7.1
	58

	Barrow 
	25
	No Report
	
	
	2.6
	

	Imnaviat Creek
	3050
	2/28/10
	2.4
	4.5
	3.4
	71

	Prudhoe Bay 
	30
	No Report
	
	
	3.4
	

	Sagwon
	1000
	No Report
	
	
	3.3
	


Kotzebue Sound

	Kivalina
	50
	2/28/10
	1.4
	---
	---
	---

	Red Dog**  

	950
	2/28/10
	2.2
	4.0
	5.6
	39


** Wyoming Shielded Gauge

STREAMFLOW FORECASTS

	   FORECAST POINT
	FORECAST 

 PERIOD
	30- YR AVERAGE  (1000AF)
	50 

PERCENTILE
	% OF 

AVERAGE
	MAX

(kaf)
	MIN

(kaf)

	Sagvanirktok River near
Pump Station 3
	Apr-Jul

	685

	570
	83
	137
	61

	Kuparuk River near Deadhorse
	Apr-Jul

	795

	605
	76
	117
	58


WATERSHED SNOWPACK ANALYSIS

	REGION / RIVER BASIN
	# COURSES AVERAGED
	PERCENT OF LAST YEAR
	PERCENT OF AVERAGE

	Arctic Coast
	No Report
	
	

	Dalton Highway
	3
	58
	58


NORTON SOUND/SOUTHWEST DELTA/BRISTOL BAY(
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Snowcover:
Norton Sound


Southwest Delta

Bristol Bay


Norton Sound / Southwest Delta / Bristol Bay

SNOWPACK DATA

	
	THIS YEAR
	LAST YEAR
	1971-2000 AVERAGE

	SNOW COURSE
	ELEV.
	DATE
	SNOW

DEPTH
	WATER

CONTENT
	SNOW DEPTH
	WATER

CONTENT
	SNOW DEPTH
	WATER

CONTENT


Bristol Bay 

	Brooks Camp 
	150
	3/04/10
	6
	1.0
	6
	1.5
	---
	---

	Fishtrap Lake
	1800
	No Survey
	
	
	---
	---
	40
	9.7

	Port Alsworth 
	270
	3/01/10
	2
	0.5
	22
	5.2
	15
	4.2

	Three Forks
	1300
	3/04/10
	7
	1.2
	12
	3.0
	---
	---

	Upper Twin Lakes
	2000
	No Survey
	
	
	---
	---
	27
	7.0


Norton Sound 

	Johnson’s Camp
	25
	2/28/10
	5
	1.0
	25
	4.5
	---
	---

	Pargon Creek
	100
	2/28/10
	10
	2.1*
	32
	6.1
	---
	---

	Rocky Point 
	500
	2/28/10
	12
	2.3*
	38
	7.0
	---
	---


PRECIPITATION DATA



INCHES ACCUMULATED SINCE OCTOBER 1ST

	Precipitation

Gauge
	
	
	
	
	71-2000
	% of

	
	Elevation
	Date
	This Year
	Last Year
	Ave
	Average

	Pargon Creek
	100
	2/28/10
	2.2
	6.0
	4.3
	51

	Rocky Point 
	500
	2/28/10
	3.4
	6.8
	4.8
	71
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COPPER BASIN(
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Snowcover:


Copper Basin

SNOWPACK DATA

	
	THIS YEAR
	LAST YEAR
	1971-2000 AVERAGE

	SNOW COURSE
	ELEV.
	   DATE
	SNOW

DEPTH
	WATER

CONTENT
	SNOW DEPTH
	WATER

CONTENT
	SNOW DEPTH
	WATER

CONTENT

	Chistochina 
	1950
	2/27/10
	20
	3.0
	25
	3.6
	22
	3.5

	Chokosna
	1550
	No Report
	
	
	16
	3.1
	---
	---

	Dadina Lake   
	2160
	No Report
	
	
	33
	6.0
	29
	5.1

	Fielding Lake
	3000
	2/27/10
	30
	5.8
	41
	9.6
	41
	10.2

	Haggard Creek
	2540
	2/27/10
	23
	3.9
	31
	5.8
	27
	5.6

	Horsepasture Pass 
	4300
	3/02/10
	21
	4.3
	21
	4.0
	28
	5.6

	Kenny Lake School 
	1300
	2/26/10
	18
	3.3
	13
	2.0
	18
	3.4

	Lake Louise   
	2400
	2/26/10
	18
	2.8
	25
	4.3
	22
	4.0

	Little Nelchina 
	2650
	2/26/10
	20
	3.6
	22
	4.0
	24
	4.6

	Long Glacier
	4820
	No Report
	
	
	---
	---
	---
	---

	May Creek
	1610
	2/28/10
	27
	3.4
	27
	5.6
	26
	4.4

	Mentasta Pass  
	2430
	2/27/10
	23
	4.3
	26
	4.2
	26
	5.8

	Monsoon Lake  
	3100
	3/02/10
	16
	2.2
	34
	5.9
	28
	5.6

	Notch
	2643
	No Report
	
	
	---
	---
	---
	---

	Paxson    
	2650
	2/27/09
	21
	3.4
	26
	7.4
	31
	6.6

	Sanford River 
	2280
	No Report
	
	
	28
	4.8
	28
	5.4

	St. Anne Lake 
	1990
	3/02/10
	20
	3.8
	22
	3.2
	25
	4.9

	Tazlina   
	1225
	2/26/10
	22
	3.7
	10
	2.0
	20
	3.7

	Tebay Lake
	1930
	No Report
	
	
	---
	---
	---
	---

	Tolsona Creek
	2000
	2/25/10
	20
	2.9
	21
	3.5
	22
	3.8

	Tsaina River
	1650
	2/26/10
	51
	12.7
	40
	11.9
	56
	15.7

	Twin Lakes 
	2400
	3/02/10
	25
	4.6
	23
	3.8
	31
	5.9

	Upper Tsaina River
	1750
	2/26/10
	64
	16.2
	47
	15.0
	64
	18.5

	Worthington Glacier
	2100
	2/26/10
	71
	21.8
	61
	20.5
	68
	21.6


*Estimate
PRECIPITATION DATA


INCHES ACCUMULATED SINCE OCTOBER 1ST

	Precipitation

Gauge
	
	
	
	
	71-2000
	% of

	
	Elev.
	Date
	This Year
	Last Year
	Ave
	Average

	May Creek
	1610
	2/28/10
	5.7
	6.9
	---
	---

	Strawberry Reef
	50
	2/28/10
	31.5
	35.7
	40.8
	77

	Upper Tsaina River   
	1750
	2/26/10
	14.5
	23.4
	23.4
	62


STREAMFLOW FORECASTS

	   FORECAST POINT
	FORECAST 

 PERIOD
	30- YR AVERAGE  (1000AF)
	50 

PERCENTILE
	% OF 

AVERAGE
	MAX

(kaf)
	MIN

(kaf)

	Gulkana River at Sourdough
	Apr- Jul
	475
	330
	69
	115
	45


WATERSHED SNOWPACK ANALYSIS

	REGION / RIVER BASIN
	# COURSES AVERAGED
	PERCENT OF LAST YEAR
	PERCENT OF AVERAGE

	Alaska Range**
	4
	58
	56

	Basin Floor
	6
	86
	78

	Chugach Range
	6
	111
	89

	Talkeetna Mountains
	3
	110
	81

	Wrangell Mountains
	1
	54
	73


**At the foot of the Alaska Range.

MATANUSKA - SUSITNA BASINS(
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Snowcover:


Matanuska - Susitna Basins

SNOWPACK DATA

	
	THIS YEAR
	LAST YEAR
	1971-2000 Average

	SNOW COURSE
	ELEV.
	DATE
	SNOW

DEPTH
	WATER

CONTENT
	SNOW DEPTH
	WATER

CONTENT
	SNOW DEPTH
	Water Content

	Alexander Lake 
	160
	3/01/10
	35
	9.0
	53
	12.5
	43
	10.7

	Archangel Road 
	2200
	3/03/10
	33
	8.1
	52
	12.9
	47
	13.5

	Bentalit Lodge
	150
	3/01/10
	31
	7.6
	41
	8.8
	35
	8.0

	Blueberry Hill 
	1200
	2/26/10
	32
	8.0
	57
	13.1
	53
	13.8

	Chelatna Lake  
	1450
	No Survey
	
	
	45
	10.0
	42
	10.0

	Clearwater Lake 
	2650
	3/02/10
	16
	2.4
	30
	4.8
	26
	5.1

	Curtis Lake
	2850
	3/02/10
	20
	3.5
	29
	5.0
	---
	---

	Denali View  
	700
	2/26/10
	30
	7.2
	50
	12.0
	46
	11.4

	Dunkle Hills
	2700
	No Survey
	
	
	39
	9.0
	---
	---

	Dutch Hills 
	3100
	No Survey
	
	
	96
	25.0
	76
	23.0

	E. Fork Chulitna
	1800
	2/26/10
	30
	6.6
	50
	11.5
	51
	12.7

	Eldridge Glacier
	3400
	No Survey
	
	
	---
	---
	---
	---

	Fishhook Basin  
	3300
	3/03/10
	33
	8.6
	68
	16.7
	58
	17.7

	Fog Lakes      
	2120
	3/02/10
	17
	2.3
	30
	4.0
	26
	5.3

	Halfway Slough
	350
	2/26/10
	20
	4.9
	34
	7.0
	---
	---

	Independence Mine 
	3550
	3/03/10
	40
	11.2
	75
	21.0
	58
	17.7

	Lake Louise       
	2400
	2/27/10
	18
	2.8
	25
	4.3
	22
	4.0

	Little Susitna 
	1700
	3/03/10
	31
	7.2
	42
	9.7
	42
	11.6

	Monahan Flat 
	2710
	2/28/10
	21
	3.6
	35
	6.0
	34
	7.4

	Moose Creek Ranch
	450
	2/27/10
	13
	2.5
	14
	2.4
	---
	---

	Nugget Bench 
	2010
	No Survey
	
	
	64
	14.7
	51
	12.9

	Ramsdyke Creek
	2220
	No Survey
	
	
	84
	20.6
	66
	18.9

	Sheep Mountain  
	2900
	2/27/10
	23
	4.8
	21
	3.6
	26
	5.4

	Skwentna       
	160
	3/01/10
	34
	8.9
	50
	11.3
	43
	10.5

	Square Lake   
	2950
	3/02/10
	18
	2.9
	23
	3.3
	22
	3.8

	Susitna Valley High
	375
	2/26/10
	27
	5.5
	40
	7.2
	39
	8.3

	Talkeetna    
	350
	2/26/10
	21
	4.5
	38
	8.5
	32
	7.6

	Tokositna Valley 
	850
	2/28/10
	36
	9.7
	53
	11.5
	67
	15.7

	Tyone River 
	2500
	No Survey
	
	
	26
	4.5
	23
	4.4

	Upper Oshetna River
	3150
	3/02/10
	19
	3.3
	21
	3.9
	---
	---

	Upper Sanona Creek
	3100
	3/02/10
	21
	3.6
	31
	5.5
	29
	5.2

	Willow Airstrip 
	200
	2/26/10
	24
	3.9
	27
	5.7
	30
	6.9


*Estimate
STREAMFLOW FORECASTS

	   FORECAST POINT
	FORECAST 

 PERIOD
	30- YR AVERAGE  (1000AF)
	50 

PERCENTILE
	% OF 

AVERAGE
	MAX

(kaf)
	MIN

(kaf)

	Little Susitna River near Palmer
	Arp-Jul

	86

	55
	64
	105
	44

	Talkeetna River near Talkeetna
	Apr-Jull
	1630

	1250
	77
	94
	59


PRECIPITATION DATA



INCHES ACCUMULATED SINCE OCTOBER 1ST

	Precipitation

Gauge
	
	
	
	
	71-2000
	% of

	
	Elevation
	Date
	This Year
	Last Year
	Ave
	Average

	Independence Mine
	3550
	2/28/10
	10.1
	15.1
	22.1
	46

	Monahan Flat
	2710
	2/28/10
	3.9
	5.7
	7.3
	53

	Susitna Valley High
	375
	2/28/10
	7.9
	10.5
	10.3
	77

	Tokositna Valley
	850
	2/28/10
	10.9
	19.6
	16.2
	67


WATERSHED SNOWPACK ANALYSIS

	REGION / RIVER BASIN
	# COURSES AVERAGED
	PERCENT OF LAST YEAR
	PERCENT OF AVERAGE

	Lower Susitna
	5
	70
	70

	Matanuska/Little Susitna
	7
	65
	59

	Peters Hills
	2
	70
	61

	Upper Susitna
	11
	65
	61


NORTHERN COOK INLET(
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Snowcover:

Northern Cook Inlet

SNOWPACK DATA


	
	THIS YEAR
	LAST YEAR
	1971-2000 AVERAGE

	SNOW COURSE
	ELEV.
	DATE
	SNOW

DEPTH
	WATER

CONTENT
	SNOW DEPTH
	WATER

CONTENT
	SNOW DEPTH
	WATER

CONTENT

	Anchorage Hillside 
	2080
	2/28/10
	36
	7.7
	37
	8.0
	35
	8.9

	Arctic Ski Bowl
	3000
	3/02/10
	26
	7.1
	21
	4.8
	38
	11.9

	Arctic Valley #1
	500
	3/02/10
	20
	4.1
	10
	1.5
	17
	3.9

	Arctic Valley #2
	1000
	3/02/10
	23
	3.9
	14
	2.7
	20
	4.6

	Arctic Valley #3
	1450
	3/02/10
	27
	7.2
	25
	5.6
	28
	6.9

	Arctic Valley #4
	2130
	3/02/10
	25
	5.9
	28
	5.6
	27
	6.9

	Chuitna Plateau
	1540
	No Survey
	
	
	84
	27.9
	68
	24.6

	Congahbuna Lake
	500
	3/01/10
	28
	7.2
	41
	10.1
	32
	8.9

	Granite Point
	250
	3/01/10
	11
	2.7
	---
	---
	22
	5.6

	Indian Pass   
	2350
	2/28/10
	52
	14.7
	75
	19.2
	64
	19.8

	Kincaid Park  
	250
	3/04/10
	17
	3.8
	13
	3.6
	17
	4.0

	Lone Ridge
	1675
	No Survey
	
	
	91
	30.5
	79
	28.8

	Moraine
	2100
	2/28/10
	34
	8.1
	25
	6.3
	27
	6.6

	Mt. Alyeska  
	1540
	2/28/10
	75
	23.6
	78
	22.2
	92
	29.7

	Point Mackenzie  
	200
	2/28/10
	16
	3.5
	23
	4.8
	19
	4.0

	Portage Valley 
	50
	3/02/10
	27
	10.0
	33
	10.9
	39
	12.9

	South Campbell Creek
	1200
	2/26/10
	31
	5.6
	12
	3.0
	26
	6.2


*Estimate
STREAMFLOW FORECASTS

	   FORECAST POINT
	FORECAST 

 PERIOD
	30- YR AVERAGE  (1000AF)
	50 

PERCENTILE
	% OF 

AVERAGE
	MAX

(kaf)
	MIN

(kaf)

	Ship Creek near Anchorage
	Apr- Jul
	58
	48
	83
	107
	59


PRECIPITATION DATA



INCHES ACCUMULATED SINCE OCTOBER 1ST
	Precipitation

Gauge
	
	
	
	
	71-2000
	% of

	
	Elevation
	Date
	This Year
	Last Year
	Ave
	Average

	Anchorage Hillside
	2080
	2/28/10
	11.1
	12.9
	11.6
	96

	Indian Pass  
	2350
	2/28/10
	18.1
	21.7
	21.1
	86

	Moraine
	2100
	2/28/10
	9.3
	9.0
	

8.5
	109

	Mt. Alyeska    
	1540
	2/28/10
	33.7
	29.6
	37.5
	90

	Point Mackenzie
	200
	2/28/10
	5.4
	8.4
	6.9
	78


*Estimate

WATERSHED SNOWPACK ANALYSIS

	REGION / RIVER BASIN
	# COURSES AVERAGED
	PERCENT OF LAST YEAR
	PERCENT OF AVERAGE

	Beluga
	2
	71
	68

	Campbell Creek
	3
	119
	88

	Ship Creek
	8
	111
	84

	Turnagain Arm
	3
	123
	90


KENAI PENINSULA(
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Snowcover:


Kenai Peninsula

SNOWPACK DATA

	
	THIS YEAR
	LAST YEAR
	1971-2000 AVERAGE

	SNOW COURSE
	ELEV.
	DATE
	SNOW

DEPTH
	WATER

CONTENT
	SNOW DEPTH
	WATER

CONTENT
	SNOW DEPTH
	WATER

CONTENT

	Anchor River Divide
	1650
	2/28/10
	35
	10.9
	28
	6.2
	40
	10.3

	Bertha Creek
	950
	2/26/10
	46
	14.3
	32
	9.7
	51
	14.7

	Bridge Creek 
	1300
	No Survey
	
	
	21
	4.6
	38
	10.2

	Cooper Lake   
	1200
	2/28/10
	40
	11.5
	25
	8.1
	50
	14.8

	Demonstration Forest 
	780
	No Survey
	
	
	20
	3.9
	28
	7.7

	Eagle Lake
	1400
	No Survey
	
	
	28
	6.5
	38
	10.7

	Grandview     
	1100
	2/28/10
	81
	26.0
	56
	17.6
	70
	21.7

	Grouse Creek Divide
	700
	2/28/10
	44
	12.5
	36
	9.5
	55
	16.7

	Jean Lake   
	620
	3/01/10
	14
	3.1
	4
	0.8
	17
	3.8

	Kachemak Creek
	1660
	2/28/10
	46
	15.6*
	24
	6.0
	48
	12.8

	Kenai Moose Pens    
	300
	2/28/10
	9
	1.7
	18
	3.7
	17
	3.8

	Kenai Summit
	1390
	2/26/10
	45
	13.8
	32
	8.2
	44
	12.3

	McNeil Canyon 
	1320
	2/28/10
	28
	9.5
	26
	6.3
	36
	8.9

	Moose Pass  
	700
	2/26/10
	15
	4.6
	12
	2.9
	22
	6.3

	Nuka Glacier 
	1250
	2/28/10
	75
	21.7*
	48
	12.6
	69
	26.9

	Port Graham  
	300
	2/28/10
	21
	5.8
	23
	6.8
	16
	4.9

	Snug Harbor Road 
	500
	3/01/10
	18
	5.3
	12
	3.0
	20
	5.1

	Summit Creek 
	1400
	2/28/10
	37
	10.2
	32
	6.4
	38
	10.5

	Turnagain Pass
	1880
	2/28/10
	98
	29.2
	71
	19.6
	92
	29.2


*Estimate
STREAMFLOW FORECASTS

	   FORECAST POINT
	FORECAST 

 PERIOD
	30- YR AVERAGE  (1000AF)
	50 

PERCENTILE
	% OF 

AVERAGE
	MAX

(kaf)
	MIN

(kaf)

	Kenai River at 
Cooper Landing
	Apr-Jul

	925

	885
	96
	112
	85


PRECIPITATION DATA 

            INCHES ACCUMULATED SINCE OCTOBER 1ST

	Precipitation

Gauge
	
	
	
	
	71-2000
	% of

	
	Elev.
	Date
	This Year
	Last Year
	Ave
	Average

	Anchor River Divide
	1650
	2/28/10
	13.1
	12.0
	16.1
	81

	Cooper Lake
	1200
	2/28/10
	20.8
	21.5
	20.7
	1.4

	Grandview 
	1100
	2/28/10
	35.5
	24.7
	31.4
	112

	Grouse Creek Divide 
	 700
	2/28/10
	34.4
	26.8
	30.6
	112

	Kachemak Creek
	1660
	2/28/10
	34.3
	23.0
	34.5
	99

	Kenai Moose Pens 
	 300
	2/28/10
	4.9
	7.3
	7.3
	67

	McNeil Canyon   
	1320      
	2/28/10
	10.7
	10.7
	13.6
	79

	Middle Fork Bradley**
	2300
	2/28/10
	25.6
	22.5
	30.6
	83

	Nuka Glacier**    
	1250
	2/28/10
	40.2
	24.7
	48.1
	84

	Port Graham
	300
	2/28/10
	38.4
	38.4
	35.1
	109

	Summit Creek      
	1400
	2/28/10
	14.3
	12.4
	14.3
	100

	Turnagain Pass    
	1880
	2/28/10
	35.0
	22.5
	34.0
	103


*Estimate
**Wyoming Shielded gauge


WATERSHED SNOWPACK ANALYSIS

	REGION / RIVER BASIN
	# COURSES AVERAGED
	PERCENT OF LAST YEAR
	PERCENT OF AVERAGE

	Bradley Lake/Southern Kenai
	3
	156
	89

	Ninilchik Dome
	2
	162
	105

	Northern Kenai Flats
	1
	46
	45

	Northern Kenai Mountains
	11
	153
	98


WESTERN GULF(
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Snowcover:


Western Gulf

SNOWPACK DATA

	
	THIS YEAR
	LAST YEAR
	1971-2000 AVERAGE

	SNOW COURSE
	ELEV.
	DATE
	SNOW

DEPTH
	WATER

CONTENT
	SNOW DEPTH
	WATER

CONTENT
	SNOW DEPTH
	WATER

CONTENT

	Exit Glacier 
	400
	2/27/10
	39
	12.9
	34
	9.4
	53
	13.7

	Grouse Creek Divide
	700
	2/28/10
	44
	12.5
	36
	9.5
	55
	16.7

	Lowe River  
	600
	2/26/10
	55
	14.9
	43
	12.5
	53
	15.1

	Mt. Eyak
	1405
	2/28/10
	61
	24.6
	65
	19.3
	67
	19.6

	Nuka Glacier  
	1250
	2/28/10
	75
	21.7*
	48
	12.6
	69
	26.9

	Sugarloaf Mountain 
	550
	2/25/10
	77
	23.2
	62
	18.8
	79
	23.3

	Tsaina River   
	1650
	2/26/10
	51
	12.7
	40
	11.9
	56
	15.7

	Upper Tsaina River
	1750
	2/26/10
	64
	16.2
	47
	15.0
	64
	18.5

	Valdez      
	50
	2/26/10
	46
	13.8
	51
	13.2
	51
	15.5

	Worthington Glacier
	2100
	2/26/10
	71
	21.8
	61
	20.5
	68
	21.6


*Estimate
PRECIPITATION DATA




INCHES ACCUMULATED SINCE OCTOBER 1ST

	Precipitation

Gauge
	
	
	
	
	71-2000
	% of

	
	Elev.
	Date
	This Year
	Last Year
	Ave
	Average

	Esther Island
	50
	2/28/10
	64.9
	67.7
	71.5
	91

	Grouse Creek Divide 
	700
	2/28/10
	34.4
	26.8
	30.6
	112

	Mt. Eyak
	1405
	2/28/10
	49.0
	50.4
	58.9
	83

	Nuka Glacier**  
	1250
	2/28/10
	38.2
	24.7
	48.1
	79

	Port San Juan
	50
	2/28/10
	69.6
	51.2
	66.0
	106

	Seal Island
	20
	2/28/10
	35.7
	31.1
	35.3
	101

	Strawberry Reef
	50
	2/28/10
	31.5
	35.7
	40.8
	77

	Sugarloaf Mountain
	550
	2/28/10
	30.6
	36.0
	35.5
	86

	Tatitlek
	50
	2/28/10
	34.1
	37.1
	33.6
	102

	Upper Tsaina River
	1750
	2/26/10
	14.5
	23.4
	23.4
	62


**Wyoming Shielded Gauge

*Estimate
WATERSHED SNOWPACK ANALYSIS

	REGION / RIVER BASIN
	# COURSES AVERAGED
	PERCENT OF LAST YEAR
	PERCENT OF AVERAGE

	Lowe River (Valdez)
	5
	117
	103

	Eyak Lake
	1
	127
	126


Southeast
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Snowcover:



SOUTHEAST
SNOWPACK DATA

	
	THIS YEAR
	LAST YEAR
	1971-2000 AVERAGE

	SNOW COURSE
	ELEV.
	DATE
	SNOW

DEPTH
	WATER

CONTENT
	SNOW DEPTH
	WATER

CONTENT
	SNOW DEPTH
	WATER

CONTENT

	Cropley Lake
	1650
	2/26/10
	53
	23.1
	98
	33.9
	70
	23.9

	Eagle Crest  
	1200
	2/26/10
	30
	12.1
	79
	23.0
	48
	16.1

	Fish Creek  
	500
	2/26/10
	0
	0.0
	32
	9.2
	20
	6.0

	Long Lake
	820
	2/28/10
	74
	26.7
	104
	38.1
	92
	34.1

	Moore Creek Bridge 
	2250
	2/27/10
	60
	19.0
	78
	23.5
	62
	21.3

	Petersburg Reservoir
	550
	3/01/10
	0
	0.0
	45
	13.6
	18
	5.8

	Petersburg Ridge
	1650
	3/01/10
	45
	18.6
	93
	28.3
	65
	21.8

	Speel River
	280
	2/28/10
	46
	17.0
	101
	39.8
	75
	26.8

	West Creek
	470
	3/01/10
	38
	9.6
	---
	---
	---
	---


STREAMFLOW FORECASTS

	   FORECAST POINT
	FORECAST 

 PERIOD
	30- YR AVERAGE  (1000AF)
	50 

PERCENTILE
	% OF 

AVERAGE
	MAX

(kaf)
	MIN

(kaf)

	Gold Creek near Juneau
	Apr-Jul


	33


	30
	91
	124
	70                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                         


PRECIPITATION DATA
INCHES ACCUMULATED SINCE OCTOBER 1ST

	Precipitation

Gauge
	
	
	
	
	71-2000
	% of

	
	Elev.
	Date
	This Year
	Last Year
	Ave
	Average

	Long Lake
	820
	2/28/10
	66.3                                                                                                                                                                                                       
	89.1
	85.9
	77

	Moore Creek Bridge
	2250
	2/27/10
	22.6
	21.9
	23.9
	95

	Snettisham   
	25
	2/28/10
	67.6
	116.0
	95.2
	71

	Swan Lake  
	50
	
	
	93.4
	77.8
	


WATERSHED SNOWPACK ANALYSIS

	REGION / RIVER BASIN
	# COURSES AVERAGED
	PERCENT OF LAST YEAR
	PERCENT OF AVERAGE

	Skagway
	1
	72
	80

	Douglas Island
	3
	53
	77

	Snettisham
	2
	56
	72

	Petersburg
	2
	44
	67


For further information contact:

NRCS Alaska web site:  www.ak.nrcs.usda.gov/snow/
Alaska Meteor Burst Communication System (AMBCS) web site:  www.ambcs.org
NRCS Anchorage Support Staff

510 L Street, Suite 270

Anchorage, Alaska  99501-1949

Telephone (907) 271-2424, Extension 113; 

Facsimile (907) 271-3951; or e-mail:  Richard.McClure@ak.usda.gov

Copper Center Field Office

Catherine Hadley, District Conservationist

Telephone:  (907) 822-4484  

Facsimile:  (907) 822-4489

e-mail: Catherine.Hadley@ak.usda.gov

Delta Junction Field Office

Catherine Hadley, District Conservationist

Telephone (907) 895-4241 x 103

Facsimile:  (907) 895-5003

e-mail: Catherine.Hadley@ak.usda.gov

Fairbanks Field Office

Joanne Kuykendall, District Conservationist

Telephone (907) 479-3159 x 110

Facsimile:  (907) 479-6998

e-mail:  Joanne.Kuykendall@ak.usda.gov

Homer Field Office

Mark Kinney, District Conservationist

Telephone (907) 235-8177 x 103

Facsimile:  (907) 235-2364

e-mail:  Mark.Kinney@ak.usda.gov

Mat-Su Field Office

District Conservationist, Keith Griswold
Telephone (907) 373-6492 x 101

Facsimile:  (907) 373-7192

e-mail: Keith.Griswold@ak.usda.gov
The large central basin varies from below normal in the eastern part to much below normal in the western part of the basin.  The Fort Yukon SNOTEL site has 12 inches of snow depth, same as last month.  The snow course at Fort Yukon located half mile away has 16 inches and 2.5 inches of water content, 78 percent of normal.  The SNOTEL site on the BLM/airport property is subject to wind.


The Coal Creek snow course in the Yukon Charlie National Park has 16 inches of snow depth with 2.4 inches of water content.  


The Forty Mile basin is 88 percent of average, exemplified by the Boundary snow course which is 87 percent of average.  


In Canada, the Porcupine River basin is 87 percent of normal with Old Crow snow course at 117 percent.  Eagle Plains and Eagle River are in the 70 to 80 percent of average range.


The Upper Nome Creek SNOTEL site has 15 inches of snow and an estimated 2.6 inches of water content, in the 50 percent of average range. 


The four White Mountains snow courses are 59 percent of average.











The west coast, Nome and Bethel and on the Beaufort Sea, Barrow received above normal precipitation for the month of February.  Less than normal was received at Bettles, 45 percent, Fairbanks, 70 percent and McGrath, 14 percent.  In South Central, the Moraine SNOTEL site received the greatest amount above normal for the month, it received 2.6 inches of precipitation with average being 1.3 inches.  The SNOTEL sites received above normal precipitation in the Northern Cook Inlet and the Kenai regions.


Southeast Alaska received much less than normal precipitation as indicated by the Snettisham Hydro-electric power plant receiving 4.9 inches, normal is 13.6 inches.











The temperatures were above normal across the state ranging generally from 5 to 10 degrees F greater than normal.  The one exception was Healy with a minus 1 deg F departure for the month of February.  On the other extreme was Eagle, which was 14 deg F above normal for the month.











North of the Alaska Range the snowpack varies to just below average near the Canadian border to minimum of records along the Dalton Highway south of the Brooks Range in the upper Koyukuk basin.


The large Central Yukon and Tanana basins vary from below normal in the eastern part to much below normal in the western part of the basin.  For the lower Tanana valley, French Creek is 37 percent of average, Bonanza Creek is 38 percent of average and the 5 snow courses summed in the lower basin are 37 percent of average.


Five snow courses in the upper Koyukuk basin have record low snow water contents.  Starting in the north is Table Mountain with 1.4 inches of snow water content, previous record low was 1.9 inches set in 1982.  Disaster Creek has 1.8 inches of water content with the previous low of 2.0 in 1979.  South and west of Bettles, Lake Todatonten has 1.9 inches of water content with the previous low being 2.2 in 1970.  On the Dalton Highway, the Bonanza Forks and Thirty Mile snow courses have had wild fires disturbing or removing the vegetation at the snow courses in 2004 and 2005 respectively.  Both of the water contents are lower than the previous record low set for both courses in 2007.


South of the Alaska Range, the Northern Kenai Mountains had a significant change in snowpack at lower elevations with the Moose Pass snow course going from 143% of average water content last month down to 73 percent of average this month, loosing 2.0 inches of water content due to rain and warm temperatures.  In contrast the Grandview SNOTEL site went from 94 percent of average to 120 percent of average, gaining 9.3 inches of water content, with most of the precipitation coming as snow.  The average water content for the 11 snow courses measured in the Northern Kenai Mountains is 98% of normal, up 3 percent from last month.


In Southeast, the two Petersburg snow courses have gone down to 67% of average water content from 94 percent last month.  The three Douglas Island snow courses are down to 77 percent of average from 110% of average water content last month.


























 The large Tanana basin is similar to the Central Yukon being below normal in the southeast to much, much below normal in the western portion of the basin.


In the upper Tanana basin, the Chisana SNOTEL site is reporting 94 percent of average water content and the Tok snow course measured 91 percent of average water content.  Beaver Creek snow course in the Yukon Territories is 72 percent of average.


For the Delta Junction area and south, the Fielding Lake snow course is 57 percent of average and Granite Creek is 84 percent of average.


For the lower Tanana valley, French Creek is 37 percent of average and Bonanza Creek is 38 percent of average.  The combined 5 snow courses in the lower basin are 37 percent of average.


The Chena basin is 47 percent of average and the Chatanika basin is 55 percent of average.












































The snow water contents in the south and east side of the basin are near average with Worthington Glacier near Thompson Pass at 100 percent of normal. The Upper Tsaina River SNOTEL site has 64 inches of snow depth with 16.2 inches of water content, 88 percent of normal.   The Kenny Lake snow course is average with 14 inches of snow depth and 3.3 inches of water content.


The Basin Floor average of 6 snow courses is 78 percent ranging from 95 percent of average at Tazlina to 78 percent of average at Haggard Creek and Lake Louise.  The Chugach Range is 89 percent of average, while the Alaska Range dropped 2 percent from last month and is 56 percent of normal with the snow course Fielding Lake at 57 percent of normal.  To the west, the Talkeetna Mountains are 81 percent of normal water content.


No report from the Wrangell Mountain snow courses.


The Gulkana River at Sourdough expected volume flow for the April through July time period is 330,000 acre-feet, 69 percent of average.











The Northern Cook Inlet region varies from 48 percent of average at Granite Point, near Tyonek, to 123 percent of average at Moraine.  The Moraine SNOTEL site, in the Eklutna watershed, has 34 inches of snow depth with 8.1 inches of water content.  The Granite Point snow course has 11 inches of snow depth with 2.7 inches of water content.


For the SNOTEL sites in the Anchorage area; Indian Pass is 74 percent of average with 52 inches of snow and 14.7 inches of water content, Anchorage Hillside is 87 percent of average reporting 36 inches of snow with 7.7 inches of water content and Mt. Alyeska has 75 inches of snow and 23.6 inches of water content, which is 79% of average.


For the west side of Cook Inlet, the aerial markers Chuitna Plateau and Lone Ridge were not read due to bad weather.  The Congahbuna Lake snow course has 28 inches of snow depth with 7.2 inches of water content, 81 percent of average.


The Snowmelt Runoff Index for the Campbell Creek near Spenard is -1.6, below average.
































The Aniak SCAN site, which is located at the Aniak Farm, has 7 inches of snow depth, it was down from 8 inches last month.  This is probably in the 50 percent of normal range.  Bethel has received a normal amount of precipitation in February to continue its above average trend for the year.


























The Imnaviat Creek SNOTEL site has recorded 2.4 inches of precipitation this water year which is 58% of average.  The Atigun Pass SNOTEL site has received 3.7 inches of precipitation since October 1st or 52 percent of average.  It has 22 inches of snow on the ground.











The Red Dog mine precipitation gauge received 2.2 inches of precipitation since October 1st, 39% of normal.  











The Rocky Point SNOTEL site has 12 inches of snow on the ground and an estimated 2.3 inches of water content. The Johnson Camp SNOTEL site, in the “blow hole” at Solomon, 30 miles east of Nome, has 5 inches of snow on the ground as of March 1st, last year there was 25 inches of snow depth.











This area appears to have very little snow with 6 inches recorded at Brooks Camp, where there was only a skiff last month.   The Three Forks aerial marker measured 7 inches of snow, while last month the depth at Three Forks was 2 inches.  














The Northern Kenai Mountains had a significant change in snowpack at lower elevations with the Moose Pass snow course going from 143% of average water content last month down to 73 percent of average this month, loosing 2.0 inches of water content due to rain and warm temperatures.  In contrast the Grandview SNOTEL site went from 94 percent of average to 120 percent of average, gaining 9.3 inches of water content, with most of the precipitation coming as snow.  The average water content for the 11 snow courses measured in the Northern Kenai Mountains is 98% of normal, up 3 percent from last month.


Northeast of Homer, the Anchor River Divide SNOTEL site reported 35 inches of snow depth with 10.9 inches of water content, and is 105% of average.


Across Kachemak Bay from Homer, Port Graham SNOTEL site has 21 inches of snow with 5.8 inches of snow water content, and is 118% of average.


The Nuka Glacier SNOTEL site has 75 inches of snow depth with an estimated 21.7 inches of water content, up 10 inches of water content from last month, and currently is 81% of average. The site has recorded 40.2 inches of accumulated precipitation since October 1st, which is only 84% of average.


The expected volume flow from snowmelt runoff for the Kenai River at Cooper Landing for the April through July time frame is 885,000 acre-ft, 96 percent of average.














The SNOTEL site at Mt. Eyak is above average, reporting 61 inches of snow depth and 24.6 inches of snow water content.


Sugarloaf Mountain SNOTEL site, perched above the Solomon Gulch Hydroelectric and the town of Valdez at 550 ft of elevation, reported 77 inches of snow depth and an estimated 23.2  inches of water content, 100% of average.  The precipitation gauge has caught 30.6 inches since October 1st, which is 86% of average.


The Esther Island precipitation gauge has caught 64.9 inches of precipitation since October 1st 91% of average with 16.7 inches being caught in the month of February.


The Strawberry Reef SNOTEL site, located east of Cordova, is 77% of average and has caught 31.5 inches of water since October 1st.














The Susitna Basin snow courses range from below average to well below average.  The 11 snow courses in the Upper Susitna Basin are below average at 62 percent. Snow water contents range from 43 percent of average at the Fog Lakes snow course to 85 percent of average at the Upper Oshetna River snow course.


For the Lower Susitna snow courses, the west side of the basin is below average as indicated by Alexander Lake which measured 9.0 inches of snow water content, 84 percent of average. The east side of the basin along the Parks Highway is well below average with the SNOTEL site at Susitna Valley High reporting 5.5 inches of water content, only 66 percent of average.


The Denali View snow course, at Mile 131 of the Parks Highway, is 63 percent of average.


The Hatcher Pass snow courses vary from 49 percent of average at the Fishhook Basin snow course to 62% of average at the Little Susitna snow course.


The Sheep Mountain snow course water content is 4.8 inches, 89 percent of average.


The Snowmelt Runoff Index for the Deshka River at mouth near Willow is -2.4, much below average.
































The snow courses vary from 127 percent of average in the Yukon basin above Whitehorse/Teslin to 63 percent of average in the Stewart/Pelly basin.   There are two snow courses at 127 percent of average, Williams Creek and Mt. McIntyre B, and as a whole the basin above Whitehorse/Teslin is 107 percent of average.  The low snow course is Pelly Farm located in the Stewart/Pelly basin. The Stewart/Pelly basin is 79 percent of average.  The Dawson basin is 74 percent of normal and the Whiter River basin is 101 percent of normal.


The expected volume flow from snowmelt runoff for the Yukon River at Eagle for the April through July time frame is 30,600,000 acre-ft, 89 percent of average.
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The Lake Minchumina and Purkeypile Mine snow courses were not measured this month, but it is suspected both sites received very little snow.  The Telaquana Lake snow course was measured after the a snow storm dropped 3 to 4 inches of new snow, it has 10 inches of snow depth with 1.7 inches of snow water content, 42 percent of average. 








The snow courses in the Innoko Wildlife Refuge range from 67 percent at Upper Innoko snow course to 112 percent of normal at Horsefly Creek.  Most are in the 80 to 90 percent of normal range.  To the north the Tozikaket snow course is 45 percent of average with 2.0 inches of snow water content, 2nd lowest on record with 1.5 inches being measured in 2003.

















Five snow courses in the upper Koyukuk basin have record low snow water contents.  Starting in the north is Table Mountain with 1.4 inches of snow water content, previous record low was 1.9 inches set in 1982.  Disaster Creek has 1.8 inches of water content with the previous low of 2.0 in 1979.  South and west of Bettles, Lake Todatonten has 1.9 inches of water content, the previous low was 2.2 in 1970.  On the Dalton Highway, the Bonanza Forks and Thirty Mile snow courses have had wild fires disturbing or removing the vegetation at the snow courses in 2004 and 2005 respectively.  Both of the water contents are lower than the previous record low set for both courses in 2007.


Near Galena, the Colville Bend snow course has 15 inches of snow depth, last year there was 45 inches.  This is similar ratio for the snow courses in the lower Koyukuk and Yukon area near Galena.


























Southeast Alaska is having a below average snow pack year after three big snow years in a row (2007, 2008, 2009). 


The Long Lake SNOTEL site is reporting 74 inches of snow and 26.7 inches of water content, which is 78% of average. 


The two Petersburg snow courses have gone down to 67% of average water content from 94 percent last month.


The three Douglas Island snow courses are down to 77 percent of average from 110% of average water content last month.


The Moore Creek Bridge snow course, north of Skagway, has 60 inches of snow depth with 17.0 inches of water content, 80 percent of average.  The precipitation received at Moore Creek since October 1st is 22.6 inches, 95 percent of average.

















( See regional summaries for the forecast period and the actual forecasted flow volumes.





( For further information contact the Natural Resources Conservation Service in Anchorage.


( For further information contact the Natural Resources Conservation Service in Fairbanks.


( For further information contact the Natural Resources Conservation Service in Fairbanks or Delta Junction.


( For further information contact the Natural Resources Conservation Service in Anchorage.


( For further information contact the Natural Resources Conservation Service in Anchorage.


( For further information contact the Natural Resources Conservation Service in Anchorage.


( For more information contact the Natural Resources Conservation Service in Copper Center, Delta Junction or Anchorage. 





( For more information contact the Natural Resources Conservation Service in Wasilla.





( For more information contact the Natural Resources Conservation Service in Wasilla or Anchorage.


( For more information contact the Natural Resources Conservation Service in Homer.


( For more information contact the Natural Resources Conservation Service in Copper Center.
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